## ASZ80 Assembler

####

    .hd64 DIRECTIVE

    Format:

            .hd64

    The  .hd64  directive enables processing of the HD64180 specific
    mnemonics not included in  the  Z80  instruction  set.   HD64180
    mnemonics  encountered  without  the  .hd64  directive  will  be
    flagged with an 'o' error.

    Z80 REGISTER SET AND CONDITIONS

       The following is a complete list of register designations and
    condition mnemonics:

            byte registers  -       a,b,c,d,e,h,l,i,r
            register pairs  -       af,af',bc,de,hl
            word registers  -       pc,sp,ix,iy

            C -     carry bit set
            M -     sign bit set
            NC -    carry bit clear
            NZ -    zero bit clear
            P -     sign bit clear
            PE -    parity even
            PO -    parity odd
            Z -     zero bit set

    L.3  Z80 INSTRUCTION SET

      The following list specifies the format for each addressing
    mode supported by ASZ80:

            #data           immediate data
                            byte or word data

            n               byte value

            rg              a byte register
                            a,b,c,d,e,h,l

            rp              a register pair
                            bc,de,hl

            (hl)            implied addressing or
                            register indirect addressing

            (label)         direct addressing

            offset(ix)      indexed addressing with
                            an offset

            label           call/jmp/jr label

    The  terms  data,  dir,  offset, and ext may all be expressions.
    The terms dir and offset are not allowed to be  external  refer-
    ences.

       Note  that  not all addressing modes are valid with every in-
    struction, refer to the Z80/HD64180  technical  data  for  valid
    modes.

       The  following  tables  list all Z80/HD64180 mnemonics recog-
    nized by the ASZ80 assembler.  The designation []  refers  to  a
    required addressing mode argument.

    Inherent Instructions

            ccf             cpd
            cpdr            cpi
            cpir            cpl
            daa             di
            ei              exx
            halt            neg
            nop             reti
            retn            rla
            rlca            rld
            rra             rrca
            rrd             scf

    Implicit Operand Instructions

            adc     a,[]            adc     []
            add     a,[]            add     []
            and     a,[]            and     []
            cp      a,[]            cp      []
            dec     a,[]            dec     []
            inc     a,[]            inc     []
            or      a,[]            or      []
            rl      a,[]            rl      []
            rlc     a,[]            rlc     []
            rr      a,[]            rr      []
            rrc     a,[]            rrc     []
            sbc     a,[]            sbc     []
            sla     a,[]            sla     []
            sra     a,[]            sra     []
            srl     a,[]            srl     []
            sub     a,[]            sub     []
            xor     a,[]            xor     []

    Load Instruction

            ld      rg,[]           ld      [],rg
            ld      (bc),a          ld      a,(bc)
            ld      (de),a          ld      a,(de)
            ld      (label),a       ld      a,(label)
            ld      (label),rp      ld      rp,(label)
            ld      i,a             ld      r,a
            ld      a,i             ld      a,r
            ld      sp,hl           ld      sp,ix
            ld      sp,iy           ld      rp,#data

            ldd                     lddr
            ldi                     ldir

    Call/Return Instructions

            call    C,label         ret     C
            call    M,label         ret     M
            call    NC,label        ret     NC
            call    NZ,label        ret     NZ
            call    P,label         ret     P
            call    PE,label        ret     PE
            call    PO,label        ret     PO
            call    Z,label         ret     Z
            call    label           ret

    Jump and Jump to Subroutine Instructions

            jp      C,label         jp      M,label
            jp      NC,label        jp      NZ,label
            jp      P,label         jp      PE,label
            jp      PO,label        jp      Z,label

            jp      (hl)            jp      (ix)
            jp      (iy)            jp      label

            djnz    label

            jr      C,label         jr      NC,label
            jr      NZ,label        jr      Z,label
            jr      label

    Bit Manipulation Instructions

            bit     n,[]
            res     n,[]
            set     n,[]

    Interrupt Mode and Reset Instructions

            im      n
            im      n
            im      n
            rst     n

    Input and Output Instructions

            in      a,(n)           in      rg,(c)
            ind                     indr
            ini                     inir

            out     (n),a           out     (c),rg
            outd                    otdr
            outi                    otir

    Register Pair Instructions

            add     hl,rp           add     ix,rp
            add     iy,rp

            adc     hl,rp           sbc     hl,rp

            ex      (sp),hl         ex      (sp),ix
            ex      (sp),iy
            ex      de,hl
            ex      af,af'

            push    rp              pop     rp

    HD64180 Specific Instructions

            in0     rg,(n)
            out0    (n),rg

            otdm                    otdmr
            otim                    otimr

            mlt     bc              mlt     de
            mlt     hl              mlt     sp

            slp

            tst     a
            tstio   #data

##### Go to the Documentation Index

####

... Exit the ASxxxx Documentation

... Home Page