Note:
This package may only be used in conjunction with Caldera DR-DOS 7.03. 
You may not use any of these files in a commercial product without 
first obtaining a license from Caldera Thin Clients Inc.

Installation:
The configuration files, located in the SAMPLE directory, are 
pre-configured for a typical installation of DR-DOS 7.03 with networking. 
Just copy the files in the BIN directory into directory c:\nwclient, 
using an "xcopy /s" command.

The Toolkit contains the sample source code and libraries needed to 
develop to the Caldera TCP/IP stack.

Documentation is found in the DOC directory and includes the following
online documentation:
TCP/IP DOS Socket Library Reference
TCP/IP DOS Utilities
TCP/IP Transport for DOS

The NE2000.COM ODI driver is set as default. You will probably need 
to replace it with the ODI driver for your card. First, edit your startnet.bat
file and enter your ODI driver. Next, edit the NET.CFG file and enter 
the Link Driver section for your ODI driver and change the binding in 
the Protocol TCPIP section. Finaly, enter appropriate IP numbers in the 
PROTOCOL TCPIP section and edit \TCP\RESOLV.CFG and enter your DNS information.  

Run startnet to load tcpip.
