## General Specifications : CineMaster DVD Playback Card

[ Table of Contents ] [ Getting Started ] [ Supported Feature Set ]

### General Specifications

- PCI 2.1 compliant bus master, 32-bit host interface
- Intel/Microsoft Plug-and-Play compliant

External Board Connectors

> Video

- S-Video analog output: 4-pin Mini-DIN Composite video
- Analog output: RCA-style phono jack / Cinch (European)

> Audio

- Analog audio output: 1/8 in. stereo mini phono jack
- S/PDIF digital: RCA-style phono audio jack, line level output

> Audio Output Formats

- Dolby Digital - AC-3 S/PDIF
- Dolby Surround - 2 channel digital audio downmixed from 5.1 channel AC-3
- Linear PCM - all modes down sampled to 48 kHz, 16-bit

Internal Board Connections

- Analog audio output: MPC-3 connector; to sound card analog audio input
- Video Port Support: AMC

Table of Contents