*********** USING  THE ATI FLASH UTILITY ***********
ATI FLASH works fine with both .BIN and .ROM files



MAKE A BOOTABLE FLOPPY DISC:


The drdflash.exe program will help you make a bootable floppy disc.

Once made, extract and copy ALL the files in the "ATI_FLASH" folder onto the boot-floppy.

Then, copy the BIOS(ez) that you wish to "flash" onto the boot-floppy, as well.



*****************************************************************************************************************



FLASH YOUR CARD:


1)  Insert the boot-disc into your floppy drive, and reboot your computer from your floppy drive.


2)  If you type "atiflash" (enter) at the A:\ prompt, you'll be shown a list of all of the possible BIOS'z that are available.


3)  Use this command to make a copy of your original BIOS at the A:\ prompt:
 
           atiflash -s 0 originalBIOS.bin (enter)    <<<<<<<< that's a ZERO before the originalBIOS


4)  Use this command to flash your BIOS with the appropriate file at the A:\ prompt:
   
           atiflash -f -p 0 BIOSname.bin (enter)    <<<<<<<< that's a ZERO before the BIOSname






THAT'S IT!!!!!!!!!!!!!!!!!!!

ENJOY!!!!!!!!!!!!!!

HAVE FUN!!!!!!!!!!!!!!!!!!!!!!


schiz
04/22/2003

