v1.6 |
siGGis H.a.R ware © M.Harašta |
Brief description: siGGis Monitor program is made for vector file *.sig (format siGGis) shapefile *.shp (format ESRI - ArcView).You can create own vector layers (e.g.: digitize imported orthofotomap - JPEG format, edit databases new layers) save they into *.sig , *.dbf (DBase III) files change the following properties for polygonal,line, point and text graphics: foreground fill and color, outLine, text, font, size, style . You can join a table to the active table based on the values of a common field found in both tables. You can open a html document on active geoObject. You can export a view to a graphics file (output formats: *.wmf, *.emf ) ASCII files (coordinate files of points) import orthofotomap - format JPEG. Attend to configuration applet's siGGis Applet and siGGis Event ( internet/ intranet - don't require any action from server, don't need JDBC/ODBC interface. You can save your work to a projectFile ( *.hgf ) with a different name. With this program it is possible to join other programs or systems ( INI type file ) and monitor events (change properties of geoObjects by mean of ASCI event file:e.g. secure of objects , flood monitor, GPS ... ). It is possible to save individual events into graphics files(*.wmf, *.emf) Properties: Viewer for Windows 9x, 2000, NT.., needs internet browser ( e.g.: MSIE 5 .x ). Hardware: 1 MB free space on HD without data files. Easy instalation: "unpack and run... :-)". Don't need Database, JDBC/ODBC interface - (dbf III... dbf V..., don't support memo,blob items..), without index files - have own simple database engine. Restriction: Don't attent to robust geoLayers ( more 10 MB). |
Description of the program: Main panel |
Contains basic features used to manipulate the geoObject layers. The File menu offers these services:: Add… - adds the selected layer in the *.shp, *.sig format (if a layer database file exists, it is loaded) and *.jpg as background - orthoFotoMap. Delete … - removes the current layer from the memory. The current layer can be selected either by clicking a geoObject in the map or by selecting the layer in Select layer service. Open … - erases all open layers from the memory and loads a newly selected *.shp, *.sig layer. Save … (*.siGGis) - saves the currently opened layer to the internal *.sig format. Open project - erases all layers from the memory and loads the selected GeoProject (static - *.hgf, dynamic - *.hge, applet config file). Save *.hgf,*.hge - saves the current state of the project under construction to the project file. Copy map to clipboard - saves the current map range to the clipboard in a vector format that can be printed in your favorite editor. Export map (metafile) - saves the current map range to a *.wmf *.emf vector format file for use in any graphics program. Import layer from ASCII - load new layer from import file. Export layer to ASCII - save layer (*.shp, *.sig ) to ASCII file (.. modifying and back import ). First row of Main panel enables basic manipulation with the map: Enlarge the map window content (it’s possible to use the mouse - click and drag) Reduce the size of map window Set the original size Second row enables project description with predefined dates: State of the first button - description Label info : if the geoObject description is defined double-click on the left button in the map will show the objects characterization State of the first button - description Label draw : if the GeoObject description is defined clicking of the left mouse button will write down information about that geoObject in to a map on a current position according to a defined description entry in a database. Right mouse button click on a described geoObject will erase information about it. Holding down the Shift key together with right mouse button edits the description: State of the first button - Label hide : hides all existing geoObjects descriptions Clear button - deletes all existing descriptions from the map. |
Switches on the Main panel : |
Window with the map - shows or hides the current map window. Map Window - import *.jpg file, digitize new layers, mapextent Top button in mapWindow:(needs install TrueType font Webdings) show / hide buttons for import/edit coordinate Images, Digitize, mapExtent modification (horizontal buttons), zooming,set layers,select geoObjests,draw labels,open/save GISprojects (horizontal buttons). Import JPEG file: Service: Menu - Add... - select JPEG image type - open file *.jpg Button: [Image] - select and open *.jpg file, only when is not imported otherwise is switched for modification bounds (move,resize) by means of mouse. If is imported JPEG file into GIS project, imageExtent is same as extent of layers otherwise is in interval: 0,10 (left,top) - 10,0 (right,bottom). Position and resize image: In mapWindow - button [Image] - up / off modification size(position) by means of mouse. DoubleClick (mouse) in bounds - set change and open window for detail modification (edit coordinate imageExtent). Digitize: MapWindow - button [Digitize] - up / off drawing in map to Import new layer. Show / Hide(not clear) window for digitize and off / up zooming. When is not empty digitizeWindow drawing (black objects) is permanent, zooming, reset map not clear it. If is selected type Line,Polygon - right button click(mouse) ended drawing current geoObject ( polygon is closed - last,first point is equal ) and allowed to make new geoObject. All coordinate new geoObjects are saved in digitizeWindow - ASCII format. DoubleClick on selected row showed current point (blink) and allows window coordinate for detail edit (soft move XY by distance, add/delete point). Button [Save as *.txt] saved content window in ASCII file. Button [Now Layer] added new geoObjects in new *.sig,*.dbf files. New layer is added in GIS project automatically . Button [Add to Layer] saved new geoObjects in selected layer. Before saving it is possible edit databaze (add, modify, delete fields). Button [Bounds] allows change mapExtent (all layers) - move GISproject in new coordinate. Database - shows/hides - window containing geoObject information of the selected layer Information about the current active geoObject: Mode full table - position of the actual geoObject in the attached database. Database can be sorted by any entry - double-click on any column.(e.g.: LABEL) Column width can be changed by before printed by dragging the border line in the column description field Description of Database window’s buttons: Set table: - Opens a window that allows to set attributes of the gird (hide unwanted items, change order of entries, change entry’s titles and connect any *.dbf files using the join entry). Order Change - drag the desired entry in the first column up or down Title Change - double-click in the second column activate the edit mode Hide/show - double-click in the third column Addition to a database : Classic way: open the database with the Open database button and choose the connection entries (main dBase - connect dBase). You can connect up to 1024 entries (memory limits) Define the action (e.g. : open html file with detail geoObject description, following reference to additional information) for double-click on a left mouse button in a database table on a description of a geoObject - dblClick - def button. …. selectData - assist to choose the database entry that will contain data for parameter generation according to database. When is fileType asociated with any program, textField (path and exeName of program) can be empty. Example : geoObject is described in the document on an address (HD) : http://city.geo.cz/lay_123/object_xx3457.html , selected entry of current database of geoObjects can contain : complete path to the document: http://city.geo.cz/lay_123/object_xx3457.html is in database field (...selectData), 2. and 4. window’s content is empty part of the path lay_123/object34567 and the rest is defined trough the 2. and 4. edit window complete path to the document http://city.geo.cz/lay_123/object_xx3457.html contains 2. edit window, entry of the database is not selected 4. window is empty ….. Confirm all changes by pressing Ok button Print the table : Print window enables to choose the font, header, and printer setting for the current database printing. Find Objects - opens dialog window for keys to find the geoObjects in the layers by the value of entered text. Finding of geoObjects can be more specified by selecting of the particular layer or by selecting particular dBase entry. Switch equal - will find the geoObjects if they contain the exact some text as entered. Switch within - will find any geoObjects that contains somewhere in description the entered string. DblClick in List - show selected geoObject Button Show all will show all corresponding geoObjects and show them in map window Make project - objects selection - enables to define GEOProjects: set of geoObjects in particular layers according to values in databases. Colors can be changed for individual geoObjects sets. The GeoProject will include defined selection only. Object selection will be preformed according to chosen database entries that corresponds with the Operator description:= equal to value ,<> unequal to,> bigger then,< less then,in value is in range of border values (including) the only allowable format : x..y entered manually to the window for limitation,geoObject color in (according to….) if the selected layer is original the goeObjects will be colored in according to default definition (set layers). If the set color value is active the color of the geoObject can be selected: If the window for selecting the entry (SES_ID) stays clear then for polygons Red ( RGB 255:0:0 ) determinates the color of the outlines and Yelow the color of the filling. For the line Yelow has no meaning and the color of the line is determinated by Red. By selecting the SES_ID entry form the database, Red determinates the color of geoObject with lowest value of SES_ID and Yellow is the color of geoObject with the highest SES_ID value. Mixed color (RedYelow) will be given to other geoObject corresponding with ratio of SES_ID. Next select: - biding of following selection : value determinates logical biding between definitions. OR means also. AND means that the selected object has to corresponds with both conditions. BLANK represents no logical value e.g.: Definition: x > 5 and x <> 8 select into group this values: 1,2,3,4,5,6,7,8,9,10,11.. Definition actualization : Select by double-clicking on the definition in the table (load the values). Change the attributes ... Apply the actualization y pressing the update line button Update/edit database table (out siGGis Monitor): drop layer from current geoProject update/edit database table of drop layer add layer into current geoProject save current geoProject Set layers: Tip: service Fill color and OutLine color. You can write your color in service's textField ( RGB model (e.g.: 218:118:218 ) - separator is :) Option enables to change the geoObject attributes in selected layers. The color, style, size (for points) of geoObject can be set. Define entry and font for geoObject’s description (any database entry can be used as a description) If the current layer is a layer of polygons or lines then type can be changed by clicking the mouse on the layer. Warning : that service works without any problems in the Polygon to line direction in the reversed direction just in case that lines creates a closed polygon. If lines doesn’t represent a polygon the result may be unpredictable. If the lines forms a polygon the filling of this polygon can be changed. The service can be used in case of : when a less important layer shields more important ones. Then the conversion allows to change the style of the outline and also disable the identification for that layer when clicked on with the mouse. Of the lines forms the polygon the polygon can have colorful filling and can have the identification attribute when clicked on that geoObject. Legend : shows/hides the window containing information about loaded layers. Offers to show and hide a layer or to change order of layers. right mouse button - edit the legend of current layer Double-click on the text switches on/off the layer Change the order : click on the icon and drag up or down Current project - show / hide window: The project file is assigned complete save of all information about the semi-finished state. It has sense just when using the Project Selection service. Add selection button offers a window for the project’s title definition and prepares it for save in to *.hgf. Actualize button enable to change the name of loaded *.hgf file. Any project can be described in a memoPanel. Project List - shows/hides the list of defined project in siGGis.INI file. Section : [Project] Count - number of projects if > 0 window containing list of defined projects will automatically open if the program was launched without any parameters. As parameters names of files (*.shp, *.hgf, *.hge) can be used. pth_x - path to the x th project prj_x - name of the x th project When the program finds a project with a path pth_x it will search the place determinates in [Path] section - pth_x - project. If the search fails it searches in the Program_siggis\data\project directory (if exists). Correspondingly works for *.shp, *.dbf files defined in individual projects. |
Menu - Options |
Language service switches between languages for program and applets (define in siGGis.INI file, section [language]). By selecting the Default service (F12) the implicit languages English and Czech are going to be prepared for default saving into siGGis.INI file. Service Properties: The whole section of all general attributes of Default F12 service can be switched off in the menu by the noConfig = 1 entry in [General] section, and turned on (enabled) by value noConfig = 0 (siGGis.INI). Save when finished if the Update INI file service is selected, the current setting of all attributes is going to be saved. Entry path to… determinates where will the program search for .shp and .dbf files that are defined in .hgf file if the program won’t find them. If it won’t find them even in those places it will search the directory of the program siGGis and it’s subdirectories ..\data\Project ( *.hgf) , .. \data\Vector\vector (*.shp,*.dbf) a ..\data\Table (other files *.dbf for connection), if existing. Redefine keyboard (HelpKey) for help : Service will define actions (launch help program describing e.g. projects, supportive database etc.). If the entry is defined the service can be reached in file menu of the program. [Czech Language] Service has sense just for Czech GIS it determinates what code page will be used to display text from database files. [Events setting] service is designed as a interface between program siGGis and other programs or systems. Using this service you can use the program as a monitor for watching changes of geoObjects outside siGGis EventFile path - file of events : determinates where will the program search for file for defined changes. If this field is empty the implicit directory of the program : data\Events\ will be searched. Export in applet: EventFile path determine location owing to appletURL: E.g.: appletURL : http://www.aaaa.bbb/ccccc/my-applet.html Address for x event.mon files: http://www.aaaa.bbb/ccccc/Data/Events/ EventFile path: Data/Events/ EventFile name : name of the file of events that will be used when activated (*.*) . EventFile generator: It is allowed to prepare - save mask eventFile. Offers complet list of eventCommands. Path (destination): path to save eventFiles Source file:determined for prepare eventFiles by content of sourceFile. service is determined for multiProcess one row represents one eventFile commands are separated (Separator define) button [Generate] saves files on HD. E.g.: from row [Static]#eventCount=1 #eLayer1=1 #eObject1=0 #eMoveXY1= 9,27947598253275|7,77838427947598|# is generated eventFile(content): [Static] eventCount=1 eLayer1=1 eObject1=0 eMoveXY1=9,27947598253275|7,77838427947598| Button [Make mask file]: prepares file mask by selected commands Interval/seconds : sets freqention for watching the changes. Event process : Single file - event changes in file event.mon. Multiple files - event changes in file X event.mon (X: 0 to EventFileCount - 1 ( 0 event.mon to 49 event.mon )). Repeat: for process Multiple files(0..49,0..49..). Reload project: - for setting Repeat - loading original setting of geoObjects - before 0 event.mon. If is disabled checkbox Default window, allows definition of appletWindows ( place, hight, width ). The service [Export] is assigned complete save of all information about the project in applet's configuration file - siGGis Applets . siGGis Monitor is determined to configuration of applets. First step: build project and save as *.hgf *.hge (check), second step: export applets Description: Export directory - determinates where will the program save all vector/database files(*.sig, *.dbf). Into vector files : All geoObjects - exports and saves complet layers , setting: Only selected geoObjects - creates vector files of geoObjects in particular layers according to values in databases . Into database files : All database fields - export only one file*.dbf for one layer *.sig (complet database with all fields - Classic way ). The Switch: Only selected fields -. create one new optimal file - *.dbf, include only showed fields( sign "Yes" - service: Set.). Warning: In the new database have to be the define fields - Objects selection. Applet setting: Config fileName - define name.* - configuration applet file. It is created prototip file name.htm (include the definition of applet running) and name.log - file of export progress . If the Layer_name.zip(In the archive must be include all vector/database files) service is selected, the cross-reference of archive file (URL_applet/Data/name.zip) is going to be saved in appletConfig file - name.cfg. Data path: - determinates where will the applet search for *.sig and *.dbf files. E.g.: The place on local net: f:\Gis\Geo123\geo123.html. When is open document, the applet is running , is readed the URL_applet : file:/f:/Gis/Geo123. The archive file (gis_1x.zip) must be place in subdirectories URL_applet: f:\Gis\Geo123\Data\gis_1x.zip. The place on internet: http://geoGis.xyz.ce/Geo123/geo123.html. When is open document, the applet is running , is readed the URL_applet: http://geoGis.xyz.ce/Geo123/. The archive file (gis_1x.zip) must be place in subdirectories URL_applet: http://geoGis.xyz.ce/Geo123/Data/gis_1x.zip. Button: [Define fileNames] - Open a window that allows to change names all files of geoProject: Button: [Define dbf action] - Open a window that allows to Define the action (e.g. : open html file with detail geoObject description, following reference to additional information, load configuration file *.cfg - other map) or fill in AppletProjects list. Example : 135 th geoObject is described in the document on an address: http://geogis.xyz.ce/fLay0/ID 135.html., selected entry of current database of geoObjects can contain : complete path to the document: http://geogis.xyz.ce/fLay0/ID 135.html is in field TERI_ID, all others column's content is empty. part of the path 135 is in field TERI_ID, and the rest is defined trough the 3. and 5. columns complete path to the document http://geogis.xyz.ce/fLay0/ID 135.html. contains 3. edit window. ….. The dbf Action may be start from applet window:. The type of Action is depend on your internet browser. A several types for MSIExplorer: Open file in MSIE: f:\Gis\Data\Geo123.html : distil: file:///f:\Gis\Data\Geo123.html Run other program with associate file: c:\Doc\Data\Geo123.doc : distil: file:///c:\Doc\Data\Geo123.doc (The file *.doc must be associate with any program when will be launch). Send e-mail to address: xxx123@email.com: distil: mailto:xxx123@email.com
Applets - siGGis Applet siGGis Event |
Brief description: siGGis Applet- is included in siGGis program. Applet is designed to viewing and presentation geographical projects through an internet browser. Applet's configuration is made by service: Export. You can export new layers (*.sig - format for internet) according to setting ( only seleced geoObjects, only displayed database's fields of all joining). You can define any action for selected geoObject (e.g.: show *.html document, run any program associated with document type, run post program and sending e-mail - is generated e-mail address is cames from geoDatabase, load other map...).All files can be pack in to archive file (ZIP).The working with applet is same as with program siGGis Monitor.The Applet was on trial through an internet browser (MSIE v5.0 - higher).Does not require any action from server(....CGI scripts etc), doesn't need JDBC/ODBC interface. When is applet loaded correctly the Load List window will be hide otherwise stay on screen and can contain Error Info. (When is find any Exception or the eventProcess/applet was not start - reload document with applet! ). Limits: Polygons - only solid or transparent fill, lines - only solid line, labels only default font, style is limited normal,italic,bold,boldItalic. siGGis Event - applet - is included in siGGis program. Is designed to join with another programs or systems and monitor events (change geoObject's properties, flood monitoring, object security guard, GPS.. ). The changes can be defined - generated another programs - in same ASCII file ( type *.INI ).Does not require any action from server(....CGI scripts etc), doesn't need JDBC/ODBC interface. Intention: Applet siGGis Event is scanning content of ASCII file - eventFile. The eventFile can be placed on a server or local PC ( URL - intranet / internet / PC ) . It can be selected a type of monitor: Continual scanning single file (e.g.:single process GPS - change of location - geoObject, state of properties, secure of objects, flood monitor ... ). Process simulaction - composite from X events ( e.g.: multiple process - gradually scanning X-1 eventFiles) Combine 1) and 2) ( e.g.: multiple process - periodic scanning 2 eventFiles: first file: check setting, second file: any events...<< repeat ) The eventFile ( siGGis Event v 1.6 )- command description: [Dynamic] - section for creating and editing new geoLayers createLayer = LAYER_NAME|POINT/LINE/POLY|LABEL|x0|y0|...xX|yY setLayerFont = LAYER_NAME|1/0{show/hide}|COLOR|SIZE|TYPE{0/1/2/3:normal/bold/italic/boldItalic}| addObject = LAYER_NAME|LABEL|x0|y0|...xX|yY modifyObject = LAYER_NAME|RECORD|LABEL|x0|y0|...xX|yY ; createLayer : create new layer LAYER_NAME, selected type, create virtualy database of geoObjects with Label field fill in of LABELcontents. If layer ; ; LAYER_NAME is not existing next commands is ignored. ; setLayerFont: set font properties (geoObject - Label) in import layer LAYER_NAME. 1/0 show/hide exist Labels, COLOR: set Label color , SIZE: set ; font size (0: not draw, -1: SIZE: 0.5 ), TYPE: font type. ; addObject: add next geoObject in layer LAYER_NAME and fill in database of LABELcontens. ; modifyObject: replace geoObject number RECORD in layer LAYER_NAME new geoObject, LABEL [Static] - sektion: static event ( !!! after [Dynamic] section if is used !!! ) load = URL/nameFile.* (siGGisMonitor- *.hgf *.hge, associate files with programs) (siGGisEvent *.cfg *.html...) - load new project file ( new mapProject ) or run one program according to associate files loadJpgFile = URL/nameFile.jpg - load new jpg file ( *.jpg must be defined in project! ) saveMetafile = path and name for saving geoProjectWindow into vekctor file ( *.wmf, *.emf ) - only siGGisMonitor interval = S - count second ( scanning frequency ) countEvent = X - count event zoom = x.x - zooming setting ( x.x <> 0 : e.g.: zoom = 1.5 or zoom = -0.5) resetMap = 0/1 - No/Yes - redraw map window ( Reset ) resetAll = 0/1 - No/Yes - reset geoObject's properties - according to last configFile *.cfg. Reset count of multiEvents - repeat process refresh = 0/1 - No/Yes - redraw map window (actual zooming) eMessage = link Main text message moveAll = 0/1 - when is eMoveXz or eMoveYz or eMoveXYz defined No/Yes - move all geoObjects in layer z loop= Y - jump on YeventFile.* (only multiProcess) eLayer[1..X] = - number of layers into project file. eObject[1..X] = - number of geoObject eObjectType[1..X] = - number of type geoObject eObjectSize[1..X] = - number of size geoObject (only point: 5..25) eRangeColor[1..X] = 0/1 - No/Yes - fill geoObject (graduated color) if eRangeColor[1..X] = 1 then fillColor will be calculated: eBeginColor[1..X] = - for minimum value eEndColor[1..X] = - tor maximum value eMaxValue[1..X] = max. value eMinValue[1..X] = min.value eValue[1..X] = value in [max .. min] if eRangeColor[1..X] = 0 then fillColor is define: eFillColor[1..X] = eOutLineColor[1..X] = - outline eDblOutLine[1..X] = 0/1 - No/Yes - double thickness outline (point,polygon), line geoObject eCentre[1..X] = 0/1 - No/Yes - centre geoObject - map window eCentreZoom[1..X] = 0/1 - No/Yes - centre + zoom geoObject - map window eBlink[1..X] = 0/1 - No/Yes - blink geoObject eReset[1..X] = 0/1 - No/Yes - reset properties of geoObject eBeep[1..X] = 0/1 - No/Yes - beep eHide[1..X] = 0/1 - No/Yes - hide/show geoObject eMoveX[1..X] = x.y - change of location X geoObject ( GPS: physical value x-coordinate - format:double ) 1) new location ( X.Y:...1234,1234... or ...1234.1234...) 2) adding/decreasing m/p : minus/plus ( e.g.: p-50,5 add value to current X: -1234.1234 + (-50,5) ) eMoveY[1..X] = y.z - change of location Y geoObject ( GPS: physical value y-coordinate - format:double). eMoveXY[1..X] = x.y|y.z - change of location XY geoObject ( GPS: physical value xy-coordinate - format:double, separator "|"). eMessage[1..X] = link text message : List Event window ( ~x,~y is replaced current X,Y of geoObject) eLabelSet[1..X] = abcd 1234 : show and set labelText of geoObject Export / Import geoObjects 1) Detail format to editing and back importing ( *.d01 ): Description - structure import ASCII file(Separator = |): Layer = LAYER_NAME Type = POINT/LINE/POLY NUM_RECORD0|NUM_POINT0|x0|y0 NUM_RECORD0|NUM_POINT1|x1|y1 : : : : NUM_RECORDX|NUM_POINTY|xZ|yZ LAYER_NAME: name new layer ( legend, comboBox...) TYPE : Type of layer - point, line ( polyline ) or simple polygon ( multipolygon a multipoint not supported) NUM_RECORDX: geoObjects number in layer (0..count_geoObjects -1) x0|y0: coordinate of current point ( integer or double) 2) Format for events (new laers, modify new geoObjects - siGGis Event - *.e01) Description - structure import ASCII file(Separator = |): createLayer = LAYER_NAME|POINT/LINE/POLY|LABEL|x0|y0|...xX|yY setLayerFont = LAYER_NAME|1/0{show/hide}|COLOR|SIZE|TYPE{0/1/2/3:normal/bold/italic/boldItalic}| addObject = LAYER_NAME|LABEL|x0|y0|...xX|yY modifyObject = LAYER_NAME|RECORD|LABEL|x0|y0|...xX|yY createLayer : create new layer LAYER_NAME, selected type, create virtualy database of geoObjects with Label field fill in of LABELcontents. If layer LAYER_NAME is not existing next commands is ignored. setLayerFont: set font properties (geoObject - Label) in import layer LAYER_NAME. 1/0 show/hide exist Labels, COLOR: set Label color , SIZE: set font size (0: not draw, -1: SIZE: 0.5 ), TYPE: font type. addObject: add next geoObject in layer LAYER_NAME and fill in database of LABELcontens. modifyObject: replace geoObject number RECORD in layer LAYER_NAME new geoObject, LABEL |
Description configuration INI file: |
;Max. length of row : 250 chars !!! [Language] fstName - first language( first menu row - item Language) nxtName - second language ( second row - item Language) actual - (0/1: first/second language) fst_1 - text - first language nxt_1 - text - second language fst_x - text - first language (x - th text) nxt_x - text v druhém jazyce (x - th text) cPage - code page ( default IBM: 6 ) [Paths] - position for vector/database files from *.hg* update - update configuration siGGis ( 0/1: no/yes) Project - path to files *.hg* Vector - path to files *.sig,*.shp, *.dbf Temp - NET set: path to tempfiles *.shp, *.sig, *.d0x, *.e0x, *.dbf dBase - path to next files *.dbf ( e.g.: for joining ) hlp1 - path with name of 1.help file(key F1) - item: hlpPar1 hlp2 - path with name of 2.help file(keys Ctrl+F1) - item: hlpPar2 hlp3 - path with name of 3.help file(keys Shift+F1) - item: hlpPar3 [General] - setting noConfig - enable/disable setting - service Properties - General (for update INI file): 0/1 - no/yes [Projects] - projects *.hg* - in projects list. count - count project files for select window Project List ( if is > 0, is open select window ) prj_1 - first project file in select window Project list pth_1 - path to first project file in select window Project list : prj_count - count project file in select window Project list pth_count - path to count project file in select window Project list |
© Milan Harašta, H.a.R ware (http://web.quick.cz/siggis) |