 The X-ThinPro 6.0/Release:20000714 Installation
   ***********************************************

To install the package, run the "setup.exe" file from the first diskette .

NOTES:
     1) the XWPNFS32/Win9x Client may be installed only by using
       the "Custom" installation mode;
     2) the beta 3 XWPNFS32 NFS-Client for Windows 2000 is installed manually.
       Please refer to the "nfsc2k_b.txt" readme file and the
       "nfsc2k_b.exe" self-extracting archive file.
       These files may be found into the directory with uncompressed
       X-ThinPro distributive.
     3) the Windows NT/2000 LPR printer driver is installaed
       by running the "lprd.exe" self-extracting archive file.
       This file may be found into the directory with uncompressed
       X-ThinPro distributive.

        Undocumented Features
 ---------------------

  1. XServer and XSettings :
     - the empty, or "255.255.255.255" or "0.0.0.0" contents
      of the "Broadcast File" field provides now the "natural"
      XDMCP broadcast mode when users need not fill in any file
      (see also the "The following enhancements have been made"/XServer
       above);
     - the "GlxExtension" box should be checked to enable
      the "GLX" extension.

  2. XServer :
     - the "Restore"/"Minimize" menu items of XServer in "Multiple+remoteWM"
      mode provides "visibility" of XServer's background into additional
      non-large window. This "background" may be used to provide control
      functionality of the windows manager used (usually it is pressing on
      mouse-buttons).

  3. NFS-Client for Windows 9x :
     - may be installed manually after X-ThinPro installation
      from "XWPNFS32.W95" subdirectory of installed X-ThinPro directory
      (see "XWPNFS32.W95\readme" text file for more information);

  4. NFS-Client for Windows 2000 :
     - may be installed only manually after X-ThinPro installation
      (see the top of this readme file).

        Known problems
        --------------

  1. XServer :
     - drawing of partial arcs may be very slow ;
     - the CDE/XDMCP of the HP-UX host may provide infinite
      waiting for connection. To avoid this, the new "HP" fonts
      alias directory should be included into the XServer FontPath;
     - the "Forced Backing Store" setting may provide wrong
      screen re-displaying in some cases (e.g., Netscape scrolling).

  2. Lpd :
     - printers on the remote Windows NT 4 hosts
      are unavailable from the local host with Windows NT 4 .

  3. NFS-Server :
     - may have problems on PCs with several IP addresses;
     - some Linux NFS-3 Clients may provide an error message
      (about wrong file ID) because of wrong packets unwrapping
      in the Linux's "nfs3xdr.c" module.

  4. NFS-Client for Windows 9x :
     - PC must restart after you changed the license
      "xwpdllid.dll" file.

  5. Uninstallation :
     - uninstallation procedure does not remove components
      which were installed in additional (non-first) installation
      sessions. Such additional components should be removed manually.

