Docklight V1.0
Copyright 2002 Flachmann und Heggelbacher (www.fuh-edv.de)

Program Description:
Docklight is a test, analysis and simulation tool for serial communication protocols (RS232, RS485/422 and others). It allows you to monitor the communication between two serial devices or to test the serial communication of a single device. Docklight is easy to use and runs on almost any standard PC using MS Windows 95/98/NT 4/2000/XP operating system.

Installation:
- Execute the "setup.exe" application

Distribution:
- See the "fuh_distribute_int.txt" file

System Requirements:
- Operating system:MS Windows 95/98//NT/2000/XP 
- Hardware requirements: Pentium processor 200 MHz or faster, minimum 32 MB RAM, minimum one COM port available. Two COM ports for monitoring communication between two serial devices. 
