IntPv100.zip    InternetPager - Send alarm over internet eMail

InternetPage have been designed to send alphanumeric alarms from a
control console to PCS or cellular phone with eMail receiving 
capability.

You could also send alphanumeric alarms to any other eMail receiver
(Internet, Intranet) because InternetPager use SMTP server to send
eMail at designated receiver.


Special requirements: Need a "null" modem to link control console to
		      the serial interface.
		      Need a valid SMTP server account and eMail sender
		      name and address.

Pre-install

1- " Unzip " compressed IntPv100.zip file in a working directory.  You will get three compressed files (.zip) : InternetPager.zip, InterfaceSerial.zip and VbSetUp.zip (Vb installer in english).

InternetPager installation.

1- " Unzip " InternetPager.zip in a working directory.  Note : as I use a french version of Visual Basic, the standard install wizard is in french, you can replace this by english version in unzipping, on the same directory, VbSetUp.zip contained in the InternetP.zip compressed file.  This unzip action replace french Setup programs on this working directory. 

2- Run Setup program and follow installation instruction provided by "installation Wizard". 

3- You are now able to customize InternetPager as you wish.  However, it is important to install InterfaceSerial (Ser_Ip) before the customisation of InternetPager.

4- " Unzip " InterfaceSerial.zip in another working directory. Note : as I use a french version of Visual Basic, the standard install wizard is in french, you can replace this by english version in unzipping, on the same directory, VbSetUp.zip contained in the InternetP.zip compressed file.  This unzip action replace french Setup programs on this working directory. 

5- Run Setup program and follow installation instruction provided by "installation Wizard". 

6- Run Ser_Ip from Start menu.

7- Use UserGuide-Ser_Ip.txt to help you in customisation of InterfaceSerial (Ser_Ip).  You must use InterfaceSerial (Ser_Ip) as a server.  These are parameters for preparing InterfaceSerial (Ser_Ip) to run with InternetPager : 
- langue : english (to obtain a user interface in english).
- mode : server.
- display : as you wish.
- Select under serial port button, the related parameters for the serial port to interface.
- Select service " 7243 " as listening port of server.
- Select exchange protocol between serial port and InterfaceSerial application.
- Select Execution on start-up.
- Click on " Start " and note window's title in running mode.  This title must be specified as a parameter to InternetPager application.

8- Run InternetPager from Start menu.

9- Specify " English " to obtain english user interface.

10- Complete InternetPager parameters as your organisation need.  Follow UserGuide-InternetPager.txt.


Robert Laflamme, 
rlafla@excite.com
http://members.wbs.net/homepages/i/n/t/intbobqcenfrancais/index.htm 