=========================================================================
Date:         Fri, 1 Mar 2002 01:50:33 -0500
Reply-To:     Ulrich Allen <Ulrich.Allen@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ulrich Allen <Ulrich.Allen@GMX.DE>
Subject:      Re: Sending SMS with post/lx?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Thanks again, Tony,
I first try to understand what you did send.
I'll compare it with my sms.scr.
But because of your hints the problem is limited now.
Uli

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 05:04:10 -0500
Reply-To:     Martin Bergvill <hplx@BERGVILL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Martin Bergvill <hplx@BERGVILL.COM>
Subject:      Re: MPG program
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Thu, 28 Feb 2002 21:19:51 -0500, Bing wrote:

> I am using HP200 to track the car consumption of gasoline.

Me too. I track both my bike and my car.

> I found two
> programs, MPGTracker and HPMILE. The former only has entry in gallons and
> miles. The later, which has better graphical display and is said to allow
> entry of kilos and litres, seems not accessable from SUPER link. Anybody
> has a copy of new version HPMILE?

I use version 2.0 sept 1998 of MPG Tracker. It works well in literes
and kilometers. I can not remember, but you choose the first time you
start the program to use gallons or liters.

I got a private email from Owen that made MPG Tracker and hopefully
there will be a new version soon. I made some requests here on this
list and hopefully before I take my bike out for a ride I am able to
track both car and bike within the same program.

Owen also said that if anyone wants to have a look at the source just
let him know.

Owen are you there? Jump in here anytime :-)

Regards

--
Martin Bergvill ,Narvik Norway

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 05:04:25 -0500
Reply-To:     Martin Bergvill <hplx@BERGVILL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Martin Bergvill <hplx@BERGVILL.COM>
Subject:      Re: HPLX links database
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Tue, 26 Feb 2002 16:10:33 +0200, Daniel Hertrich wrote:

> Hi friends,

Hello there

> How nice it would be to have an online form where everone could add a
> link he has found and thinks it could be intersting to HPLX users.

Great idea. There is also a webring isn't it?

Collecting all good links is a great idea.

Regards

--
Martin Bergvill ,Narvik Norway

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 05:04:47 -0500
Reply-To:     Martin Bergvill <hplx@BERGVILL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Martin Bergvill <hplx@BERGVILL.COM>
Subject:      Fwd: Ol' Eddie Archive Was: Re: Minix on the 200LX natively -
              longer,posting.
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi

Found this in my folder from may last year.

I have not checked Bill's website out, but if Bill sends a copy of his
cdr's to Daniel or any other of the Superteam we could put them on
Super?

Regards

--
Martin Bergvill ,Narvik Norway

--- begin of forwarded message ---

Date:         Sun, 20 May 2001 10:41:53 -0700
From: Bill Childers <childers@GARLIC.COM>
Subject:      Ol' Eddie Archive Was: Re: Minix on the 200LX natively - longer
              posting.
To: HPLX-L@UCONNVM.UConn.Edu

Yep.  My lil' repository at clove.garlic.com is no longer - the website
server was hacked and the data got nuked.  (Thanks, Microsoft, for having
such $%&@ security.)

Anyhow, this did happen some time ago, and I've since got my own website,
www.nulldevice.net.  I absolutely forgot all about the old HPLX archive
since I moved to a Palm Vx for my daily activities, but - I do have all
the data on CD-R.  When I get some time I'll put a section up on
nulldevice.net pertaining to the LX.  I'll toss the Eddie stuff and Minix
there as well.

Sorry about this -- All this happened about the same time my daughter was
born, and it kinda got put on the back burner.  I'll keep the list
informed when I make some progress.

-- Bill


On Sun, 20 May 2001, Laust Brock-Nannestad wrote:

> On Sun, 20 May 2001, Tamas Feher wrote:
>
> > It was at <http://minix.hplx.net>, which links to a site called
> > garlic.something.??? , which was under construction two
> > days ago.
>
> garlic.clove.com. This was Bill Childers' web-site. He hosted not only the
> Minix files but also copies of long-gone LX-related ftp sites,
> eddie.mit.edu for instance. ISTR that Bill's site was hacked, and taken
> down, destined to be brought online again "some day". If Bill is still
> reading the list, then perhaps he can let us know when/if the archive will
> be back up or if there is another way to get a copy of the files. I
> personally wouldn't mind a complete copy of the Eddie archive, since
> garlic.clove.com is now the official location according eddie.mit.edu
> (which no longer hosts the archive but refers to garlic.clove.com!).
>
>
> bye,
>
> Laust

--- end of forwarded message ---

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 05:05:30 -0500
Reply-To:     Martin Bergvill <hplx@BERGVILL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Martin Bergvill <hplx@BERGVILL.COM>
Subject:      Re: TDMA and GSM
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Mon, 13 Aug 2001 21:26:31 +0200, Daniel Hertrich wrote:

> Hi Martin,

Hello Daniel

Having some time to clean up my POST/LX folder and found this from you.

> > 90199462. The cellphone swithc knows where I am. If you are outside
> > Norway then you call the norwegian swithc and the norwegian switch puts
> > you through to my phone wherever I am.
>
> Yes, same here.
> 901 seems to be your network's area code (or only 90?), seems like
> cell phone netwprk provides love the "9".

No in Norway we do not have area codes. The first two or three numbers
does not indicate where you are in Norway. It used to indicate on which
network you are. But that was up until 1. November 2001. Now you can
take phonenumber with you to a different network provider.

> Sorry, folks, if this is off topic, but I find it very interesting to
> discuss that here!

It is. I found out not long ago that the bug in Ericsson's phones where
it would not log on again after it was out of range has been fixed in
the latest firmware version.

The problem was that if you had "Preferred services" set to Gsm _and_
Gprs it would not log on again to the network. This only happend to
T39/T65/T68 used on Telenor which uses Nokia hardware in their BS.

This problem should now be fixed. (Or so I am told by Telenor here in
Norway)

Regards

--
Martin Bergvill ,Narvik Norway

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 14:18:19 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: MPG program
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> track the car consumption of gasoline.

This is a combination of calculation and documentation, isn't it? That imho
is exactly what spreadsheets are for and good at. I use Lotus 123 for this
and on my desktop Atari something quite similar which can also draw line
graphs.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 14:25:33 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: MPG program
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> but you choose the first time you start the program
> to use gallons or liters.

Does it also offer a choice of real gallons and American ones?
Do these programs do anything a very simple spreadsheet can't do just as
well or better?
I would recommend rolling your own. Start with the simplest way to do what
you need - you can always get more fancyful later (i.e. in my case adding
foreign currencies or oil for my two stroke) and you will have the
advantage to always know exactly what you are doing and not having to put
up with other people's ideosyncrasies. (Why after all are we preferring a
system we can understand to coloured Wince?)

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 08:27:48 -0500
Reply-To:     "Striegel, Alan" <Striegel@PIOS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Striegel, Alan" <Striegel@PIOS.COM>
Subject:      Re: IDE adapter info for PCMCIA and CF ATA flash cards
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

If you're not so handy with the soldering iron and are willing to pay the
price, you can just buy a very well done Compact Flash adapter for $59 US
(or $49 if you're a member of TAPR - Tucson Amateur Packet Radio.  For
membership details $20/year, see
http://www.tapr.org/tapr/html/Fmembership.html).   See
http://www.tapr.org/tapr/html/Fcfa.html

Alan Striegel

-----Original Message-----
From: Michel Bel [mailto:michel.bel@ZONNET.NL]
Sent: Thursday, February 28, 2002 5:13 PM

Those looking hard for a fast adapter to backup their CF or PCMCIA flash
cards to their desktop PC's, and are not too scared of soldering, should
look at the following pages describing how to connect your flash cards to a
desktop IDE connector

http://www.ant-computing.com/v0/v0-flash.html  for adapting a CF adapter,
and

http://www.wau.nl/hemeltje/temporary/personal/miscelaneous/cfadapter.html
for some more info

Michel ( off to soldering....)

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 08:28:30 -0500
Reply-To:     Steve <novosad@SERVER030.FWB.SAIC.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Steve <novosad@SERVER030.FWB.SAIC.COM>
Subject:      Re: PC Card Partitions with 200LX ?
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Michael Kopplin wrote:

> >   Did anyone try more than one partition with the Minix
> > distribution for the 200LX?

> The minix that works on the LX uses the dos-file-as-partition
> scheme, so it doesn't actually use real partitions. I have run
> it using two files, for extra "partitions" but that's not the
> same. Once minix is running it can't see anything of the card
> beyond the dos files.

  Oh.  Okay then, that makes sense.

> Perhaps real partitions would work using Dubbs method, but I
> have never tried to get it working. Maybe that's another thing
> I'll add to my list of things to look at if I ever can find the
> time.

  That's what I was thinking of.  He made a replacement for the
INT 13H disk services.  But I guess the original palmtop Minix
was unstable.

Steve

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 14:54:03 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: HPLX links database
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends

On Fri, 1 Mar 2002 05:04:25 -0500, Martin Bergvill <hplx@BERGVILL.COM> wrote:

> > How nice it would be to have an online form where everone could add a
> > link he has found and thinks it could be intersting to HPLX users.
>
> Great idea. There is also a webring isn't it?
>
> Collecting all good links is a great idea.

Seems as if the idea wasn't new. <g>

You won't believe what I just found on palmtop.net: Exactly what I
suggested.
Go to http://www.palmtop.net/links/links.htm and look!
Unfortunately, this doesn't work. But I know we can make it work, if
someone who has experience in perl script and html programming helps me
with that.

There seems to be exactly one html file (links.htm) and one perl script
involved. Nothing more. Ah, and a file called database.txt, which seems
to be created automatically.

We had to change the categories, add a few form fields (date,
comment...) and make the whole thing work. That's all.

Who is willing to help me? I don't dare to ask Laust once more, because
he did so much in the past to make SUPER work better, so maybe anyone
else this time?

Thanks
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 16:20:03 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: IDE adapter info for PCMCIA and CF ATA flash cards
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Michel and others

On Thu, 28 Feb 2002 23:12:37 +0100, Michel Bel <michel.bel@ZONNET.NL> wrote:

> Those looking hard for a fast adapter to backup their CF or PCMCIA flash
> cards to their desktop PC's, and are not too scared of soldering, should
> look at the following pages describing how to connect your flash cards to a
> desktop IDE connector

You can also buy such adapters. They occasionally appear on ebay. I got
mine together with a 170 MB PCMCIA hard drive for my old Omnibook 430.

However, the big disadvantage of these adapters is that IDE is not
hot-pluggable. So you have to restart your computer everytime you want
to attach / detach a flash card.

And, of course, you must have access to the IDE port, either using a
removable hard disk mounter or by leading an IDE cable out of the
computer case.

But OTOH this is a very fast and reliable method to transfer data to /
from a flash card.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 16:20:04 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      SUPER update
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

next SUPER apdate applied.

Changes:

*14-FEB-02
added ipcalc.pl (IP subnet calculator)
added GNUPLOT

*26-FEB-02
DOCHTML Sourceforge link added
PalDRAW Homepage link added

*27-FEB-02
XECHO133 added

*03/01/02
EDRUGS.ZIP (drugs.gdb) added
FELIXFON added
MAKEDOC added


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 08:20:57 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: IDE adapter info for PCMCIA and CF ATA flash cards
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

The ant-computing.com site has a link to a company called ES&S in Viersen at
the Niederrhein, Germany (http://www.esskabel.de), that makes a nice, small
CF-IDE adapter board in two versions -- 40 pin (with separate 4 pin power
connector) and 44 pin (with integrated power). Don't know how much they
cost, but it looks like it shouldn't be too much if they sell them
individually. Can anyone in Germany check this out?

Bob

-----Original Message-----
From: Michel Bel [mailto:michel.bel@ZONNET.NL]
Sent: Thursday, February 28, 2002 4:13 PM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: IDE adapter info for PCMCIA and CF ATA flash cards


Those looking hard for a fast adapter to backup their CF or PCMCIA flash
cards to their desktop PC's, and are not too scared of soldering, should
look at the following pages describing how to connect your flash cards to a
desktop IDE connector

http://www.ant-computing.com/v0/v0-flash.html  for adapting a CF adapter,
and

http://www.wau.nl/hemeltje/temporary/personal/miscelaneous/cfadapter.html
for some more info

Michel ( off to soldering....)

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 11:13:31 -0500
Reply-To:     Bill Sprague <eugarps@ATTGLOBAL.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bill Sprague <eugarps@ATTGLOBAL.NET>
Subject:      WANT: Connectivity Pack for  200LX
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Hi,

Anyone have one for sale?

Thanks,

Bill

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 17:25:05 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Web site updated
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

I have updated my homepage:

http://www.daniel-hertrich.de/mob_hplx

now contains more info about

* GPRS
* PostPDU
and some other goodies.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 18:21:24 +0100
Reply-To:     furlan@gmx.net
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Dr. Werner Furlan" <furlan@GMX.NET>
Organization: OE9FWV
Subject:      public transport map of Munich
MIME-Version: 1.0
Content-type: text/plain; charset=ISO-8859-15
Content-transfer-encoding: Quoted-printable

hello or Gr=FCss Gott for all bavarians on the list,

I use Stefan Peichls Lxmap program sometimes, and there is a very
good qualitiy map for M=FCnchen subway, but it is a little outdated.
They built some new stations.
Does anybody know of a more recent map?

txs,
Werner

--
Powered by Pegasus Mail - free at http://www.pmail.com
Homepage: http://www.qsl.net/oe9fwv
SMS: +436646340014@text.mobilkom.at

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 12:33:41 -0500
Reply-To:     "David M. Solinas" <solinas@FASTMAIL.FM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "David M. Solinas" <solinas@FASTMAIL.FM>
Subject:      WWW/LX With Verizon's Mobile Office (USA)
In-Reply-To:  <20020225050153.EEE1B39408E@fastmail.fm>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Hi all.  I've been carrying around my trusty HP200LX since
mid-1995, and I've been carrying around a digital cell phone
for a year or so.  So I finally got around to trying to connect
the two, and I figured that my experience might be useful to
someone, someday.

Here's my equipment:
HP200LX 8MB DS
HP serial cable
Audiovox CDM-9000 (tri-mode CDMA cell phone)
Audiovox DIC-4000 data cable (mid-$40's on eBay)
Ratshack 9-pin null-modem adapter and 9-pin M-M gender changer

Verizon Wireless has a free service called Mobile Office.  This is
different than their paid Mobile Web service, which lets you use a
web-enabled phone as a web browser.  Mobile Office lets you connect
to their circuit-switched network at 14.4Kbps, when you're on their
digital cell network, without using a separate ISP.  You do, however,
consume normal plan minutes when connected.

I connected the phone to the HP, and tried issuing "AT" commands
via datacomm.  No luck, until I disabled the "lighton" TSR that let's
me use Daniel 's excellent LCD light.  Then I fired up WWW/LX 2,
and tried calling my ISP.  I used the init string "ATZV1S7=90", which
I found in Verizon's .inf file for their Mobile Office windoze software.
I set the Baud to 19,200.  It worked, on and off -- I'd often have to
recycle the HP and/or the phone.  Then I tried changing the Dial
string to #777, which uses the Mobile Office ISP (and connects very
quickly), and couldn't connect at all.

Finally, I downloaded and installed WWW/LX 3, just for laughs, and
sure enough it works perfectly -- both with my ISP and the #777 one.
Once I told Post/LX3 my ISP's login and password, I was good to go
for Email.  WWW, ftp, telnet, ping, and even the ftp server all work.
I'm ordering WWW/LX 3 right away.

I hope someone finds this useful.  And thanks to D&A Soft for their
excellent software!

Dave Solinas

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 13:52:52 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: Ol' Eddie Archive Was: Re: Minix on the 200LX natively -
              longer,posting.
In-Reply-To:  <HPLX-L%2002030105044696@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

I'd be willing to host them on my site. I finally got around to putting =
up my linux box and setting up dynamic dns so that it's available. So =
far comcast is not blocking ftp (they do block http! the bastards...). I =
got a few gigabytes I can spare.



> Martin Bergvill

>=20
> Hi
>=20
> Found this in my folder from may last year.
>=20
> I have not checked Bill's website out, but if Bill sends a copy of his
> cdr's to Daniel or any other of the Superteam we could put them on
> Super?

> From: Bill Childers <childers@GARLIC.COM>

> www.nulldevice.net.  I absolutely forgot all about the old HPLX =
archive
> since I moved to a Palm Vx for my daily activities, but - I do have =
all
> the data on CD-R.  When I get some time I'll put a section up on
> nulldevice.net pertaining to the LX.  I'll toss the Eddie stuff and =
Minix
> there as well.
>=20
> Sorry about this -- All this happened about the same time my daughter =
was
> born, and it kinda got put on the back burner.  I'll keep the list
> informed when I make some progress.
>=20
> -- Bill
>=20
> > On Sun, 20 May 2001, Tamas Feher wrote:
> >
> > > It was at <http://minix.hplx.net>, which links to a site called
> > > garlic.something.??? , which was under construction two
> > > days ago.
> >
> > garlic.clove.com. This was Bill Childers' web-site. He hosted=20
> not only the
> > Minix files but also copies of long-gone LX-related ftp sites,
> > eddie.mit.edu for instance. ISTR that Bill's site was hacked, and =
taken
> > down, destined to be brought online again "some day". If Bill is =
still
> > reading the list, then perhaps he can let us know when/if the=20
> archive will
> > be back up or if there is another way to get a copy of the files. I
> > personally wouldn't mind a complete copy of the Eddie archive, since
> > garlic.clove.com is now the official location according =
eddie.mit.edu
> > (which no longer hosts the archive but refers to garlic.clove.com!).
> >
> >
> > bye,
> >
> > Laust
>=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 12:20:07 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Microsoft Mouse?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

Has anyone had success using a Microsoft mouse with the 200LX? I can get the
driver to recognize the mouse and install properly, but I get no response
(neither cursor movement nor button clicks). The serial port works with
CPack, so I know it's good. I have also tried an Appoint Pen Mouse, which is
MS compatible, with the same results. Could it be that the mouse needs more
power than the LX serial port can supply?

Bob

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 20:25:58 +0100
Reply-To:     gonter+usenet@wu-wien.ac.at
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Gerhard Gonter <gonter@ZECHINE.WU-WIEN.AC.AT>
Subject:      Re: HPLX links database
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Daniel Hertrich wrote:
> [HP-LX link database]
> Who is willing to help me? I don't dare to ask Laust once more, because
> he did so much in the past to make SUPER work better, so maybe anyone
> else this time?

Well, there is also DMOZ:

  http://dmoz.org/Computers/Systems/Handhelds/Hewlett-Packard/MS-DOS/

You can submit links there and an editor can review and file the
link in an appropriate category.  You can also apply as an editor
to speed up this process.

+gg

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 13:06:15 -0800
Reply-To:     "Martin G. Ramirez" <mramirez@LMU.EDU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Martin G. Ramirez" <mramirez@LMU.EDU>
Subject:      Re: Microsoft Mouse?
In-Reply-To:  <D8020D6F0DB8D211B99A0008C7C59CFE0FD8F727@cormails1.jdedwar
              ds.com>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

LXers,

I seem to be having the same problem right now with a Microsoft serial
mouse.  As outlined in an earlier post this week, my connection set up is...

200LX ---> HP serial cable (F1015-80002) ---> HP null modem adapter
(5181-6639) ---> Mouse

The MOUSE.COM driver loads ok in DOS, but I too get no response from the
mouse (no cursor movement, no mouse clicks).  I know the LX port works, as
it use it with Transfile & Intellisync almost everyday, and I have the port
set to ON in DOS mode via Setup.  So, if this problem is indeed a case of
the mouse not getting enough power from the LX serial port, could those who
have managed to get mice/trackpads/trackballs/etc. working with the LX
share with us what BRANDS/MODELS of these things they are using?

Thanks,
Martin G. Ramirez

At 12:20 pm 3/1/2002 -0700, you wrote:
>Has anyone had success using a Microsoft mouse with the 200LX? I can get the
>driver to recognize the mouse and install properly, but I get no response
>(neither cursor movement nor button clicks). The serial port works with
>CPack, so I know it's good. I have also tried an Appoint Pen Mouse, which is
>MS compatible, with the same results. Could it be that the mouse needs more
>power than the LX serial port can supply?
>
>Bob
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

============================
Dr. Martin G. Ramirez
Department of Biology
Loyola Marymount University
One LMU Drive, MS 8220
Los Angeles, CA  90045-2659, U.S.A.
(310) 338-5120
FAX: (310) 338-4479
e-mail: mramirez@lmu.edu
=============================




NTMail K12 - the Mail Server for Education

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 22:18:47 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Microsoft Mouse?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Bob

On Fri, 1 Mar 2002 12:20:07 -0700, "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM> wrote:

> Has anyone had success using a Microsoft mouse with the 200LX? I can get the
> driver to recognize the mouse and install properly, but I get no response
> (neither cursor movement nor button clicks). The serial port works with
> CPack, so I know it's good. I have also tried an Appoint Pen Mouse, which is
> MS compatible, with the same results. Could it be that the mouse needs more
> power than the LX serial port can supply?

DId you make sure that the COM port is set up properly?
I recommend Stefan Peichl's SETCOM1 for that.
Also, don't try to use the mouse under System Manager.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 13:21:16 -0800
Reply-To:     Harry Mulcahey <harrym@LVCM.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Harry Mulcahey <harrym@LVCM.COM>
Subject:      Re: help!
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

>Your HP: check the com jack for damage of the pins.
>use cic100 to power on / off the port.
>can you check if the port works with another >device (modem)
I dont have a modem, the com jack is not damaged, and I do not have cic100.
----- Original Message -----
From: "Dr. Werner Furlan" <furlan@gmx.net>
To: "Harry Mulcahey" <harrym@LVCM.COM>
Sent: Friday, March 01, 2002 9:35 AM
Subject: Re: help!


> hi Harry,
>
> > It seems that my HP200LX now hates my PC. Whenever I try to scan the
> > COM ports, or connect to the HP, it says it does not detect it. I have
> > the filer app running, server mode is enabled, it is connected to the
> > HP and the PC. When I scan the COM ports, because I have the correct
> > speed when I start the scan, it says it cannot connect to the HP200LX.
> > Please help me.
> >
> the problem could have many reasons, software and Hardware.
> To track it down you have to check both - the HP, the Desktop and the
> cable of course.
>
> Can you check the comport on your desktop with another device?
> A modem for example?
> Is it possible that another software locks the comport?
>
> Your HP: check the com jack for damage of the pins.
> use cic100 to power on / off the port.
> can you check if the port works with another device (modem)
>
> Do you have CPACK or a Norton Commander version for DOS?
> They are also useful to copy file from the HP.
>
> HTH
> Werner
>
>
> --
> Powered by Pegasus Mail - free at http://www.pmail.com
> Homepage: http://www.qsl.net/oe9fwv
> SMS: +436646340014@text.mobilkom.at
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 14:25:38 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: Microsoft Mouse?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

I believe the port was set OK, as it works for CPack. Also, the mouse driver
recognizes the mouse.

I get the same results in straight DOS or DOS via the System Manager.

BTW, I am using the same cabling as Martin.

-----Original Message-----
From: Daniel Hertrich [mailto:daniel.hertrich@GMX.DE]
Sent: Friday, March 01, 2002 2:19 PM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: Microsoft Mouse?


Hi Bob

On Fri, 1 Mar 2002 12:20:07 -0700, "Feldman, Robert"
<Robert_Feldman@JDEDWARDS.COM> wrote:

> Has anyone had success using a Microsoft mouse with the 200LX? I can get
the
> driver to recognize the mouse and install properly, but I get no response
> (neither cursor movement nor button clicks). The serial port works with
> CPack, so I know it's good. I have also tried an Appoint Pen Mouse, which
is
> MS compatible, with the same results. Could it be that the mouse needs
more
> power than the LX serial port can supply?

DId you make sure that the COM port is set up properly?
I recommend Stefan Peichl's SETCOM1 for that.
Also, don't try to use the mouse under System Manager.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 13:34:31 -0800
Reply-To:     "James P. Grenert, MD, PhD" <grenert@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "James P. Grenert, MD, PhD" <grenert@YAHOO.COM>
Subject:      LX serial connection
Comments: To: harrym@LVCM.COM
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii

Hi.
Here are some things to check:
1.  Make sure no other PC programs/hardware are trying to use the COM# of the
serial port.
2.  Make sure your 200LX serial port is on.
3.  Set the LX serial port speed in Filer to nothing higher than 57600.
4.  I know you don't have to be in Server mode on the LX.  I'm not sure it
hurts, but you may want to try connecting just by being in Filer with the
serial port active.

Good luck.
J. P. Grenert
grenert@yahoo.com



__________________________________________________
Do You Yahoo!?
Yahoo! Greetings - Send FREE e-cards for every occasion!
http://greetings.yahoo.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 16:54:17 -0500
Reply-To:     Owen Samuelson <owensamuelson@COX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Owen Samuelson <owensamuelson@COX.NET>
Subject:      Re: MPG program
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Bing,
I wrote MPG Tracker and it will do kilos and liters but it's not set up to
change back and forth. You specify which one to use initially. I'm in the
process of updating my programs and contact info at SUPER.
Owen S.

----- Original Message -----
From: "Bing" <bxu2@UWO.CA>
Sent: Thursday, February 28, 2002 9:19 PM
Subject: MPG program


> I am using HP200 to track the car consumption of gasoline. I found two
> programs, MPGTracker and HPMILE. The former only has entry in gallons and
> miles.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 17:01:39 -0500
Reply-To:     Owen Samuelson <owensamuelson@COX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Owen Samuelson <owensamuelson@COX.NET>
Subject:      Re: MPG program
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

----- Original Message -----
From: "Axel Berger" <Axel-Berger@NEXGO.DE>
Subject: Re: MPG program


> Does it also offer a choice of real gallons and American ones?

No, but it could.

> Do these programs do anything a very simple spreadsheet can't do just as
> well or better?

I don't know. I just wrote mine because it was fun to do (for me). If anyone
wants to use it and/or modify/change it, that's fine with me. I used
Microsoft Quick C and the PAL library. The source code will be included in
the next SUPER update.

Best Regards,
Owen S.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 00:20:14 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: Microsoft Mouse?
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Just one question (and it is genuine interest, not a snotty nosed snide
remark):
What do you actually want the mouse for?
I have of course enabled a DOS mouse driver on my games console (Win98,
bells, whistles, internet, etc.), but under DOS I never use it at all. To
the contrary, I have found a list of key commands for windows and do a lot
more than is usually thought possible without having to reach over to that
thing. So honestly, what do you actually want it for on a LX?

Danke
        Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 00:30:41 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: MPG program
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> I don't know. I just wrote mine because it was fun to do (for me).

Please don't take my remarks as criticism - they are not meant that way. It
is just that for many years I used to program utility stuff in BASIC on my
Atari (and before the Atari in a Sharp 1401 calculator) and never knew
spreadsheets. When I began to use an Atari Portfolio (before giving that up
for an LX last year) I first began to use Lotus mostly because the
Calculator was useless (as in the HP IMHO). But after I found how simple
some things - and especially stuff like mileage and cost tables - can be
done there, I have never bothered to program for things like that any more.
Of course undoubtedly programming allows much more than a simple
spreadsheet does, thus my question if you actually do more than I.
Would anyone like my Lotus table as a template and are small attachments
accepted here?

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 23:58:43 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: MPG program
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Axel Berger wrote:
> Does it also offer a choice of real gallons and American ones?

Does it offer a choice of gallons that most people use or those
Imperial ones?

Cheers... Russ   :-)

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 19:49:02 -0500
Reply-To:     Owen Samuelson <owensamuelson@COX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Owen Samuelson <owensamuelson@COX.NET>
Subject:      Re: MPG program
Comments: To: Axel.Berger@NexGo.De
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

----- Original Message -----
From: "Axel Berger" <Axel-Berger@NEXGO.DE>
Sent: Friday, March 01, 2002 6:30 PM

> Please don't take my remarks as criticism - they are not meant that way.

> Of course undoubtedly programming allows much more than a simple
> spreadsheet does, thus my question if you actually do more than I.
> Would anyone like my Lotus table as a template and are small attachments
> accepted here?
>
> Axel

Axel,
No problem about the comments. Just wanted you to know my reasons for doing
the program were for fun more than utility. HPLX doesn't like attachments.
Send me your template directly so I can check it out.

Thanks,
Owen

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 1 Mar 2002 17:50:10 -0800
Reply-To:     "Martin G. Ramirez" <mramirez@LMU.EDU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Martin G. Ramirez" <mramirez@LMU.EDU>
Subject:      Microsoft Mouse - Success!
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

LXer's,

I have good news to report about the problem with the Microsoft mouse, the
details of which I reported earlier today (see below).  Well, I just went
to drawer full of Microsoft serial mice in my lab and picked out another
and connected it up as below - and it works!!!   As far as I know, all the
mice I have are good (they have all been used on other systems), so it may
be useful to note the info about the mouse I had earlier today that did NOT
work with the LX and the one that DOES.  So, here's the info:

        + mouse that would not work - "Serial - Mouse Port Compatible Mouse", part
no. 55305

        + mouse that does work - "Serial Mouse 2.0A", part no. 50674

Hope this info helps,
Martin G. Ramirez


====================================================================
LXers,

I seem to be having the same problem right now with a Microsoft serial
mouse.  As outlined in an earlier post this week, my connection set up is...

200LX ---> HP serial cable (F1015-80002) ---> HP null modem adapter
(5181-6639) ---> Mouse

The MOUSE.COM driver loads ok in DOS, but I too get no response from the
mouse (no cursor movement, no mouse clicks).  I know the LX port works, as
it use it with Transfile & Intellisync almost everyday, and I have the port
set to ON in DOS mode via Setup.  So, if this problem is indeed a case of
the mouse not getting enough power from the LX serial port, could those who
have managed to get mice/trackpads/trackballs/etc. working with the LX
share with us what BRANDS/MODELS of these things they are using?

Thanks,
Martin G. Ramirez

At 12:20 pm 3/1/2002 -0700, you wrote:
>Has anyone had success using a Microsoft mouse with the 200LX? I can get the
>driver to recognize the mouse and install properly, but I get no response
>(neither cursor movement nor button clicks). The serial port works with
>CPack, so I know it's good. I have also tried an Appoint Pen Mouse, which is
>MS compatible, with the same results. Could it be that the mouse needs more
>power than the LX serial port can supply?
>
>Bob
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

============================
Dr. Martin G. Ramirez
Department of Biology
Loyola Marymount University
One LMU Drive, MS 8220
Los Angeles, CA  90045-2659, U.S.A.
(310) 338-5120
FAX: (310) 338-4479
e-mail: mramirez@lmu.edu
=============================




NTMail K12 - the Mail Server for Education

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

============================
Dr. Martin G. Ramirez
Department of Biology
Loyola Marymount University
One LMU Drive, MS 8220
Los Angeles, CA  90045-2659, U.S.A.
(310) 338-5120
FAX: (310) 338-4479
e-mail: mramirez@lmu.edu
=============================




NTMail K12 - the Mail Server for Education

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 11:23:57 +0800
Reply-To:     SM Ling <piclister@yahoo.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         SM Ling <piclister@YAHOO.COM>
Subject:      IDE to CF adapter
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I think the best deal is on the eBay, there is one that has a plastic case
that let it be mounted like a floppy drive so it can be assesible without
opening out the PC case.  I have not tried that version, and not sure about
he hot-plugging issue.

Which bring me to the question about 3V3 and 5V CF that the previous site
mentioned, how does one differentiate them by appearance or form factor?
Because so far for the CFs I bought, this information is not printed on the
packaging.

Cheers, Ling SM

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 11:33:07 +0800
Reply-To:     SM Ling <piclister@yahoo.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         SM Ling <piclister@YAHOO.COM>
Subject:      SerialBert and something similar
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Frontier Test Equipment has some very powerful serial line testing software,
however they are too expensive.

You can find them here:  http://www.fte.com/download.asp .

The demo one is just a graphical display without real IO.  Anyone knows is
there a cheaper software or freeware that can do simple BERT (Bit Error Rate
test) or pattern testing and detection?

Cheers, Ling SM

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 11:41:54 +0800
Reply-To:     SM Ling <piclister@yahoo.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         SM Ling <piclister@YAHOO.COM>
Subject:      Portest on 200LX
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I am trying out porttest.exe on 200LX.  This is a serial and parallel port
testing software.

It is working but after a while, the internal digital loopback will fail.
When this happen, nothing can recover it unless I remove all the batteries
including the button standby battery.  I am not sure is it the software, or
is it the 200LX protecting its port from some spike.

Anyone can comment on this?  Thanks in advance.

Cheers, Ling SM

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 01:57:31 -0800
Reply-To:     j_vanderstel@JUNO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John J Vander Stel <j_vanderstel@JUNO.COM>
Subject:      Free AT compatible serial port peer-to-peer network software
              called Easy-Net
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Hi all,

While still exploring the far reaching corners of my hard drive, I ran
across some old software that might be of interest to some here.

Here is a paragraph from one of its text files:

"These files contain SHAREABLE SOFTWARE for EasyNet's ShareLan computer
networking system - a two-user version - ideal for lap-top to desktop
connections.  EasyNet ShareLan (ESL) is a full PEER-to PEER network
system for
two PCs.  EasyNet ShareLan will allow two PCs to share, programs, disk
drives,
Ram disks and printers connected to either machine, even if the machine
you
want to contact is currently in an application such as wordprocessing or
accounting.  EasyNet ShareLan is a full MULTI-TASKING, MULTI-USER network
system."

I don't know how fast the simple Zip serial transfer program on SUPER is,
but Easy-Net will only run at a maximum speed of 56K.  I know that the
LBL network software that I used on my HP200LX long ago was much faster
than that, but the setup for Easy-Net truly *is* easy.

I'm currently without the necessary hardware to test the Easy-Net
software and will only have email access for a while, but if anyone would
like to check out how it works on their HP200LX and would be willing to
post about the experience to this list , I would be happy to send the
archive to them as an attachment to a private email. (Sorry, I have no
idea where or when I found it. It might have even been uploaded to my old
BBS, long ago)

Cheers!

John Vander Stel
Grand Rapids, Michigan
________________________________________________________________
GET INTERNET ACCESS FROM JUNO!
Juno offers FREE or PREMIUM Internet access for less!
Join Juno today!  For your FREE software, visit:
http://dl.www.juno.com/get/web/.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 09:50:10 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Microsoft Mouse - Success!
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Martin

On Fri, 1 Mar 2002 17:50:10 -0800, "Martin G. Ramirez" <mramirez@LMU.EDU> wrote:

> mice I have are good (they have all been used on other systems), so it may
> be useful to note the info about the mouse I had earlier today that did NOT
> work with the LX and the one that DOES.  So, here's the info:

It may be a matter of power consumption.
The LX's serial port doesn't provide the same voltage and current as a
"normal" serial port. Thus the power which can be sucked off the port
is much much lower than the power you can get out of a PC serial port.

I will use your mouse info on my RS232-page if you agree
(http://www.daniel-hertrich.de/rs232 in the mouse section). Maybe this
helps others to avoid frustration.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 03:03:35 -0800
Reply-To:     hobchi@hotmail.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         hobchi <hobchi@YAHOO.COM>
Subject:      Re: Short battery life in an upgraded 200lx
Comments: To: Paulo Custodio <paulocustodio@YAHOO.COM>
In-Reply-To:  <HPLX-L%2002013119525215@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii

To those of yu that don want the
upgraded 96 MB unit, I'd be happee
to trade yu for a lesser unit or
otherwise kompensate yu for it.

regards,
yor pal al..............



__________________________________________________
Do You Yahoo!?
Yahoo! Sports - sign up for Fantasy Baseball
http://sports.yahoo.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 15:02:56 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: WWW/LX With Verizon's Mobile Office (USA)
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi David

On Fri, 1 Mar 2002 12:33:41 -0500, "David M. Solinas" <solinas@FASTMAIL.FM> wrote:

> HP200LX 8MB DS
> HP serial cable
> Audiovox CDM-9000 (tri-mode CDMA cell phone)
> Audiovox DIC-4000 data cable (mid-$40's on eBay)
> Ratshack 9-pin null-modem adapter and 9-pin M-M gender changer

> I connected the phone to the HP, and tried issuing "AT" commands
> via datacomm.  No luck, until I disabled the "lighton" TSR that let's
> me use Daniel 's excellent LCD light.  Then I fired up WWW/LX 2,

Did you have to _unload_ lighton, or was it enough to press the hotkey
to switch the light off?

> I hope someone finds this useful.  And thanks to D&A Soft for their
> excellent software!

In order to let others make use of your info, it would be great if you
allowed me to put it on http://www.daniel-hertrich.de/mob_hplx (along
with your email address, in case someone has questions).

Would that be okay for you?

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 10:21:45 -0800
Reply-To:     Alfred1520 <alfred1520@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Alfred1520 <alfred1520@YAHOO.COM>
Subject:      Re: SerialBert and something similar
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

What is you need?  I have a program that send a packet of data, receive the
looped back, check for error, and repeat indefinitely.  Email me for more
details if interested.

Best Regards,
Alfred Lee

-----Original Message-----
From: SM Ling <piclister@YAHOO.COM>
To: HPLX-L@UConnVM.UConn.Edu <HPLX-L@UConnVM.UConn.Edu>
Date: Friday, March 01, 2002 7:42 PM
Subject: SerialBert and something similar


>Frontier Test Equipment has some very powerful serial line testing
software,
>however they are too expensive.
>
>You can find them here:  http://www.fte.com/download.asp .
>
>The demo one is just a graphical display without real IO.  Anyone knows is
>there a cheaper software or freeware that can do simple BERT (Bit Error
Rate
>test) or pattern testing and detection?
>
>Cheers, Ling SM
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 15:37:59 -0500
Reply-To:     Ulrich Allen <Ulrich.Allen@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ulrich Allen <Ulrich.Allen@GMX.DE>
Subject:      WWW/LX+NOKIA6310+GPRS
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Now I am trying to get Www/lx connected to GPRS.
With Dial=3D*99# there appears CONNECTED on the screen
and NEGOCIATING LCP is started.
The end is: Can't establish PPP...
Is that the same problem which happend to the T68 some
time ago?
Uli

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 3 Mar 2002 08:00:21 +0800
Reply-To:     Oliver Chua <bud@MINDGATE.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Oliver Chua <bud@MINDGATE.NET>
Subject:      gsmssend translation
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

>3. GSMSSEND: an SMS sending tool which works without WWW/LX, but only
>for cable connections and SMS Text mode.

Daniel and friends,

Anyone kind enough to translate this program in english?  I for one would
like to try this program out since I've tried PDU before over cable without
success.

regards,

Oliver

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 19:37:11 -0800
Reply-To:     j_vanderstel@JUNO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John J Vander Stel <j_vanderstel@JUNO.COM>
Subject:      Re: Free AT compatible serial port peer-to-peer network software
              called Easy-Net
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Bob Christopher,

Thanks for volunteering to test Easy-Net.  I hope it ends up warranting a
place on SUPER.

Cheers!

John Vander Stel
Grand Rapids, Michigan
________________________________________________________________
GET INTERNET ACCESS FROM JUNO!
Juno offers FREE or PREMIUM Internet access for less!
Join Juno today!  For your FREE software, visit:
http://dl.www.juno.com/get/web/.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 19:54:48 -0500
Reply-To:     Bill Sprague <eugarps@ATTGLOBAL.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bill Sprague <eugarps@ATTGLOBAL.NET>
Subject:      Re: I'm doing something wrong..What?
In-Reply-To:  <NFBBLLFMJLBAFDKAJOBLMEACCBAA.eugarps@attglobal.net>
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Hi,

Never mind.... I got it!  Must have been some duplicate and corrupted files
giving the OL2LX software a haasle.  I manually purged a number of my
contacts and the conversion went smoothly.

Thanks,

Bill

-----Original Message-----
From: HPLX Mailing List [mailto:HPLX-L@UConnVM.UConn.Edu]On Behalf Of
Bill Sprague
Sent: Thursday, February 28, 2002 7:30 PM
To: HPLX-L@UConnVM.UConn.Edu
Subject: Re: I'm doing something wrong..What?


Update:

Just tried again and now I get: "OL2LX caused an invalid page fault in
module HPDB.DLL at 0177:01914abe."

I don't pretend to know Windoze.  That's why I have an HP200LX!

Thanks again.


Hi,

I've downloaded and installed OL2LX, installed it, updated VR, etc. to my
Libretto 110CT which is running Windoze 98 and Outlook 2000.

Here's MY problem (MY, because I'm sure there's nothing wrong with the
program... but rather, I'm sure it's something I'm doing wrong.)....

I keep getting and error message that says "Error: unable to load data into
phone.pdb from text file."

What am I doing wrong?

Thanks,

Bill

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 17:08:43 -0800
Reply-To:     Larry Mittell <lmittel@ATTGLOBAL.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Larry Mittell <lmittel@ATTGLOBAL.NET>
Subject:      OT: 128MB CF for $40
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

For those of you with a Fry's store near you, I picked up a
generically-labeled 128MB CF card at the Manhattan Beach store for $39.95.
My digital camera likes it just fine. It looked like that's the normal
price; i.e., it wasn't on sale so far as I know.

Larry Mittell

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 3 Mar 2002 03:02:19 +0100
Reply-To:     Alexander Schreiber <als@THANGORODRIM.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Alexander Schreiber <als@THANGORODRIM.DE>
Subject:      Re: MiniLinux (Was: Re:      Re: PC Card Partitions with 200LX ?)
Comments: To: Dario Draiman <dario200@MAIL.COM>
In-Reply-To:  <20020228232554.22540.qmail@mail.com>
Mime-Version: 1.0
Content-Type: text/plain; charset=iso-8859-1
Content-Transfer-Encoding: 8bit

On Thu, Feb 28, 2002 at 06:25:54PM -0500, Dario Draiman wrote:
> Anyone tried MiniLinux? It works under DOS but I don't remember if needs 286 or 386 to work.

The regular Linux kernel for Intel x86 needs at least a 386 CPU to run.
There is the ELKS (Embededable Linux Kernel Subset) project, which should
run on 8086, but I have no idea wether it will run on the HPLX or not.

Regards,
      Alex.
--
9./10. Mdrz 2002: 4. Chemnitzer Linux-Tag http://www.tu-chemnitz.de/linux/tag/
"I sense much NT in you. NT leads to Blue Screen, Blue Screen leads to
downtime, downtime leads to suffering. NT is the path to the Dark Side."
                                               -- Ellsworth, one small voice

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 2 Mar 2002 21:46:01 -0600
Reply-To:     Tim <palmtop@N-LINK.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tim <palmtop@N-LINK.COM>
Subject:      FS: KeyMate and Mini-Keyboard
In-Reply-To:  <5.0.2.1.2.20020302170307.0392cc60@pop1.attglobal.net>
MIME-Version: 1.0
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: 7bit

Hi All,

I'd like to sell:

KeyMate kit for the 200LX  - $60
"Great Quality" Mini-Keyboard - $60

Plus Shipping (we can work that out to be the online postal estimate plus
about $3 for me to wrap it SO WELL that you could drop it out of the second
story of a building!). You can "upgrade" your shipping to as much as you're
willing to pay....

Details:

The KeyMate is the adapter kit that allows you to use any keyboard w/ your
LX. It takes an internal 9 volt battery (not included.... I would, if I had
one in my gadget room), or the INCLUDED A/C adapter (looks like it's U.S.
voltage only and is really small). This kit also has an IR input that works
w/ WinCE devices (only) and the Thaddeus-provided disk w/ the LX driver.

The Mini-Keyboard is REALLY cool. It's about 3/4 sized, membrane-mechanism
KB w/ almost no use. Its big "draw" is the low current draw (sold to me by
the KeyMate developer as the lowest power-use KB he could find ... the box
says "Input Power: 5Vdc, 50mA"). The dimensions are listed in millimeters:
287(L) x 143(W) x 28 (H). I'll trust you to pull out your LX for the
conversion!

I used the combination once, prob. two-three years ago (when I bought it)
and then shelved it saying, "That's cool, I'll have to use that more often."
Well, I'm cleaning house and haven't used the combo and want them to go to a
good home.

The good news is that means they're "like new."

I'll respond to questions on or off the list, but direct email will work
fastest for me. I can accept PayPal [email there is: ttraymond@hotmail.com
so don't be surprised], but postal money orders are fine.

Thanks!!

--tim

PS. Operating on a standard "first come (in my inbox), first serve," since I
don't have an eBay-like "bid-server" on a website.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 3 Mar 2002 11:27:37 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      mail web interface
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends

I have found a universal web interface for email which might work on
the palmtop.
It is a derivate of the service mail2web.com.

Go to www.mail2pda.com and have a look. I just tried it with Netscape,
and the pages look as they could be displayed by HV. Only the URLs are
very long and thus might limit the usablilty.

Maybe Arachne/LX will support long URLs.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 3 Mar 2002 12:28:57 +0100
Reply-To:     Tamas Feher <etomcat@FREEMAIL.HU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tamas Feher <etomcat@FREEMAIL.HU>
Subject:      Re: PC Card Partitions with 200LX ?
MIME-Version: 1.0
Content-type: text/plain; charset=US-ASCII
Content-transfer-encoding: 7BIT

Hello,

>>Perhaps real partitions would work using Dubbs method, but I
>>have never tried to get it working.
>
>That's what I was thinking of.  He made a replacement for the
>INT 13H disk services. But I guess the original palmtop Minix
>was unstable.

No, the original stock Minix 2.0, which also comes as CD-inset in
the Tanenbaum's "Operating Systems" book, was the one crashing
on the palmtop.

R. L. Dubbs made his native partition experiment before Mack fixed
Minix for the palmtop. If there is a list of Minix files, which needed
to be modified to stabilize Minix on the 200LX, one could install
Minix in a native partition, patch it and then run it OK. Did Mack
Bagette tell us, which particular files were changed in Minix for
HPLX compliance? I have only seen ready-made installs for DOS-
guest partition.

However Dubb's method supposedly does not help in implementing
multi-partition flashcard support for 200LX, he said he was unable
to make a second partition visible.

I guess we could try to contact the Intel and Phoenix people, who
made the 200LX CPU / BIOS, and torture them to reveal some info
about multi-partition support issues.

By the way, what kind of multiple partitions did you try to put unto
the flashcard for 200LX experiment?
1., one primary DOS+ one extended DOS with logical drives inside
2., multiple primaries ?

I have a crazy idea: use a real laptop computer to prepare a
flashcard according to method 1., (primary DOS then extended
DOS partition + logical drives) and then manually delete only the
primary DOS partition with some hexa diskeditor.
Then check if the 200LX still sees the logical drive(s) inside the
extended DOS partition. If yes, you could try to put a non-DOS
partition into the empty space, where primary DOS part used to be
and utilize it for native Minix or ELKS or other OS which runs on
8086 (QNXv2, Xenix?)

Sincerely: Tamas Feher.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 3 Mar 2002 19:45:50 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Memory configurations
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

on http://www.daniel-hertrich.de/stuff

I have created a table with all possible memory configurations of 100LX
and 200LX models. I would like to add a column for the 700LX and one
for the 1000CX, but I don't know details about them. Could anyone who
knows these details please give me hints?
Is it correct that the 100LX never came out with 2 MB _on_board_
memory? (i.e. the 2MB models of the 100LX always had an 1 MB
daughterboard)?

Also, if you find errors in the table, please correct them!

Thanks
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 3 Mar 2002 11:37:54 -0800
Reply-To:     Gary Jacek <gary-jacek@SHAW.CA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Gary Jacek <gary-jacek@SHAW.CA>
Organization: @Shaw
Subject:      Re: Memory configurations (and EMM200/EMM240 for 5MB Palmtop)
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-version: 1.0
Content-type: text/plain; charset=us-ascii
Content-transfer-encoding: 7BIT

Hi Daniel

Your list of possible memory configurations reminded me of
something I have always wanted to try.  That is the EMM200
program on SUPER.  Unfortunately, my 200LX is the 5MB variety.

Has anyone gotten around to rewriting Hiroyuki Sekiya's
EMM200/EMM240
to support the 5 megabyte configuration of the palmtop?

Thanks
Gary

Daniel Hertrich wrote:
>
> Hi friends,
>
> on http://www.daniel-hertrich.de/stuff
>
> I have created a table with all possible memory configurations of 100LX
> and 200LX models.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 3 Mar 2002 21:58:18 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

An interesting (private) site with information about all HP calculators,
palmtops etc in German, with pictures:

http://www.hp-collection.org/hewlettpackard.htm

and especially:

http://www.hp-collection.org/hewlettpackard.htm#organizer

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 04:56:52 +0100
Reply-To:     Nathalie Bugeaud <tps-seti@WANADOO.FR>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nathalie Bugeaud <tps-seti@WANADOO.FR>
Subject:      Re: Question regarding Quick/LX
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

 >Norbert:
 >I tested Quick/LX and find it really good.

Quick/LX is the main reason why i use DOS-based editors to do e-mail.
Q: does it run on a WinCE J720?

 >However, after several problems came up:
 >- the 'starting/stop charging' message delayed to more then 30 seconds.
 >- 1-2-3 macros could not be stopped anymore.
 >I changed the TSR's position in AUTOEXEC.BAT with no success.

this has nothing to do with Quick/LX
you can also turn it off any time you want:
 -insert start-
If  you  press  Ctrl-Q  in any situation, other than immediately
after entering a word,  QUICK/LX  will  display  a  small  setup
status  window  that  will  show  the  text:  "Setup: QBlD". The
letters indicate whether certain features are enabled or not:
 * Q: QUICK/LX is enabled
   q: QUICK/LX is disabled (does not make any suggestions)
  -insert end-
Nathalie

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 10:37:32 +0100
Reply-To:     castrobarco@wol.es
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Josi A. de Castro" <castrobarco@YAHOO.COM>
Subject:      ArachneLX?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Please:
Wath is Arachne/LX?


-----Mensaje original-----
De: HPLX Mailing List [mailto:HPLX-L@UConnVM.UConn.Edu]En nombre de
Daniel Hertrich
Enviado el: domingo 3 de marzo de 2002 10:28
Para: HPLX-L@UConnVM.UConn.Edu
Asunto: mail web interface


Hi friends

I have found a universal web interface for email which might work on
the palmtop.
It is a derivate of the service mail2web.com.

Go to www.mail2pda.com and have a look. I just tried it with Netscape,
and the pages look as they could be displayed by HV. Only the URLs are
very long and thus might limit the usablilty.

Maybe Arachne/LX will support long URLs.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 21:25:49 +1100
Reply-To:     Russell Hemery <rhemery@POWERUP.COM.AU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russell Hemery <rhemery@POWERUP.COM.AU>
Subject:      Eddie archive
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

At 01:52 PM 01/03/02 -0500, you wrote:
>I'd be willing to host them on my site. I finally got around to putting up
my linux box and setting up dynamic dns so that it's available. So far
comcast is not blocking ftp (they do block http! the bastards...). I got a
few gigabytes I can spare.
>
>
>
>> Martin Bergvill

Hi all

Just an idea.. I dont know how many CD's are for the eddie archive but what
about using Morpheus to distribute the files if there are too many for one
person on the list to hold them available online. That way there could be a
web page listing the files and where available. For those that dont know
Morpheus is like napster but all sorts of files distributed on many peoples
computers.

I have a couple of gig I could spare for this and cable so online all the
time.

Cheers

Russell

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 21:45:07 +1100
Reply-To:     Russell Hemery <rhemery@POWERUP.COM.AU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russell Hemery <rhemery@POWERUP.COM.AU>
Subject:      Voltage of new Energiser lithiums
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Hi all

I was wondering if anyone else on the list has tried the "new" E2 Energiser
photo lithiums? The silver blue packaging thats supposed to replace the
"old" red tops.

This morning I checked the voltage and got an incredible shock. My LX said
the voltage was 3.22 volts after about 10 hours of use. I removed them and
checked the individual battery's voltages after 12 hours rest out of the
palmtop with my multimeter and they register 1.72 volts a piece!!!!!!  I
did not check the voltages before using these battery's but the labelling
says 1.5 volts.  I want to know if there is any knowledge on the list as to
how this much overvoltage might affect the LX or if it is designed to
handle this overage. Also if anyone has similar experiences or if these
particular batteries are a "super set".

TIA

Russell

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 14:05:40 +0100
Reply-To:     hpstaber@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         HP Staber <hpstaber@COMPUSERVE.COM>
Subject:      Re: Question regarding Quick/LX
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Nathalie Bugeaud wrote:
>
> Quick/LX is the main reason why i use DOS-based editors to do e-mail.
> Q: does it run on a WinCE J720?

It should run although I have not yet tried. However PalEdit is very
slooow on the J720 so the overall interest in using both PE and
Quick/LX on the J720 is low.

HP Staber/Salzburg

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 14:23:41 +0100
Reply-To:     Michel Bel <michel.bel@ZONNET.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michel Bel <michel.bel@ZONNET.NL>
Subject:      How would I upgrade by piggybacking?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Just a brainwave - I might just try it someday.
Assuming I have a few 2MB memory chips like ones in the newer 2MB 200LX's.
(From a large older16/32 MB SIMM..)
IIRC one could piggyback one chip on the other. Now to recognise the
extension I would assume that one only has to keep the chips CAS floating
and connect it to the LCAS at the extension pins/solder pads. Is this
correct? And even sillier, piggyback one more, and connect the other CAS to
UCAS.
Please tell me , right or wrong?

Michel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 07:23:06 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: Microsoft Mouse - Success!
MIME-Version: 1.0
Content-Type: text/plain

I, too, can report success. On my way home Friday, I stopped off at my local
Value Village resale shop, and they happened to have an old serial mouse for
$1. I got it and tried it out later Friday evening (about the same time
Martin got his mouse to work!). It still didn't work, but its test program
showed that the button clicks were recognized, but the pointer didn't move.
I double-checked the port settings in Setup, and they were OK. I then
thought to check the port in Buddy -- I had the serial port locked in Buddy.
I unlocked it, and the mouse worked. My Appoint pen mouse also works, but a
clone mouse that I have rebuilt as the circuit for a track ball here at work
doesn't work (although the buttons are also recognized with this one). So,
there do appear to be differences based on the mouse electronics. The clone
mouse that works for me has a small circuit board, while the one that
doesn't has a full sized board with nore discrete components. It also has
larger phototransistors on the sensor wheels.

So, if your mouse doesn't work, make sure the serial port is _on_ and
_unlocked_. Even then, you might need to try a different mouse.

BTW, I'm loading my mouse driver in Config.sys, and it works both in
straight DOS and in DOS run from the Sys manager. It also works in Windows
3.0 using the standard Windows mouse.drv.

Bob

P.S. The Appoint pen mouse is a handy one to use with the LX, as the ball is
on the end of a pen-like stylus. You can use it on small surfaces such as a
pad or paper, or even your pants leg, as the ball is more exposed. It costs
only $10 plus shipping from California Digital. The only drawback is that it
is pink and says "Barbie" on it -- it comes with the "Barbie PC Fashion
Design & Color" software package.

-----Original Message-----
From: Martin G. Ramirez [mailto:mramirez@LMU.EDU]
Sent: Friday, March 01, 2002 7:50 PM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Microsoft Mouse - Success!


LXer's,

I have good news to report about the problem with the Microsoft mouse, the
details of which I reported earlier today (see below).  Well, I just went
to drawer full of Microsoft serial mice in my lab and picked out another
and connected it up as below - and it works!!!   As far as I know, all the
mice I have are good (they have all been used on other systems), so it may
be useful to note the info about the mouse I had earlier today that did NOT
work with the LX and the one that DOES.  So, here's the info:

        + mouse that would not work - "Serial - Mouse Port Compatible
Mouse", part
no. 55305

        + mouse that does work - "Serial Mouse 2.0A", part no. 50674

Hope this info helps,
Martin G. Ramirez

<snip>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 09:35:28 -0500
Reply-To:     Dario Draiman <dario200@MAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dario Draiman <dario200@MAIL.COM>
Subject:      Re: ArachneLX?
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit
MIME-Version: 1.0

> Please:
> Wath is Arachne/LX?
>

It's a DOS based web browser. The author is supposedly working to develop a LX version.

>
> -----Mensaje original-----
> De: HPLX Mailing List [mailto:HPLX-L@UConnVM.UConn.Edu]En nombre de
> Daniel Hertrich
> Enviado el: domingo 3 de marzo de 2002 10:28
> Para: HPLX-L@UConnVM.UConn.Edu
> Asunto: mail web interface
>
>
> Hi friends
>
> I have found a universal web interface for email which might work on
> the palmtop.
> It is a derivate of the service mail2web.com.
>
> Go to www.mail2pda.com and have a look. I just tried it with Netscape,
> and the pages look as they could be displayed by HV. Only the URLs are
> very long and thus might limit the usablilty.
>
> Maybe Arachne/LX will support long URLs.
>
> GTX
> daniel
>
> --
> http://www.daniel-hertrich.de/contact
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

--

_______________________________________________
Sign-up for your own FREE Personalized E-mail at Mail.com
http://www.mail.com/?sr=signup

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 09:39:31 -0500
Reply-To:     Dario Draiman <dario200@MAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dario Draiman <dario200@MAIL.COM>
Subject:      Re: How would I upgrade by piggybacking?
Comments: To: michel.bel@ZONNET.NL
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit
MIME-Version: 1.0

Check out http://www.upl.cs.wisc.edu/~orn/tech/200lx.html

-----Original Message-----
From: Michel Bel <michel.bel@ZONNET.NL>
Date:         Mon, 4 Mar 2002 14:23:41 +0100
To: HPLX-L@UConnVM.UConn.Edu
Subject:      How would I upgrade by piggybacking?


> Just a brainwave - I might just try it someday.
> Assuming I have a few 2MB memory chips like ones in the newer 2MB 200LX's.
> (From a large older16/32 MB SIMM..)
> IIRC one could piggyback one chip on the other. Now to recognise the
> extension I would assume that one only has to keep the chips CAS floating
> and connect it to the LCAS at the extension pins/solder pads. Is this
> correct? And even sillier, piggyback one more, and connect the other CAS to
> UCAS.
> Please tell me , right or wrong?
>
> Michel
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

--

_______________________________________________
Sign-up for your own FREE Personalized E-mail at Mail.com
http://www.mail.com/?sr=signup

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 16:59:46 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: How would I upgrade by piggybacking?
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

What you suggest is exactly the way it used to be done on Atari ST boards
(although if possible and present a separate RAS should also be used) so
yes, you should be correct.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 11:02:24 -0500
Reply-To:     Steve <novosad@SERVER030.FWB.SAIC.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Steve <novosad@SERVER030.FWB.SAIC.COM>
Subject:      Re: PC Card Partitions with 200LX ?
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Tamas Feher wrote:

> I guess we could try to contact the Intel and Phoenix people, who
> made the 200LX CPU / BIOS, and torture them to reveal some info
> about multi-partition support issues.

  Actually, I think the Developer's Guide says that it is
Microsoft's CardBIOS specification and was written by HP as
CardDrv.  If someone wants to search a Microsoft developer
site for "CARDDRV BIOS Interface" and provide a link here,
that would be a start.  However, HP modified the code, and
it's in ROM, so I'm not sure what that would tell you.

> By the way, what kind of multiple partitions did you try to put unto
> the flashcard for 200LX experiment?
> 1., one primary DOS+ one extended DOS with logical drives inside
> 2., multiple primaries ?

  When I tried, I did #1.  At which point the card was not
recognized at all.

Steve

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 09:59:51 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: PC Card Partitions with 200LX ?
MIME-Version: 1.0
Content-Type: text/plain

The LXREF documentation (mentioned a few days ago) contains the following:

<begin quotes>
12. DOS
Disk Device Drivers
Plug-in Card Disk Driver (drive A)

The plug-in card disk driver is Microsoft CARDDRV with extensions.

CARDDRV uses the CardBIOS layer to actually read and write data, learn of
card changes, etc. ...CARDDRV uses drive letters A and B. Drive letter B is
used for the second partition on a plug-in card, but partitions of this sort
are never used in practice so drive B is never used in practice. This is not
a loss since drive letter B needed to be used up somehow so that the RAM
disk, which acts like the palmtop's hard disk, would be the industry
standard hard disk drive C.

If a two-slot version of the HP palmtop had ever been made, it is likely
that drive B would have been changed to be used for that slot.


14. Hardware Overview
Introduction

10. A CPU bus interface and memory controller. ...can support up to five
ROM/RAM devices and 2 plug-in PCMCIA memory cards, and I/O cards.
<end quotes>

Interesting but confusing. Just what "drive letter B needed to be used up
somehow" means and how it was done, I hvae no idea. It does suggest that
there is a potential to get a second partition active.

Bob


-----Original Message-----
From: Steve [mailto:novosad@SERVER030.FWB.SAIC.COM]
Sent: Monday, March 04, 2002 10:02 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: PC Card Partitions with 200LX ?


Tamas Feher wrote:

> I guess we could try to contact the Intel and Phoenix people, who
> made the 200LX CPU / BIOS, and torture them to reveal some info
> about multi-partition support issues.

  Actually, I think the Developer's Guide says that it is
Microsoft's CardBIOS specification and was written by HP as
CardDrv.  If someone wants to search a Microsoft developer
site for "CARDDRV BIOS Interface" and provide a link here,
that would be a start.  However, HP modified the code, and
it's in ROM, so I'm not sure what that would tell you.

> By the way, what kind of multiple partitions did you try to put unto
> the flashcard for 200LX experiment?
> 1., one primary DOS+ one extended DOS with logical drives inside
> 2., multiple primaries ?

  When I tried, I did #1.  At which point the card was not
recognized at all.

Steve

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 11:27:54 -0600
Reply-To:     John McCaskill <jmccask@POWERCHOKES.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John McCaskill <jmccask@POWERCHOKES.COM>
Subject:      PC Card Partitions with 95LX, 100LX, 200LX
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Back in the early 95LX days, the ACE 2 mB DoubleCard had a funky format. I
don't remember all the details, but you had to boot the card and it then had
a driver which read the compressed data on the card. The original card was
"A" but became "B" after bootup. The compressed format card was then "A" and
the RAM drive "C". You could read either "A" or "B" from filer. Or, I could
be hallucinating. It was a long time ago. I also think I recall that "D" was
also part of the RAM drive where you could copy a new config.sys.

John

-----Original Message-----
From: HPLX Mailing List [mailto:HPLX-L@UConnVM.UConn.Edu]On Behalf Of
Feldman, Robert
Sent: Monday, March 04, 2002 11:00 AM
To: HPLX-L@UConnVM.UConn.Edu
Subject: Re: PC Card Partitions with 200LX ?


The LXREF documentation (mentioned a few days ago) contains the following:

<begin quotes>
12. DOS
Disk Device Drivers
Plug-in Card Disk Driver (drive A)

The plug-in card disk driver is Microsoft CARDDRV with extensions.

CARDDRV uses the CardBIOS layer to actually read and write data, learn of
card changes, etc. ...CARDDRV uses drive letters A and B. Drive letter B is
used for the second partition on a plug-in card, but partitions of this sort
are never used in practice so drive B is never used in practice. This is not
a loss since drive letter B needed to be used up somehow so that the RAM
disk, which acts like the palmtop's hard disk, would be the industry
standard hard disk drive C.

If a two-slot version of the HP palmtop had ever been made, it is likely
that drive B would have been changed to be used for that slot.


14. Hardware Overview
Introduction

10. A CPU bus interface and memory controller. ...can support up to five
ROM/RAM devices and 2 plug-in PCMCIA memory cards, and I/O cards.
<end quotes>

Interesting but confusing. Just what "drive letter B needed to be used up
somehow" means and how it was done, I hvae no idea. It does suggest that
there is a potential to get a second partition active.

Bob


-----Original Message-----
From: Steve [mailto:novosad@SERVER030.FWB.SAIC.COM]
Sent: Monday, March 04, 2002 10:02 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: PC Card Partitions with 200LX ?


Tamas Feher wrote:

> I guess we could try to contact the Intel and Phoenix people, who
> made the 200LX CPU / BIOS, and torture them to reveal some info
> about multi-partition support issues.

  Actually, I think the Developer's Guide says that it is
Microsoft's CardBIOS specification and was written by HP as
CardDrv.  If someone wants to search a Microsoft developer
site for "CARDDRV BIOS Interface" and provide a link here,
that would be a start.  However, HP modified the code, and
it's in ROM, so I'm not sure what that would tell you.

> By the way, what kind of multiple partitions did you try to put unto
> the flashcard for 200LX experiment?
> 1., one primary DOS+ one extended DOS with logical drives inside
> 2., multiple primaries ?

  When I tried, I did #1.  At which point the card was not
recognized at all.

Steve

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

John

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 19:55:39 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      ANN: Syslog 1.0
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Attention Linux freaks:

I have written a little utility called "syslog" which writes messages
into a system-wide central log file (like /var/log/messages ;-) ).

Simply use it in a batch file like this

c:\bin\syslog.exe "Starting Software Carousel"

and in the logfile c:\syslog.txt appears a line with a time stamp and
the message "Starting Software Carousel".

This way you can collect all info from your system batch files, like
nightly backups, or whatever. You can of course also log online runs
with WWW/LX (although WWW/LX comes already with a logging feature ;-)
)...

Once the syslog file gets too large, simply delete it or zip it to
another drive, and the next time syslog is called it will create a new
file.

http://www.daniel-hertrich.de/download

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 20:03:58 +0100
Reply-To:     Michael Lennartz <lennartz-mi@GMX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Lennartz <lennartz-mi@GMX.NET>
Subject:      Just a question
Mime-Version: 1.0
Content-Type: text/plain; charset="ISO-8859-1"
Content-Transfer-Encoding: quoted-printable

Hallo all,

is there anybody, who tried to use WWW/LX and POST/LX (and Arachne)
on a Olivetti Quaderno XT (this with a 20 MByte HD) or the identical
Highscreen Laptalk?



Mit freundlichem Gru=DF / Regards / Saluton

Michael Lennartz
lennartz-mi@gmx.net
Fax: +49 89 244 34 52 57

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 14:14:34 -0500
Reply-To:     "Striegel, Alan" <Striegel@PIOS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Striegel, Alan" <Striegel@PIOS.COM>
Subject:      Re: PC Card Partitions with 95LX, 100LX, 200LX
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

Well, that was using Stacker software.  ACE had a version of it installed on
the RAM cards that let you mount the (hidden) STACVOL.ACE file for roughly
double the native storage capacity.

But that did not have any more than a single partition.  In fact, since it
was a RAM card, it could not literally be partitioned as a Compact Flash or
ATA Flash card can.

Alan Striegel

>From: John McCaskill [mailto:jmccask@POWERCHOKES.COM]
>Sent: Monday, March 04, 2002 12:28 PM
>
>Back in the early 95LX days, the ACE 2 mB DoubleCard had a funky format. I
>don't remember all the details, but you had to boot the card and it then
had
>a driver which read the compressed data on the card. The original card was
>"A" but became "B" after bootup. The compressed format card was then "A"
and
>the RAM drive "C". You could read either "A" or "B" from filer. Or, I could
>be hallucinating.
>...
>Bob

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 20:19:57 +0100
Reply-To:     "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Organization: www.Compuseum.de
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

> http://www.hp-collection.org/hewlettpackard.htm

Nice collection, indeed :-)

BTW: So there are more differences between the 200lx and the 700lx: The
200lx has a 8088 CPU and the 700lx has the 80186.

regards,
Oliver

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 12:44:25 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

No, the 200LX also has an 80186.

-----Original Message-----
From: Oliver W. Leibenguth [mailto:Oliver@COMPUSEUM.DE]
Sent: Monday, March 04, 2002 1:20 PM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: HP collection


> http://www.hp-collection.org/hewlettpackard.htm

Nice collection, indeed :-)

BTW: So there are more differences between the 200lx and the 700lx: The
200lx has a 8088 CPU and the 700lx has the 80186.

regards,
Oliver

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 13:43:31 -0600
Reply-To:     "David R. Birch" <dbirch@WI.RR.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "David R. Birch" <dbirch@WI.RR.COM>
Subject:      Re: HP collection
Comments: To: "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

"Oliver W. Leibenguth" wrote:
>
> > http://www.hp-collection.org/hewlettpackard.htm
>
> Nice collection, indeed :-)
>
> BTW: So there are more differences between the 200lx and the 700lx: The
> 200lx has a 8088 CPU and the 700lx has the 80186.
>
> regards,
> Oliver

AFAIK, the processor in the 200LX and the 700LX is the same, they
both emulate the 80186. I think the main difference between the
two is that the 700LX lacks the software in ROM, all it has is
the DOS 5.0 OS.

David

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 21:21:31 +0100
Reply-To:     Michel Bel <michel.bel@ZONNET.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michel Bel <michel.bel@ZONNET.NL>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

----- Original Message -----
From: "David R. Birch" <dbirch@WI.RR.COM>
> AFAIK, the processor in the 200LX and the 700LX is the same, they
> both emulate the 80186. I think the main difference between the
> two is that the 700LX lacks the software in ROM, all it has is
> the DOS 5.0 OS.

Slightly wrong again:

The 'Hornet' chip in the 100, 200 and 700 is an extended chip with a 186 CPU
core plus extra's such as serial i/o ports, pcmcia hw drivers, LCD driver
etc all onchip. It does not 'emulate' an 186.  It is really a '186 PC on a
chip', just needing some line drivers for serial I/O, and a rom to boot from
to work as a pc ( plus power of course...). The 700 has an extended 200LX
rom, with SMS and FAX sw as well, plus a second PCMCIA slot (strictly I/O
wired)..

Michel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 15:49:50 -0500
Reply-To:     Eduardo Seudonimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudonimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: HP collection
Comments: To: "David R. Birch" <dbirch@WI.RR.COM>
In-Reply-To:  <3C83CE63.D0798430@wi.rr.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: quoted-printable

>AFAIK, the processor in the 200LX and the 700LX is the same, they
> both emulate the 80186. I think the main difference between the
> two is that the 700LX lacks the software in ROM, all it has is
> the DOS 5.0 OS.

I think the 1000CX is the software-less one. the 700 is that one with =
the phone docking cradle.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 23:55:09 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: Microsoft Mouse - Success!
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> The Appoint pen mouse is a handy one to use with the LX, as the
> ball is on the end of a pen-like stylus. You can use it on small
> surfaces such as a pad or paper, or even your pants leg, as the
> ball is more exposed. It costs only $10 plus shipping from
> California Digital.

Thanks a lot for that hint. You might have added the URL and the fact that
to find this mouse one has to look under software:
        http://www.cadigital.com/software.htm
One more point:
This only distributor still offering official CP/M licences for sale is one
of those nutters who only show you a blank screen unless you invite viruses
and popups by not disabling Javascript.

Axel

P.S: And sorry Robert, I didn't mean to impolitely mail and post, I just
forgot (again) to alter the list's default.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 00:05:33 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> I think the main difference between the
> two is that the 700LX lacks the software in ROM, all it
> has is the DOS 5.0 OS.

Quite the opposite is true it has a lot of phone specific software on top
of what the 200 has, fax and SMS mainly - although it seems to me that
those programs are less well written and more carelessly and incompletely
documented than the original HP ones.

Axel

P.S: Did it again, sorry - blame it on my advanced years, please.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 15:30:11 -0500
Reply-To:     theise@netins.net
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: Microsoft Mouse - Success!

Feldman, Robert writes:

> P.S. The Appoint pen mouse is a handy one to use with the LX, as the ball is
> on the end of a pen-like stylus. You can use it on small surfaces such as a
> pad or paper, or even your pants leg, as the ball is more exposed. It costs
> only $10 plus shipping from California Digital. The only drawback is that it
> is pink and says "Barbie" on it -- it comes with the "Barbie PC Fashion
> Design & Color" software package.

This is *hilarious*!  You ought to get an action pic to post on SUPER.

--
Theodore W. Heise   <theise@netins.net>    West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 18:36:41 -0500
Reply-To:     Dario Draiman <dario200@MAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dario Draiman <dario200@MAIL.COM>
Subject:      Re: HP collection
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: 7bit
MIME-Version: 1.0

David, you are confusing the 700LX with the 1000LX. The HP1000LX is the one having only DOS and no rom goodies.

-----Original Message-----
From: "David R. Birch" <dbirch@WI.RR.COM>
Date:         Mon, 4 Mar 2002 13:43:31 -0600
To: HPLX-L@UConnVM.UConn.Edu
Subject:      Re: HP collection


> "Oliver W. Leibenguth" wrote:
> >
> > > http://www.hp-collection.org/hewlettpackard.htm
> >
> > Nice collection, indeed :-)
> >
> > BTW: So there are more differences between the 200lx and the 700lx: The
> > 200lx has a 8088 CPU and the 700lx has the 80186.
> >
> > regards,
> > Oliver
>
> AFAIK, the processor in the 200LX and the 700LX is the same, they
> both emulate the 80186. I think the main difference between the
> two is that the 700LX lacks the software in ROM, all it has is
> the DOS 5.0 OS.
>
> David
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

--

_______________________________________________
Sign-up for your own FREE Personalized E-mail at Mail.com
http://www.mail.com/?sr=signup

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 15:39:39 -0800
Reply-To:     Ian Butler <ianb@HPLX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ian Butler <ianb@HPLX.NET>
Subject:      Re: HP collection
Comments: To: Dario Draiman <dario200@MAIL.COM>
In-Reply-To:  <20020304233641.26966.qmail@mail.com>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Mon, 4 Mar 2002, Dario Draiman wrote:

> David, you are confusing the 700LX with the 1000LX. The HP1000LX is
> the one having only DOS and no rom goodies.

That's the 1000CX, not the 1000LX.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 20:09:44 -0500
Reply-To:     Owen Samuelson <owensamuelson@COX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Owen Samuelson <owensamuelson@COX.NET>
Subject:      Re: Voltage of new Energiser lithiums
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

That's about what I've gotten (3.2 V), using these batteries. When I sent in
my palmtop for upgrade from Thaddeus, they returned it with a set of these
installed. I've never had any problems using them.
Owen

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 21:37:25 -0500
Reply-To:     steve@CARDERFAMILY.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Steve Carder <steve@CARDERFAMILY.NET>
Subject:      Re: Voltage of new Energiser lithiums
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

> This morning I checked the voltage and got an incredible shock. My LX =
said
> the voltage was 3.22 volts

So, 3.22 volts is enough to give you an incredible shock <g>.

 Steve Carder <steve@carderfamily.net>
 PGP public key on the server at http://pgp.mit.edu

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 02:53:32 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: ANN: Syslog 1.0
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Daniel Hertrich wrote:
> I have written a little utility called "syslog" which writes messages
> into a system-wide central log file (like /var/log/messages ;-) ).
>
> Simply use it in a batch file like this
>
> c:\bin\syslog.exe "Starting Software Carousel"
>
> and in the logfile c:\syslog.txt appears a line with a time stamp and
> the message "Starting Software Carousel".

I've been doing this for a long time with the following Rexx
program.  Call it from BAT files like:

rexx ts Starting Software Carousel


/** TS.Rex - TimeStamp **/
parse value date('S')time()date('W') with 3 yymm 7 dd 9 hhmm 14 . 17 dow 19 .
file = 'C:\TS'yymm'.LOG'
if arg(1) <> '' then call lineout file, dow dd hhmm space(arg(1))
call lineout file  /* close file */
exit


Besides being a nice language by itself Rexx can also act a
super utility to make your BAT files more useful.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 03:51:20 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      T2T drivers
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

I just had a 2M 200LX I bought used, upgraded to 32M and double
speed.  This is now my primary LX and my single speed 32M 200LX
will become its backup.  (With my original 200LX-4M backing them
both up.)

I noticed that the software drivers included with the upgrade
weren't the very latest. (Hey Hal, Thaddeus should ship the
latest drivers with an upgrade.)

I got the latest drivers from Mack at Times2Tech to be sure I
was up to date.  Here's a DIR listing of their files so you can
see if you have the most recent ones on your T2T upgraded LX...

Cheers... Russ

----------------------------------
 Volume in drive C is Times2_Tech
 Directory of d:

RDT2T    EXE      2391 10-21-00  10:53a
RDT2T    TXT      4780 04-01-99  12:40a
RDSWAP   EXE       942 10-14-98  12:59p
LICENSE  TXT      6319 04-13-96   7:52p
CONFIG   T2T       180 06-03-99   9:53a
        7 file(s)      14612 bytes
----------------------------------
 Volume in drive C is Times2_Tech
 Directory of d:

SPD31    EXE      3100 03-14-01  11:38p
SPD31S   SYS       585 04-19-01   7:48a
SPD31    TXT      8332 03-14-01  10:33p
SPDALRM  TSR       196 01-27-00   7:13a
CHRG     COM        85 12-16-99   1:38p
README   TXT      1901 02-19-99   9:09a
LICENSE  TXT      6319 04-13-96   7:52p
        9 file(s)      20518 bytes
----------------------------------
 Volume in drive C is Times2_Tech
 Directory of d:

TREMM    EXE      4515 10-28-00   8:28a
TREMM    TXT      5547 03-31-99  11:32p
INSTEMM  EXE     15269 10-18-00   4:08p
TRCHECK  COM      1290 08-17-98   8:53a
TRCHECK  TXT      1945 03-31-99  11:33p
        7 file(s)      28566 bytes
----------------------------------

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 11:57:18 +0800
Reply-To:     SM Ling <piclister@yahoo.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         SM Ling <piclister@YAHOO.COM>
Subject:      200lx and handheld scanner
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

The archive and FAQ do not have this information.  IIRC serial handheld
scanner used to be quite popular, has anyone tried one with 200LX?  This
type of scanner seem impossible to be seem nowsaday, does anyone know where
can get one?

Cheers, Ling SM

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 23:13:09 -0500
Reply-To:     Dario Draiman <dario200@MAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dario Draiman <dario200@MAIL.COM>
Subject:      Problems with Mocha PPP
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit
MIME-Version: 1.0

Does anyone have it working? I've set up a 38400 bps connection but it's extremely slow and doesn't complete the transmissions. Other speeds doesn't work at all. The configuration is the one at Daniel's page.

Dario

--

_______________________________________________
Sign-up for your own FREE Personalized E-mail at Mail.com
http://www.mail.com/?sr=signup

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Mar 2002 23:36:56 -0500
Reply-To:     Dario Draiman <dario200@MAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dario Draiman <dario200@MAIL.COM>
Subject:      Spanish spelling tool (Ortografo)
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit
MIME-Version: 1.0

For those of you being interested in spanish language, here is a "Ortografo" that work
under DOS. I tried to make it work on the LX but it complains that need to be executed from a hard drive (even when I use assign, subst or lxsubst).

Any ideas?

http://www.mirror.ac.uk/collections/hensa-micros/local/msdos/languages/ort.zip


Dario

--

_______________________________________________
Sign-up for your own FREE Personalized E-mail at Mail.com
http://www.mail.com/?sr=signup

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 09:58:06 +0100
Reply-To:     Michel Bel <michel.bel@ZONNET.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michel Bel <michel.bel@ZONNET.NL>
Subject:      Re: How would I upgrade by piggybacking?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Dario wrote

> Check out http://www.upl.cs.wisc.edu/~orn/tech/200lx.html
to mine
> Subject:      How would I upgrade by piggybacking?
>
Sorry, doesn't help. Different onboard chip.. I want to solder one on top of
the 2MB onboard chip..

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 04:42:07 -0800
Reply-To:     hobchi@hotmail.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         hobchi <hobchi@YAHOO.COM>
Subject:      Stacka
In-Reply-To:  <HPLX-L%2002011909213939@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii

Listen up...
OK so none of youse guys like staka no more
kause y'all got BIG 220-512+ flash drives.
However it still good for the C: and F: drive
for those that got upgraded 32/64 n even
96MB C/Fs   Reelee

yor pal al............................


=====
.
       o__
      _.>/)_
     (_) \(_)
Woman, that's warm...
  Semper Mobilus

__________________________________________________
Do You Yahoo!?
Try FREE Yahoo! Mail - the world's greatest free email!
http://mail.yahoo.com/

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 07:48:47 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: Spanish spelling tool (Ortografo)
Comments: To: Dario Draiman <dario200@MAIL.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

The readme text says that it won't work on floppies, partitioned hard drives
or removable disks ("Nota: El programa no trabaja en disquetes, discos duros
compartidos o discos removibles.") From the installation instructions, it
looks like the program will only work if installed on Drive C: .

It does look like an interesting program, though.

Bob

-----Original Message-----
From: Dario Draiman [mailto:dario200@MAIL.COM]
Sent: Monday, March 04, 2002 10:37 PM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Spanish spelling tool (Ortografo)


For those of you being interested in spanish language, here is a "Ortografo"
that work
under DOS. I tried to make it work on the LX but it complains that need to
be executed from a hard drive (even when I use assign, subst or lxsubst).

Any ideas?

http://www.mirror.ac.uk/collections/hensa-micros/local/msdos/languages/ort.z
ip


Dario

--

_______________________________________________
Sign-up for your own FREE Personalized E-mail at Mail.com
http://www.mail.com/?sr=signup

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 10:18:36 -0500
Reply-To:     Bruce_Martin@MANULIFE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bruce Martin <Bruce_Martin@MANULIFE.COM>
Subject:      Re: ANN: Syslog 1.0
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

>> I have written a little utility called "syslog" which writes messages
>> into a system-wide central log file (like /var/log/messages ;-) ).
>>
>> Simply use it in a batch file like this
>>
>> c:\bin\syslog.exe "Starting Software Carousel"
>>
>> and in the logfile c:\syslog.txt appears a line with a time stamp and
>> the message "Starting Software Carousel".
>>
> I've been doing this for a long time with the following Rexx
> program.  Call it from BAT files like:
>
> rexx ts Starting Software Carousel
>
I have a 5K utility called NOW.EXE (I think it may be from PC Magazine)
which allows me to do this in 2 batch file lines:

echo now >> startup.log
echo Starting Software Carousel >> startup.log

Bruce in Toronto

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 16:24:58 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

... well, I know, there are many. ;-)

But I need a special one.

I am looking for the English word for the German "Werksstudent", i.e. a
person, who is still studying at a university, but who works for a
company some hours a month, to make experiences in the job, to get a
little bit of money (not much), to be able to begin his career already
during the studies.

Thanks a lot
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 09:45:56 -0600
Reply-To:     TomSalwasser@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tom Salwasser <TomSalwasser@COMPUSERVE.COM>
Subject:      Re: OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Daniel,

One word for this is intern.

Monica Lewinski was a White House intern a few years ago...

Regards,
TomSalwasser

> I am looking for the English word for the German "Werksstudent", i.e. a
> person, who is still studying at a university, but who works for a
> company some hours a month, to make experiences in the job, to get a
> little bit of money (not much), to be able to begin his career already
> during the studies.
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 10:52:20 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: Looking for an English word
In-Reply-To:  <HPLX-L%2002030510222359@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Sounds like 'Intern'. (U.S. English).=20


intern =20
.
.

6. Chiefly U.S.a student or recent graduate receiving practical training =
in a working environment.


internship (`=80nt=87:n=89=80p)  n. U.S. and Canadian. the position of =
being an intern or the period during which a person is an intern.




> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@uconnvm.uconn.edu]On Behalf Of
> Daniel Hertrich
> Sent: Tuesday, March 05, 2002 9:25 AM
> To: HPLX-L@uconnvm.uconn.edu
> Subject: OT: Looking for an English word
>=20
>=20
> ... well, I know, there are many. ;-)
>=20
> But I need a special one.
>=20
> I am looking for the English word for the German "Werksstudent", i.e. =
a
> person, who is still studying at a university, but who works for a
> company some hours a month, to make experiences in the job, to get a
> little bit of money (not much), to be able to begin his career already
> during the studies.
>=20
> Thanks a lot
> daniel
>=20
> --
> http://www.daniel-hertrich.de/contact
>=20
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 10:52:20 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: Spanish spelling tool (Ortografo)
In-Reply-To:  <D8020D6F0DB8D211B99A0008C7C59CFE0FD8F735@cormails1.jdedwards.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

I remember using norton disk editor on programs to change A: to C: and =
such to bypass these issues.=09

> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@uconnvm.uconn.edu]On Behalf Of
> Feldman, Robert
> Sent: Tuesday, March 05, 2002 9:49 AM
> To: HPLX-L@uconnvm.uconn.edu
> Subject: Re: Spanish spelling tool (Ortografo)
>=20
>=20
> The readme text says that it won't work on floppies, partitioned=20
> hard drives
> or removable disks ("Nota: El programa no trabaja en disquetes,=20
> discos duros
> compartidos o discos removibles.") From the installation instructions, =
it
> looks like the program will only work if installed on Drive C: .
>=20
> It does look like an interesting program, though.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 09:01:15 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

I also suggested "intern" to Daniel, but I still feel it's not quite the
right word. Since the program is called "work-study", is a "work-student"
(not a correct English construction) an "intern" -- I don't think so, but I
can't think of the correct term.

Bob

-----Original Message-----
From: Tom Salwasser [mailto:TomSalwasser@COMPUSERVE.COM]
Sent: Tuesday, March 05, 2002 9:46 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: OT: Looking for an English word


Daniel,

One word for this is intern.

Monica Lewinski was a White House intern a few years ago...

Regards,
TomSalwasser

> I am looking for the English word for the German "Werksstudent", i.e. a
> person, who is still studying at a university, but who works for a
> company some hours a month, to make experiences in the job, to get a
> little bit of money (not much), to be able to begin his career already
> during the studies.
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 10:11:53 -0600
Reply-To:     TomSalwasser@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tom Salwasser <TomSalwasser@COMPUSERVE.COM>
Subject:      OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

My Collins dictionary says:

6) Chiefly US, a student or recent graduate receiving practical training in a
working environment.

Tom

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 10:14:00 -0600
Reply-To:     TomSalwasser@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tom Salwasser <TomSalwasser@COMPUSERVE.COM>
Subject:      OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

OOPS...


 My Collins dictionary says:

Intern:
 6) Chiefly US, a student or recent graduate receiving practical training in a
 working environment.

 Tom

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 17:19:11 +0100
Reply-To:     Michel Bel <michel.bel@ZONNET.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michel Bel <michel.bel@ZONNET.NL>
Subject:      Re: Looking for an English word
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

It definitely _is_  'intern'


Michel
----- Original Message -----
From: "Daniel Hertrich" <daniel.hertrich@GMX.DE>
To: <HPLX-L@UCONNVM.UCONN.EDU>
Sent: Tuesday, March 05, 2002 3:24 PM
Subject: OT: Looking for an English word


> ... well, I know, there are many. ;-)
>
> But I need a special one.
>
> I am looking for the English word for the German "Werksstudent", i.e. a
> person, who is still studying at a university, but who works for a
> company some hours a month, to make experiences in the job, to get a
> little bit of money (not much), to be able to begin his career already
> during the studies.
>
> Thanks a lot
> daniel
>
> --
> http://www.daniel-hertrich.de/contact
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 11:23:52 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: OT: Looking for an English word
Comments: To: "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
In-Reply-To:  <D8020D6F0DB8D211B99A0008C7C59CFE0FD8F738@cormails1.jdedwards.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Apprentice?


> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@uconnvm.uconn.edu]On Behalf Of
> Feldman, Robert
> Sent: Tuesday, March 05, 2002 11:01 AM
> To: HPLX-L@uconnvm.uconn.edu
> Subject: Re: OT: Looking for an English word
>=20
>=20
> I also suggested "intern" to Daniel, but I still feel it's not quite =
the
> right word. Since the program is called "work-study", is a =
"work-student"
> (not a correct English construction) an "intern" -- I don't think=20
> so, but I
> can't think of the correct term.
>=20
> Bob
>=20
> -----Original Message-----
> From: Tom Salwasser [mailto:TomSalwasser@COMPUSERVE.COM]
> Sent: Tuesday, March 05, 2002 9:46 AM
> To: HPLX-L@UCONNVM.UCONN.EDU
> Subject: Re: OT: Looking for an English word
>=20
>=20
> Daniel,
>=20
> One word for this is intern.
>=20
> Monica Lewinski was a White House intern a few years ago...
>=20
> Regards,
> TomSalwasser
>=20
> > I am looking for the English word for the German "Werksstudent", =
i.e. a
> > person, who is still studying at a university, but who works for a
> > company some hours a month, to make experiences in the job, to get a
> > little bit of money (not much), to be able to begin his career =
already
> > during the studies.
> >
>=20
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>=20
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 10:31:54 -0600
Reply-To:     Chris Lott <rclott@ro.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Chris Lott <rclott@RO.COM>
Subject:      Re: OT: Looking for an English word (fwd)
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

I don't want you guys to flounder any further.  Here is the reply I
sent Daniel:

> We call these "co-op" students.  Short for "Cooperative", as they
> belong to what is called at most Universities the "Cooperative Program",
> I suppose because they cooperate with various industries.


-Chris Lott

--

************************************************************************
R. Christopher Lott, P.E.                                  rclott@ro.com
Alpha Beta Technologies, Inc.
3112 12th Ave S.W.                                   PHONE: 256-534-9067
Huntsville, Alabama 35805                              FAX: 256-534-9069
************************************************************************

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 11:41:01 -0500
Reply-To:     Ed <edwardp@SYMPATICO.CA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ed <edwardp@SYMPATICO.CA>
Subject:      Re: OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

There a university in Canada which offers a program of alternating work and
study terms for its accounting degree.  They refer to this as a "co-op"
program, and the student is a co-op student.  Perhaps this is closer to the
German phrase than intern?

Ed


----- Original Message -----
From: "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Tuesday, March 05, 2002 11:01 AM
Subject: Re: OT: Looking for an English word


> I also suggested "intern" to Daniel, but I still feel it's not quite the
> right word. Since the program is called "work-study", is a "work-student"
> (not a correct English construction) an "intern" -- I don't think so, but
I
> can't think of the correct term.
>
> Bob
>
> -----Original Message-----
> From: Tom Salwasser [mailto:TomSalwasser@COMPUSERVE.COM]
> Sent: Tuesday, March 05, 2002 9:46 AM
> To: HPLX-L@UCONNVM.UCONN.EDU
> Subject: Re: OT: Looking for an English word
>
>
> Daniel,
>
> One word for this is intern.
>
> Monica Lewinski was a White House intern a few years ago...
>
> Regards,
> TomSalwasser
>
> > I am looking for the English word for the German "Werksstudent", i.e. a
> > person, who is still studying at a university, but who works for a
> > company some hours a month, to make experiences in the job, to get a
> > little bit of money (not much), to be able to begin his career already
> > during the studies.
> >
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 10:56:33 -0600
Reply-To:     TomSalwasser@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tom Salwasser <TomSalwasser@COMPUSERVE.COM>
Subject:      OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I hadn't considered apprentice, but I like it.

Is co-op primarily used in Canadian schools or is that used in US schools too?
It' such a clumsy word, especially to the English as a second language person.

My how easily I am distracted! d;-)

From: Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>

Apprentice?

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 12:05:18 -0500
Reply-To:     Ed <edwardp@SYMPATICO.CA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ed <edwardp@SYMPATICO.CA>
Subject:      Re: OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Apparently it is used in the US as well as Chris Lott from Alabama suggested
co-op (short for co-operative) as well.

Ed

----- Original Message -----
From: "Tom Salwasser" <TomSalwasser@COMPUSERVE.COM>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Tuesday, March 05, 2002 11:56 AM
Subject: OT: Looking for an English word


> I hadn't considered apprentice, but I like it.
>
> Is co-op primarily used in Canadian schools or is that used in US schools
too?
> It' such a clumsy word, especially to the English as a second language
person.
>
> My how easily I am distracted! d;-)
>
> From: Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
>
> Apprentice?
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 11:13:26 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: PC Card Partitions with 200LX ?
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Feldman, Robert wrote:
> Interesting but confusing. Just what "drive letter B
> needed to be used up somehow" means and how
> it was done, I hvae no idea. It does suggest that
> there is a potential to get a second partition active.

I think I remember that on any single floppy PC you can specify
drive B: and it will ask you to insert the disk in drive A: and
will use A: as B: until A: is asked for.  I also think I tried
this on the 200lx years ago and it worked.  I don't remember any
details of how or why I did it.  Probably just curiosity.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 12:18:44 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: OT: Looking for an English word
In-Reply-To:  <002b01c1c464$89ad6360$9a0110ac@hypn.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Educated cheap labor?=09

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 11:16:59 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Oliver W. Leibenguth:
> BTW: So there are more differences between the
> 200lx and the 700lx: The 200lx has a 8088 CPU and
> the 700lx has the 80186.

The 200lx has an 80186 CPU.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 10:32:29 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: PC Card Partitions with 200LX ?
MIME-Version: 1.0
Content-Type: text/plain; charset="windows-1252"

If I type "B:<enter> on my 95LX, I get "Insert the card for Drive B: and
strike any key when ready". When I do that on my 200LX, I get "Not ready
reading drive B:  Abort, Retry, Fail?".  I am pretty sure that the first
message comes from the SunDisk driver I have installed on the 95LX, not from
DOS. It might  be possible to do a driver for the 200LX that does the same.

Another interesting point is that when booting the 200LX, there is the
following message:

   "Microsoft Device Driver for BIOS Services Version 2.0
    Copyright (C) Microsoft Corp 1989-1992. All rights reserved.

    The Device Driver system installed 02 drive(s): A: - B:."

This message appears before Config.Sys runs.

Bob

-----Original Message-----
From: Barry [mailto:barry@FBTC.NET]
Sent: Tuesday, March 05, 2002 11:13 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: PC Card Partitions with 200LX ?


Feldman, Robert wrote:
> Interesting but confusing. Just what "drive letter B
> needed to be used up somehow" means and how
> it was done, I hvae no idea. It does suggest that
> there is a potential to get a second partition active.

I think I remember that on any single floppy PC you can specify
drive B: and it will ask you to insert the disk in drive A: and
will use A: as B: until A: is asked for.  I also think I tried
this on the 200lx years ago and it worked.  I don't remember any
details of how or why I did it.  Probably just curiosity.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 10:49:11 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: PC Card Partitions with 200LX ?
MIME-Version: 1.0
Content-Type: text/plain; charset="windows-1252"

I just tried using the HP95SDP.SYS driver in my 200LX. I can switch been A:
and B:, but _both_ drives give the "Not ready
reading drive X:  Abort, Retry, Fail?" message. Might be progress, though.

How do I partition my Flash card? The FDISK.EXE I have on my Win2K laptop
gives me a "Wrong DOS Version" error.

Bob

-----Original Message-----
From: Feldman, Robert [mailto:Robert_Feldman@JDEDWARDS.COM]
Sent: Tuesday, March 05, 2002 11:32 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: PC Card Partitions with 200LX ?


If I type "B:<enter> on my 95LX, I get "Insert the card for Drive B: and
strike any key when ready". When I do that on my 200LX, I get "Not ready
reading drive B:  Abort, Retry, Fail?".  I am pretty sure that the first
message comes from the SunDisk driver I have installed on the 95LX, not from
DOS. It might  be possible to do a driver for the 200LX that does the same.

<snip>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 18:50:42 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

When I did it with Bayer Leverkusen years ago, it was not to gain any
insight or practice - I did that as a "Praktikant" - but work on the
factory floor as a labourer during the university summer holidays for money
only (and not paying social insurance or taxes good money it was too). At
that time it was not the common thing for students to live in bigger and
better flats and drive more expensive cars than the professors as it is
now, and that money went a long way.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 19:03:58 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      A or nor A - how to ask the question?
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

My AUTOEXEC.BAT on C: contains the line

path a:\dos;c:\dos;d:\;d:\bin;d:\dos

which produces an error whenever there is no A: card inserted.
I have tried
IF EXIST A:\DOS\VC.COM
but that too does not say "no" but Error. Is there any known workaround?

Danke
        Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 05:15:22 +1100
Reply-To:     Russell Hemery <rhemery@POWERUP.COM.AU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russell Hemery <rhemery@POWERUP.COM.AU>
Subject:      Re: OT: Looking for an English word
In-Reply-To:  <HPLX-L%2002030510222359@UCONNVM.UCONN.EDU>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

>But I need a special one.
>
>I am looking for the English word for the German "Werksstudent", i.e. a
>person, who is still studying at a university, but who works for a
>company some hours a month, to make experiences in the job, to get a
>little bit of money (not much), to be able to begin his career already
>during the studies.

Hi all

In Australia the term apprentice is used for a person who is hired to be
trained in a trade and does some technical training at a college as well as
practical with the company. ie apprentice plumber, apprentice mechanic etc.

Intern is mainly used here for the medical profession as a term for a
graduate that is studying as they work. ie mentors oversee their practical
efforts after they have learned the intellectual stuff.

There are similar positions in the arts (understudy) and the legal
profession as well as copilot etc.

I think the situation Daniel describes is where full time students go out
to get some life experiences in return for a bit of pocket change. Here in
Oz the students go out for work-experience sometimes for no money at all.
They "test" professions they may be interested in pursuing for a career.
That seems the closest I can think of. They can then apply for their first
job quoting work-experience with xyz Company for x time and abc company for
x time etc with references as to how they did.

Hope this is of benefit ;-)

Russell

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 05:22:52 +1100
Reply-To:     Russell Hemery <rhemery@POWERUP.COM.AU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russell Hemery <rhemery@POWERUP.COM.AU>
Subject:      FYI Lithium initial voltage
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Hi all

As a follow on to my post a couple of days ago I measured "out of the pack"
voltage on the new E2 eveready AA photo lithiums and they read 1.79V x2 =
3.58V in the LX.

I'm doing a battlog and will post runtime etc once I have it.

Regards

Russell

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 05:34:19 +1100
Reply-To:     Russell Hemery <rhemery@POWERUP.COM.AU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russell Hemery <rhemery@POWERUP.COM.AU>
Subject:      Re: A or nor A - how to ask the question?
In-Reply-To:  <3C85088E.6ACA870F@NexGo.De>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

At 07:03 PM 05/03/02 +0100, you wrote:
>My AUTOEXEC.BAT on C: contains the line
>
>path a:\dos;c:\dos;d:\;d:\bin;d:\dos
>
>which produces an error whenever there is no A: card inserted.
>I have tried
>IF EXIST A:\DOS\VC.COM
>but that too does not say "no" but Error. Is there any known workaround?

Hi Axel and list

What if you have 2 Autoexec.bat. One on A: with A references as well as C:
and another on C without A: references. That way boot from A: if its there
and boot from C: if its not. I "think" this will be automatic if you choose
boot from A: in the startup menu.

Hope this helps

Russell

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 21:00:01 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: A or nor A - how to ask the question?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Axel

On Tue, 5 Mar 2002 19:03:58 +0100, Axel Berger <Axel-Berger@NEXGO.DE> wrote:

> path a:\dos;c:\dos;d:\;d:\bin;d:\dos
>
> which produces an error whenever there is no A: card inserted.
> I have tried
> IF EXIST A:\DOS\VC.COM
> but that too does not say "no" but Error. Is there any known workaround?

IIRC this can be done using

IF EXIST A:\NUL PATH A:\BIN;...
IF NOT EXIST A:\NUL PATH C.\BIN;...

At least this works for directories.

Otherwise lxcic may help you since it returns errorlevels depending on
the card type inserted into the slot. So ask for the Flash card
errorlevel and if true, you can be sure there is an A: drive.
THEN you can use your IF EXIST to see if it is the correct card.


GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 21:00:02 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

Thanks for al your suggestions!

Here is what I collected from your replies:

co-op: probably means a direct cooperation (on a certain project?)
between university and company. Not meant here. No such direct
relation, although the subject of my work is essentially the same as my
studying subject.

Intern: Seems to be something like "Praktikant" (Monica Lewinsky).
That's something different I think. You have to be an intern(al?) for
some time to be able to graduate. What I do is not a must.

Educated cheap labor: That was the best! :-) "trifft den Nagel auf den
Kopf" ("hits the nail onto the head").

work-student: My English teacher suggested "working student", but I
don't think this is a common work. work-student is also a little
strange... But it would be the most accurate translation.

fellow(ship): too general in my opinion.

trainee: Maybe kind of. But not exactly.

apprentice: No. To be an apprentice here is an alternative to be a
student. But I am also a student.


Maybe co-op is still the best term, and it probably impresses most. ;-)
I'll go for that one, I think.

Thanks a lot to you all
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 14:51:34 -0500
Reply-To:     Andrew <andrewaa@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Andrew <andrewaa@EARTHLINK.NET>
Subject:      Re: Appoint pen mouse drivers?
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Automatic digest processor wrote:
> Subject: Re: Microsoft Mouse - Success!
> Date: Mon, 4 Mar 2002 07:23:06 -0700
> From: "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
<SNIP>
> P.S. The Appoint pen mouse is a handy one to use with the LX, as the ball is
> on the end of a pen-like stylus. You can use it on small surfaces such as a
> pad or paper, or even your pants leg, as the ball is more exposed. It costs
> only $10 plus shipping from California Digital. The only drawback is that it
> is pink and says "Barbie" on it -- it comes with the "Barbie PC Fashion
> Design & Color" software package.

Bob
What drivers does the Apoint mouse use?
I like the shape, it seems as if it would feel a lot like my Kurta
tablet (but smaller).
I suppose I could always paint it if I felt unmanly.
Actually if I don't paint it it will end up on my daughters computer.

Thanks

--
Andrew King
Ann Arbor Michigan
technology is the answer, what was the question?

NOTE:  NEW E-MAIL ADDRESS, andrewaa@earthlink.net is working,
comcast and mediaone addresses will be gone by march

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 21:03:52 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> It definitely _is_  'intern'

I'd say definitely not. I do not know a better term but in my other post I
have just explained what a "Werkstudent" is taken to be, and it is
something quite different.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 12:26:32 -0800
Reply-To:     Ian Butler <ianb@HPLX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ian Butler <ianb@HPLX.NET>
Subject:      FLUFF: Re: Looking for an English word
In-Reply-To:  <3C8524A8.56E36532@NexGo.De>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Tue, 5 Mar 2002, Axel Berger wrote:

> > It definitely _is_  'intern'
>
> I'd say definitely not. I do not know a better term but in my other
> post I have just explained what a "Werkstudent" is taken to be, and it
> is something quite different.

What Daniel described was basically the an internship -- a student working
for free (or for very little money, at least) to gain experience in their
field.  But what you described sounds more like an ordinary student summer
job to make as much money as possible, even if the job isn't in your
chosen career field. (presumably to help out with tuition and school
living expenses).

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 21:29:53 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: A or nor A - how to ask the question?
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Russell Hemery wrote:
> That way boot from A: if its there and boot from C: if its not.

That is what I do mostly. The main reason for there not being an A: is a
modem in the socket. In that case I need loads of RAM for Nettamer and do
not start "700" (equivalent to "200" on a 700 LX) among other things. Now I
may want to have RAM with an A: drive present, e.g. to play chess. The
easiest and fastest way is <Alt><2> on booting, and then I do want A: in
the path.

Daniel Hertrich wrote:
> THEN you can use your IF EXIST to see if it is the correct card.

No such thing as a wrong card - it is no card, thus no A: or the right one.

> Otherwise lxcic may help
Thanks, I'll check that out, you suggestion of
> IF EXIST A:\NUL
did not help. It tries to read from A:, thus no A = error

Danke
        Axel

P.S: Any reason why replies are not defaulted to the group? I keep and keep
forgetting

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 15:31:50 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: OT: Looking for an English word
In-Reply-To:  <HPLX-L%2002030514572919@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Someone should put together a list of responses, create an NDB file and =
post it on super.... :^/ or maybe not.

> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@uconnvm.uconn.edu]On Behalf Of
> Daniel Hertrich
> Sent: Tuesday, March 05, 2002 2:00 PM
> To: HPLX-L@uconnvm.uconn.edu
> Subject: Re: OT: Looking for an English word
>=20
>=20
> Hi friends,
>=20
> Thanks for al your suggestions!
>=20
> Here is what I collected from your replies:
>=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 13:44:39 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: A or nor A - how to ask the question?
MIME-Version: 1.0
Content-Type: text/plain

Because there was a nasty flame war a while back. The thought was that it
would take a conscious act by the flamer to send the post to the whole list
rather than just to the flamee.

Bob

-----Original Message-----
From: Axel Berger [mailto:Axel-Berger@NexGo.De]
Sent: Tuesday, March 05, 2002 2:30 PM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: A or nor A - how to ask the question?

<snip>

P.S: Any reason why replies are not defaulted to the group? I keep and keep
forgetting

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 16:14:11 -0500
Reply-To:     Ed <edwardp@SYMPATICO.CA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ed <edwardp@SYMPATICO.CA>
Subject:      Re: OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

This from the University website I mentioned to hopefully clarify, but I
think co-op is a good choice for your situation:

"The Co-op system of study involves alternating terms of work and study in
approved work settings. Four successfully completed work terms are required
for the granting of a Co-op degree. The first Co-op work term will follow
completion of the 2A academic term."

The students do not work on special projects, they are just part of the
general company staff and treated the same way as other staff with a similar
level of experience.  Its good for the students because they make a little
bit of money and get work experience directly applicable to their future
careers.  Many are in fact ultimately hired by the company they do their
work terms for.  The school likes it because the workterms enhance the
academic studies of the students with practical experience in the field.
The companies like it because they get a constant supply of cheap and
(usually) keen young labour.

Hope that helps.

Ed



----- Original Message -----
From: "Daniel Hertrich" <daniel.hertrich@GMX.DE>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Tuesday, March 05, 2002 2:00 PM
Subject: Re: OT: Looking for an English word


> Hi friends,
>
> Thanks for al your suggestions!
>
> Here is what I collected from your replies:
>
> co-op: probably means a direct cooperation (on a certain project?)
> between university and company. Not meant here. No such direct
> relation, although the subject of my work is essentially the same as my
> studying subject.
>
> Intern: Seems to be something like "Praktikant" (Monica Lewinsky).
> That's something different I think. You have to be an intern(al?) for
> some time to be able to graduate. What I do is not a must.
>
> Educated cheap labor: That was the best! :-) "trifft den Nagel auf den
> Kopf" ("hits the nail onto the head").
>
> work-student: My English teacher suggested "working student", but I
> don't think this is a common work. work-student is also a little
> strange... But it would be the most accurate translation.
>
> fellow(ship): too general in my opinion.
>
> trainee: Maybe kind of. But not exactly.
>
> apprentice: No. To be an apprentice here is an alternative to be a
> student. But I am also a student.
>
>
> Maybe co-op is still the best term, and it probably impresses most. ;-)
> I'll go for that one, I think.
>
> Thanks a lot to you all
> daniel
>
> --
> http://www.daniel-hertrich.de/contact
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 22:48:23 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      ANN: Syslog 1.1
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

as always, a short time after v1.0 there is a version 1.1 of my new
program. Thanks to Paulo Custodio I could remove a few "bugs" (not
really, but it is safer now).

http://www.daniel-hertrich.de/download

and it will soon appear on SUPER.

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 5 Mar 2002 15:26:51 -0700
Reply-To:     Bob Christopher <bob@PALMTOP.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Christopher <bob@PALMTOP.COM>
Subject:      MODEM PROBLEM FIXED
Comments: To: Longden_Loo@candle.com
Mime-Version: 1.0
Content-Type: text/plain; charset=iso-8859-1
Content-Transfer-Encoding: 8bit

Longden & List,

Problem fixed. I am now running Goin' Postal email program in a
DOS Window just fine. Problem turned out to be a semi-defective
XJ1144 PCMCIA modem that worked on the OB430 (or at least seated
better in the PCMCIA slot) but was not registering on the OB-800
at all. In its place I'm using the 56K modem I got for my HP200LX
and it works great. Love the speed but hate the dongle business.
Thanks, Longden.

Bob
 Bob Christopher . Littleton, Colorado USA . bob@palmtop.com
   HP 200-LX Palmtop . Minox Cameras . All The Small Stuff

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 05:53:08 +0100
Reply-To:     Nathalie Bugeaud <tps-seti@WANADOO.FR>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nathalie Bugeaud <tps-seti@WANADOO.FR>
Subject:      Lotus 123 - where to store macros
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

my accounting file, called my-money.wk1 has 2 macros which i saved into E1
and H1 respectively. Without any data the file is 19,745 (zipped 4114). If i
save the macros in row 1 and hide it, would the file reduce in size to an
acceptable 2k?  Any Lotus-lovers out there?
Filer does not a good job viewing (F8) Lotus files.
tip: For instant viewing  without loading Lotus itself use XTGOLD.
Nat .. still with flat tyres

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 08:21:32 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: A or nor A - how to ask the question?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Axel

On Tue, 5 Mar 2002 21:29:53 +0100, Axel Berger <Axel-Berger@NEXGO.DE> wrote:

> Daniel Hertrich wrote:
> > THEN you can use your IF EXIST to see if it is the correct card.
>
> No such thing as a wrong card - it is no card, thus no A: or the right one.

As I said - use LXCIC to see IF there is a card and THEN (If there is a
Flash card) use IF EXIST to determine if it is the card you want or
not.

> P.S: Any reason why replies are not defaulted to the group? I keep and keep
> forgetting

Reason: The FROM field of the emails contain the poster's address.
Solution: Use Post/LX and press "t" to reply to list messages. This
puts the contents of the "to" field into the new "to" field, i.e. the
list address.

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 09:26:23 +0100
Reply-To:     Geert van Wirdum <v.wirdum@HCCNET.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Geert van Wirdum <v.wirdum@HCCNET.NL>
Subject:      Re: OT: Looking for an English word
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

It was interesting to see the various views on students taking paid jobs. My
first association would be the one given by Axel, and I would assume "work
student" (without a hyphen) would raise similar associations in the UK.
"Working student" would probably also do, although, depending on the
context, this could as well indicate the student was actively studying,
rather than doing a different job at that very moment.

The paid work of a "werkstudent" most often bears no relation to his or her
study. My three daughters are post sorters and postmen in the weekends, one
also did cucumber packing, street interviewing for Green Peace, and
servant's work in a theahouse. My water-bound son works as a guide in a
maritime museum, a watchman on a wharf, sailor on a tourist boat, etc. The
money is used for "luxury", even an LX in my son's case. When I was at the
University, in the 60s, I was lucky enough to get a job in one of the
laboratories. Being a "werkstudent" then was to pay your living and study.
Many of my friends would work as tomato pickers, dish cleaners, pizza
couriers or, preferably, night watchmen (and meanwhile learn for
examinations, being working students and work students in the same
instance!).

Geert.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 04:39:15 -0600
Reply-To:     TomSalwasser@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tom Salwasser <TomSalwasser@COMPUSERVE.COM>
Subject:      OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Geert,

In common usage in the US, intern is the best transaltion of werkstudent.  Co-op
is another possibility, although it is clumsy and not really a word.

My Collins dictionary says:

Intern:
 6) Chiefly US, a student or recent graduate receiving practical training in a
 working environment.

Regards,
Tom

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 12:00:53 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      pdf viewer?
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Is there any way how to view PDF files on 200lx? There is Acrobat reader ver 1.0 for DOS, but apparently needs VGA.

Radek

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 08:14:27 -0500
Reply-To:     Keith Grider <k.grider@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Keith Grider <k.grider@EARTHLINK.NET>
Subject:      Re: OT: Looking for an English word
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Daniel,

The best word is Co-op. It does not mean directly working on a specific
project, but can mean general employment at a lower than prevailing wage and
is only open to university students. I co-oped at GE Aircraft engines while
studying engineering. The co-op lasted over a couple of years and happened
every other quarter for my Sophomore and Junior years.

KeithG
(former student at Universitaet Hamburg as well)
----- Original Message -----
From: "Daniel Hertrich" <daniel.hertrich@GMX.DE>
Sent: Tuesday, March 05, 2002 2:00 PM
Subject: Re: OT: Looking for an English word


> Hi friends,
>
> Thanks for al your suggestions!
>
> Here is what I collected from your replies:
>
> co-op: probably means a direct cooperation (on a certain project?)
> between university and company. Not meant here. No such direct
> relation, although the subject of my work is essentially the same as my
> studying subject.
>
> Intern: Seems to be something like "Praktikant" (Monica Lewinsky).
> That's something different I think. You have to be an intern(al?) for
> some time to be able to graduate. What I do is not a must.
>
> Educated cheap labor: That was the best! :-) "trifft den Nagel auf den
> Kopf" ("hits the nail onto the head").
>
> work-student: My English teacher suggested "working student", but I
> don't think this is a common work. work-student is also a little
> strange... But it would be the most accurate translation.
>
> fellow(ship): too general in my opinion.
>
> trainee: Maybe kind of. But not exactly.
>
> apprentice: No. To be an apprentice here is an alternative to be a
> student. But I am also a student.
>
>
> Maybe co-op is still the best term, and it probably impresses most. ;-)
> I'll go for that one, I think.
>
> Thanks a lot to you all
> daniel
>
> --
> http://www.daniel-hertrich.de/contact
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 07:24:37 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: pdf viewer?
MIME-Version: 1.0
Content-Type: text/plain

No, there is AFIK, no PDF viewer that will work with a 80186 and CGA. There
are web-based services that will do conversions. I don't remember the URLs,
but you can search the LX list archives.

One program that seems to have potential for modification (unless it is
outdated) is Ghostscript, which was a project to do an open source pdf
reader. The recent versions need an 80386 or better, or Unix, but versions
around 2.6 could be compiled for DOS. It's a big program and I haven't taken
the time to look at the source code to see if it could be made to work on
the 200LX.

Bob

-----Original Message-----
From: Radek Svagr [mailto:radek.svagr@LGPHILIPS-DISPLAYS.COM]
Sent: Wednesday, March 06, 2002 5:01 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: pdf viewer?


Is there any way how to view PDF files on 200lx? There is Acrobat reader ver
1.0 for DOS, but apparently needs VGA.

Radek

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 15:35:12 +0100
Reply-To:     Juan Belmonte <jbmbhs@eresmas.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Juan Belmonte <jbmbhs@ERESMAS.COM>
Subject:      Re: pdf viewer?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Bad news: ACRODOS Also needs 386+

Instead, I'm using GhostSript to convert PDF's to monochrome PCX's at 72 or
96 dpi.
And use the EXCELLENT Peichl's LXPIC...
I'm using by to read datasheets of IC's and microcontrollers.

For main text PDF's I use the accesibility plugin of Acrobat Reader 4 to
extract all text in pdf to TXT file but formatting it's VERY UGLY and
dificult to read if (example) two columns by page...


It's the best solution I found... If anyone knows best... PLEASE, Tell me!

Regards


----- Original Message -----
From: "Radek Svagr" <radek.svagr@LGPHILIPS-DISPLAYS.COM>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Wednesday, March 06, 2002 12:00 PM
Subject: pdf viewer?


> Is there any way how to view PDF files on 200lx? There is Acrobat reader
ver 1.0 for DOS, but apparently needs VGA.
>
> Radek

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 08:36:36 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: A or nor A - how to ask the question?
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Axel Berger wrote:
> My AUTOEXEC.BAT on C: contains the line
>
> path a:\dos;c:\dos;d:\;d:\bin;d:\dos
>
> which produces an error whenever there is no A:
> card inserted.  I have tried
> IF EXIST A:\DOS\VC.COM
> but that too does not say "no" but Error. Is there
> any known workaround?

Put an autoexec.bat in C: that leaves A: out of the path.  Keep
the existing autoexec.bat in A:.  Also have a config.sys on
both.

When you boot it looks first on A: and then on C: for config.sys
and it uses the autoexec.bat where it firsts finds a config.sys.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 08:44:32 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Russell Hemery wrote:
> In Australia the term apprentice is used for a person
> who is hired to be trained in a trade and does some
> technical training at a college as well as practical with
> the company. ie apprentice plumber, apprentice
> mechanic etc.
>
> Intern is mainly used here for the medical profession as a
> term for a graduate that is studying as they work. ie mentors
> oversee their practical efforts after they have learned the
> intellectual stuff.
>
> There are similar positions in the arts (understudy) and the
legal
> profession as well as copilot etc.

I don't think understudy and copilot are used in quite the same
way.  An understudy is someone already fully capable who can
take over if the performer is ill.

A copilot is also a fully qualified pilot, able to do everything
the pilot can do.  Someone has to be in charge and that's the
pilot, but they're really expected to be equal in ability, or
nearly so.

The company I retired from was in the stock market and we had
intern traders.  They were postgraduate students who came and
did the job of a trader during the summer, but with much
supervision.  A few of them, when they graduated, came to work
for us as traders later.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 08:52:35 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Daniel Hertrich wrote:
> Intern: Seems to be something like "Praktikant" (Monica
Lewinsky).
> That's something different I think. You have to be an
intern(al?) for
> some time to be able to graduate. What I do is not a must.

Our interns didn't have to serve as interns to graduate.  Our
company looked for promising students and offered this as an
opportunity.  They worked during the summer and learned the
business and we got to take a look at them and see if we wanted
to keep them.

I think the problem is that everyone is trying to attach shades
of meanings to each word but they're often interchangable.

I'm not familiar with co-op but I think "apprentice" and
"intern" can be used interchangably.  Probably intern is used
more in professional positions and apprentice is used more in
craft positions, but I think they're interchangable.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 10:02:26 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: Lotus 123 - where to store macros
Comments: To: Nathalie Bugeaud <tps-seti@WANADOO.FR>
In-Reply-To:  <004e01c1c4cc$cee3e9a0$b2e8f8c1@oemcomputer>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Isn't there a way to store macros in a seperate spreadsheet under a =
named range and then refer to it  from another spreadsheet? It's been a =
long time since I've messed with 1-2-3 on a regular basis but I remember =
doing something like this.

> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@uconnvm.uconn.edu]On Behalf Of
> Nathalie Bugeaud
> Sent: Tuesday, March 05, 2002 11:53 PM
> To: HPLX-L@uconnvm.uconn.edu
> Subject: Lotus 123 - where to store macros
>=20
>=20
> my accounting file, called my-money.wk1 has 2 macros which i saved =
into E1
> and H1 respectively. Without any data the file is 19,745 (zipped=20
> 4114). If i
> save the macros in row 1 and hide it, would the file reduce in size to =
an
> acceptable 2k?  Any Lotus-lovers out there?
> Filer does not a good job viewing (F8) Lotus files.
> tip: For instant viewing  without loading Lotus itself use XTGOLD.
> Nat .. still with flat tyres
>=20
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 09:25:12 -0600
Reply-To:     TomSalwasser@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tom Salwasser <TomSalwasser@COMPUSERVE.COM>
Subject:      OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

I feel I'm running the risk of being flamed, so I'm very sorry to say this will
be my last addition to this discussion. d;-)

Daniel needs to translate the word werkstudent. I think we can all agree that a
werkstudent is not a co-op. A werkstudent is an intern in a co-operative
educational program, or co-op. A person is not a co-op, a person is an intern. A
co-op is a program. How does that sound!

Best Regards,
Tom Salwasser

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 10:28:53 -0500
Reply-To:     Ed <edwardp@SYMPATICO.CA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ed <edwardp@SYMPATICO.CA>
Subject:      Re: OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

This is my last post too.

Tom, you are wrong.

I know of a co-op program where the students are referred to as co-op
students.  I guess you should send them all an email telling them they are
all actually interns and they should stop calling themselves co-op students.
Then, I suggest you duck.

Regards,

Ed

----- Original Message -----
From: "Tom Salwasser" <TomSalwasser@COMPUSERVE.COM>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Wednesday, March 06, 2002 10:25 AM
Subject: OT: Looking for an English word


> I feel I'm running the risk of being flamed, so I'm very sorry to say this
will
> be my last addition to this discussion. d;-)
>
> Daniel needs to translate the word werkstudent. I think we can all agree
that a
> werkstudent is not a co-op. A werkstudent is an intern in a co-operative
> educational program, or co-op. A person is not a co-op, a person is an
intern. A
> co-op is a program. How does that sound!
>
> Best Regards,
> Tom Salwasser
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 08:45:29 -0700
Reply-To:     Bob Christopher <bob@PALMTOP.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Christopher <bob@PALMTOP.COM>
Subject:      Re: A or nor A - how to ask the question?
Mime-Version: 1.0
Content-Type: text/plain; charset=iso-8859-1
Content-Transfer-Encoding: 8bit

If I understand the problem correctly, the system is faulting
simply because it is searching for drive A first as it works its
way through the DOS calls in Axel's autoexec.bat file.

A solution that does not require duplicate autoexec.bat files or
other workarounds is to simply move the A:\; to the end of the
path statement and you will avoid the error.

By placing it at the end of the statement, all your DOS calls in
your autoexec.bat file follow the stream of the path, ie the
search begins at c:\dos;c:\;d:\;d:\bin;c:\dos and then finally to
A:\; but only if what you are calling via autoexec.bat hasn't
already been found in the previous path string.

If there is no pcmcia card in Drive A, you will not get an error
unless you have a DOS call in your autoexec.bat that cannot be
satisfied by the path string.

Bob
 Bob Christopher . Littleton, Colorado USA . bob@palmtop.com
   HP 200-LX Palmtop . Minox Cameras . All The Small Stuff

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 17:05:54 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: A or nor A - how to ask the question?
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Barry wrote:
> Put an autoexec.bat in C: that leaves A: out of the path.  Keep
> the existing autoexec.bat in A:.  Also have a config.sys on
> both.
As I explained, there are sometimes reasons for booting from C: with an A:
card in place and then and only then will I want A: in the path.

The solution was Daniel's suggestion of Stefan Peichl's excellent LXCIC.
Replacing stuff from ROM (I already use SUBST insead of ASSIGN) seems a
terrible shame and a waste, but when it is as superiour as this. I have
also now installed ABC for the batteries and this will hopefully stop them
from being overcharged and cooked in a very short time.

Thank you all
                Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 17:15:19 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      eMail
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Having put you all to a lot of trouble with my last problem, why not do it
again?
I have currently installed nettamer which although being an excellent piece
of work is somewhat clumsy and unwieldy for my needs.
I do not really have a use for HTML and FTP on my LX but do want to use my
reserved address Berger.mobil@Web.De (no binaries!) on the move. That
means, one eMail account with one pop and one smtp server, but lots of
differnt modems on lots of different ports and several differnt provider
dial ins for all of them. At first glance postLX seems to be the best
choice, especially as it seems to be an all in one, while cclxpop seems to
require installation of at least three separate packages.

Any advice?

Danke
                Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 10:40:01 -0500
Reply-To:     theise@netins.net
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: OT: Looking for an English word

Tom Salwasser writes:
> Geert,
>
> In common usage in the US, intern is the best transaltion of werkstudent.  Co-op
> is another possibility, although it is clumsy and not really a word.

From what Daniel and Geert have said, it sounds as if the German term
refers to students who are working in some job, not related to their
study, to make ends meet, raise their standard of living, or avoid
taking out loans.  I don't think either intern or co-op are appropriate
since they describe work that is related to the career being pursued.

Geert's description makes me think of the old song with the lines, "I'm
working my way through college..."  Seems like "working student" is the
best match I've heard so far.

Ted

--
Ted Heise     <theise@netins.net>     West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 09:47:04 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: PC Card Partitions with 200LX ?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

Hello All,

Here's something interesting that others might follow up on:

I copied CSMAPPER.SYS and CARDDRV.EXE from a Win95 computer to my flash card
(normally drive A:) and then ran them on my 200LX by putting the following
in my CONFIG.SYS

     DEVICE=A:\CSMAPPER.SYS
     DEVICE=A:\CARDDRV.EXE /PART=2

Surprisingly, both devices appear to have installed, and CARDDRV reports
that it installed 4 drives, F: - I: . I can still read my flash card as
drive A:, but none of the "new" drives will work. BTW, I have a 20MB SunDisk
card with only one partition on it.

Bob

P.S. Win95 documentation says the CARDDRV switch is /SLOT=n, where n is the
number of PCMCIA slots, but internally, CARDDRV says the switch is /PART=n,
where n is the maximum number of card partitions. You can view this message
by running CARDDRV from a DOS prompt with no switches, or by viewing the
contents of CARDDRV with Windows NotePad.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 18:26:17 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: eMail
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Axel

On Wed, 6 Mar 2002 17:15:19 +0100, Axel Berger <Axel-Berger@NEXGO.DE> wrote:

> I do not really have a use for HTML and FTP on my LX but do want to use my
> reserved address Berger.mobil@Web.De (no binaries!) on the move. That
> means, one eMail account with one pop and one smtp server, but lots of
> differnt modems on lots of different ports and several differnt provider
> dial ins for all of them. At first glance postLX seems to be the best
> choice, especially as it seems to be an all in one, while cclxpop seems to
> require installation of at least three separate packages.

Have you tried Goin' Postal? This is said to be easy to set up, needs
not so much disk space, is free, and easy to handle.

I don't know about its capability regarding different connection setup
handling, but I assume it is possible to develop some mechanisms
similar to setcom.bat used in the www/lx setup. See also
http://www.daniel-hertrich.de/wwwlx

If GP doesn't support such mechanisms by itself, you can maybe write
some batch files which recognize the kind of connection, chooses the
dependant ISP and modifies the config file of GP...
No idea if this would work, since I don't know GP, but if it uses ASCII
config files, this should work in some way.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 12:26:28 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: eMail
In-Reply-To:  <HPLX-L%2002030612234046@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Wed, 6 Mar 2002, Daniel Hertrich wrote:

> On Wed, 6 Mar 2002 17:15:19 +0100, Axel Berger <Axel-Berger@NEXGO.DE> wrote:
>
> > I do not really have a use for HTML and FTP on my LX but do want to use my
> > reserved address Berger.mobil@Web.De (no binaries!) on the move. That
> > means, one eMail account with one pop and one smtp server, but lots of
> > differnt modems on lots of different ports and several differnt provider
> > dial ins for all of them.

> Have you tried Goin' Postal? This is said to be easy to set up, needs
> not so much disk space, is free, and easy to handle.
>
> I don't know about its capability regarding different connection setup
> handling, but I assume it is possible to develop some mechanisms
> similar to setcom.bat used in the www/lx setup.

Actually, GP is quite good at managing multiple dial-up methods.
If e-mail is your only interest, it would be a good bet.  If you
also want Usenet news, you might have a look at LXTCP/PNR.  If you
search the archives, you should find a thread on this topic from a
few months ago.

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 13:37:21 -0500
Reply-To:     "Striegel, Alan" <Striegel@PIOS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Striegel, Alan" <Striegel@PIOS.COM>
Subject:      Re: OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain

Our firm has hired some people under similar terms.  We always referred to
this as a 'work-study program'.  The individuals were considered to be
employees (possibly with some special categories, such as part-time or
exempt) but I don't think we ever called them co-ops or interns.

If they made references to this experience on their resumes, it would
probably be best to say they were employed in a work-study program.  Their
employee titles were no different than other employees in the department at
that level.

Alan Striegel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 12:04:17 -0700
Reply-To:     "Robert K. Meyer" <bmeyer@UNION-TEL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Robert K. Meyer" <bmeyer@UNION-TEL.COM>
Subject:      Re: OT: Looking for an English word
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Work-study student is a term applied to students at the
University of Wyoming when they work inside the university
generally in the college of their persuing degree.

Bob

Daniel Hertrich wrote:
>
> ... well, I know, there are many. ;-)
>
> But I need a special one.
>
> I am looking for the English word for the German "Werksstudent", i.e. a
> person, who is still studying at a university, but who works for a
> company some hours a month, to make experiences in the job, to get a
> little bit of money (not much), to be able to begin his career already
> during the studies.
>
> Thanks a lot
> daniel
>
> --
> http://www.daniel-hertrich.de/contact
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

--
R.K. Meyer MSEE K7PPC bmeyer@union-tel.com Elk Mountain WY
http://w3.union-tel.com/~bmeyer/   His name...  Isaiah 9:6

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 19:38:44 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      SPD31.EXE Shift-Ctrl-Del Slowdown?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

The doc for SPD31.EXE, the speed driver from Times2Tech,
mentions several keys strokes that control various feature
including Shift-Ctrl-Del to slow down.  I've tried this without
any apparent change.  Should I detect something or am I missing
something?

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 01:57:30 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

-----Original Message-----
From: Oliver W. Leibenguth <Oliver@COMPUSEUM.DE>
Date: Tuesday, March 05, 2002 3:10 PM



>BTW: So there are more differences between the 200lx and the 700lx: The
>200lx has a 8088 CPU and the 700lx has the 80186.


is THAT so ? makes the lx200 an XT and an
lx700 an AT ? wow !

..pk

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 02:00:42 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

-----Original Message-----
From: Michel Bel <michel.bel@ZONNET.NL>
Date: Tuesday, March 05, 2002 3:10 PM


> The 700 has an extended 200LX
>rom, with SMS and FAX sw as well, plus a second PCMCIA slot (strictly I/O
>wired)..


a SECOND pcmcia slot .. mine is missing ..
i have only one :-((

..pk

>Michel
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 22:01:09 +0100
Reply-To:     "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Subject:      AW: HP collection
In-Reply-To:  <006701c1c54d$ca28a6e0$6574c5cb@q20>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

> > The 700 has an extended 200LX
> >rom, with SMS and FAX sw as well, plus a second PCMCIA slot (strictly I/O
> >wired)..
> a SECOND pcmcia slot .. mine is missing ..
> i have only one :-((

I guess, the second PCMCIA slot is for the built-in datacard and not a
_real_ slot.

regards,
oliver

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 22:02:02 +0100
Reply-To:     "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Subject:      AW: HP collection
In-Reply-To:  <005e01c1c54d$57486340$6574c5cb@q20>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

> is THAT so ? makes the lx200 an XT and an
> lx700 an AT ? wow !

I think it's a typo. They both must have the same cpu...

regards,
Oliver

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 13:12:32 -0800
Reply-To:     Ian Butler <ianb@HPLX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ian Butler <ianb@HPLX.NET>
Subject:      Re: HP collection
In-Reply-To:  <006701c1c54d$ca28a6e0$6574c5cb@q20>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Thu, 7 Mar 2002, pksharma wrote:

> > The 700 has an extended 200LX
> >rom, with SMS and FAX sw as well, plus a second PCMCIA slot (strictly I/O
> >wired)..
>
> a SECOND pcmcia slot .. mine is missing ..
> i have only one :-((

The second slot is inside the shell of the 700LX.  Take the 700LX apart
and you can remove the datacard from it and end up with a second slot, but
I don't think it works as a normal slot (i.e., I don't think a flash card
works in it).  I could be wrong, though.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 17:59:23 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Ol' Eddie Archive
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Did anybody ever get their hands on the Eddie files? I can host them if =
it's not more'n a few gigs.


I got  some minix stuff on there to start. If you want minix go get it:

ftp://badeddie.no-ip.com/pub/eddie/

Looks like I can spare about 4 gigs.

BTW: I think I got a pretty tight FTP server setup but let know if you =
see any security issues.

Thanks,

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 00:00:17 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> a SECOND pcmcia slot .. mine is missing ..

No it isn't, though quite hidden. When I first openen up my 700 I was quite
surprised to find, that the phone is not connected via something customized
and proprietary but rather a standard Nokia Cellular Data Card exactly the
same as I had bought for my notebook. This being a PCMCIA card makes its
connector a PCMCIA slot. I have not tried to fit another card there -
though for certain usages a flashdisk might come handy, especially if the
700 innards could be made to fit inside a 200 case.

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 23:55:29 +0000
Reply-To:     castorlw@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Larry Castor <castorlw@YAHOO.COM>
Subject:      Re: Problems with Mocha PPP
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Dario,
  I've set it up and it works fine on my home PC using Win98 &, 33600modem=
.  Can't get it to work at by business PC which is connected to the =
company lan.  In the later case, it appears to connect but then times out =
because I don't have the right script?
  I6m also using 38400 bps and it is very stable.
  What platform are you using?

Larry


> Does anyone have it working? I've set up a 38400 bps connection but =
it's extremely slow and doesn't complete the transmissions. Other speeds =
doesn't work at all. The configuration is the one at Daniel's page.
>
> Dario
>
> --
>
> _______________________________________________
> Sign-up for your own FREE Personalized E-mail at Mail.com
> http://www.mail.com/?sr=3Dsignup
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 20:36:58 -0500
Reply-To:     Dario Draiman <dario200@MAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dario Draiman <dario200@MAIL.COM>
Subject:      Re: Problems with Mocha PPP
Content-Type: text/plain; charset="ISO-8859-1"
Content-Transfer-Encoding: 7bit
MIME-Version: 1.0

I'm using Windows 98, 56700 bps modem and my 200LX connected in COM1 with the F1015 cable (the same I use with Transfile). I set up WWW/LX in the same way as Daniel explained on his page. I tried telnet and HV. Telnet connect, ask for a login but stop
transfer when it ask for a password (and it's not a server problem). HV says "Connected...Receiving..." but the download of the page never ends.
In Mocha the "bytes from palm" grow faster than the "bytes to palm".

Dario


-----Original Message-----
From: Larry Castor <castorlw@YAHOO.COM>
Date:         Wed, 6 Mar 2002 23:55:29 +0000
To: HPLX-L@UConnVM.UConn.Edu
Subject:      Re: Problems with Mocha PPP


> Dario,
>   I've set it up and it works fine on my home PC using Win98 &, 33600modem.  Can't get it to work at by business PC which is connected to the company lan.  In the later case, it appears to connect but then times out because I don't have the right
script?
>   I6m also using 38400 bps and it is very stable.
>   What platform are you using?
>
> Larry
>
>
> > Does anyone have it working? I've set up a 38400 bps connection but it's extremely slow and doesn't complete the transmissions. Other speeds doesn't work at all. The configuration is the one at Daniel's page.
> >
> > Dario
> >
> > --
> >
> > _______________________________________________
> > Sign-up for your own FREE Personalized E-mail at Mail.com
> > http://www.mail.com/?sr=signup
> >
> > ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

--

_______________________________________________
Sign-up for your own FREE Personalized E-mail at Mail.com
http://www.mail.com/?sr=signup



** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 22:23:26 -0500
Reply-To:     David Heath <downeast@VOL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         David Heath <downeast@VOL.COM>
Subject:      Re: INSTALLATION ISSUES/ HISWORD/OLBIBLE
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Bob,

I went to the Online Bible web site and downloaded the following DOS
software:  Revised Easton's Bible Dictionary; Electic Bible Notes; Geneva
Bible Verse in Modern English; Lexicon (Thayer, Brown Driver Briggs);
Matthew Henry';s Concise Commentary; Spurgeon's "Morning and Evening" Daily
Readings; Topics containing Thompson Chain, New Topical Text Book, and other
material; Treasury of Scripture Knowledge; Bible in Basic English.

I want to use this software with the hisword software.  So I installed this
software using Online Bible installation program.   However, the
installation program didn't set up the software to work with hisword.  If
you have any or all of these programs working with hisword, I would like to
have a copy of the installed version.

Also, I would like to have the installed version of AV-NIV.  I will obtain
the necessary unlock disk.

If you will send me an email with your address, I will be glad to send you
some blank CD-R or CD-RWs.  Also, I'll be glad to pay the postage.

Dave

----- Original Message -----
From: "Robert K. Meyer" <bmeyer@union-tel.com>
To: "David Heath" <downeast@VOL.COM>
Sent: Thursday, February 28, 2002 9:44 PM
Subject: Re: INSTALLATION ISSUES/ HISWORD/OLBIBLE


> I have the AV-NIV combination. I don't have a convenient
> place to upload it at present. I could burn a CD. I would
> really like to put together the OLB and all files on a CD,
> but I'm pretty slow at getting around to stuff.
>
> Let me if there is anything else present you want. I could
> even burn my HP200LX flash setup. You would need the unlock
> disk for the NIV.
>
> Bob
> >
> > ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
> --
> R.K. Meyer MSEE K7PPC bmeyer@union-tel.com Elk Mountain WY
> http://w3.union-tel.com/~bmeyer/   His name...  Isaiah 9:6
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 6 Mar 2002 17:21:55 +0200
Reply-To:     davidb@netmedia.net.il
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         David Becher <davidb@NETMEDIA.NET.IL>
Subject:      Re: Problems with Mocha PPP
Content-transfer-encoding: 7BIT

Dario Draiman writes:
> Does anyone have it working? I've set up a 38400 bps connection but it's extremely slow and doesn't complete the transmissions. Other speeds doesn't work at all. The configuration is the one at Daniel's page.

I have it working fine. If you have a single speed HPLX you wont be able
to go over 19200.

What software are you using on the HPLX?

--
** David Becher
** davidb@netmedia.net.il   davidb@cimatron.co.il
** www.cimatron.co.il

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 10:36:17 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: SPD31.EXE Shift-Ctrl-Del Slowdown?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Russel

On Wed, 6 Mar 2002 19:38:44 +0000, Russel Brooks <rlbrooks@POBOX.COM> wrote:

> The doc for SPD31.EXE, the speed driver from Times2Tech,
> mentions several keys strokes that control various feature
> including Shift-Ctrl-Del to slow down.  I've tried this without
> any apparent change.  Should I detect something or am I missing
> something?

If I press Sh-Ctrl-Del while reading your email with Post/LX, I see a
big difference in scrolling speed.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 10:36:18 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi PK

On Thu, 7 Mar 2002 02:00:42 +0530, pksharma <pksharma@CAL.VSNL.NET.IN> wrote:

> a SECOND pcmcia slot .. mine is missing ..
> i have only one :-((

The second one is in inside the LX (screen half) and a Mokia Datacard
is mounted there. It is wired only for I/O purposes, so it is
unfortunately not possible to use it to hold a permanent drive like a
flash card.

But I think it would be possible to let it hold a modem mermanently
(since the Noia Datacard is something similar). Has anyone tried that?
So if you swap often between a modem and a flash card, you could use a
700LX, mount the modem permanently into the Datacard slot (if you don't
need the datacard), and use the regular PCMCIA slot for the flash disk.

What does LXCIC say if invoked on a 700LX? Does it recignize the Nika
Datacard in the second slot as well as any card in the first slot?

GT
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 10:36:19 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Axel

On Thu, 7 Mar 2002 00:00:17 +0100, Axel Berger <Axel-Berger@NEXGO.DE> wrote:

> connector a PCMCIA slot. I have not tried to fit another card there -
> though for certain usages a flashdisk might come handy, especially if the
> 700 innards could be made to fit inside a 200 case.

How is a second PCMCIA slot connected to the motherboard? Just in
parallel to the first one? If so, it should be no too big problem to
solder a CF card (or the innards of one) permanently to the PCMCIA
contacts of the motherboard.
Does anyone have a spare 200LX motherboard and a small CF card to try?
Maybe it would even fit into the 200LX then. I have not taken a CF card
apart yet, but if you don't have any memory expansion board in your LX,
there is eventually enough room for the circuit board of a CF card.

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 11:33:34 +0100
Reply-To:     Erwann ABALEA <erwann@ABALEA.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Erwann ABALEA <erwann@ABALEA.COM>
Organization: Halfling Soft
Subject:      Re: PC Card Partitions with 200LX ?
In-Reply-To:  <D8020D6F0DB8D211B99A0008C7C59CFE0FD8F746@cormails1.jdedwards.com>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=iso-8859-1
Content-Transfer-Encoding: quoted-printable

On Wed, 6 Mar 2002, Feldman, Robert wrote:

> Here's something interesting that others might follow up on:
>
> I copied CSMAPPER.SYS and CARDDRV.EXE from a Win95 computer to my flash=
 card
> (normally drive A:) and then ran them on my 200LX by putting the follow=
ing
> in my CONFIG.SYS
>
>      DEVICE=3DA:\CSMAPPER.SYS
>      DEVICE=3DA:\CARDDRV.EXE /PART=3D2
>
> Surprisingly, both devices appear to have installed, and CARDDRV report=
s
> that it installed 4 drives, F: - I: . I can still read my flash card as
> drive A:, but none of the "new" drives will work. BTW, I have a 20MB Su=
nDisk
> card with only one partition on it.

Stupid question: did you specify a LASTDRIVE=3D directive in your config.=
sys
file?

--=20
Erwann ABALEA <erwann@abalea.com> - RSA PGP Key ID: 0x2D0EABD5
-----
Je viens d'adopter une limace (elle s'appele "Chompie"), et j'ai trouve
des infos sur un site qui n'a pas ete mis a jour depuis des siecles!
Meme si l'auteur ne s'y interesse plus, le site garde tout son interet.
-+- P in : Guide du Neuneu d'Usenet - L'=EAre des limaces m=E9dia -+-

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 12:10:58 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

This is cool idea, disassembled CF card should fit in to 200lx without big problems. Then the PCMCIA slat can be used for something else than a memory.
I have at home schematics of Sharp PC3100 palmtop which has two PCMCIA slots, I can look how they are connected, but they are
release 1 so it can be different.

I don't have a small CF card for eventual destruction so I can't try it on my 200lx.

Radek




                    Daniel Hertrich
                    <daniel.hertrich           To:  HPLX-L@UConnVM.UConn.Edu
                    @GMX.DE>                   cc:  (bcc: Radek Svagr/HRC/COMP/PHILIPS)
                    Sent by: HPLX              Subject:  Re: HP collection
                    Mailing List
                    <HPLX-L@UConnVM.           Classification:
                    UConn.Edu>


                    2002-03-07 09:36
                    AM
                    Please respond
                    to Daniel
                    Hertrich






Hi Axel

On Thu, 7 Mar 2002 00:00:17 +0100, Axel Berger <Axel-Berger@NEXGO.DE> wrote:

> connector a PCMCIA slot. I have not tried to fit another card there -
> though for certain usages a flashdisk might come handy, especially if the
> 700 innards could be made to fit inside a 200 case.

How is a second PCMCIA slot connected to the motherboard? Just in
parallel to the first one? If so, it should be no too big problem to
solder a CF card (or the innards of one) permanently to the PCMCIA
contacts of the motherboard.
Does anyone have a spare 200LX motherboard and a small CF card to try?
Maybe it would even fit into the 200LX then. I have not taken a CF card
apart yet, but if you don't have any memory expansion board in your LX,
there is eventually enough room for the circuit board of a CF card.

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 16:15:58 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> What does LXCIC say if invoked on a 700LX? Does it recignize the Nika
> Datacard in the second slot as well as any card in the first slot?

No, at least it does not say so in any way.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 22:23:17 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      OT : Video Viewer for working in DOS on a DESKTOP
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Any one have any idea if there exists
a viewer for viewing video clips ( .avi,
.dat) in dos ?

..pk

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 22:26:02 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      OT : Any idea what is CODEVIEW & where to get it ?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I need codeview (needed by a
friend back from usa , italy , )
to analyse and improve a small
exe and a small .com program ..
probably needs codeview .. any
idea where to get it ? is it free ?
if not, what does it cost ? any
sellers ? what is the size ?

..pk

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 12:06:33 -0500
Reply-To:     Dennis Bell <doppelbike@EMAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dennis Bell <doppelbike@EMAIL.COM>
Subject:      Re: PDF Viewer...
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit
MIME-Version: 1.0

I have a copy of a DOS program which will convert
PDF files to text.  It is called PDFTOTEXT (v0.80) by
Derek Noonburg.

There are a few shortcomings, the biggest of which
is that it will NOT run on the LX.  It also does not
handle 2-column text very well, which means a fair
bit of post-processing is necessary to make a
readable text file.

I can send it to the SUPER-master if folks would like
to see it there.

Dennis Bell

--

_______________________________________________
Sign-up for your own FREE Personalized E-mail at Email.com
http://www.email.com/?sr=signup

Travelocity.com is giving away two million travel miles.
http://ad.doubleclick.net/clk;3969773;6991039;g?http://svc.travelocity.com/promos/millionmiles_main/0,,TRAVELOCITY,00.html

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 19:50:16 +0100
Reply-To:     Norbert_Giese@T-Online.de
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Norbert Giese <Norbert_Giese@T-ONLINE.DE>
Subject:      Re: Question regarding Quick/LX
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Nathalie,

thank you for confirming that Quick/LX runs without problems on
your machine.

I have read the instructions word by word. However, installing
Quick/LX raises the described problems, removing it and restarting
lets the problems disappear.

My assumption now is that my machine must be differently configured.
Would you mind sending me your CONFIG and AUTOEXEC for comparison?
It might ease to diagnose the cause?

Thanks
 Norbert
--
Norbert Giese, A.Stifter-Weg 10, 71116 Gaertringen

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 20:28:22 +0100
Reply-To:     Juan Belmonte <jbmbhs@eresmas.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Juan Belmonte <jbmbhs@ERESMAS.COM>
Subject:      CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Daniel Hertrich on Thursday, March 07, 2002 9:36 wrote:

> How is a second PCMCIA slot connected to the motherboard? Just in
> parallel to the first one? If so, it should be no too big problem to
> solder a CF card (or the innards of one) permanently to the PCMCIA
> contacts of the motherboard.

Looks very good...

> Does anyone have a spare 200LX motherboard and a small CF card to try?
> Maybe it would even fit into the 200LX then. I have not taken a CF card
> apart yet, but if you don't have any memory expansion board in your LX,
> there is eventually enough room for the circuit board of a CF card.

Three questions:
    1.- If it's possible to connect one internal CF card...  LXCIC may
recognice it?

    2.- Mine is an older HP200LX ( SG5* ) 2Mb model (1Mb on motherboard and
1Mb daughtercard). If first question its succesful, mine can be converted to
an 1Mb + 64 Mb internal CF leaving free the PCcard slot but getting out the
daughtercard?

    3.- I'm still not enough crazy to test with my main (and only!!)
palmtop. For testing pusposes; Two unassembled CF to PCcard adaptor and two
standard CF cards, soldering iron to test it external and get working two CF
cards before do anything inside the palmtop

Regards

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 14:28:47 -0500
Reply-To:     Bing <bxu2@UWO.CA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bing <bxu2@UWO.CA>
Subject:      Desktop<->lx
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

Can I install a PCMCIA driver in the desktop PC so I can transfer files
faster. Using Tfwin200 and serial port is too slow, and using CF in a
PCMCIA adapter is only to my laptop.
Bing

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 13:44:18 -0600
Reply-To:     TomSalwasser@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tom Salwasser <TomSalwasser@COMPUSERVE.COM>
Subject:      Re: Desktop<->lx
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Bing, I use the Actiontec PC-750 PC card reader in my desktop, it works very
well.
http://www.cdw.com/shop/products/default.asp?EDC=213488

The PC-750 uses a PCI slot, the PC-700 uses an ISA slot.


>
> Can I install a PCMCIA driver in the desktop PC so I can transfer files
> faster. Using Tfwin200 and serial port is too slow, and using CF in a
> PCMCIA adapter is only to my laptop.
> Bing
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 14:10:37 -0600
Reply-To:     "David R. Birch" <dbirch@WI.RR.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "David R. Birch" <dbirch@WI.RR.COM>
Subject:      Re: Desktop<->lx
Comments: To: Bing <bxu2@UWO.CA>
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Bing wrote:
>
> Can I install a PCMCIA driver in the desktop PC so I can transfer files
> faster. Using Tfwin200 and serial port is too slow, and using CF in a
> PCMCIA adapter is only to my laptop.
> Bing

Yes, I picked up a card and drive combo on Ebay. The ISA card has
two Type II sockets, and a ribbon cable goes to a second pair
that fit in a 3.5" floppy bay. If you're interested, I have
another combo that doesn't have the sockets in the ISA card, just
two sockets that fit in a 3.5' bay. I accidentally bid on and won
both in my first time on Ebay. Fortunately it was a fairly cheap
lesson, but now I have a spare PCMCIA setup. $20 plus shipping.

David

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 15:30:28 -0500
Reply-To:     Martin Bergvill <hplx@BERGVILL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Martin Bergvill <hplx@BERGVILL.COM>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Sun,  3 Mar 2002 21:58:18 +0200, Daniel Hertrich wrote:

> An interesting (private) site with information about all HP calculators,
> palmtops etc in German, with pictures:
>
> http://www.hp-collection.org/hewlettpackard.htm
>
> and especially:
>
> http://www.hp-collection.org/hewlettpackard.htm#organizer

Thanks..I found my old calculator on that site.. I thought it was the
32s I had a long time ago ,but it was a 38s with led display..almost
brought a tear to my eye seeing it again :-)

(I think I have also had a 32s..)

Regards

--
Martin Bergvill ,Narvik Norway

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 11:10:28 +1300
Reply-To:     Roger Whitmarsh <lodger@NZ1.IBM.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Roger Whitmarsh <lodger@NZ1.IBM.COM>
Subject:      What is VBRJP200.DLL?
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Does anyone know what piece of software the above belongs to?

Cheers...Roger

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 17:37:39 -0500
Reply-To:     Martin Bergvill <hplx@BERGVILL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Martin Bergvill <hplx@BERGVILL.COM>
Subject:      Re: Ol' Eddie Archive
Comments: To: childers@GARLIC.COM
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Wed,  6 Mar 2002 17:59:23 -0500, Eduardo Seudsnimo wrote:

Hi Eduardo And Bill

> Did anybody ever get their hands on the Eddie files? I can host them if
> it's not more'n a few gigs.

I have no idea how big it is. I just found the message From Bill which
I forwarded to the list in my inbox.

I have sent a copy of this message to his emailadress. Not sure if he
is active here at the moment.

Bill:

You sent a email to the Hplx-l a long time ago where you talked about
the Eddie archives. How big are they and are you willing to send them
off to Eduardo or maybe the Superteam?

You talked about putting them on the web somewhere and now we have a
volunteer to put them on his site. How about it?

What are in the Eddie archives?

Not sure if you are still on the Hplx-l so I am sending this to the
address you posted with a long time ago.

> I got  some minix stuff on there to start. If you want minix go get it:
>
> ftp://badeddie.no-ip.com/pub/eddie/
>
> Looks like I can spare about 4 gigs.
>
> BTW: I think I got a pretty tight FTP server setup but let know if you see any security issues.
>
> Thanks,

We just have to see if we get any response.

Thanks for your suggestion.

Regards

--
Martin Bergvill ,Narvik Norway

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 23:11:11 +0100
Reply-To:     Norbert_Giese@T-Online.de
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Norbert Giese <Norbert_Giese@T-ONLINE.DE>
Subject:      Re: Lotus 123 - where to store macros
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Hi Nathalie,

about 19K for a WK1 file with only two cells filled is far too much.
Hiding rows does not change the file size. I guess there is more.

My tip: Open a new sheet, and do a Transfer, Copy, Named Range, etc.
to get the data (cells E1 and H1) into the new sheet. Save it
and you will be surprised.

If you still have trouble with the file, I can have a look.

Norbert

--
Norbert Giese, A.Stifter-Weg 10, 71116 Gaertringen

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 15:58:31 -0800
Reply-To:     Terry Matson <ttmatson@earthlink.net>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Terry Matson <ttmatson@EARTHLINK.NET>
Subject:      Transfile / Connectivity Pack on IMAC
MIME-Version: 1.0
Content-Type: multipart/alternative;
              boundary="----=_NextPart_000_002F_01C1C5F0.EDAAC820"

This is a multi-part message in MIME format.

------=_NextPart_000_002F_01C1C5F0.EDAAC820
Content-Type: text/plain;
        charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Has (or is it even possible) anyone using the Transfile and Connectivity =
Pack
on an IMAC?

I am aware there are "window emulators" for the Mac and IF it is =
possible
to run the above programs which of these emulators would you recommend?

I am seriously considering a IMAC as I am very tired of windoze - so any
insight would be helpful (though tired of windoze NOT willing to give up
the HP<g>).

Many THANKS in advance for any advice received : )
terry

------=_NextPart_000_002F_01C1C5F0.EDAAC820
Content-Type: text/html;
        charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0 Transitional//EN">
<HTML><HEAD>
<META http-equiv=3DContent-Type content=3D"text/html; =
charset=3Diso-8859-1">
<META content=3D"MSHTML 6.00.2712.300" name=3DGENERATOR>
<STYLE></STYLE>
</HEAD>
<BODY bgColor=3D#ffffff>
<DIV><FONT face=3DArial size=3D2>Has (or is it even possible) anyone =
using the=20
Transfile and Connectivity Pack</FONT></DIV>
<DIV><FONT face=3DArial size=3D2>on an IMAC?</FONT></DIV>
<DIV><FONT face=3DArial size=3D2></FONT>&nbsp;</DIV>
<DIV><FONT face=3DArial size=3D2>I am aware there are "window emulators" =
for the Mac=20
and IF it is possible</FONT></DIV>
<DIV><FONT face=3DArial size=3D2>to run the above programs which of =
these emulators=20
would you recommend?</FONT></DIV>
<DIV><FONT face=3DArial size=3D2></FONT>&nbsp;</DIV>
<DIV><FONT face=3DArial size=3D2>I am seriously considering a IMAC as I =
am very=20
tired of windoze - so any</FONT></DIV>
<DIV><FONT face=3DArial size=3D2>insight would be helpful (though tired =
of windoze=20
NOT willing to give up</FONT></DIV>
<DIV><FONT face=3DArial size=3D2>the HP&lt;g&gt;).</FONT></DIV>
<DIV><FONT face=3DArial size=3D2></FONT>&nbsp;</DIV>
<DIV><FONT face=3DArial size=3D2>Many THANKS in advance for any advice =
received :=20
)</FONT></DIV>
<DIV><FONT face=3DArial size=3D2>terry</FONT></DIV></BODY></HTML>

------=_NextPart_000_002F_01C1C5F0.EDAAC820--

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 01:11:02 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: eMail
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> Actually, GP is quite good at managing multiple dial-up methods.

I have now copied GP to the LX and started installing it on my games
console (my old eyes you know). It is far more concise than nettamer and
the logic with separate sets of mailhosts and locales fits my mobile needs
perfectly. Only snag is: I won't ever be able to send mail with it!

My email servers are separate from the providers and I expect to use their
smtp either via smtp after pop or with a password. I could use a provider's
smtp instead - though that is inconvenient, as I might ask somebody to use
his dialup when abroad instead of making an international GSM call - as GP
wants me to, *BUT* with all my providers the username for smtp is different
from that used for logon and the password ought to be.

Is there any way to reach the author?

Danke
        Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 00:44:38 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: SPD31.EXE Shift-Ctrl-Del Slowdown?
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Daniel Hertrich wrote:
> On Wed, 6 Mar 2002 19:38:44 +0000, Russel Brooks <rlbrooks@POBOX.COM> wrote:
> > The doc for SPD31.EXE, the speed driver from Times2Tech,
> > mentions several keys strokes that control various feature
> > including Shift-Ctrl-Del to slow down.  I've tried this without
> > any apparent change.  Should I detect something or am I missing
> > something?
>
> If I press Sh-Ctrl-Del while reading your email with Post/LX, I see a
> big difference in scrolling speed.

If I press it while reading your post I get asked if I want to
delete mail on the host.  Why isn't SPD31 seeing it?
If you're lurking Mack, any ideas?

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 02:54:42 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: eMail
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

The following hasn't come through in about two hours. Sorry in advance
should it now be sent twice:

> Actually, GP is quite good at managing multiple dial-up methods.

I have now copied GP to the LX and started installing it on my games
console (my old eyes you know). It is far more concise than nettamer and
the logic with separate sets of mailhosts and locales fits my mobile needs
perfectly. Only snag is: I won't ever be able to send mail with it!

My email servers are separate from the providers and I expect to use their
smtp either via smtp after pop or with a password. I could use a provider's
smtp instead - though that is inconvenient, as I might ask somebody to use
his dialup when abroad instead of making an international GSM call - as GP
wants me to, *BUT* with all my providers the username for smtp is different
from that used for logon and the password ought to be.

Is there any way to reach the author?

Danke
        Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 03:18:23 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Going Postal
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Problem: Doesn't do anything.

I have set up everything as well as I am capable and tried to log on. The
modem is iniatialized:

ATZ1
OK

and then - nothing. Why doesn't the damn thing try to dial? What can it be
waiting for? I know no modem that says anything else but "OK" on receiving
config commands. Any ideas?

Danke
        Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 23:54:40 -0600
Reply-To:     Curtis Cameron <curtc@AIRMAIL.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Curtis Cameron <curtc@AIRMAIL.NET>
Organization: None
Subject:      Re: OT : Video Viewer for working in DOS on a DESKTOP
Comments: To: pksharma <pksharma@CAL.VSNL.NET.IN>
In-Reply-To:  <004001c1c5f8$955c4ce0$2facc8cb@q20>
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

On Thu, 7 Mar 2002 22:23:17 +0530 pksharma wrote:
>Any one have any idea if there exists
>a viewer for viewing video clips ( .avi,
>.dat) in dos ?

The web site "Interesting DOS Programs" has at least two listed. Along
with MP3 players, RealAudio players, CD Burners, disk utilities, and
lots more. It's at http://www.opus.co.tt/dave/index.htm .

--
Curtis Cameron

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 7 Mar 2002 21:58:35 -0800
Reply-To:     Alfred1520 <alfred1520@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Alfred1520 <alfred1520@YAHOO.COM>
Subject:      Re: OT : Any idea what is CODEVIEW & where to get it ?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Codeview is the symbolic debugger of Microsoft's 16-bit C
compiler.  I doubt it is still available for sale.  There's probably
is no way of getting it unless you can find it on the Net (which
I have't tried.)

Best Regards,
Alfred


-----Original Message-----
From: pksharma <pksharma@CAL.VSNL.NET.IN>
To: HPLX-L@UConnVM.UConn.Edu <HPLX-L@UConnVM.UConn.Edu>
Date: Thursday, March 07, 2002 1:18 PM
Subject: OT : Any idea what is CODEVIEW & where to get it ?


>I need codeview (needed by a
>friend back from usa , italy , )
>to analyse and improve a small
>exe and a small .com program ..
>probably needs codeview .. any
>idea where to get it ? is it free ?
>if not, what does it cost ? any
>sellers ? what is the size ?
>
>..pk
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 08:51:45 +0100
Reply-To:     hpstaber@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         HP Staber <hpstaber@COMPUSERVE.COM>
Subject:      Re: SPD31.EXE Shift-Ctrl-Del Slowdown?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

> Daniel Hertrich wrote:
> > On Wed, 6 Mar 2002 19:38:44 +0000, Russel Brooks <rlbrooks@POBOX.COM> =
wrote:
> > > The doc for SPD31.EXE, the speed driver from Times2Tech,
> > > mentions several keys strokes that control various feature
> > > including Shift-Ctrl-Del to slow down.  I've tried this without
> > > any apparent change.  Should I detect something or am I missing
> > > something?
> >
> > If I press Sh-Ctrl-Del while reading your email with Post/LX, I see a
> > big difference in scrolling speed.
>
> If I press it while reading your post I get asked if I want to
> delete mail on the host.  Why isn't SPD31 seeing it?
> If you're lurking Mack, any ideas?

Russ,

I also notice a considerable difference in speed when scrolling,
sorting etc. The shft-ctrl-del really toggles the speed.

HP Staber/Salzburg

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 08:46:30 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      Re: CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Somebody has mentioned here a kind of device which makes two pcmcia slots from one. What is inside it? A new PCMCIA controller, or just paralel
slots + external power ? I was looking on PCMCIA BUS pinout:

pin 7: /CE1         ... card enable1
pin 36: /CD1        ... card detect 1
pin 42: /CE2        ... card enable 2
pin 67: /CD2        ... card detect 2

If there will be a confirmation that PCMCIA controler in 200lx can theoreticaly handle two cards, I am crazy enough to test it with my only 200lx and my 128MB CF card...

Does anyone know what PCMCIA controler is inside of our 200lx?

Radek




                    Juan Belmonte
                    <jbmbhs@ERESMAS.           To:  HPLX-L@UConnVM.UConn.Edu
                    COM>                       cc:  (bcc: Radek Svagr/HRC/COMP/PHILIPS)
                    Sent by: HPLX              Subject:  CF inside HP200LX  ( was: Re: HP collection
                    Mailing List
                    <HPLX-L@UConnVM.           Classification:
                    UConn.Edu>


                    2002-03-07 08:28
                    PM
                    Please respond
                    to Juan Belmonte






Daniel Hertrich on Thursday, March 07, 2002 9:36 wrote:

> How is a second PCMCIA slot connected to the motherboard? Just in
> parallel to the first one? If so, it should be no too big problem to
> solder a CF card (or the innards of one) permanently to the PCMCIA
> contacts of the motherboard.

Looks very good...

> Does anyone have a spare 200LX motherboard and a small CF card to try?
> Maybe it would even fit into the 200LX then. I have not taken a CF card
> apart yet, but if you don't have any memory expansion board in your LX,
> there is eventually enough room for the circuit board of a CF card.

Three questions:
    1.- If it's possible to connect one internal CF card...  LXCIC may
recognice it?

    2.- Mine is an older HP200LX ( SG5* ) 2Mb model (1Mb on motherboard and
1Mb daughtercard). If first question its succesful, mine can be converted to
an 1Mb + 64 Mb internal CF leaving free the PCcard slot but getting out the
daughtercard?

    3.- I'm still not enough crazy to test with my main (and only!!)
palmtop. For testing pusposes; Two unassembled CF to PCcard adaptor and two
standard CF cards, soldering iron to test it external and get working two CF
cards before do anything inside the palmtop

Regards

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 01:23:24 -0700
Reply-To:     Kiyoshi Akima <k_akima@HOTMAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Kiyoshi Akima <k_akima@HOTMAIL.COM>
Subject:      CodeView
Mime-Version: 1.0
Content-Type: text/html

<html><div style='background-color:'><DIV>&gt; I need codeview (needed by a<BR>&gt; friend back from usa , italy , )<BR>&gt; to analyse and improve a small<BR>&gt; exe and a small .com program ..<BR>&gt; probably needs codeview .. any<BR>&gt; idea where
to get it ? is it free ?<BR>&gt; if not, what does it cost ? any<BR>&gt; sellers ? what is the size ?<BR><BR>CodeView is (was) the debugger shipped with the Microsoft compilers back in the days before everything ran under Windows. AFAIK it was never a
separate product on its own. I don't have a copy handy so I can't tell you how big it is, but it should run on the LX since early versions ran fine on XTs.</DIV>
<DIV>&nbsp;</DIV>
<DIV>Good luck finding it. If you can find a pre-Windows Microsoft compiler, you may be able to get it that way.</DIV>
<DIV>&nbsp;</DIV>
<DIV>Kiyoshi Akima</DIV></div><br clear=all><hr>Get your FREE download of MSN Explorer at <a href='http://g.msn.com/1HM105401/13'>http://explorer.msn.com</a>.<br></html>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 01:27:49 -0700
Reply-To:     Kiyoshi Akima <k_akima@HOTMAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Kiyoshi Akima <k_akima@HOTMAIL.COM>
Subject:      PC Card problem
Mime-Version: 1.0
Content-Type: text/html

<html><div style='background-color:'><DIV>I have a 1995 vintage IBM 40MB PC card that has seen daily use in my LX. All of a sudden it failed today. I put it in the slot and the system can't read it. After several cycles of removal and reinsertion, it will
eventually work. The same thing happens on several laptops from different manufacturers as well as on a WinCE machine (yes, I'll admit to owning one of those).</DIV>
<DIV>&nbsp;</DIV>
<DIV>Is the card simply "worn out"? Dirty or eroded contacts? Any ideas other than replacing it?</DIV>
<DIV>&nbsp;</DIV>
<DIV>Thanx in advance,</DIV>
<DIV>Kiyoshi Akima</DIV></div><br clear=all><hr>Get your FREE download of MSN Explorer at <a href='http://g.msn.com/1HM105401/13'>http://explorer.msn.com</a>.<br></html>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 19:34:00 +1100
Reply-To:     Paul Johnson <paulj@SILCHIP.COM.AU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Paul Johnson <paulj@SILCHIP.COM.AU>
Subject:      Re: pdf viewer?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Juan Belmonte wrote:
> Bad news: ACRODOS Also needs 386+
>
> Instead, I'm using GhostSript to convert PDF's to monochrome PCX's at 72 or
> 96 dpi.
> And use the EXCELLENT Peichl's LXPIC...
> I'm using by to read datasheets of IC's and microcontrollers.
>

I'm about to scurry to the desktop PC to read the docs about GhostScript
converting to PCX, sounds like a excellent way to view some PDFs. There
is a GhostScript available for DOS isn't there ? Are you using
GhostScipt on the LX ?

> For main text PDF's I use the accesibility plugin of Acrobat Reader 4 to
> extract all text in pdf to TXT file but formatting it's VERY UGLY and
> dificult to read if (example) two columns by page...
>
> It's the best solution I found... If anyone knows best... PLEASE, Tell me!
>
> Regards
>

Well I wouldn't call it a better solution, as it is still not
completely "on" the LX, but a PDF can be emailed to a PDF to Text
translator at:

 <pdf2txt@sun.trace.wisc.edu>

This also produces a sometimes difficult to read result, like using
Acrobat and extracting the text, but sometimes anything is better than
nothing.

Or if you have one of the many methods of viewing a HTML file on the LX
and you think it will produce a more suitable result, theres a PDF to
HTML translator at:

 <pdf2html@sun.trace.wisc.edu>

Again, this can be a bit ugly sometimes. The resulting file is normally
processed very promptly, and emailed back to you. Its not something I'd
normally use, but it has come in handy a couple of times.

Paul Johnson


> ----- Original Message -----
> From: "Radek Svagr" <radek.svagr@LGPHILIPS-DISPLAYS.COM>
> To: <HPLX-L@UConnVM.UConn.Edu>
> Sent: Wednesday, March 06, 2002 12:00 PM
> Subject: pdf viewer?
>
> > Is there any way how to view PDF files on 200lx? There is Acrobat reader
> ver 1.0 for DOS, but apparently needs VGA.
> >
> > Radek
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 10:14:53 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Going Postal
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Axel

On Fri, 8 Mar 2002 03:18:23 +0100, Axel Berger <Axel-Berger@NEXGO.DE> wrote:

> ATZ1
> OK
>
> and then - nothing. Why doesn't the damn thing try to dial? What can it be
> waiting for? I know no modem that says anything else but "OK" on receiving
> config commands. Any ideas?

What modem do you use for this test?
If it is a mobile phone with data cable, it is probably a missing DCD
line on the data cable. The only way to get around it is to either
build your own data cable as I describe on
http://www.daniel-hertrich.de/s25_hplx of connect the DCD line (pin 1)
of the HP-side plug with another line which is "1" during the whole
call (probably DSR, but I am not sure).

Did you try is also with a normal landline modem?

What cabeling do you use? HP cable, null modem adapter, modem/phone
cable? What null modem adapter? There are some models lacking important
handshaking lines. See http://www.daniel-hertrich.de/rs232

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 10:14:55 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Transfile / Connectivity Pack on IMAC
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Terry

On Thu, 7 Mar 2002 15:58:31 -0800, Terry Matson <ttmatson@EARTHLINK.NET> wrote:

> I am aware there are "window emulators" for the Mac and IF it is possible
> to run the above programs which of these emulators would you recommend?
>
> I am seriously considering a IMAC as I am very tired of windoze - so any
> insight would be helpful (though tired of windoze NOT willing to give up
> the HP<g>).

Aren't the new Macs (also IMACs?) shippied with MAC OS X, which is a
UNIX derivate? If so, you can probably run lxtools for Linux on it. See
SUPER...

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 10:14:56 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: SPD31.EXE Shift-Ctrl-Del Slowdown?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Russell

On Fri, 8 Mar 2002 00:44:38 +0000 (GMT), Russel Brooks <rlbrooks@pobox.com> wrote:

> If I press it while reading your post I get asked if I want to
> delete mail on the host.  Why isn't SPD31 seeing it?
> If you're lurking Mack, any ideas?

Which version of SPD31 do you use?
AFAIK the .SYS file only supports the basic things like all the timing
corrections, but no hot keys. The EXE version is the one for all the
features. (Or am I wrong?).

I have the following as the first line in my config.sys:

device=\drivers\t2t\speed\spd31.exe /M /C /K /N

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 10:14:59 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: ANN: Syslog 1.0
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Bruce

On Tue, 5 Mar 2002 10:18:36 -0500, Bruce Martin <Bruce_Martin@MANULIFE.COM> wrote:

> I have a 5K utility called NOW.EXE (I think it may be from PC Magazine)
> which allows me to do this in 2 batch file lines:
>
> echo now >> startup.log
> echo Starting Software Carousel >> startup.log

Too complicated. ;-)

I wanted to have a 1-EXE-file utility which does the job using a very
simple call in a batch file, because so it's easy to keep batch files
simple, but generate lots of syslog entries from them.

Now, a line

syslog "this is written to the syslog file"

is enough.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 10:15:00 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: ANN: Syslog 1.0
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Russel

On Tue, 5 Mar 2002 02:53:32 +0000, Russel Brooks <rlbrooks@POBOX.COM> wrote:

> I've been doing this for a long time with the following Rexx
> program.  Call it from BAT files like:
>
> rexx ts Starting Software Carousel
>
> /** TS.Rex - TimeStamp **/
> parse value date('S')time()date('W') with 3 yymm 7 dd 9 hhmm 14 . 17 dow 19 .
> file = 'C:\TS'yymm'.LOG'
> if arg(1) <> '' then call lineout file, dow dd hhmm space(arg(1))
> call lineout file  /* close file */
> exit
>
> Besides being a nice language by itself Rexx can also act a
> super utility to make your BAT files more useful.

Thanks for the idea!

Rexx is definitely a powerful tool and I wanted to learn it for a long
time ;-)

But for such a purpose, isn't it too slow? Doesn't the whole
interpreter have to be loaded for just one ts call in a batch file?

How big is the interpreter executable?

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 09:59:25 +0100
Reply-To:     Alan Krempler <alan@oeh.tu-graz.ac.at>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Alan Krempler <alan@SBOX.TU-GRAZ.AC.AT>
Subject:      CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

i could donate a 10mb sandisk cf card (with a few irrepairably bad blocks)
for experiments

alan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 05:14:39 -0500
Reply-To:     Larry Tachna <ltachna@ATT.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Larry Tachna <ltachna@ATT.NET>
Subject:      Re: CodeView
In-Reply-To:  <F119IZfSp1J106zPpPk0000f380@hotmail.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

codeview v3.11 is 508k the help file that goes with it is 231k and yes as I
recall it does run on the 100/200

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 05:14:17 -0700
Reply-To:     kwmiller@azbcs.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "ABCS INC." <kwmiller@AZBCS.COM>
Subject:      200lx ethernet adapter
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Anyone have a current source for Ethernet adapters that work with a
doublespeed 200lx palmtop?  I haven't been able to find the Accton En2216-1
card anywhere..

thx

Kevin Miller
ABCS INC.
kwmiller@azbcs.com <mailto:kwmiller@azbcs.com>
602-943-0159
www.azbcs.com <http://www.azbcs.com>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 13:21:23 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Alan

On Fri, 8 Mar 2002 09:59:25 +0100, Alan Krempler <alan@SBOX.TU-GRAZ.AC.AT> wrote:

> i could donate a 10mb sandisk cf card (with a few irrepairably bad blocks)
> for experiments
>

This would be great! I will let you know when testing begins.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 13:21:21 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Radek

On Fri, 8 Mar 2002 08:46:30 +0100, Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM> wrote:

> Somebody has mentioned here a kind of device which makes two pcmcia slots from one. What is inside it? A new PCMCIA controller, or just paralel
> slots + external power ? I was looking on PCMCIA BUS pinout:

It was the Accurite DoubleSlot.
I'm currently talking with the people at Accurite about that problem.
They say, it is not just two parallel ports, but there has to be a
special logic, but the 200LX has this logic built-in.

I'm still waiting for some more info from them, and if I have it, I
will report.

> pin 7: /CE1         ... card enable1
> pin 36: /CD1        ... card detect 1
> pin 42: /CE2        ... card enable 2
> pin 67: /CD2        ... card detect 2

So, this seems to be the necessary logic! :-)

Stefan, do you know if the card services software in the LX supports
two slots (the CE2 / CD2 signals)? How does LXCIC handle that?

> If there will be a confirmation that PCMCIA controler in 200lx
> can theoreticaly handle two cards, I am crazy enough to test it
> with my only 200lx and my 128MB CF card...

I thought about testing it first with an old 200LX motherboard and a
cheap 4MB CF card. ;-) But every other testing is welcome, of course!


> Does anyone know what PCMCIA controler is inside of our 200lx?

It is not one of the standards used today (intel 82365 ot Databook
TCIC).

GTX
daniel
--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 07:00:11 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: 200lx ethernet adapter
In-Reply-To:  <BLENKJJKIJHGOGCHGNNNAEBBENAA.kwmiller@azbcs.com>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Fri, 8 Mar 2002, ABCS INC. wrote:

> Anyone have a current source for Ethernet adapters that work with a
> doublespeed 200lx palmtop?  I haven't been able to find the Accton En2216-1
> card anywhere..

Back in December I was able to pick up an Accton EN2216-1-J1 for
$20.00 from gretchen_tai@yahoo.com.  She had a number of them at the
time.  The card was new and the package unopened--it came with a
Japanese user manual (the J1 part?), but seems to work fine.

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 14:32:55 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: PC Card problem
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Kiyoshi

please turn off HTML when posting to the list!

On Fri, 8 Mar 2002 01:27:49 -0700, Kiyoshi Akima <k_akima@HOTMAIL.COM> wrote:

> <html><div style='background-color:'><DIV>I have a 1995 vintage IBM 40MB PC card that has seen daily use in my LX. All of a sudden it failed today. I put it in the slot and the system can't read it. After several cycles of removal and reinsertion, it
w
> ill eventually work. The same thing happens on several laptops from different manufacturers as well as on a WinCE machine (yes, I'll admit to owning one of those).</DIV>
> <DIV>&nbsp;</DIV>
> <DIV>Is the card simply "worn out"? Dirty or eroded contacts? Any ideas other than replacing it?</DIV>

It can be dirty contacts, of course, as well as maybe a loose contact
inside the card. All in all, if you can afford the money, I would
strongly suggest you to buy aa new one, since your data is not safe
anymore. Even if it is inly a loose contact or dirt, it can damage your
file system seriously.

If you don't want to buy a now card, first try compressed air to blow
out dirt, then try a _very_small_ amount of contact spray, maybe
applied with a needle to every hole.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 14:32:56 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: 200lx ethernet adapter
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Kevin

On Fri, 8 Mar 2002 05:14:17 -0700, "ABCS INC." <kwmiller@AZBCS.COM> wrote:

> Anyone have a current source for Ethernet adapters that work with a
> doublespeed 200lx palmtop?  I haven't been able to find the Accton En2216-1
> card anywhere..

There seem to be other kinds of adapters that work well.
I have found one, which is described (with picture) on
http://www.daniel-hertrich.de/stuff
which works with the same software setup as the Accton EN2216-1 does.

Best would be, if you have the chance, to try a few before you buy one.

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 14:35:14 +0100
Reply-To:     Feher Tamas <feher.tamas@2FKFT.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Feher Tamas <feher.tamas@2FKFT.COM>
Subject:      Re: partitioned flashcard in the 200LX.
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-2"
Content-Transfer-Encoding: 7bit

Hello all,

>I copied CSMAPPER.SYS and CARDDRV.EXE from a Win95 computer
>to my flashcard (normally drive A:) and then ran them on my 200LX by
>putting the following in my CONFIG.SYS
>
>      DEVICE=3DA:\CSMAPPER.SYS
>      DEVICE=3DA:\CARDDRV.EXE /PART=3D2

You could look at the files under this directory, there is a
cardbios.exe, etc inside ZIP.:
ftp://ziatech.com/Tech_support/STD/8921/

Sincerely Yours: Tamas Feher.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 08:52:23 -0500
Reply-To:     Steve <novosad@SERVER030.FWB.SAIC.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Steve <novosad@SERVER030.FWB.SAIC.COM>
Subject:      Re: Ol' Eddie Archive
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

   I would think the ideal solution would be for it to
be held at Palmtop.Net.  I.e. at

http://www.palmtop.net/eddie

With the usual link and description at http://www.palmtop.net/
Is that possible?

Regards

Steve

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 07:12:36 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: PC Card Partitions with 200LX ?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

Lastdrive=J, so that should not be a problem.

BTW, since I have only one partition on my flash card, I didn't expect it to
be read as additional drives. It still was readable as a:.

Which brings up my earlier question: How do you partition a flash card on a
Win2K system?

Bob

-----Original Message-----
From: Erwann ABALEA [mailto:erwann@ABALEA.COM]
Sent: Thursday, March 07, 2002 4:34 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: PC Card Partitions with 200LX ?
<snip>

Stupid question: did you specify a LASTDRIVE= directive in your config.sys
file?
<snip>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 15:43:10 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: Going Postal
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> What modem do you use for this test?
> Did you try is also with a normal landline modem?
A Zyxel 1496 on COM1 of my desktop. As I said, for trying stuff out first I
prefer the easy and readability of the big screen. It might have something
to do with that: GP started in a DOS window freezes the whole machine
completely (reset button only!), only booting directly to DOS (BOOTGUI=0)
works and produces the result described.

> it is probably a missing DCD line on the data cable.
The line is present, but "0" as per the instruction. There can't be a
carrier before dialing thus there must not be a carrier detect. "DCD
follows carrier" is what the manual sais and it is what my modems are
always (those with manual, i.e. the older ones from the time when users
could read) configured to do.

Danke
        Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 09:46:19 -0500
Reply-To:     Andrew <andrewaa@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Andrew <andrewaa@EARTHLINK.NET>
Subject:      Re: Transfile alternative for MAC, try Maclink Plus
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> Subject: Transfile / Connectivity Pack on IMAC
>   Date: Thu, 7 Mar 2002 15:58:31 -0800
>   From: Terry Matson <ttmatson@EARTHLINK.NET>
>
>Has (or is it even possible) anyone using the Transfile and Connectivity Pack
>on an IMAC?

terry
I have used a program called Maclink Plus for HP palmtop to connect my
200LX to a MAC Plus and a 520 powerbook. I imagine it would probably
work with a power PC machine.
You'll need a palmtop to MAC serial cable, I can post pin-out
information if anyone's interested.

The information on the disks is:
DataVis Inc.
55 Corporate Drive
Trumbull CT  06611
203-268-0030
fax 268-4345

No web site listed (the disks are that old....)

--
Andrew King
Ann Arbor Michigan
technology is the answer, what was the question?

NOTE:  NEW E-MAIL ADDRESS, andrewaa@earthlink.net is working,
comcast and mediaone addresses will be gone by march

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 15:56:01 +0100
Reply-To:     Jacques Belin <jbelin@ALTERN.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jacques Belin <jbelin@ALTERN.ORG>
Subject:      Re: Going Postal
In-Reply-To:  <HPLX-L%2002030804134730@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset="ISO-8859-1"
Content-Transfer-Encoding: quoted-printable

Le Fri, 8 Mar 2002 10:14:53 +0200
Daniel Hertrich <daniel=2Ehertrich@GMX=2EDE> a =E9crit:

> What modem do you use for this test?
> If it is a mobile phone with data cable, it is probably a missing DCD
> line on the data cable=2E=20

I don't think he has a DCD line problem=2E In GP, it arrives much later,
after that the connexion is established=2E

Anyway, if he uses a GSM phone, I think he will have the DCD problem,
as most of the phones don't manage the DCD line (the only exception is
the Ericsson phones with the DRS-11 cable=2E Don't buy the DRS-10, which
don't activate the DCD line)=2E

Jacques=2E

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 15:56:06 +0100
Reply-To:     Jacques Belin <jbelin@ALTERN.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jacques Belin <jbelin@ALTERN.ORG>
Subject:      Re: Going Postal
In-Reply-To:  <3C881F6F.1E679E37@NexGo.De>
MIME-Version: 1.0
Content-Type: text/plain; charset="ISO-8859-1"
Content-Transfer-Encoding: quoted-printable

Le Fri, 8 Mar 2002 03:18:23 +0100
Axel Berger <Axel-Berger@NEXGO=2EDE> a =E9crit:

> Problem: Doesn't do anything=2E
>=20
> I have set up everything as well as I am capable and tried to log on=2E Th=
e
> modem is iniatialized:
>=20
> ATZ1
> OK
>=20
> and then - nothing=2E Why doesn't the damn thing try to dial? What can it =
be
> waiting for? I know no modem that says anything else but "OK" on receiving
> config commands=2E Any ideas?

Did you put "DT" in the "Dial Command" line of your modem setting ?

If yes, it eems to me that you have a problem with your "locale" setup,
which is not recognized=2E Try to create a new one=2E=2E=2E

Jacques=2E

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 10:19:33 -0500
Reply-To:     albert.kind@uconn.edu
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Al Kind <MCHEM1@UCONNVM.UCONN.EDU>
Subject:      Feb Archives Posted
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Hi All:

The Logs from Feb are on http://list.hplx.net

Cheers...AJKind

Al Kind
Technical Lab Manager, Microchemistry Lab CANR
3113 Horsebarn U4193, Storrs CT 06269-4193
ph (860)486-6126  eFAX (413)826-8780

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 12:07:50 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      LXTOOLS on SUPER
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

Hi folks,

I've tried on two different systems to unpack the LXTOOLS tar file
with no luck.  It unzips fine, but on a Digital UNIX V4.0E system
"tar x filename" runs with no result and on my Red Hat 7.2 system
it runs without ever exiting.  Is it possible the tar package is
somehow corrupt?  Or am I doing something wrong?

Thanks for hints!

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 00:27:56 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: OT : Video Viewer for working in DOS on a DESKTOP
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

an astonishingly good site ..
for dos programs that do wonders ..
i got 2 video viewers ..
and finally could make a very simple
foxbase program for managing/hear/see
music, family pics, family videos(.dat format)

works like a charm .. i'm so happy ..

on the desktop of course ..

tks everybody

..pk

-----Original Message-----
From: Curtis Cameron <curtc@AIRMAIL.NET>
Date: Friday, March 08, 2002 11:30 AM


>The web site "Interesting DOS Programs" has at least two listed. Along
>with MP3 players, RealAudio players, CD Burners, disk utilities, and
>lots more. It's at http://www.opus.co.tt/dave/index.htm .

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 21:09:03 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: Transfile alternative for MAC, try Maclink Plus
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Please help the dumb:
I have got Transfile 200 installed, but have never used it really. As far
as I could find out it is totally braindead and can't do anything except
copy files. The program from the connectivity pack OTOH is not only able to
convert from and to comma separated ASCII and thus enable data exchange
which transfile can't, it also allows running the LX programs on the dektop
which quite often comes in handy.

I am not sure about the status of that software, very probably it is not to
be copied freely, but it can often be found reasonably priced at eBay. Of
course, Transfile is free, but then I for one would prefer being served in
a restaurant even if McDonalds were to officially allow me to avail myself
of their trashcans for free.

My two Euro-cents (used to be two Pfennig, that's inflation for you)

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 09:13:03 +1300
Reply-To:     Roger Whitmarsh <lodger@NZ1.IBM.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Roger Whitmarsh <lodger@NZ1.IBM.COM>
Subject:      Re: What is VBRJP200.DLL?
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Curtis Cameron wrote:
>There was a file called VBRUN200.DLL, which was the run-time library
>for Visual Basic version 2. How big is the file? My VBRUN200.DLL is
>349kB. My guess is either it's related to VB, or someone just renamed
>the file.

Bob Feldman wrote:
>Open the file in Wordpad or Notepad and look for plain-text messages,
>usually found near the beginning and end of the file. These messages might
>give some clue as to the dll's use.

Thanks to both. The file is a runtime VB component, according to internal
text. God only knows why it was on my LX. Perhaps the 'JP' part of the
name hints at one of the Japanese utilities?

Cheers, Roger

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 20:48:31 -0000
Reply-To:     "Richard E. McEvoy" <remce@GOFREE.INDIGO.IE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Richard E. McEvoy" <remce@GOFREE.INDIGO.IE>
Subject:      Re: OT: Looking for an English word
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I haven't looked at my e-mail for several days; hence this late posting. It
is worth leaving here all that Russel Hemery has said on this topic because
it sums up precisely the position here in Ireland and the UK. There is no
one word to correspond to Werkstudent. University students here get
work experience in the manner he describes. The important part is that the
work is related to their studies and the careers they hope to follow.

"Co-op" in the UK and Ireland is the abbreviation for any co-operative
enterprise, mostly consumer co-ops as reinvented ( Rochdale, 1844) in the
19th century. Members are charged the regular retail prices but have any
profits credited to them in proportion to their purchases.

Work-study in the UK and Ireland (and probably Europe) is Time and Motion
study which was pioneered in the US by Gilbreth and Taylor and which
involves the analysis and redesign of work methods. I was a practitioner at
one time :))

Richard

> In Australia the term apprentice is used for a person who is hired to be
> trained in a trade and does some technical training at a college as well
as
> practical with the company. ie apprentice plumber, apprentice mechanic
etc.
>
> Intern is mainly used here for the medical profession as a term for a
> graduate that is studying as they work. ie mentors oversee their practical
> efforts after they have learned the intellectual stuff.
>
> There are similar positions in the arts (understudy) and the legal
> profession as well as copilot etc.
>
> I think the situation Daniel describes is where full time students go out
> to get some life experiences in return for a bit of pocket change. Here in
> Oz the students go out for work-experience sometimes for no money at all.
> They "test" professions they may be interested in pursuing for a career.
> That seems the closest I can think of. They can then apply for their first
> job quoting work-experience with xyz Company for x time and abc company
for
> x time etc with references as to how they did.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 21:56:41 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: LXTOOLS on SUPER
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Ted

On Fri, 8 Mar 2002 12:07:50 -0600, Theodore Heise <theise@NETINS.NET> wrote:

> I've tried on two different systems to unpack the LXTOOLS tar file
> with no luck.  It unzips fine, but on a Digital UNIX V4.0E system
> "tar x filename" runs with no result and on my Red Hat 7.2 system
> it runs without ever exiting.  Is it possible the tar package is
> somehow corrupt?  Or am I doing something wrong?
>

Try a

tar xvf filename

does that work?

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 15:44:35 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: LXTOOLS on SUPER
In-Reply-To:  <HPLX-L%2002030815553254@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Fri, 8 Mar 2002, Daniel Hertrich wrote:

> Try a
>
> tar xvf filename
>
> does that work?

Yes it does, thanks!  I thought I had tried that combination, but
apparently not.

Thanks again!

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 17:36:14 -0500
Reply-To:     Sales@Systems-Consulting.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Systems-Consulting <Systems-Consulting@COX.NET>
Subject:      Re: What is VBRJP200.DLL?
In-Reply-To:  <OF7455EB6F.B0AF725D-ONCC256B75.0079FA48@nz.ibm.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Visual Basic Japanese v2.0 Runtime package



Thanks,

Systems-Consulting - here since 1992
89 Main Street, Broad Brook CT 06016-9701
tel:(860)627-5393 fax:(860)627-5393
web: http://Systems-Consulting.com
mailto:Sales@Systems-Consulting.com
Paul Anderson
President
Maximizing the results of Information Systems
Certified Novell Salesperson
Your ALPS MD Printer Supplies Source


> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@UConnVM.UConn.Edu]On Behalf Of
> Roger Whitmarsh
> Sent: Thursday, March 07, 2002 5:10 PM
> To: HPLX-L@UConnVM.UConn.Edu
> Subject: What is VBRJP200.DLL?
>
>
> Does anyone know what piece of software the above belongs to?
>
> Cheers...Roger
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 22:51:13 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: ANN: Syslog 1.0
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Daniel Hertrich wrote:
> On Tue, 5 Mar 2002 02:53:32 +0000, Russel Brooks <rlbrooks@POBOX.COM> wrote:
> > I've been doing this for a long time with the following Rexx
> > program.  Call it from BAT files like:
> >
> > rexx ts Starting Software Carousel
>
> But for such a purpose, isn't it too slow? Doesn't the whole
> interpreter have to be loaded for just one ts call in a batch file?
> How big is the interpreter executable?

Rexx.exe 132K for Personal Rexx.  There are other versions such
as the that is included with IBM's PCDOS.

Yes, there is a delay loading and running Rexx.  Personal Rexx
can be loaded resident to speed up loading but then it uses up
memory.  Basically you don't use Rexx for tasks where
performance is critical.

One advantage to Rexx is that it is an interpreted language.  I
can always look at the executable to see what it does; you may
not be able to that with a .COM/.EXE if you've lost the source.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 22:51:16 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: SPD31.EXE Shift-Ctrl-Del Slowdown?
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Daniel Hertrich wrote:
> On Fri, 8 Mar 2002 00:44:38 +0000 (GMT), Russel Brooks <rlbrooks@pobox.com> wrote:
> > If I press it while reading your post I get asked if I want to
> > delete mail on the host.  Why isn't SPD31 seeing it?
>
> Which version of SPD31 do you use?

I'm using the latest SPD31.EXE from T2T, not the .SYS version.

> AFAIK the .SYS file only supports the basic things like all the timing
> corrections, but no hot keys. The EXE version is the one for all the
> features. (Or am I wrong?).

No, you're correct.

> I have the following as the first line in my config.sys:
> device=\drivers\t2t\speed\spd31.exe /M /C /K /N

I don't specify any option switches.  Do I need to?

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 8 Mar 2002 22:51:19 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: SPD31.EXE Shift-Ctrl-Del Slowdown?
Comments: To: hpstaber@COMPUSERVE.COM
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

HP Staber wrote:
> I also notice a considerable difference in speed when scrolling,
> sorting etc. The shft-ctrl-del really toggles the speed.

I must be running something which is stealing the keystrokes
before SPD31.EXE can see them.  I'll have to start commenting
things out and rebooting to see if it changes.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 01:21:04 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: pdf viewer?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

-----Original Message-----
From: Paul Johnson <paulj@SILCHIP.COM.AU>
Date: Friday, March 08, 2002 2:15 PM


>Well I wouldn't call it a better solution, as it is still not
>completely "on" the LX, but a PDF can be emailed to a PDF to Text
>translator at:
>
> <pdf2txt@sun.trace.wisc.edu>
>
>This also produces a sometimes difficult to read result, like using
>Acrobat and extracting the text, but sometimes anything is better than
>nothing.


i second that .. in absence of a better alternative ..
something is definitely better than nothing ..
but i couln't find it 'something' good enough to
use except to just satisfy myself that .. well .. that
it CAN be done .. at least .. the results were far
away from desirable

>Or if you have one of the many methods of viewing a HTML file on the LX
>and you think it will produce a more suitable result, theres a PDF to
>HTML translator at:
>
> <pdf2html@sun.trace.wisc.edu>
>
>Again, this can be a bit ugly sometimes. The resulting file is normally
>processed very promptly, and emailed back to you. Its not something I'd
>normally use, but it has come in handy a couple of times.


again, i'll second that too .. but with the same comments ..
So ! there IS a need for these kind of converters .. an
unfulfilled need ..

but they ARE faaaasst .. the speed with which the email
comes back .. a definite model to take lesson from ..
very very prompt .. sometimes almost like send the file ..
and bang ! .. it lands as an email .. before you know it ..

ONE MORE THING .. the converters i tried from the
above URLs accepted a URL as an input too ! excellent
feature .. no time consuming up loading the file ..

..pk

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 23:50:53 +1300
Reply-To:     Tony Hutchins <th@PARADISE.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Hutchins <th@PARADISE.NET.NZ>
Subject:      ANN: CLOCKS
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Sat,  9 Mar 2002 23:46:33 +1300 (NZDT)

If you want to see a few clock faces on your palmtop, you will
find "CLOCKS" at

http://homepages/paradise.net.nz/th/

Also, the latest ROBOWEB/LX is there.

- Tony

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 11:16:52 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: SPD31.EXE Shift-Ctrl-Del Slowdown?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Well I tried commenting out a bunch of things in my Autoexec.Bat
then rebooted and the Shift-Ctrl-Del started working.  So I
started adding them back one at a timeand rebooting until it
stopped working again.

Now here's the odd part...

...it didn't stop working.

The SPD31.EXE slow down keys now work and I'm running all the
same startup stuff I was before.  Very weird.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 14:45:01 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: LXTOOLS on SUPER
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Ted

On Fri, 8 Mar 2002 15:44:35 -0600, Theodore Heise <theise@NETINS.NET> wrote:

> > tar xvf filename
> >
> > does that work?
>
> Yes it does, thanks!  I thought I had tried that combination, but
> apparently not.

You can also do the unzip process in combination with the untar process
by using

tar xvzf filename.tar.gz

Important: the f must be the last parameter, because it mist be
directly followed by the filename.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 15:04:59 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: SPD31.EXE Shift-Ctrl-Del Slowdown?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Russ

On Sat, 9 Mar 2002 11:16:52 +0000, Russel Brooks <rlbrooks@POBOX.COM> wrote:

> Now here's the odd part...
>
> ...it didn't stop working.
>
> The SPD31.EXE slow down keys now work and I'm running all the
> same startup stuff I was before.  Very weird.

Weird, indeed..

Did you reboot BEFORE you began to comment something out and tried it
after a reboot?
Maybe you have started a program which stopped the drriver from
detecting the hotkey(s) and after a reboot it would have worked again
even without commenting out other TSRs.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 08:08:51 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: LXTOOLS on SUPER
In-Reply-To:  <HPLX-L%2002030908435670@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Sat, 9 Mar 2002, Daniel Hertrich wrote:

> You can also do the unzip process in combination with the untar process
> by using
>
> tar xvzf filename.tar.gz
>
> Important: the f must be the last parameter, because it mist be
> directly followed by the filename.

I had also tried that combination of letters, but probably didn't put
the f last.  Now that you mention it, I seem to recall the man page even
saying something about it.  duh.  That's one I won't forget!

Thanks again,

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 15:35:01 +0100
Reply-To:     Nels.Sennmark@TELIA.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Digest Tomas Moberg <Nels.Sennmark@TELIA.COM>
Subject:      Re: OT : Video Viewer for working in DOS on a DESKTOP
Comments: To: pksharma <pksharma@CAL.VSNL.NET.IN>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Yes
EVE plays uncompressed AVI on th HP200lx
I found it on SUPER once.

> Any one have any idea if there exists
> a viewer for viewing video clips ( .avi,
> .dat) in dos ?
>
> ..pk
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 14:09:21 +0100
Reply-To:     Lillebjorn Nilsen <bjni@ONLINE.NO>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Lillebjorn Nilsen <bjni@ONLINE.NO>
Subject:      Post/LX files
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

What are the *.red files in Post/LX?
They seem to keep track of various
folders. And keep groing. Can they
safely be deleted?

 -----------------
 Lillebjorn Nilsen, Oslo Norway
 http://bjni.home.online.no

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 08:44:28 -0800
Reply-To:     Alfred1520 <alfred1520@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Alfred1520 <alfred1520@YAHOO.COM>
Subject:      Re: ANN: CLOCKS
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Try http://homepages.paradise.net.nz/th/

Regards,
Alfred

-----Original Message-----
From: Tony Hutchins <th@PARADISE.NET.NZ>
To: HPLX-L@UConnVM.UConn.Edu <HPLX-L@UConnVM.UConn.Edu>
Date: Saturday, March 09, 2002 5:23 AM
Subject: ANN: CLOCKS


>Sat,  9 Mar 2002 23:46:33 +1300 (NZDT)
>
>If you want to see a few clock faces on your palmtop, you will
>find "CLOCKS" at
>
>http://homepages/paradise.net.nz/th/
>
>Also, the latest ROBOWEB/LX is there.
>
>- Tony
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 17:59:16 +0000
Reply-To:     Stefan.Peichl@T-ONLINE.DE
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Stefan Peichl <Stefan.Peichl@T-ONLINE.DE>
Subject:      Re: CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Daniel Hertrich wrote:

> Stefan, do you know if the card services software in the LX supports
> two slots (the CE2 / CD2 signals)? How does LXCIC handle that?

the PCMCIA card is accessed through Socket Services.
The 200LX SDK says:

 From Socket Services viewpoint, the HP palmtop has one adapter
 (number 0) and the adapter has one socket (number 1), which is
 the PCMCIA card slot.

LXCIC always only uses the socket number 1. I don't know, if
the 700LX for example has a socket 1 and a socket 2, or if it
has 2 adapters with one socket each, or if the built in Nokia
modem card is accessed completely different.

The SDK also states, that a Socket, which has been used for
something else than a memory card, is reset to generic memory
card operation after the card has been removed. IMHO this
implies, that after removing the Nokia data card from the 700LX
the slot should be available and setup for memory cards, which
it is obviously not. Therefore I think it is handled different
to the external PCMCIA socket.

Stefan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 12:29:53 -0500
Reply-To:     Keith Grider <k.grider@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Keith Grider <k.grider@EARTHLINK.NET>
Subject:      Re: 200lx ethernet adapter
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

The 'socket.com' low power Ethernet card is probably the best solution that
I have seen. It is an ne2000 based card and seems to work fine with the
lxeth drivers (rod whitby's drivers on Super). It is even lower power than
the Accton card. I went to a comp. store, popped it in the CF adapter and
then into the PCMCIA slot and loaded the driver. It all seemed to be fine.

KeithG
----- Original Message -----
From: "ABCS INC." <kwmiller@AZBCS.COM>
Sent: Friday, March 08, 2002 7:14 AM
Subject: 200lx ethernet adapter


> Anyone have a current source for Ethernet adapters that work with a
> doublespeed 200lx palmtop?  I haven't been able to find the Accton
En2216-1
> card anywhere..
>
> thx
>
> Kevin Miller
> ABCS INC.
> kwmiller@azbcs.com <mailto:kwmiller@azbcs.com>
> 602-943-0159
> www.azbcs.com <http://www.azbcs.com>
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 19:45:12 +0100
Reply-To:     Jacques Belin <jbelin@ALTERN.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jacques Belin <jbelin@ALTERN.ORG>
Subject:      OT: HP To Resume calculator Production ?
MIME-Version: 1.0
Content-Type: text/plain; charset="US-ASCII"
Content-Transfer-Encoding: 7bit

Just seen a thread in the forum section of hpmuseum.org about the fact
that HP would release an HP41 successor :

http://www.hpmuseum.org/cgi-sys/cgiwrap/hpmuseum/forum.cgi?read=15299

If they do that, perhaps there is a chance we can convince them to
release an HP200 successor ?  ;-)


Jacques.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 19:47:55 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: SPD31.EXE Shift-Ctrl-Del Slowdown?
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Daniel Hertrich wrote:
> Weird, indeed..
>
> Did you reboot BEFORE you began to comment something out and tried it
> after a reboot?
> Maybe you have started a program which stopped the drriver from
> detecting the hotkey(s) and after a reboot it would have worked again
> even without commenting out other TSRs.

Yeah I rebooted before and after each change.  I made enough
changes and reboots without carefully recording what I was doing
that I don't remember each step now.

Oh well, I won't worry unless it comes back and I doubt I use
the slow down function much to ever notice it doesn't work
again.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 09:41:02 +1300
Reply-To:     Tony Hutchins <th@PARADISE.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Hutchins <th@PARADISE.NET.NZ>
Subject:      Re: ANN: CLOCKS
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Sun, 10 Mar 2002 08:45:53 +1300 (NZDT)

03h01m25s ago ...
On Sat,  9 Mar 2002 08:44:28 -0800, Alfred1520 wrote:

> Try http://homepages.paradise.net.nz/th/

Thanks for the correction Alfred!

- Tony

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 09:41:04 +1300
Reply-To:     Tony Hutchins <th@PARADISE.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Hutchins <th@PARADISE.NET.NZ>
Subject:      Re: Post/LX files
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Sun, 10 Mar 2002 08:51:28 +1300 (NZDT)

06h42m07s ago ...
On Sat,  9 Mar 2002 14:09:21 +0100, Lillebjorn Nilsen wrote:

> What are the *.red files in Post/LX?

---------------------------
From: Help - Appendix
Subject: Files

The following file extensions are used by POST/LX:

 EXE          executable program files
 I            inbox file
 O            outbox file
 I1, O1       level 1 index for inbox/outbox
 I2, O2       level 2 index for inbox/outbox
 OLD          keeps IDs of messages already downloaded
 DOW          keeps IDs of messages to be downloaded
 DEL          keeps IDs of messages to be deleted
 RED          keeps IDs of messages to be marked as read (IMAP4)
 URE          keeps IDs of messages to be marked as unread (IMAP4)
 TMP          temporary file (multi-purpose)
 TMA, TMB...  temporary files for message composition
 TPL          template files for message composition
 HED          file with headers of current message
 ADR          address list
-------------
> They seem to keep track of various
> folders. And keep groing. Can they
> safely be deleted?

Lillebjorn,

Yup they can be deleted. They are only used if your mailbox is
an IMAP4 box.

- Tony

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 17:58:04 -0500
Reply-To:     LEONG Ka Tai <leongkt@HKIPP.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         LEONG Ka Tai <leongkt@HKIPP.ORG>
Subject:      Re: Transfile / Connectivity Pack on IMAC
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

There is a program called "Virtual PC" which emulates a
pentium PC on the Mac. With that you can choose to start a
DOS, Windoze or Linux session, if you have the systems
installed. Made by Connectix (?).

Ka Tai


Terry Matson wrote:

> Has (or is it even possible) anyone using the Transfile and Connectivity=
 Pack
> on an IMAC?
>
> I am aware there are "window emulators" for the Mac and IF it is =
possible
> to run the above programs which of these emulators would you recommend?
>
> I am seriously considering a IMAC as I am very tired of windoze - so =
any
> insight would be helpful (though tired of windoze NOT willing to give =
up
> the HP<g>).
>
> Many THANKS in advance for any advice received : )
> terry
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 00:02:27 +0100
Reply-To:     Yves Leurquin <leurquin@BIGFOOT.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Yves Leurquin <leurquin@BIGFOOT.COM>
Subject:      Re: Stacker on PCMCIA cards
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

PK,

> you could do that .. or try out the stacker program which i have
> .. it came especially with a stacpalm software .. very suited
> to the palmtop environment .. and guess what .. it works
> when i put it in my Toshiba Satellite Pro pcmcia slot .. needed
> to put the right lines in my config.sys file though !

1. So you managed to mount a Stack volume on a Flash card and access at =
the same
time the uncompressed partition of the flash card (e.g. for copying from =
the
compressed to the uncompressed part) ?

2. Also, you manage to read a stack volume on your laptop. It it running =
Win95
or above.

As you know I am using JAM which allows 1. but not 2.

 \/
 /ves



_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 9 Mar 2002 18:10:59 -0500
Reply-To:     Martin Bergvill <hplx@BERGVILL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Martin Bergvill <hplx@BERGVILL.COM>
Subject:      Re: Ol' Eddie Archive
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Fri,  8 Mar 2002 08:52:23 -0500, Steve wrote:

Hi Steve

>    I would think the ideal solution would be for it to
> be held at Palmtop.Net.  I.e. at
>
> http://www.palmtop.net/eddie

Yes that is probably the best solution.


> With the usual link and description at http://www.palmtop.net/
> Is that possible?

I hope so.. I have not gotten any reply from Bill Childers yet. And I
have not seen him post here for a long time.

Do anybody have a emailadress that weknow he uses?

Regards

--
Martin Bergvill ,Narvik Norway

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 03:39:40 +0100
Reply-To:     Axel Berger <Axel-Berger@NEXGO.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Going Postal
Mime-Version: 1.0
Content-Type: text/plain; charset=iso-8859-1
Content-Transfer-Encoding: 8bit

The best news first: I works!
This very post was sent to my mobile account and retrieved and
forwarded using gp (with a bit of extra mangling, as the list would not
accept mail from my mobile account and I don't want that flooded.)

But then, it was a long, long way to go, which probably only shows my own
incompetence and nothing else. Still, I will tell about the pitfalls I
encountered:
For the much faster turnaround times on changing settings and the nice big
screen, I prefer trying things out on the big machines first.
W98 games console, DOS window: freezes everything including keyboard reset,
requires hard reset.
W98 booted to DOS without GUI: doesn't work. COM port seems to lose
characters, can't dial.
Now I got my ultimate DOS machine, a 486DX66 notebook with 8 MB, MSDOS 5.0
and WIN 3.11, which was given to me but not yet used in earnest. Very bad
news: COM loses characters. In another terminal (DSZ in terminal mode) it
became especially visible with AT&V: the first two or three characters of
every line are missing!
 -> Any helpful hints for that one? I was hoping to use the thing for
        montoring undocumented serial connections with proprietary
        hardware drivers.
The last thing I tried was the DOS window invoked from WIN 3.11, and lo and
behold: success!
So then I set everything up started it, dialled, got to PPP negotiation
flash onto the screen, then hangup and nothing in the debug logfile.

After thoroughly getting fed up with that I decided to try the HP after
all. Setting up does require more patience! But the plus side of being very
much slower: I could now read the screen and found: "DNS server not found"
or something like that. Looking very, very carefully and zooming to the
larges print I finally saw why:
I had copied the files after the first trials and setup on the big games
console. German keyboards have a comma in the numeric field. In Windows I
have replaced that with the far more sensible and international point, but
not yet found how in DOS. So, you guessed it, commas in the DNS instead of
points!

One problem remains, and that is one I am currently talking about with
Steven Lawson:
Of my four ISPs only one offers unauthentificated smtp access. Normally I
use the smtp not of the isp but of the mailserver, either via smtp after
pop or with password authentification. Perhaps he'll do something about
that, if not I'm stuck with the one, which is one more or infinitely more
than none.

So now I can save scarce and valuable room on C: by deleting nettamer from
there.

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 13:25:41 +0200
Reply-To:     Nigel R <nigel@KEEPSMILING.CO.ZA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nigel R <nigel@KEEPSMILING.CO.ZA>
Organization: STRATEGIC ALLIANCE CONSULTING
Subject:      Transfer of data using IR from HP95 to Siemens S35
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Greetings from sunny South Africa :-)

Apologies if the following has already been answered in a previous posting.

I would like to transfer appointment book entries from my HP95 to a Siemens
S35i appointment book using the infra red link capabilities of both devices.
Logic tells me that this procedure should be possible but so far I have not
been able to progress beyond locking up the 95 (requiring removal of all
power, reformatting drive 'C' and then restoring system using back-up
contained on PCMCIA memory card) when trying to use ir.exe  :-(

Assuming I eventually have an application running on the 95 (am going to try
the only other application located thus far [IR-Print  v1 copyright (c) 1993
by Thomas Rundel] and format S35 data as a print file) that will establish
some form of communication with the S35, the next issue is the format of
what is being transferred!  The idea I have is to mark HP appointment book
entries that I want to appear in the S35 appointment list with a flag in the
'Notes' field (or use tagging function from within 'Notepad' application as
developed by Charles Hayden) and then run whatever is required to effect the
transfer and updating of the S35i entries.  Am I expecting too much?  Would
an alternative to be use HP95 > Desk PC and then PC > phone application(s)
using serial connections? Is the protocol for data transfer to the S35
freely available and if so
where?

Hopefully someone somewhere has ALL the answers for me (and anyone else
interested in linking the two devices <g>!

Looking forward to some the solution but until then, KEEP SMILING:-)

All the best from Nigel R

P.S.  Is the world-wide LX user database available yet?

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 07:17:12 +0100
Reply-To:     hpstaber@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         HP Staber <hpstaber@COMPUSERVE.COM>
Subject:      Re: Post/LX files
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Lillebjorn Nilsen wrote:
>
> What are the *.red files in Post/LX?
> They seem to keep track of various
> folders. And keep groing. Can they
> safely be deleted?

From posthelp.i :

RED          keeps IDs of messages to be marked as read (IMAP4)


HP Staber/Salzburg

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 12:09:10 -0500
Reply-To:     Bob Penick <bpenick@MYREALBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Penick <bpenick@MYREALBOX.COM>
Subject:      OT - Joseph Buford = Digest's #2002-73, 43, &42
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Sorry folks for sending this to the list.

Joseph, I've tried replying to your email and my messages get bounced back
from your mail serveer as "Spam".
(My email address is provided by Novell and is firmly committed against
"Spam" and virus transmission.)

I'm getting your messages so please privately send me another way that I can
contact you and get you the info you requested.

Thanks,
bob

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 20:45:00 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Transfer of data using IR from HP95 to Siemens S35
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Nigel

On Sun, 10 Mar 2002 13:25:41 +0200, Nigel R <nigel@KEEPSMILING.CO.ZA> wrote:

> I would like to transfer appointment book entries from my HP95 to a Siemens
> S35i appointment book using the infra red link capabilities of both devices.
> Logic tells me that this procedure should be possible but so far I have not

Which logic do you apply? ;*)
I would be interested in it!

> using serial connections? Is the protocol for data transfer to the S35
> freely available and if so
> where?

The problem is:
S35 speaks IrDA, but the 95LX IR port only supports SIR and even that
only up to 2400 baud! I am not sure the S35 can use IrDA at so low
speeds.
So, with the normal protocols (IrDA protocol spec should be available
at www.irda.org) you will probably not succeed. But as always, I can be
wrong, and I would be glad to be proven wrong here!

> P.S.  Is the world-wide LX user database available yet?

Not yet, but soon it will be available.
Bob has sent me the version with all the "around the world" info and I
am currently making some design changes. Then we will put it online
somewhere.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 20:02:43 -0000
Reply-To:     Chris Randle <chris@AMLOG.CO.UK>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Chris Randle <chris@AMLOG.CO.UK>
Subject:      Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

-----Original Message-----
>From: "Martin Bergvill" <hplx@BERGVILL.COM>
>Sent: 07/03/02 8:33:26 PM

>Thanks..I found my old calculator on that site.. I thought it was the
>32s I had a long time ago ,but it was a 38s with led display..almost
>brought a tear to my eye seeing it again :-)

If you don't already know it, check out:
http://www.hpmuseum.org

--=20
Chris Randle

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 21:19:27 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: Transfer of data using IR from HP95 to Siemens S35
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> S35 speaks IrDA, but the 95LX IR port only supports SIR and
> even that only up to 2400 baud!

That was my first idea too. But then there is the HP supplied printer-only
IRDA driver, perhaps
> [IR-Print  v1 copyright (c) 1993 by Thomas Rundel]
(BTW: your header does not supply RID information, I had to look for the
article you replied to instead of just jumping to it as is customary)
is something similar. With clip there is some control over the format to be
"printed", so perhaps this idea is not as silly as I too at first thought
it to be.

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 15:55:13 -0500
Reply-To:     Dario Draiman <dario200@MAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dario Draiman <dario200@MAIL.COM>
Subject:      Program to organize students classes
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit
MIME-Version: 1.0

Hi everyone!
Does anyone knows about a program that would organize courses for students? For example, if I have to attend let say 4 courses and each one has several classes with their own timetables, it would be nice to enter all the information into a program and it
would suggest all possibilities without superimpose classes for the whole week. That way I get a classes fixture I have to subscribe.

Thanks.

Dario

--

_______________________________________________
Sign-up for your own FREE Personalized E-mail at Mail.com
http://www.mail.com/?sr=signup

Travelocity.com is giving away two million travel miles.
http://ad.doubleclick.net/clk;3969773;6991039;g?http://svc.travelocity.com/promos/millionmiles_main/0,,TRAVELOCITY,00.html

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 23:16:22 +0100
Reply-To:     Josef Meyer <meyerj@SWISSONLINE.CH>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Josef Meyer <meyerj@SWISSONLINE.CH>
Subject:      How to change email adrdress in list subscription?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

I have changed my email address. Can anybody tell me the procedure to
change the email address in the HPLX-L subscription? Do I have to
unsubscribe with the old email address and then subscribe again with
new new address, or is there a simpler way?

Josef Meyer

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 03:36:18 +0000
Reply-To:     castorlw@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Larry Castor <castorlw@YAHOO.COM>
Subject:      Re: Problems with Mocha PPP
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Dario,

> I'm using Windows 98, 56700 bps modem and my 200LX connected in COM1 =
with the F1015 cable (the same I use with Transfile). I set up WWW/LX in =
the same way as Daniel explained on his page. I tried telnet and HV. =
Telnet connect, ask for a login but stop > transfer when it ask for a =
password (and it's not a server problem). HV says "Connected...Receiving..=
." but the download of the page never ends.
> In Mocha the "bytes from palm" grow faster than the "bytes to palm".


 Don't know.  Seems like it must be set up right if it is connecting as =
you say.  The times that I have used it is to go straight to postlx.  You =
might try that.

Larry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 21:05:32 -0800
Reply-To:     Marta Pierce <Marta1@attbi.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marta Pierce <Marta1@ATTBI.COM>
Organization: Family
Subject:      Personal Food Analyst
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Hello HPLX,

  I have purchased this little program, and it seems to be what I want
  and need.  2 questions, is there an updated database that I can
  find/get/download from somewhere? and 2nd, I can't seem to save any
  info.  When I fill in a day's food info, and then save to my user
  name, I lose all the data from the food.  I can still see the list
  of the food I inputed, but non of the caloric values and amount are
  saved.  I get this message,
          file fragmented or invalid file header
          a:\database.db4

 I get that when ever I try to save or retrieve info that I placed
 into the program.  I have it currently on my A drive, in a dos
 software carrousel area.  There is plenty of room in the area. Also,
 I had the same problem when I moved it to the C drive.  I
 have a 32 db speed machine.

 What it looks like is that the database.db4 isn't saving any info. I
 tried to manually enter a new food, and it wouldn't save it.

 any one know this software?

 TIA

 Marta

--
Best regards,
 Marta                          mailto:Marta1@attbi.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 18:22:52 +1300
Reply-To:     Tony Hutchins <th@PARADISE.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Hutchins <th@PARADISE.NET.NZ>
Subject:      Re: ANN: CLOCKS
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Mon, 11 Mar 2002 18:19:20 +1300 (NZDT)

CLOCKS V2.1 is at:

http://homepages.paradise.net.nz/th/

It is more interactive now, using number keys and +/-, and
shows more info.

- Tony

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 10 Mar 2002 23:57:46 -0800
Reply-To:     "Douglas Tucker, M.D." <dtucker@ITSA.UCSF.EDU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Douglas Tucker, M.D." <dtucker@ITSA.UCSF.EDU>
Subject:      100LX to HP Jornada 568 conversion
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

I'm contemplating getting the 568, which runs the Pocket PC 2002 OS, but
I'm concerned about having to reenter all my phonebook, appointment, and
memo entries.  Is there some way to do a simple conversion using the
connectivity pack (or anything else)?
-Doug

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 15:03:05 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      CF inside the LX
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

as expected, the people at Accurite are a little bit reserved giving
away information about how I can connect a second PCMCIA card to the
200LX's PCMCIA port. They wanted to make me buy a DoubleSlot. ;-)

But they helped me a bit, I quote the message of the support person
here:

> From: "Richard Kelly" <rkelly@accurite.com>
> To: <daniel.hertrich@gmx.de>
> Subject: Re: PCMCIA: technical question
> Date: Thu, 7 Mar 2002 15:02:38 -0800
>
> Hi Daniel
>
> > Please tell me: If I have one PCMCIA slot and want to make two out of it, do I
> > only need two physical slots and connect them in parallel to the one original
> > slot? Or is there any additional logic involved, or some line voltage
> > regulation / blocking...?
>
> Answer:
>
> No, there has to be separate control logic for each slot and the operating
> system has to know many slots there are in order to assign system resources
> (interrupts,I/O ports and memory) to avoid conflicts. The Double Slot ships
> with a software driver that filters and redirects control signals to the PC
> Card slots. The Double Slot is designed for the HP 100/200 machines only and
> will not work any other model computer. The reason the DoubleSlot works on the
> HP handheld computers is that there is logic for two slots but only one slot
> was supported.
>
> Hope this helps Regards Richard Kelly


So, without any software enhancement the project "CF card inside the
LX" cannot be realized, I guess.
Could anyone open his double slot and look if the two PCMCIA slots are
jsut in parallel or if there is more logic? If these slots are in
parallel (only the Card enable / Card detect 1/2 signals are for one
slot only), the Accurite driver might work. Otherwise, I don't see any
way to make it possible to use an internal mounted CF memory and in
addition use the PCMCIA slot as usual.

Thanks
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 15:03:07 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Transfer of data using IR from HP95 to Siemens S35
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Axel

On Sun, 10 Mar 2002 21:19:27 +0100, Axel Berger <Axel-Berger@NEXGO.DE> wrote:

> That was my first idea too. But then there is the HP supplied printer-only
> IRDA driver, perhaps
> > [IR-Print  v1 copyright (c) 1993 by Thomas Rundel]

I don't know this driver, but if it works for the 95LX, maybe it is
really possible to do something like that.

> (BTW: your header does not supply RID information, I had to look for the
> article you replied to instead of just jumping to it as is customary)

As I said before, I do not have the possibility to control the
behaviour of Post/LX related to RIDs.
Or do I? Do you know how to enable that?
You are the first one who complains about that. And many people post
here using Post/LX.

> is something similar. With clip there is some control over the format to be
> "printed", so perhaps this idea is not as silly as I too at first thought
> it to be.

I didn't think the idea way silly.
I only thought it wasn't possible.
But if it is, I wouldb e glad to see a solution!

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 15:03:08 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: How to change email adrdress in list subscription?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Josef

On Sun, 10 Mar 2002 23:16:22 +0100, Josef Meyer <meyerj@SWISSONLINE.CH> wrote:

> I have changed my email address. Can anybody tell me the procedure to
> change the email address in the HPLX-L subscription? Do I have to
> unsubscribe with the old email address and then subscribe again with
> new new address, or is there a simpler way?

When you subscribed, you got a short introduction into listserv usage.
This introduction sais how to order a reference card of listserv
commands. One of these commands lets you change the subscription
address.
It was something like
CHANGE HPLX-L newaddress

or something liks that. Since I'm not sure, please have a look at the
reference card.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 15:03:10 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Problems with Mocha PPP
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Dario

On Mon, 11 Mar 2002 03:36:18 +0000, Larry Castor <castorlw@YAHOO.COM> wrote:

>  Don't know.  Seems like it must be set up right if it is connecting as you say.  The times that I have used it is to go straight to postlx.  You
> might try that.

Another problem might be a firewall or Proxy the LAN you connected to is
behind. Ask the LAN administrator.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 15:03:11 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Going Postal
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Axel

On Sun, 10 Mar 2002 03:39:40 +0100, Axel Berger <Axel-Berger@NEXGO.DE> wrote:

> One problem remains, and that is one I am currently talking about with
> Steven Lawson:
> Of my four ISPs only one offers unauthentificated smtp access. Normally I
> use the smtp not of the isp but of the mailserver, either via smtp after
> pop or with password authentification. Perhaps he'll do something about
> that, if not I'm stuck with the one, which is one more or infinitely more
> than none.

SMTP after POP should be relatively easy to implement, but SMTP-AUTH
requires more work.

In case Steven will not implement one of the two, you could simulate
SMTP after POP by once going online only with POP access and then going
online once more using SMTP, if Going Postal allows that. But it dows
only work if you use the same internet connection (i.e. don't redial),
because your IP address would probably change and the SMTP recognizes
you by letting the POP server store your IP address.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 15:03:12 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Juan

On Thu, 7 Mar 2002 20:28:22 +0100, Juan Belmonte <jbmbhs@ERESMAS.COM> wrote:

> Three questions:
>     1.- If it's possible to connect one internal CF card...  LXCIC may
> recognice it?

Software is still an issue we must talk about. See my other message.

>     2.- Mine is an older HP200LX ( SG5* ) 2Mb model (1Mb on motherboard and
> 1Mb daughtercard). If first question its succesful, mine can be converted to
> an 1Mb + 64 Mb internal CF leaving free the PCcard slot but getting out the
> daughtercard?

Yes. I don't think that both a CF card board and a RAM daughterboard will fit
into the LX.

>     3.- I'm still not enough crazy to test with my main (and only!!)
> palmtop. For testing pusposes; Two unassembled CF to PCcard adaptor and two
> standard CF cards, soldering iron to test it external and get working two CF
> cards before do anything inside the palmtop

IF it works, proably not with two CF Flash cards, but only with one CF
flash card and one I/O card, as in the 700LX. For two CF cards, we
would have a similar problem as the one discussed a week ago with the
Flash card partitioning, I guess.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 15:03:14 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Stefan

On Sat, 9 Mar 2002 17:59:16 +0000, Stefan Peichl <Stefan.Peichl@T-ONLINE.DE> wrote:

> LXCIC always only uses the socket number 1. I don't know, if
> the 700LX for example has a socket 1 and a socket 2, or if it
> has 2 adapters with one socket each, or if the built in Nokia
> modem card is accessed completely different.

Couldn't you simply modify LXCIC so that it also asks for info on
socket 2? This way we could test that.

> The SDK also states, that a Socket, which has been used for
> something else than a memory card, is reset to generic memory
> card operation after the card has been removed. IMHO this
> implies, that after removing the Nokia data card from the 700LX
> the slot should be available and setup for memory cards, which
> it is obviously not. Therefore I think it is handled different
> to the external PCMCIA socket.

Well, as far  as I have heard, the second slot in the700LX is strictly
I/O wired. So no way to put a flash card into it.

But in a few days I will get a 700LX, and then I can look for the
wiring. :-)

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 15:03:15 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Ol' Eddie Archive
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Steve

On Fri, 8 Mar 2002 08:52:23 -0500, Steve <novosad@SERVER030.FWB.SAIC.COM> wrote:

> http://www.palmtop.net/eddie
>
> With the usual link and description at http://www.palmtop.net/
> Is that possible?


It depends on how much data it is and if David is willing to host all
that data on his machine.

But once we have the CDs from Bill, we can decide what to do with the
data.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 15:03:16 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: PDF Viewer...
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Dennis

On Thu, 7 Mar 2002 12:06:33 -0500, Dennis Bell <doppelbike@EMAIL.COM> wrote:

> I have a copy of a DOS program which will convert
> PDF files to text.  It is called PDFTOTEXT (v0.80) by
> Derek Noonburg.
>
> [...]
>
> I can send it to the SUPER-master if folks would like
> to see it there.

Yes, please do so. super@palmtop.net
I will put it there with the next update.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 15:03:18 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Batch programming tips and utilities
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

everyone interested in batch programming: Have a look into Prof. Timo
Salmi's collection of DOS batch programming Tips:

ftp://garbo.uwasa.fi/pc/ts/tsbat73.zip

Especially the FAQ file is very recommended! Almost everything
regarding batch tricks is covered there!
Great ressource!

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 15:26:15 +0100
Reply-To:     xmarc@free.fr
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marc BERLIOUX <xmarc@FREE.FR>
Subject:      Re: 100LX to HP Jornada 568 conversion
In-Reply-To:  <20020311080125.BWYC1147.rwcrmhc52.attbi.com@doug-desktop>
Content-Type: text/plain; charset="iso-8859-1"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit

Le Lundi 11 Mars 2002 08:57, Douglas Tucker, M.D. a icrit :
> I'm contemplating getting the 568, which runs the Pocket PC 2002
> OS, but I'm concerned about having to reenter all my phonebook,
> appointment, and memo entries.  Is there some way to do a simple
> conversion using the connectivity pack (or anything else)?
> -Doug
>

you gotta find a common file format to export-import your datas.
try to find out if your Pocket can at least import text-based files
such as .CSV(comma separated values) or .LDIF

It's always the same problem
Why don't they use a common file structure?

i'm working on making converters from-to XML

--
Marc BERLIOUX
Pologne : "Boire ou conduire ? de toutes fagons on a pas de voitures"

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 11:04:12 -0500
Reply-To:     Sales@Systems-Consulting.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Systems-Consulting <Sales@SYSTEMS-CONSULTING.COM>
Subject:      test
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

test

Thanks,

Paul Anderson, Pres, Systems-Consulting here since 1992
89 Main Street, Broad Brook CT 06016 tel:(860)627-5393
web: http://Systems-Consulting.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 17:30:45 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      CamWork
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

did you know CamWork? It is a DOS utility to transfer images from
digital cameras, according to the requirement info, it should work on
the LX. It is said to work with Agfa, Olympus and Epson cameras.

http://members.tripod.com/~tawba/camwork.htm

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 14:00:58 -0500
Reply-To:     Bruce_Martin@MANULIFE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bruce Martin <Bruce_Martin@MANULIFE.COM>
Subject:      New DOS (Win, Linux, etc.) handheld
MIME-Version: 1.0
Content-type: text/plain; charset=iso-8859-1
Content-transfer-encoding: quoted-printable

http://www.appliancemagazine.com/news.cfm?newsid=3D1608


                        First Handheld Computer to Run Windows, Linux o=
r
Unix OS to Be
                        Unveiled at CeBIT

                        March 8, 2002. eightythree, said to be the firs=
t
computer that combines the portability of a
                        handheld with the functionality and software
compatibility of a Windows/Linux/UNIX PC,
                        will be unveiled at the opening of CeBIT next w=
eek
by Tiqit Computers.

                        According to Tiqit, although this feature was
previously considered impossible to engineer,
                        the eightythree is not a concept product. Inste=
ad,
Tiqit says it has built ? a mass produced --
                        a fully functioning x86 handheld device out of
cutting-edge but available parts, designed
                        specifically for enterprise use and immediate
production. The computer will be introduced at
                        CeBIT, the world's largest telecommunications a=
nd
IT conference, scheduled for next week,
                        March 13-20, in Hannover, Germany.

                        According to the company, eightythree offers cl=
ear
benefits to the enterprise community.
                        Workers reportedly gain increased mobility and
function with a device that allows them to
                        depend on a single operating system, and compan=
ies
can reduce their total cost of ownership.
                        Possessing the storage capacity and processing
power to enable the extension of many
                        software services to areas formerly unreachable=
,
the eightythree also has the flexibility of
                        using all of the software and hardware extensio=
ns
currently available in the mainstream PC
                        market, Tiqit maintains.

                        "This product will greatly accelerate adoption =
and
use of handhelds in the enterprise," said
                        Ian Blasch, CEO, Tiqit Computers. "It uses stan=
dard
operating systems -- Windows XP,
                        Linux or UNIX -- and is compatible with all
associated applications, including legacy
                        software. Almost anything you can do on a lapto=
p or
PC, you can do on eightythree -- only
                        it is smaller and more mobile."

                        The eightythree form factor is 5.4-in long, 4-i=
n
wide, 1.1-in thin and weighs 20 oz. It is the
                        size of a large PDA, has laptop-quality screen
resolution, SMS keyboard, thumb-operated
                        micro joystick with mouse buttons, touchscreen,=
 a
cardbus PC card slot to support all
                        standard wireless modems, a USB port, a Secure
Digital (SD) slot and internal speaker.
                        Therefore, says Tiqit, it connects with other
standard devices, from digital cameras to bar
                        code scanners to docking stations. On the softw=
are
end, it incorporates all the applications
                        you would find on a laptop or PDA, including vo=
ice
communication, e-mail, web access,
                        PIM, enterprise applications and the ability to=

download attachments.

                        In terms of components, eightythree's CPU is th=
e
National Semiconductor Geode, 266-300
                        MHz, RAM is 128 MB or 256 MB, and there is a 10=
 GB
hard drive. The screen is a 4-in
                        640X480 TFT (18-bit color) with touchscreen and=

backlight. The external monitor displays
                        up to 1280 x 1024 at 75 Hz, 1024 x 768 at 85 Hz=
.
eightythree is powered by an internal
                        lithium ion rechargeable battery.

PDF brochure at: http://www.tiqit.com/TiqitBrochure.pdf

=

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 08:24:13 +1300
Reply-To:     Tony Hutchins <th@PARADISE.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Hutchins <th@PARADISE.NET.NZ>
Subject:      Re: Transfer of data using IR from HP95 to Siemens S35
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Tue, 12 Mar 2002 07:58:17 +1300 (NZDT)

05h55m10s ago ...
On Mon, 11 Mar 2002 15:03:07 +0200, Daniel Hertrich wrote:

> > (BTW: your header does not supply RID information, I had
> > to look for the article you replied to instead of just
> > jumping to it as is customary)
>
> As I said before, I do not have the possibility to control
> the behaviour of Post/LX related to RIDs.  Or do I? Do you
> know how to enable that?

Hi Daniel,

If a "References:" header is added to the mailbox template
then, when replying to a message, POST/LX will send the
Message-ID from the parent e-mail . While reading
messages in POST/LX pressing "Alt-T" (T for "thread") and then
"P" will find the Parent message (if it is still in the
mailbox<G>).

When composing a new message then the "References:" part of
the template is not filled and not sent. So, it works well.

- Tony

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 00:35:43 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: New DOS (Win, Linux, etc.) handheld
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Its a fully fledged complete
working desktop equivalent but in a very
small form factor .. a MatchboxPC
.. MPC .. the connectors are much larger
than the mother board .. but what is a
SMS keyboard ?

..pk

(i've been following Tiquit's progress casually
.. its short form for The Ubiquitous computer..
very very well conceived and designed .. uses
a pcmcia card as the hdd .. so ANY OS can be
loaded onto it .. the color screen is a good
addition .. especially the touch screen part ..
the one thing which i intensely like on the
hp lx320 and upwards ..

but does this run on batteries .. if yes .. then
its gonna bomb .. color screen sucks the life
out of batteries .. a b&w touch screen could
have been much much better .. like the lx200's
screen .. virtually no power needed for it ..
the color .. wellll all things have some short
comings .. but a good beginning .. a real good
beginning ..

LXers .. be on the look out .. me .. i'll wait for
the prices to come down .. at the last look the
prices were almost double of an equivalent
desktop .. that's absurd to say the least ..
but then cost of research has to be recoverd ..
what a tragedy !

..pk

-----Original Message-----
From: Bruce Martin <Bruce_Martin@MANULIFE.COM>
Date: Tuesday, March 12, 2002 12:35 AM


http://www.appliancemagazine.com/news.cfm?newsid=1608


                        First Handheld Computer to Run Windows, Linux or
Unix OS to Be
                        Unveiled at CeBIT

                        March 8, 2002. eightythree, said to be the first
computer that combines the portability of a
                        handheld with the functionality and software
compatibility of a Windows/Linux/UNIX PC,
                        will be unveiled at the opening of CeBIT next week
by Tiqit Computers.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 21:17:31 +0100
Reply-To:     hpstaber@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         HP Staber <hpstaber@COMPUSERVE.COM>
Subject:      Re: 100LX to HP Jornada 568 conversion
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Douglas Tucker, M.D. wrote:
>
> I'm contemplating getting the 568, which runs the Pocket PC 2002 OS, =
but
> I'm concerned about having to reenter all my phonebook, appointment, =
and
> memo entries.  Is there some way to do a simple conversion using the
> connectivity pack (or anything else)?

I have neither 100LX nor J568 - my gear is 200LX an J720. The issue, I
gues, is how to convert databases and appointments into PocketOutlook.

You should use your desktop Outlook to import comma separated text
databases. It is quite intuitive to assign the fields of one database
to the fields in Outlook. In the next step you can sync Outlook with
PocketOutlook and you should be set.

I assume that you know how to create comma separated text files on the
palmtop.

HP Staber/Salzburg

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 4 Feb 2002 14:09:03 -0700
Reply-To:     "Robert K. Meyer" <bmeyer@UNION-TEL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Robert K. Meyer" <bmeyer@UNION-TEL.COM>
Subject:      Re: New DOS (Win, Linux, etc.) handheld
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

AA's & long battery life are necessary IMHO for an LX
replacement.

Bob
--
R.K. Meyer MSEE K7PPC bmeyer@union-tel.com Elk Mountain WY
http://w3.union-tel.com/~bmeyer/   His name...  Isaiah 9:6

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 14:52:43 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: New DOS (Win, Linux, etc.) handheld
MIME-Version: 1.0
Content-Type: text/plain

Also, 4x5x1 inch will not (easily) fit in a pocket. A numerical keypad would
be nice, too.

But then again, it might be a good machine (if anyone picks it up and starts
manufacturing it).

Bob

-----Original Message-----
From: Robert K. Meyer [mailto:bmeyer@UNION-TEL.COM]
Sent: Monday, February 04, 2002 3:09 PM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: New DOS (Win, Linux, etc.) handheld


AA's & long battery life are necessary IMHO for an LX
replacement.

Bob

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 23:00:00 +0100
Reply-To:     Michel Bel <michel.bel@ZONNET.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michel Bel <michel.bel@ZONNET.NL>
Subject:      Re: CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Well, to mimic a 'DoubleSlot' IMHO  e.g. drive a second socket. This
might be an approach:

a) Create a driver to catch requests to PCMCIA socket 2.
When this is requested, instead of asserting CE1 and CE2, assert A9 and A10
of the PCMCIA slot.( Or any other two address lines).

b) Rewire A9 and A10 from the PCMCIA socket to the CE1 and CE2 of the CF
card.
e.g. assert A9 and A10 (inverted?) on the PCMCIA, while pulling _REG high.
( The address and CE logic use exactly the same timings, so this should
work.


Then the second card is normally addressed and handled.

OR: Find out which two lines on the Hornet drive the CE1 and CE2 on the
second slot. This can be done by ohming out pins 7 and 42 of the second
PCMCIA socket of a 700LX with the Hornet's pins. Connect these to the CF's
CE1 and CE2, and they should work without problems.

Alternatively, use a small i/o address coder for asserting IO read and IO
write, and connect the CF to (mostly) the memory extension socket in 'True
Ide' mode, again, CE1 and 2 to address lines. Needs a small IDE driver, but
avoids most PCMCIA troubles.

Michel



----- Original Message -----
From: "Daniel Hertrich" <daniel.hertrich@GMX.DE>
To: <HPLX-L@UCONNVM.UCONN.EDU>
Sent: Monday, March 11, 2002 2:03 PM
Subject: Re: CF inside HP200LX ( was: Re: HP collection


> Hi Stefan
>
> On Sat, 9 Mar 2002 17:59:16 +0000, Stefan Peichl
<Stefan.Peichl@T-ONLINE.DE> wrote:
>
> > LXCIC always only uses the socket number 1. I don't know, if
> > the 700LX for example has a socket 1 and a socket 2, or if it
> > has 2 adapters with one socket each, or if the built in Nokia
> > modem card is accessed completely different.
>
> Couldn't you simply modify LXCIC so that it also asks for info on
> socket 2? This way we could test that.
>
> > The SDK also states, that a Socket, which has been used for
> > something else than a memory card, is reset to generic memory
> > card operation after the card has been removed. IMHO this
> > implies, that after removing the Nokia data card from the 700LX
> > the slot should be available and setup for memory cards, which
> > it is obviously not. Therefore I think it is handled different
> > to the external PCMCIA socket.
>
> Well, as far  as I have heard, the second slot in the700LX is strictly
> I/O wired. So no way to put a flash card into it.
>
> But in a few days I will get a 700LX, and then I can look for the
> wiring. :-)
>
> GTX
> daniel
>
>
> --
> http://www.daniel-hertrich.de/contact
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 23:51:34 +0100
Reply-To:     Jacques Belin <jbelin@ALTERN.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jacques Belin <jbelin@ALTERN.ORG>
Subject:      Re: New DOS (Win, Linux, etc.) handheld
In-Reply-To:  <3C5EF86F.5B26FE55@union-tel.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="ISO-8859-1"
Content-Transfer-Encoding: quoted-printable

Le Mon, 11 Mar 2002 16:08:17 EST
"Robert K=2E Meyer" <bmeyer@UNION-TEL=2ECOM> a =E9crit:

> AA's & long battery life are necessary IMHO for an LX
> replacement=2E

Yes=2E 4 hours is definitely not enough for me=2E=2E=2E

Same electronical architecture (not talking about this awful form factor), b=
ut
only a 100 Mhz processor, 64 Mb Ram, B&W screen, Flash technology hard
drive, etc=2E=2E=2E could perhaps increase the autonomy, but to which level =
?

Jacques=2E

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 23:51:35 +0100
Reply-To:     Jacques Belin <jbelin@ALTERN.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jacques Belin <jbelin@ALTERN.ORG>
Subject:      Re: New DOS (Win, Linux, etc.) handheld
In-Reply-To:  <001801c1c92f$bf807fc0$5774c5cb@q20>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Le Tue, 12 Mar 2002 00:35:43 +0530
pksharma <pksharma@CAL=2EVSNL=2ENET=2EIN> a =E9crit:

> a b&w touch screen could
> have been much much better =2E=2E=20

BTW (beside the power consumption point), do you have noticed the screen
resolution : 640x480 (x 3 color "elements" / pixel), in a size which
could nearly fit to the HPLX form factor ?

Let's dream=2E=2E=2E=2E

Jacques=2E

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 23:51:36 +0100
Reply-To:     Jacques Belin <jbelin@ALTERN.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jacques Belin <jbelin@ALTERN.ORG>
Subject:      Re: New DOS (Win, Linux, etc.) handheld
In-Reply-To:  <001801c1c92f$bf807fc0$5774c5cb@q20>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Le Tue, 12 Mar 2002 00:35:43 +0530
pksharma <pksharma@CAL=2EVSNL=2ENET=2EIN> a =E9crit:

> but what is a SMS keyboard ?

It's one of these very small keyboards that can be connected to cellular
phone to write SMS=2E=2E=2E=20


Well, do you remember that the main grief made against the HPLX was that
the keyboard was too small ?  <g>

If they can sell "that", we can get a point to ask HP to resume the HPLX
line=2E=2E=2E=2E  ;-)

Jacques=2E

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 16:29:59 -0700
Reply-To:     Bob Christopher <bob@PALMTOP.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Christopher <bob@PALMTOP.COM>
Subject:      Re: New DOS (Win, Linux, etc.) handheld
Mime-Version: 1.0
Content-Type: text/plain; charset=iso-8859-1
Content-Transfer-Encoding: 8bit

PK - SMS stands for Short Message Service (like alphanumeric
pagers utilize).

As an aside, funny how closely the convergence of technologies
can resemble a collision. This "brick" may run any OS, but it's
going to take an extra large pair of cargo pants to carry it
around!

Bob
 Bob Christopher . Littleton, Colorado USA . bob@palmtop.com
  Palmtop Computers . Minox Cameras . All The Small Stuff

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 01:50:43 +0000
Reply-To:     Stefan.Peichl@T-ONLINE.DE
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Stefan Peichl <Stefan.Peichl@T-ONLINE.DE>
Subject:      ANN: LXPIC 7.1
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Steve Novosad found two bugs in LXPIC 7.0 and also supplied me
with the solutions:

- On some VESA implementations, V7.0 showed color errors in
  high and true color modes.
- The DOS shell didn't work under all Windows versions.

Hopefully both bugs are fixed now. Many thanks to Steve for
tracing down what was wrong. And I'd like to thank Tamas Feher
for explaining how to use LXPIC under Win NT/2000/XP.

Version 7.1  -DOS shell works now for all Windows versions
(10-MAR-02)  -High and True color bug fixed for some VESAs
             -Added Windows NT/2000/XP under "HOW TO USE LXPIC"

Download from

http://peichl.hplx.net/lxpic.zip

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 11 Mar 2002 21:35:54 -0800
Reply-To:     patrick@west.net
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Patrick West <francis_patrick_west@YAHOO.COM>
Subject:      Palm are looking more interesting
Mime-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

A palm OS machine with a keyboard!

< =
 http://www.sony.co.jp/sd/products/Consumer/PEG/PEG-NR70V/index.h=
tml  >

--
Patrick West, patrick@west.net on 03/11/2002



_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 01:24:07 -0500
Reply-To:     Francois Gurin <matrix@SHOT.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Francois Gurin <matrix@SHOT.ORG>
Subject:      intel's next gen handheld processor
Mime-Version: 1.0
Content-Type: text/plain; charset=us-ascii

I don't have any urls handy to point people to, but since there has been a
good deal of discussion on alternate handhelds lately, i thought people
may want to start looking into the upcoming intel processor for portable
devices.

If i remember right, it's called the x-scale, and intel has been working
it out so it will be supported by linux, palmos, and epoch among others.

also, for those who don't speak japanese,
http://www.palminfocenter.com/view_Story.asp?ID=3123
covers the new sony palms previously mentioned.

--francois

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 08:01:24 -0500
Reply-To:     Steve <novosad@SERVER030.FWB.SAIC.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Steve <novosad@SERVER030.FWB.SAIC.COM>
Subject:      Re: CF inside HP200LX
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Daniel Wrote:

> Well, as far  as I have heard, the second slot in the700LX is strictly
> I/O wired. So no way to put a flash card into it.

   Can't a flash card be accessed as a hard drive, I/O rather
than memory access?  Isn't that what Dr. Dubs did with the Minix
installation he did?  Anyone with a 700LX want to load up Minix?

Greetings

Steve

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 11:14:18 -0500
Reply-To:     albert.kind@uconn.edu
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Al Kind <MCHEM1@UCONNVM.UCONN.EDU>
Subject:      test
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

testing...1...2...3

Al Kind
Technical Lab Manager, Microchemistry Lab CANR
3113 Horsebarn U4193, Storrs CT 06269-4193
ph (860)486-6126  eFAX (413)826-8780

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 21:39:20 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: New DOS (Win, Linux, etc.) handheld
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

-----Original Message-----
From: Bob Christopher <bob@PALMTOP.COM>
Date: Tuesday, March 12, 2002 5:08 AM


>As an aside, funny how closely the convergence of technologies
>can resemble a collision. This "brick" may run any OS, but it's
>going to take an extra large pair of cargo pants to carry it
>around!


and bob knows ! his bottom line also includes :
"All The Small Stuff"


..pk

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 19:05:45 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      PLEASE EMAIL ME PRIVATELY
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

it seems that I have problems to get list emails. No list email since
about 24h now, but Al Kind says the list server is okay.

So, please, if you send / sent any replies to my postings to the list,
CC to my private email address!

Thanks!

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 19:14:34 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      TEST
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

test. please ignore.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 19:21:45 +0100
Reply-To:     Tomas Moberg <Tomas.Moberg@ABC.SE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tomas Moberg <Tomas.Moberg@ABC.SE>
Subject:      Re: 100LX to HP Jornada 568 conversion
Comments: To: "Douglas Tucker, M.D." <dtucker@ITSA.UCSF.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Use Camerons conversion tool. I moved my appointments  and phonebook to
my PocketPC with it.
For database I used Handbase for PocketPC.

Douglas Tucker, M.D. wrote:
> I'm contemplating getting the 568, which runs the Pocket PC 2002 OS, =
but
> I'm concerned about having to reenter all my phonebook, appointment, =
and
> memo entries.  Is there some way to do a simple conversion using the
> connectivity pack (or anything else)?
> -Doug
>

      /tomas moberg
                       Uppsala

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 14:19:19 -0500
Reply-To:     Bing <bxu2@UWO.CA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bing <bxu2@UWO.CA>
Subject:      pocket quicken and quicken files
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

I am using 200lx to keep my financial activities. You know, you can
download your financial account activities from most of web financing
sites in the form of Quicken file with extension of .qfx, or CSV
files. But the Quicken files are not read by 200lx's Pocket Quicken
(with .PDT files). Are they the same file format? Or any way to convert
the Quicken or other downloadable account files, say, Money or CSV etc. to
Pocket Quicken files, .PDT files?
Bing

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 20:44:02 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Another test
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

I'm sorry for the wasted bandwidth, but it's really strange:
My friend Konstantin also receives no list emails. He is also a GMX
member. Any other GMXers out there who _receive_ the list?

I have subscribed now with another address. Let's see if that works.

If in the last 24h messages have been posted which were meant to be
read by me, please send them to me once more in private email.

Thanks

daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 15:02:08 -0500
Reply-To:     Bing Xu <bxu2@UWO.CA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bing Xu <bxu2@UWO.CA>
Subject:      Re: PLEASE EMAIL ME PRIVATELY
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I got the email.
----- Original Message -----
From: "Daniel Hertrich" <daniel.hertrich@GMX.DE>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Tuesday, March 12, 2002 12:05 PM
Subject: PLEASE EMAIL ME PRIVATELY


> Hi friends,
>
> it seems that I have problems to get list emails. No list email since
> about 24h now, but Al Kind says the list server is okay.
>
> So, please, if you send / sent any replies to my postings to the list,
> CC to my private email address!
>
> Thanks!
>
> GTX
> daniel
>
> --
> http://www.daniel-hertrich.de/contact
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 15:16:37 -0500
Reply-To:     Ed <edwardp@SYMPATICO.CA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ed <edwardp@SYMPATICO.CA>
Subject:      Re: pocket quicken and quicken files
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

You need a PC version of Quicken on your desktop that will allow you to open
the .qfx file.  The desktop quicken has a function allowing you to export it
into a .qif (quicken interchange format) file ( File/Export) .  Pocket
quicken on the lx can then import the .qif file using the File/Import
function.

Ed

----- Original Message -----
From: "Bing" <bxu2@UWO.CA>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Tuesday, March 12, 2002 2:19 PM
Subject: pocket quicken and quicken files


> I am using 200lx to keep my financial activities. You know, you can
> download your financial account activities from most of web financing
> sites in the form of Quicken file with extension of .qfx, or CSV
> files. But the Quicken files are not read by 200lx's Pocket Quicken
> (with .PDT files). Are they the same file format? Or any way to convert
> the Quicken or other downloadable account files, say, Money or CSV etc. to
> Pocket Quicken files, .PDT files?
> Bing
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 13:53:58 -0800
Reply-To:     "Martin G. Ramirez" <mramirez@LMU.EDU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Martin G. Ramirez" <mramirez@LMU.EDU>
Subject:      Com1 address & interrupt
In-Reply-To:  <008c01c1ca00$ca64d0e0$7ee36481@acec15>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

LXers,

For a 200LX, what should the values be for port address and interrupt for
COM1 in Setup?

Martin G. Ramirez



============================
Dr. Martin G. Ramirez
Department of Biology
Loyola Marymount University
One LMU Drive, MS 8220
Los Angeles, CA  90045-2659, U.S.A.
(310) 338-5120
FAX: (310) 338-4479
e-mail: mramirez@lmu.edu
=============================




NTMail K12 - the Mail Server for Education

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 22:34:51 +0000
Reply-To:     fjkaufman@WORLDNET.ATT.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "F. Kaufman" <fjkaufman@WORLDNET.ATT.NET>
Subject:      Re: 100LX to HP Jornada 568 conversion
Comments: To: "Douglas Tucker, M.D." <dtucker@ITSA.UCSF.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

> I'm contemplating getting the 568, which runs the Pocket PC 2002 OS, but
> I'm concerned about having to reenter all my phonebook, appointment, and
> memo entries.  Is there some way to do a simple conversion using the
> connectivity pack (or anything else)?


If the 568 is an hp unit (sounds like it), in the past they shipped a
program on the cd which allowed a conversion between the 100/200 format
and the newer format.  I would suspect that they still do but I'm not
sure of it.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 22:35:06 +0000
Reply-To:     fjkaufman@WORLDNET.ATT.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "F. Kaufman" <fjkaufman@WORLDNET.ATT.NET>
Subject:      Re: Personal Food Analyst
Comments: To: Marta Pierce <Marta1@attbi.com>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

>  I get that when ever I try to save or retrieve info that I placed
>  into the program.  I have it currently on my A drive, in a dos
>  software carrousel area.  There is plenty of room in the area. Also,
>  I had the same problem when I moved it to the C drive.  I
>  have a 32 db speed machine.
>
>  What it looks like is that the database.db4 isn't saving any info. I
>  tried to manually enter a new food, and it wouldn't save it.
>
>  any one know this software?

I may have posted something like this before:


I have not really used it in a long time but I do recall saving my own
stuff.  There was a second or professional version but I don't know if
they are still producing it and how updated.

I do remember doing some odd locational stuff to get it to work.  I
don't think it could just be moved off of its card.

Here's my strucutre on the A: drive

a:\P

.              <DIR>        01-05-01  9:21a .
..             <DIR>        01-05-01  9:21a ..
A        BAT            69  03-08-97 11:48p A.BAT
D        DB4           279  03-08-97 11:48p D.DB4
P        SAV         5,279  03-08-97 11:48p P.SAV
PFA      KEY         8,497  03-08-97 11:48p PFA.KEY
P              <DIR>        01-05-01  9:21a P
         4 file(s)         14,124 bytes

A:\P\P

.              <DIR>        01-05-01  9:21a .
..             <DIR>        01-05-01  9:21a ..
D        DB4       379,206  03-08-97 11:50p D.DB4
D        QIK       106,002  03-08-97 11:52p D.QIK
PFA      EXE       174,111  03-08-97 11:51p PFA.EXE
         3 file(s)        659,319 bytes

Total files listed:
         7 file(s)        673,443 bytes
         5 dir(s)        4,476.16 MB free

A.bat mostly changes the screen size and passed some keystrokes to get
me directly somewhere (but I don't recall where) then ran pfa in that
doubled down subdirectory:

ECHO OFF
zoomtest c4
ks \z/ 1g/l2
a:\p\p\pfa
zoomtest c8
esc

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 20:20:12 -0500
Reply-To:     Dario Draiman <dario200@MAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dario Draiman <dario200@MAIL.COM>
Subject:      Re: Com1 address & interrupt
Comments: To: "Martin G. Ramirez" <mramirez@LMU.EDU>
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: 7bit
MIME-Version: 1.0

Mine is I/O 02F8 INT 4.


----- Original Message -----
From: "Martin G. Ramirez" <mramirez@LMU.EDU>
Date:         Tue, 12 Mar 2002 13:53:58 -0800
To: HPLX-L@UConnVM.UConn.Edu
Subject:      Com1 address & interrupt


> LXers,
>
> For a 200LX, what should the values be for port address and interrupt for
> COM1 in Setup?
>
> Martin G. Ramirez
>
>
>
> ============================
> Dr. Martin G. Ramirez
> Department of Biology
> Loyola Marymount University
> One LMU Drive, MS 8220
> Los Angeles, CA  90045-2659, U.S.A.
> (310) 338-5120
> FAX: (310) 338-4479
> e-mail: mramirez@lmu.edu
> =============================
>
>
>
>
> NTMail K12 - the Mail Server for Education
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

--

_______________________________________________
Sign-up for your own FREE Personalized E-mail at Mail.com
http://www.mail.com/?sr=signup

Travelocity.com is giving away two million travel miles.
http://ad.doubleclick.net/clk;3969773;6991039;g?http://svc.travelocity.com/promos/millionmiles_main/0,,TRAVELOCITY,00.html

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 17:37:25 -0800
Reply-To:     lfast@NATIVELAW.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Lawrence Fast <lfast@NATIVELAW.COM>
Subject:      GSM/GPRS DOS based PDA-Phone
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Convergence does indeed lead to some strange products.  The RIM Blackberry
is about to be released in a GSM/GPRS phone version.  It has an SMS style
keyboard and is DOS based.  If only it had a proper (100LX or 200LX) case
and keyboard, a compact flash slot, and the ability to load and run DOS
programmes, then Nirvana would be close indeed.  Take a look at
http://www.blackberry.net/

Having the technical ability of a stunted marmot, I would not even dream of
taking on this kind of a project.  However, would it be possible to
cannibalize the Blackberry, stuff its electronics into a 200LX box, attach
a standard screen and a card slot and then have a fully functional DOS
based PDA - phone combination?  Better yet, would anyone be interested in
approaching RIM to see if they would be interested in producing such a
desirable gadget?

Lawrence Fast

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 10:35:38 +0800
Reply-To:     SM Ling <piclister@yahoo.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         SM Ling <piclister@YAHOO.COM>
Subject:      Dos emulator on Arm machine
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I am curious on how well can non-808x PDA runs DOS programs though emulator,
particularly the winCE machines.  Any comments?

I hope this does not start a flame.  Not on a proud HP200LX sss owner.

Thanks.

Ling SM

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 12 Mar 2002 21:35:57 -0800
Reply-To:     hobchi@hotmail.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         hobchi <hobchi@YAHOO.COM>
Subject:      Pleethora of DOS/LX pgms
In-Reply-To:  <HPLX-L%2002030719433966@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: multipart/alternative; boundary="0-515054666-1015997757=:12982"

--0-515054666-1015997757=:12982
Content-Type: text/plain; charset=us-ascii


 http://www.filelibrary.com/Contents/DOS/19/1.html
yor pal al...................



.
       o__
      _.>/)_
     (_) \(_)
Woman, that's warm...
  Semper Mobilus


---------------------------------
Do You Yahoo!?
Try FREE Yahoo! Mail - the world's greatest free email!
--0-515054666-1015997757=:12982
Content-Type: text/html; charset=us-ascii

<P> <A href="http://www.filelibrary.com/Contents/DOS/19/1.html">http://www.filelibrary.com/Contents/DOS/19/1.html</A>
<P>yor pal al...................
<P>&nbsp;</P><BR><BR>.<br>       o__       <br>      _.&gt;/)_    <br>     (_) \(_) <br>Woman, that's warm...<br>  Semper Mobilus<p><br><hr size=1><b>Do You Yahoo!?</b><br>
Try FREE <a href="$rd_url/tag/http://mail.yahoo.com/">Yahoo! Mail</a> - the world's greatest free email!
--0-515054666-1015997757=:12982--

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 01:25:06 EST
Reply-To:     AHA2K@AOL.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         AHA2K@AOL.COM
Subject:      Beg./Int.lvl.user wants to get back UAR.
MIME-Version: 1.0
Content-Type: text/plain; charset="US-ASCII"
Content-Transfer-Encoding: 7bit

Craftsman, not in computer industry seeks consultation in reintegrating LX
into operations. After some catastrophic losses of primary and b/u data, and
a long pause in between, I am looking for assistance in getting back up and
running. I need suggestions on routines for utilizing and preserving data.
Are there any FAQs or readmes on integrating HPLX use in ordinary affairs? I
tried to utilize a hand-me-down Palm, but the interface was too frustrating-
mastering Graffiti was not very satisfying. Would accept any on-line or in
person evaluation and direction.
Thank you,
Adam in NYC

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 09:05:53 +0100
Reply-To:     Juergen Korthof <hplx@0800CALLING.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Juergen Korthof <hplx@0800CALLING.DE>
Subject:      Fluff: No list-mails
In-Reply-To:  <HPLX-L%2002030917584108@UCONNVM.UCONN.EDU>
Mime-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

I don=B4t receive any listmail since Sunday 10.March 2002 00:03

I have already unsubscribed und subscribed again. The
Listserver replies.
But no listmail anyway.
I will look in the archive whether my mail goes in.

Happy LXing
Juergen.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 09:34:21 +0100
Reply-To:     Michael Lennartz <lennartz-mi@GMX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Lennartz <lennartz-mi@GMX.NET>
Subject:      Re: Another test
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
In-Reply-To:  <HPLX-L%2002031214424888@UCONNVM.UCONN.EDU>
Mime-Version: 1.0
Content-Type: text/plain; charset="ISO-8859-1"
Content-Transfer-Encoding: 8bit

Hallo Daniel,

I get all the mails including yours.

Mit freundlichem Gru_ / Regards / Saluton

Michael Lennartz
lennartz-mi@gmx.net
Fax: +49 89 244 34 52 57

Daniel Hertrich schrieb am 12.03.2002:
>Hi friends,
>
>I'm sorry for the wasted bandwidth, but it's really strange:
>My friend Konstantin also receives no list emails. He is also a GMX
>member. Any other GMXers out there who _receive_ the list?
>
>I have subscribed now with another address. Let's see if that works.
>
>If in the last 24h messages have been posted which were meant to be
>read by me, please send them to me once more in private email.
>
>Thanks
>
>daniel
>
>--
>http://www.daniel-hertrich.de/contact
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 11:36:12 +0100
Reply-To:     Erwann ABALEA <erwann@ABALEA.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Erwann ABALEA <erwann@ABALEA.COM>
Organization: Halfling Soft
Subject:      Re: Dos emulator on Arm machine
In-Reply-To:  <013101c1ca37$c3531aa0$f8ad15a5@amd>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=iso-8859-1
Content-Transfer-Encoding: quoted-printable

On Wed, 13 Mar 2002, SM Ling wrote:

> I am curious on how well can non-808x PDA runs DOS programs though emul=
ator,
> particularly the winCE machines.  Any comments?
>
> I hope this does not start a flame.  Not on a proud HP200LX sss owner.

Just look at the Bochs project and some others. There's one that works
like vmware (emulating a PC on a PC), and another that emulates a PC on
any other architecture. I don't remember who does what.

--=20
Erwann ABALEA <erwann@abalea.com> - RSA PGP Key ID: 0x2D0EABD5
-----
Quand je passe par le bios et que je lui dit de booter sur C, il boot
sur le PM en C:\ et il met le SM en D:\. Quand le lui dit de booter sur
D, il boot sur le SM en C:\ et il met le PM en D:\.  Ca c'est g=E9nial.
-+- FP in: Guide du Neuneu d'Usenet - Le bonheur, c'est simple -+-

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 12:39:30 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      One more test
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

why don't I get ANY mail from the list???

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 00:46:52 +1300
Reply-To:     Tony Hutchins <th@PARADISE.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Hutchins <th@PARADISE.NET.NZ>
Subject:      Re: ANN: CLOCKS
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Thu, 14 Mar 2002 00:26:41 +1300 (NZDT)

CLOCKS V3.0 is there now. This one will run forward or
backward at varing rates, can be stopped or be set to a
specific date or time. Clocks can be rearranged, edited and
re-stored, and recalled. Also does daylight savings
adjustments. See the included clocks.doc.

- Tony

2 days 06h03m49s ago ...
On Mon, 11 Mar 2002 18:22:52 +1300 (NZDT), Tony Hutchins wrote:

> Mon, 11 Mar 2002 18:19:20 +1300 (NZDT)
>
> CLOCKS V2.1 is at:
>
> http://homepages.paradise.net.nz/th/

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 06:00:24 -0800
Reply-To:     Longden_Loo@CANDLE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Longden Loo <Longden_Loo@CANDLE.COM>
Subject:      Re: Beg./Int.lvl.user wants to get back UAR.
Comments: cc: AHA2K@AOL.COM
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

> Craftsman, not in computer industry seeks consultation in reintegrating
LX
> into operations. After some catastrophic losses of primary and b/u data,
and
> a long pause in between, I am looking for assistance in getting back up
and
> running. I need suggestions on routines for utilizing and preserving
data.

Get a flash card (PCMCIA or Compact Flash), create an automatic recurring
appointment on the LX to make a nightly backup copy of your primary data
onto the card.

Every couple of days (or weekly), manually copy the card's contents onto
your notebook or desktop computer, preferably keeping each successive file
in a separate directory or filename.

There are some good variations on this scheme, but they are primarily icing
on the cake.  The important point is to make the daily backup automatic,
and to keep long term storage of your backups in a separate location.

The exact best way to do this will depend on the extent of your computer
skills, and your available resources (ie, time and money).

My $.03

- Longden

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 08:20:04 -0600
Reply-To:     John McCaskill <jmccask@POWERCHOKES.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John McCaskill <jmccask@POWERCHOKES.COM>
Subject:      Re: Beg./Int.lvl.user wants to get back UAR.
In-Reply-To:  <OFBD619A2C.3143234C-ON88256B7B.004C0584@candle.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

"...create an automatic recurring appointment on the LX to make a nightly
backup copy of your primary data
onto the card."

I don't know how to do this.
Where can I find FAQ or instructions?
I have a 100LX 1 MB with 16mB FC.
I'm running Buddy100, otherwise standard HP apps.

John

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 06:54:32 -0800
Reply-To:     paul <paul@PYARNELL.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         paul <paul@PYARNELL.NET>
Subject:      Test
Content-Type: text/plain
Content-Transfer-Encoding: 7bit
Mime-Version: 1.0

New account test
--
I'd be a Libertarian, if they weren't all a bunch of tax-dodging
professional whiners.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 09:05:35 -0600
Reply-To:     melancon@microgear.net
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Mike Melancon <melancon@MICROGEAR.NET>
Subject:      To Daniel and the list (was: One more test)
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
In-Reply-To:  <HPLX-L%2002031306381577@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-type: text/plain; charset=US-ASCII
Content-transfer-encoding: 7BIT

Daniel

In case this helps - I am sending this reply to you directly and to the list -
just to see if one or both make it to you.

Mike

> why don't I get ANY mail from the list???
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 09:50:12 -0600
Reply-To:     John McCaskill <jmccask@POWERCHOKES.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John McCaskill <jmccask@POWERCHOKES.COM>
Subject:      Re: Beg./Int.lvl.user wants to get back UAR.
In-Reply-To:  <NFBBIDBHCLHDDBEKCHHDMEIMCMAA.jmccask@powerchokes.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Never mind, I figure out how to do it by reading the Palmtop paper archives.
I created a batch file & launched it from a  recurring appointment. Next
question: How do I set up a recurring appointment to exit all open apps?

Thanks

John

-----Original Message-----
From: HPLX Mailing List [mailto:HPLX-L@UConnVM.UConn.Edu]On Behalf Of
John McCaskill
Sent: Wednesday, March 13, 2002 8:20 AM
To: HPLX-L@UConnVM.UConn.Edu
Subject: Re: Beg./Int.lvl.user wants to get back UAR.


"...create an automatic recurring appointment on the LX to make a nightly
backup copy of your primary data
onto the card."

I don't know how to do this.
Where can I find FAQ or instructions?
I have a 100LX 1 MB with 16mB FC.
I'm running Buddy100, otherwise standard HP apps.

John

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 09:17:06 -0800
Reply-To:     Joe Buford <cpt_kludge@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Joe Buford <cpt_kludge@YAHOO.COM>
Subject:      OT-Buford & Digests
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii

First,

My thanks to Laurence Harvey and Bob Penick for their
help. It seems that the SMT server hear at Boeing has
a  wild hair up its @#$@!!!

Some messages from the HPLX-L Listserv seem to be
bouncing due to spam..... I never even know they have
been sent, but the sender gets a message similar to
the below:

--- MAILER-DAEMON@yahoo.com wrote:
> Date: 12 Mar 2002 23:38:27 -0000
> From: MAILER-DAEMON@yahoo.com
> To: cpt_kludge@yahoo.com
> Subject: failure delivery
>
> Message from  yahoo.com.
> Unable to deliver message to the following
> address(es).
>
> <joseph.buford@hsc.com>:
> 192.161.36.24 failed after I sent the message.
> Remote host said: 552 Message identified as spam....
>
> --- Original message follows.
>
> Return-Path: <cpt_kludge@yahoo.com>
>
> The original message is over 5k.  Message truncated
> to 1K.
>
> Message-ID:
> <20020312233812.7699.qmail@web20309.mail.yahoo.com>
> Received: from [128.152.20.33] by
> web20309.mail.yahoo.com via HTTP; Tue, 12 Mar 2002
> 15:38:12 PST
> Date: Tue, 12 Mar 2002 15:38:12 -0800 (PST)
> From: Joe Buford <cpt_kludge@yahoo.com>
> Subject: test
> To: joseph.buford@hsc.com
> MIME-Version: 1.0
> Content-Type: multipart/mixed;
> boundary="0-1850720966-1015976292=:7097"
>
> --0-1850720966-1015976292=:7097
> Content-Type: text/plain; charset=us-ascii
> Content-Disposition: inline
>
> test

In the short term I have set up a yahoo acct and
subscribed to the list from there. I should be able to
get the digests from there and use that acct to try to
figure out why the boeing server considers some of the
HPLX-L digests as spam. In the long term I have an
open ticket with our IT group to look at the problem.

If anyone has tried to reach me and ether I have not
responded or you rx an error msg, please contact me at
the cpt_kludge@yahoo.com address IN ADDITION to my
regular address at joseph.buford@hsc.com or
joseph.e.buford@boeing.com. This way at least I will
know when I have missed msg's even if I have to pick
them up from yahoo.

The weird thing about the errors is that if someone
tries to send a digest (that originally bounced to me)
then it will still bounce even when coming from
someone other than the HPLX-L listserv(ie:Laurence or
Bob). Same thing if I send it to my boeing acct from
my yahoo acct. However, if I split into 2 messages and
send  both at the same time to my boeing acct, they
get thru fine. This seems to indicate that the size of
the msg may be part(or all) of the problem. However, I
have rx lots of HPLX-L msg's that are way larger than
the ones that errored(ie:#42), with no problems. I
also am subscribed to an Electric Vehicle list that
usually has msg's >50K and I rarely have a problem rx
them.

If anyone has an idea as to what may be going on or
any other help and/or suggestions, please let me know.

Thanks

Joe Buford





__________________________________________________
Do You Yahoo!?
Try FREE Yahoo! Mail - the world's greatest free email!
http://mail.yahoo.com/

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 19:43:59 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: AW: Fluff: No list-mails
Comments: To: Juergen Korthof <hplx@0800calling.de>,
          mchem1@uconnvm.uconn.edu, konstantin.witzleben@gmx.de
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hello Juergen, Al, Konstantin and list,

On Wed, 13 Mar 2002 17:49:12 +0100, "Juergen Korthof" <hplx@0800calling.de> wrote:

> Hi Al,
> hi Daniel,
>
> since I am not connected via GMX but at my own domain at
> strato.de
> I don4t think it is a similar Problem at our ends.
>
> My Mailer is Outlook 2000 and I did4nt changed anything since
> the last
> received Listmail on Sunday Night.
>
> I have no idea, what I could do on my side.

I have no problems receiving any email via GMX, just no list email are
arriving.

It is NOT related to GMX, because I have subscribed with other
addresses (kanfu23 at onlinehome.de and mikeoldfield at gmx.net). No
list mails, either.

It is NOT a spam filter problem, because I disabled all spam filters at
GMX, still no messages.

So I think the problem must be at the list server. Al, please, please
investigate what the problem could be.

I also have sent me an email with a FROM header similar to the one
created by the list server (HPLX-L#UCONNVM.UCONN.EDU). It arrived.

I can also post TO the list without any problem. So my subscription is
still alive.

I have no idea anymore what the problem could be.

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 19:59:56 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: To Daniel and the list (was: One more test)
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Mike

On Wed, 13 Mar 2002 09:05:35 -0600, "Mike Melancon" <melancon@microgear.net> wrote:

> In case this helps - I am sending this reply to you directly and to the list -
> just to see if one or both make it to you.

Thanks.
Only one arrived here. :-(
GTX
daniel
--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 19:05:24 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: Fluff: No list-mails
Comments: To: Juergen Korthof <hplx@0800CALLING.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

As far as I know I'm not missing any of the list.  I subscribe
to receive each post instead of the digest

Did your ISPs put the list behind a spam filter or something
similar?  It is odd that several folks seem to be having this
problem all at once.

Cheers... Russ

Juergen Korthof wrote:
> I don4t receive any listmail since Sunday 10.March 2002 00:03
>
> I have already unsubscribed und subscribed again. The
> Listserver replies.
> But no listmail anyway.
> I will look in the archive whether my mail goes in.
>
> Happy LXing
> Juergen.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 19:05:27 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: One more test
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Daniel Hertrich wrote:
> why don't I get ANY mail from the list???

I don't know, I'm seeing your posts Ok.
Can you communicate with the list 'server'?

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 19:27:26 -0000
Reply-To:     Philip Pemberton <philpem@ZETNET.CO.UK>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Philip Pemberton <philpem@ZETNET.CO.UK>
Subject:      D&A ABC-LX and Kodak 1600mAH NiMH batteries
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Hi,
    I've just put a pair of 1600mAH Kodak "PhotoLife" NiMHs in my 700LX and
I'm having some trouble getting ABC-LX to let me enter the battery capacity.
I can enter anything up to 1200mAH fine, but if I try and enter 1600, ABC-LX
politely tells me to try again...

I know some D&A reps frequent HPLX-L, so can any of them (or anyone else for
that matter) please tell me how to fix this so I can use my NiMHs? It would
be a great shame to have to use my old Uniross 700mAH NiCads again,
especially when I've got these NiMHs...

Thanks.
--
Phil.
philpem@bigfoot.com
http://www.philpem.btinternet.co.uk/

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 20:51:07 +0100
Reply-To:     Etienne Lemaire <etienne.lemaire@pandora.be>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Etienne Lemaire <etienne.lemaire@PANDORA.BE>
Subject:      Re: To Daniel and the list (was: One more test)
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

No idea if this applies, but since specific names seem to be
involved:

my address is stelem at attglobal.net

Yesterday I received a mail that was sent to stelem at
"something else"

 that should never have arrived in my box. I thought it wasn't
worth thinking about, but how could this happen???

.00000000002 cents


Etienne
----- Original Message -----
From: "Daniel Hertrich" <daniel.hertrich@GMX.DE>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Wednesday, March 13, 2002 06:59 PM
Subject: Re: To Daniel and the list (was: One more test)


| Hi Mike
|
| On Wed, 13 Mar 2002 09:05:35 -0600, "Mike Melancon"
<melancon@microgear.net> wrote:
|
| > In case this helps - I am sending this reply to you directly
and to the list -
| > just to see if one or both make it to you.
|
| Thanks.
| Only one arrived here. :-(
| GTX
| daniel
| --
| http://www.daniel-hertrich.de/contact
|
| ** HPLX-L LIST Info at
http://www.sp.uconn.edu/~mchem1/HPLX.shtml
|
|

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 21:00:46 +0100
Reply-To:     Juergen Korthof <hplx@0800CALLING.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Juergen Korthof <hplx@0800CALLING.DE>
Subject:      AW: Fluff: No list-mails
Comments: To: Russel Brooks <rlbrooks@pobox.com>
In-Reply-To:  <200203131905.UAA13257@post.webmailer.de>
Mime-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Hi Russ,

thank you for replying to my adress too.
I still don=B4t receive any List-Mails.


Happy LXing
Juergen.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 14:15:08 -0600
Reply-To:     John McCaskill <jmccask@POWERCHOKES.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John McCaskill <jmccask@POWERCHOKES.COM>
Subject:      Recurring command to save and close all open apps in LX100
In-Reply-To:  <NFBBIDBHCLHDDBEKCHHDOEIOCMAA.jmccask@powerchokes.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I figured out how to copy all C: files to A: backup directory automatically
on a recurring basis for appt.

Next question: How do I set up a recurring appointment to exit all open apps
before the copy occurs?

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 14:19:48 -0600
Reply-To:     Tim <palmtop@N-LINK.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tim <palmtop@N-LINK.COM>
Subject:      FLUFF: FA: A Photo-Negative to Video imager
In-Reply-To:  <HPLX-L%2002030908435670@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Keeping this short: Trying to list a lot of things on eBay.... ONE or two
will be of more interest to the LX community, but thought that someone here
might like to see a Fujix FV-7 Video imager I'm auctioning (sending to LX
list; 'cause I know there are those of us with more than one hobby).

It lets you take negatives or slides and send the image to a video input
(TV, video card etc.).

It's at:

http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=1339246791

Thought you might enjoy!

--tim

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 15:15:46 -0500
Reply-To:     albert.kind@uconn.edu
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Al Kind <MCHEM1@UCONNVM.UCONN.EDU>
Subject:      Re: AW: Fluff: No list-mails
Comments: To: Daniel Hertrich <daniel.hertrich@gmx.de>,
          Juergen Korthof <hplx@0800calling.de>, konstantin.witzleben@gmx.de
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I just contacted the ListServer maintainer. We'll see if he has any ideas?

Cheers...AJKind

-----Original Message-----
From: Daniel Hertrich [mailto:daniel.hertrich@gmx.de]
Sent: Wednesday, March 13, 2002 12:44 PM
To: Juergen Korthof; mchem1@uconnvm.uconn.edu; HPLX-L@UCONNVM.UCONN.EDU;
konstantin.witzleben@gmx.de
Subject: Re: AW: Fluff: No list-mails


Hello Juergen, Al, Konstantin and list,

On Wed, 13 Mar 2002 17:49:12 +0100, "Juergen Korthof" <hplx@0800calling.de>
wrote:

> Hi Al,
> hi Daniel,
>
> since I am not connected via GMX but at my own domain at
> strato.de
> I don4t think it is a similar Problem at our ends.
>
> My Mailer is Outlook 2000 and I did4nt changed anything since
> the last
> received Listmail on Sunday Night.
>
> I have no idea, what I could do on my side.

I have no problems receiving any email via GMX, just no list email are
arriving.

It is NOT related to GMX, because I have subscribed with other
addresses (kanfu23 at onlinehome.de and mikeoldfield at gmx.net). No
list mails, either.

It is NOT a spam filter problem, because I disabled all spam filters at
GMX, still no messages.

So I think the problem must be at the list server. Al, please, please
investigate what the problem could be.

I also have sent me an email with a FROM header similar to the one
created by the list server (HPLX-L#UCONNVM.UCONN.EDU). It arrived.

I can also post TO the list without any problem. So my subscription is
still alive.

I have no idea anymore what the problem could be.

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 15:26:19 -0500
Reply-To:     Bob Penick <bnj@MYREALBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Penick <bnj@MYREALBOX.COM>
Subject:      Re: To Daniel and the list (was: One more test)
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

----- Original Message -----
From: "Etienne Lemaire"
Sent: Wednesday, March 13, 2002 2:51 PM
Subject: Re: To Daniel and the list (was: One more test)


> Yesterday I received a mail that was sent to stelem at
> "something else"
****************************************
FWIW
Don't know about ATT but I have an account with a local ISP that "resells"
access and email that is provided by Infoave.net.  Infoave "wholesales"
their services through lots of small telephone companies primarily across
the southeast United States.  My account is bpenick at pbtcomm.net.  But
they alias the email address using just the bpenick.  Because of this they
cannot use the bpenick part with any other local ISP they service, as it is
already taken by me.  Any email sent to bpenick at any of the other domain
names Infoave hosts will show up in my mailbox.  So in effect I have MANY
email addresses with just one mailbox.  It's only painful when the Spammers
pick up on it.  This is not the primary email account I use as you may
guess.
So Etienne, you may be in a similar situation.
bob

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 21:47:24 +0100
Reply-To:     "Helmuth E. Guenther" <h_e_guenther@ATTGLOBAL.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Helmuth E. Guenther" <h_e_guenther@ATTGLOBAL.NET>
Subject:      Re: AW: Fluff: No list-mails
Comments: To: daniel.hertrich@gmx.de
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

A couple of month ago Tony Hutchins did send me some emails to my
attglobal account. The message bounce telling that I am not a customer
of attglobal. At the same time I get charged from attglobal for their
service. If Tony and myself wouldn't stay in close contact, I, the one
who pays for the service, would never get notice of being denied.

This was addressed to the hotline of ATTGLOBAL about 4 weeks ago. No
answer up to now. After 14 days I did ask for an answer. The only
written answer I got was: "I told you before you need to be patient".
And that's it.

Maybe some strange things are going on here too.

At the time I have no argument, why you should not be reachable from
the list.

Kind regards

Helmuth

> I just contacted the ListServer maintainer. We'll see if he has any ideas?
>
> Cheers...AJKind
>
> -----Original Message-----
> From: Daniel Hertrich [mailto:daniel.hertrich@gmx.de]
> Sent: Wednesday, March 13, 2002 12:44 PM
> To: Juergen Korthof; mchem1@uconnvm.uconn.edu; HPLX-L@UCONNVM.UCONN.EDU;
> konstantin.witzleben@gmx.de
> Subject: Re: AW: Fluff: No list-mails
>
> Hello Juergen, Al, Konstantin and list,
>
> On Wed, 13 Mar 2002 17:49:12 +0100, "Juergen Korthof" <hplx@0800calling.de>
> wrote:
>
> > Hi Al,
> > hi Daniel,
> >
> > since I am not connected via GMX but at my own domain at
> > strato.de
> > I don4t think it is a similar Problem at our ends.
> >
> > My Mailer is Outlook 2000 and I did4nt changed anything since
> > the last
> > received Listmail on Sunday Night.
> >
> > I have no idea, what I could do on my side.
>
> I have no problems receiving any email via GMX, just no list email are
> arriving.
>
> It is NOT related to GMX, because I have subscribed with other
> addresses (kanfu23 at onlinehome.de and mikeoldfield at gmx.net). No
> list mails, either.
>
> It is NOT a spam filter problem, because I disabled all spam filters at
> GMX, still no messages.
>
> So I think the problem must be at the list server. Al, please, please
> investigate what the problem could be.
>
> I also have sent me an email with a FROM header similar to the one
> created by the list server (HPLX-L#UCONNVM.UCONN.EDU). It arrived.
>
> I can also post TO the list without any problem. So my subscription is
> still alive.
>
> I have no idea anymore what the problem could be.
>
> GTX
> daniel
>
> --
> http://www.daniel-hertrich.de/contact
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 12:59:38 -0800
Reply-To:     Joseph.Buford@HSC.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Joseph Buford <Joseph.Buford@HSC.COM>
Subject:      Removing Icons under " More Applications"
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

I remember that there is a process and program (on Super?) that can remove
the hotkey applications from the " More Applications" list allowing more
non-hotkey icons. Can someone let me know the name of the program and where
I can locate it?

Thanks

Joe

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 16:40:31 -0500
Reply-To:     Sales@Systems-Consulting.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Systems-Consulting <Sales@SYSTEMS-CONSULTING.COM>
Subject:      Re: FLUFF: FA: A Photo-Negative to Video imager
In-Reply-To:  <000a01c1cacc$6cdce6c0$6401a8c0@gadgetbase>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I bought it!



Thanks,

Systems-Consulting - here since 1992
89 Main Street, Broad Brook CT 06016-9701
tel:(860)627-5393 fax:(860)627-5393
web: http://Systems-Consulting.com
mailto:Sales@Systems-Consulting.com
Paul Anderson
President
Maximizing the results of Information Systems
Certified Novell Salesperson
Your ALPS MD Printer Supplies Source


> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@UConnVM.UConn.Edu]On Behalf Of
> Tim
> Sent: Wednesday, March 13, 2002 3:20 PM
> To: HPLX-L@UConnVM.UConn.Edu
> Subject: FLUFF: FA: A Photo-Negative to Video imager
>
>
> Keeping this short: Trying to list a lot of things on eBay.... ONE or two
> will be of more interest to the LX community, but thought that
> someone here
> might like to see a Fujix FV-7 Video imager I'm auctioning (sending to LX
> list; 'cause I know there are those of us with more than one hobby).
>
> It lets you take negatives or slides and send the image to a video input
> (TV, video card etc.).
>
> It's at:
>
> http://cgi.ebay.com/aw-cgi/eBayISAPI.dll?ViewItem&item=1339246791
>
> Thought you might enjoy!
>
> --tim
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 22:52:09 +0100
Reply-To:     Daniel Hertrich <hplx-l@DANIEL-HERTRICH.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <hplx-l@DANIEL-HERTRICH.DE>
Subject:      and one more test
Content-Type: text/plain; charset="iso-8859-15"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit

forgive me please...
I'm so persistent because I have sent so much message  s to the list recently
and now I am mot able to read the replies...

I just subscribed with a totally different kind of email address, which
doesn't involve GMX at all. Maybe this allows me to receive list emails again.

I'll let you know.

GTX
daniel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 14:18:52 -0800
Reply-To:     Ian Butler <ianb@HPLX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ian Butler <ianb@HPLX.NET>
Subject:      FLUFF: Re: No list-mails
In-Reply-To:  <MABBICONLJEBNNFHDFJLOEGHCHAA.mchem1@uconnvm.uconn.edu>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Wed, 13 Mar 2002, Al Kind wrote:

> I just contacted the ListServer maintainer. We'll see if he has any
> ideas?

I may be wrong, but all the accounts that are having trouble - aren't they
all in Germany?  Maybe that's relevant somehow...

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 23:32:24 +0100
Reply-To:     Dummy Name <hplx-l@DANIEL-HERTRICH.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dummy Name <hplx-l@DANIEL-HERTRICH.DE>
Subject:      fluff: test
Content-Type: text/plain; charset="iso-8859-15"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit

this is my last attempt.
i  resubscribed with a dummy name.
if that doesn't work, I really don't know.
i still get no messages from the list.
sorry for all the tests, but as long as I still post more useful messages
than tests, i hope you forgive me. ;-)
gtx
daniel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 00:51:14 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: t2t drivers
Comments: To: Bk361kb@aol.com
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Bk361kb@aol.com wrote:
> Yours on subject reminded me.  I had a crash & I'm not sure my 2x is working.
> How do I check to be sure?

Bill,
I'm also answering via the list as there may be better answers
out there than mine.

Since I own both a single and double LX I decided to time how
long it took for "dir d:\*.* /s" to complete.  This should use
only ROM resources so should only be influenced by the speed of
the processor.

Single speed was about 6 seconds.
Double speed was about 10 seconds.

Interesting the faster unit wasn't twice as fast.  (?)

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 03:00:57 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: Removing Icons under " More Applications"
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Joseph Buford wrote:
> I remember that there is a process and program (on Super?) that can remove
> the hotkey applications from the " More Applications" list allowing more
> non-hotkey icons. Can someone let me know the name of the program and where
> I can locate it?

I'm curious, which one(s) would you delete?

I wonder if removing Filer would stop it from starting at boot?

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 03:00:59 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: fluff: test
Comments: To: Dummy Name <hplx-l@DANIEL-HERTRICH.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Dummy Name wrote:
> this is my last attempt.
> i  resubscribed with a dummy name.

Keep trying Daniel, we don't want to lose you!
Whatever the problem it'll get fixed.
Al's starting to look at the server end.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 05:49:24 +0100
Reply-To:     Nathalie Bugeaud <tps-seti@WANADOO.FR>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nathalie Bugeaud <tps-seti@WANADOO.FR>
Subject:      Fluff: Conclusions
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

with the amount of LX users complaining about lack of ability to focus [on
the small screen] i conclude that most of you [not me] must be over 40 and
needing advice on how to prevent heart attacks. This is what i found out as
a medical doctor reading the latest health reports:

(A) The Japanese and Koreans eat very little fat and suffer fewer heart
attacks than the British or Americans.
(B) On the other hand, the French and Portugese eat a lot of fat and also
suffer fewer heart attacks than the British or Americans.
(C) The Japanese and Chinese drink very little red wine and suffer fewer
heart attacks than the British or Americans.
(D) The Italians and French drink excessive amounts of red wine and also
suffer fewer heart attacks than the British or Americans.
(E) Conclusion: Eat & drink what you like. It's speaking English that kills
you. :)

nat (in the process of fixing her bike to prevent having to drink red wine)

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 13 Mar 2002 22:36:37 -0700
Reply-To:     Jeff <hplx@sirveiss.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jeff <hplx@SIRVEISS.COM>
Subject:      DS HP200LX not using full battery capacity
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

Hi all!

I have an HP200LX DS 32M that as of a few months ago, is going through
batteries like there's no tomorrow.  I'm changing them just over once a
day.  I'd estimate I'm getting about 2-3 hours out of a set.  I believe
when I first got the DS upgrade a few years ago, I would last at least
a week or more.

I know that DS palmtops use more battery life, but when I take out the
alkaline batteries and test them (with a battery tester and the one
built into the battery), they're still good!  But the palmtop thinks
the main batteries are low.

Thanks in advance for all your help!

-Jeff

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 04:11:41 -0500
Reply-To:     Owen Samuelson <owensamuelson@COX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Owen Samuelson <owensamuelson@COX.NET>
Subject:      Re: Removing Icons under " More Applications"
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

See if this will help. http://www.palmtoppaper.com/ptphtml/45/45c00010.htm
And this: http://www.palmtoppaper.com/ptphtml/45/45c00011.htm
Best Regards,
Owen

----- Original Message -----
From: "Joseph Buford" <Joseph.Buford@HSC.COM>
Sent: Wednesday, March 13, 2002 3:59 PM
Subject: Removing Icons under " More Applications"


> I remember that there is a process and program (on Super?) that can remove
> the hotkey applications from the " More Applications" list allowing more
> non-hotkey icons. Can someone let me know the name of the program and
where
> I can locate it?

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 10:37:30 +0100
Reply-To:     Michael Lennartz <lennartz-mi@GMX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Lennartz <lennartz-mi@GMX.NET>
Subject:      Re: and one more test
Comments: To: Daniel Hertrich <hplx-l@DANIEL-HERTRICH.DE>,
          Daniel Hertrich <daniel.hertrich@GMX.DE>
In-Reply-To:  <E16lGeO-0005YW-00@mrvdom03.kundenserver.de>
Mime-Version: 1.0
Content-Type: text/plain; charset="ISO-8859-1"
Content-Transfer-Encoding: 8bit

Hallo Daniel,

I have a GMX-account and _no_ problems. This mail goes to:

HPLX-L(at)UConnVM.UConn.Edu
hplx-l(at)DANIEL-HERTRICH.DE
daniel.hertrich(at)GMX.DE

Mit freundlichem Gru_ / Regards / Saluton

Michael Lennartz
lennartz-mi@gmx.net
Fax: +49 89 244 34 52 57

Daniel Hertrich schrieb am 13.03.2002:
>forgive me please...
>I'm so persistent because I have sent so much message  s to the list
>recently
>and now I am mot able to read the replies...
>
>I just subscribed with a totally different kind of email address,
>which
>doesn't involve GMX at all. Maybe this allows me to receive list
>emails again.
>
>I'll let you know.
>
>GTX
>daniel
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 12:12:45 +0100
Reply-To:     Etienne Lemaire <etienne.lemaire@pandora.be>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Etienne Lemaire <etienne.lemaire@PANDORA.BE>
Subject:      Re: Removing Icons under " More Applications"
Comments: To: Joseph.Buford@HSC.COM
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I knew a made a note about of a relevant posting, a long time
ago; here it is:
............
< have just removed Stopwatch, Datacomm, and Lotus 123 from my
APPMGR.DAT file. Here is how:
1.)  copy APPMGR.DAT APPMGR.BAK (backup)
2.)  start Datacomm (or what you like) and transfer APPMGR.DAT
to your desktop. (I do this because I'm using Xtree Gold and
it's too big to carry around on my palmtop.  Xtree has a HEX
editor built-in. You could use Debug, but I'm not that good.)
3.)  Using a HEX editor (Xtree) find the first letter of the
application you want to remove in the APPMGR.DAT file. (first
letter includes & if used as a hot-key "tag")
4.)  Count back, using the first letter as Zero, ten(10)
characters. (remember, the & counts as a character if it's used
to underline (hot key) the first letter of the application
title.)
NOTE: Depending on the location of the application on your
desktop, you should see (in the 11th position) a value (HEX)
that corresponds to the location of the application on your
desktop.
5.)  Starting with the 10th character ( -10 from the first char
of the application ) Overtype (replace, not delete) the next 115
chars with 00 HEX (zeros).
WARNING: The APPMGR.DAT file _must_ remain the same length!
ANOTHER NOTE: You won't have to put zeros in all 115 characters,
it looks like only the applications that have notes use the last
part of the "slot".
6.)  Save the new (edited) APPMGR.DAT file.
7.)  Transfer the new APPMGR.DAT file to your  palmtop. (put the
new file in the c:\_DAT directory)
8.)  Re-boot the palmtop. (a re-boot causes the Desktop to
re-read the APPMGR.DAT file.)
9.)  Open the Desktop (MORE key, you know :)
10.) Look at the location of the application you targeted, it
should have no title and a random icon.
11.) Move the selector box to this "weird" icon and press the
delete (DEL) key.
12.) Blink a few times in relief.  :)
If you could follow my instructions (more likely problems in my
typing style) you should now be able to remove any icon /
application from the desktop. Please remember to do a backup of
the APPMGR.DAT file, and it wouldn't hurt to back-up the entire
palmtop as well.
....................

Never tried myself, hth

Etienne
----- Original Message -----
From: "Joseph Buford" <Joseph.Buford@HSC.COM>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Wednesday, March 13, 2002 09:59 PM
Subject: Removing Icons under " More Applications"


| I remember that there is a process and program (on Super?)
that can remove
| the hotkey applications from the " More Applications" list
allowing more
| non-hotkey icons. Can someone let me know the name of the
program and where
| I can locate it?
|
| Thanks
|
| Joe
|
| ** HPLX-L LIST Info at
http://www.sp.uconn.edu/~mchem1/HPLX.shtml
|
|

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 06:40:53 -0700
Reply-To:     mike <kopplin@TECHNOIR.NU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         mike <kopplin@TECHNOIR.NU>
Subject:      DHCP and LXTCP
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

Anyone using DHCP and LXTCP?

It looks like I'll have to start using DHCP at work. I've never
had to use it before so this is new to me. DHCP with WWW/LX
seems straightforward enough, using dhcp.exe from dasoft. The
LXTCP docs mention that DHCP is supported but undocumented.
Looking at the source, it seems all I need is "my_ip=dhcp" in
tcp.cfg. Is this correct?

Regards,
Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 06:58:13 -0700
Reply-To:     Michael Kopplin <kopplin@TECHNOIR.NU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Kopplin <kopplin@TECHNOIR.NU>
Subject:      Re: fluff: test
In-Reply-To:  <E16lHHM-0007Z5-00@mrvdom03.kundenserver.de>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

> this is my last attempt.
> i  resubscribed with a dummy name.
> if that doesn't work, I really don't know.
> i still get no messages from the list.

Just testing something for Daniel.

Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 08:08:02 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: DHCP and LXTCP
In-Reply-To:  <Pine.LNX.4.33.0203140632470.10338-100000@hal.technoir.nu>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Thu, 14 Mar 2002, mike wrote:

> Anyone using DHCP and LXTCP?

I am <grin>

I'm on a Netware LAN at work and use the drivers and setup from
Nori that I got from hplx.net.  The first line of my tcp.cfg file
says "include=c:\prgms\net\ipaddr.cfg" where the "prgms\net" is my
path.  (my_ip= is commented out)

The batch file below loads all the drivers.  Give me a holler if
you have questions, I'll try to help.

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA


[netup.bat]

copy \prgms\lxtcp\tcp.%1 \prgms\lxtcp\tcp.cfg
cd \prgms\net
op2216
pd2212 0x62 5
pdipx
if '%1'=='hom' goto home
netx
dhcp
call ip-up
echo my_ip=%MYIP% > ipaddr.cfg

:home
cd \prgms\lxtcp
ntime sundial.columbia.edu

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 09:09:41 -0500
Reply-To:     "Striegel, Alan" <Striegel@PIOS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Striegel, Alan" <Striegel@PIOS.COM>
Subject:      Re: FLUFF: Re: No list-mails
MIME-Version: 1.0
Content-Type: text/plain

The symptoms look to me like somebody may have added the source domain to a
'black-hole' list, such as is used to reject mail from spammers and open
relays.

Alan Striegel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 07:42:20 -0700
Reply-To:     Michael Kopplin <kopplin@TECHNOIR.NU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Kopplin <kopplin@TECHNOIR.NU>
Subject:      Re: DHCP and LXTCP
In-Reply-To:  <Pine.OSF.4.33.0203140801390.13068-100000@worf.netins.net>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Thu, 14 Mar 2002, Theodore Heise wrote:
> On Thu, 14 Mar 2002, mike wrote:
>
> > Anyone using DHCP and LXTCP?
>
> I am <grin>

So you're using dhcp.exe. I had thought about that, but what I
was really asking about is DHCP support built into the wattcp
component of LXTCP programs. I'll keep this in mind but I like
the simplicity of built-in support if I can get it to work.

Thanks,
Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 06:42:55 -0800
Reply-To:     Longden_Loo@CANDLE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Longden Loo <Longden_Loo@CANDLE.COM>
Subject:      Re: Recurring command to save and close all open apps in LX100
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Using the built-in features, it's not exactly straight-forward.  There are
programs (I think) that close open apps, but I have a system macro set up
to do this.

The appointment triggers the macro (Alt-7 for me, which is invoked from
Appt Book via "||7" in the description).  The macro closes all apps
(more/menu/application/close all) and then invokes an icon in AppMgr which
I created that actually does the subsequent pkzip and copies.  I have this
appointment set up as recurring daily at 1:30am.

Maybe after Daniel's list mail troubles subside, he can elaborate on his
methods which are much more detailed.

- Longden


<<I figured out how to copy all C: files to A: backup directory
automatically
on a recurring basis for appt.

Next question: How do I set up a recurring appointment to exit all open
apps
before the copy occurs?
>>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 08:53:04 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: DHCP and LXTCP
In-Reply-To:  <Pine.LNX.4.33.0203140728370.10441-100000@hal.technoir.nu>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Thu, 14 Mar 2002, Michael Kopplin wrote:

> So you're using dhcp.exe. I had thought about that, but what I
> was really asking about is DHCP support built into the wattcp
> component of LXTCP programs. I'll keep this in mind but I like
> the simplicity of built-in support if I can get it to work.

If you do, please let us know.

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 06:54:00 -0800
Reply-To:     Longden_Loo@CANDLE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Longden Loo <Longden_Loo@CANDLE.COM>
Subject:      Re: D&A ABC-LX and Kodak 1600mAH NiMH batteries
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

ABC/LX is limited to 1200mAH (probably the state of the technology when it
was written), and this had been discussed before when 1300mAH cells first
started appearing.  You just have to declare them as 1200mAH.

I don't know what others do with their setups, but I have 1600mAH NiMH
cells and just charge to a max of 2.84v, or stall at 6hr, or max of 16hrs.
My LX is usually plugged in at work all day (it's my calendar and
calculator after all) and I usually top the charge off whenever I feel like
it.  I'm probably not getting the maximum charge that I should, but who has
16+ hrs to spare in the day waiting for a battery to juice up anyway?  To
get a max charge, I probably should pull the cells and put them into my
nifty external Ray-O-Vac charger, but I dislike fumbling with the LX
battery door and the general nuisance of that process.

- Longden


<<
    I've just put a pair of 1600mAH Kodak "PhotoLife" NiMHs in my 700LX and
I'm having some trouble getting ABC-LX to let me enter the battery
capacity.
I can enter anything up to 1200mAH fine, but if I try and enter 1600,
ABC-LX
politely tells me to try again...

I know some D&A reps frequent HPLX-L, so can any of them (or anyone else
for
that matter) please tell me how to fix this so I can use my NiMHs? It would
be a great shame to have to use my old Uniross 700mAH NiCads again,
especially when I've got these NiMHs...
<<

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 07:57:13 -0700
Reply-To:     mike <kopplin@TECHNOIR.NU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         mike <kopplin@TECHNOIR.NU>
Subject:      Re: DHCP and LXTCP
In-Reply-To:  <200203141417.g2EEHxeN184728@mail.hiwaay.net>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Thu, 14 Mar 2002, Chris Lott wrote:
> > It looks like I'll have to start using DHCP at work. I've never
> > had to use it before so this is new to me. DHCP with WWW/LX
> > seems straightforward enough, using dhcp.exe from dasoft. The
> > LXTCP docs mention that DHCP is supported but undocumented.
> > Looking at the source, it seems all I need is "my_ip=dhcp" in
> > tcp.cfg. Is this correct?
>
> I thought you said "my_ip=bootp".  This works in other WATTCP
> based applications I run on DOS computers here at work.  As I
> understand it, dhcp is a superset of bootp.

I don't know if it's really a superset, or just that
implementations of dhcp include support for bootp for backwards
compatibility. The dhcp setup at my work will be not be
configured to answer bootp requests though.

In the wattcp source, when tcp.cfg is read, if my_ip= is
followed by a 'b' or a 'd' it turns on bootp support, thus my
assumption that "my_ip=dhcp" should work. I have tried this and
it didn't work, so I am trying to figure out if it is a problem
with lxtcp/wattcp or with the network. Only Win98+ is supported
at work so I'm on my own troubleshooting this.

Regards,
Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 10:03:19 -0500
Reply-To:     Bruce_Martin@MANULIFE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bruce Martin <Bruce_Martin@MANULIFE.COM>
Subject:      Re: Recurring command to save and close all open apps in LX100
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

> I figured out how to copy all C: files to A: backup directory
automatically
> on a recurring basis for appt.
>
> Next question: How do I set up a recurring appointment to exit all open
apps
> before the copy occurs?
>

To close all the palmtop's built-in apps via an Appointment, you could use
the built-in System Macro application to write a macro with a key sequence
that opens the AppMgr ("More Applications"), and presses [Menu],
[A]pplication, C[L]ose All. It should look something like this:
"(More)(Menu)al".

If, for example, you assign this macro to [F9], you can then launch the
macro via an Appointment with the Description "||9" and the Location "Q".

To make this happen before Appointments runs your backup batch, just set
this Start Time to a minute earlier. Remember that these operations are
executed in place of the alarm going off, which means they can happen
*before* the Appointment time if you have a Leadtime set.

Bruce in Toronto

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 16:27:15 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      delivery problems
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

okay, I'm getting messages again, but this is only because Mike was so
kind to set up an account for me on his machine, subscribed it to
HPLX-L and lets it forward the messages to me.

If it helps tracking down the problem:

The messages arrive although they are forwarded by him to my new email
address

palmtop at daniel-hertrich dot de, this one forwards to
daniel dot hertrich at gmx dot de and this one filters spam and forwards
list messages to
danielhertrich at compuserve dot de, where the messages finally appear.

So GMX and any anti-spam of filetering mechanis cannot be the problem.

I hope the real problem can be found soon, as I don't want to annoy
Mike longer than necessary with my problems.

Thanks, Mike!
I'll let you know when I get list message duplicates (because this will
mean that normal delivery works again).

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 07:33:33 -0800
Reply-To:     Joseph.Buford@HSC.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Joseph Buford <Joseph.Buford@HSC.COM>
Subject:      Re: Removing Icons under " More Applications"
Comments: To: Etienne Lemaire <etienne.lemaire@pandora.be>
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Etienne,

Thanks for the instructions. I will add them to my HPLX-Tips.gdb, then see
if I can make it work.

Joe

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 16:43:53 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Recurring command to save and close all open apps in LX100
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends

On Thu, 14 Mar 2002 06:42:55 -0800, Longden Loo <Longden_Loo@CANDLE.COM> wrote:

> Maybe after Daniel's list mail troubles subside, he can elaborate on his
> methods which are much more detailed.

Actually, it is all described on
http://www.daniel-hertrich.de/lxbackup

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 07:59:46 -0800
Reply-To:     Joseph.Buford@HSC.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Joseph Buford <Joseph.Buford@HSC.COM>
Subject:      Re: electric vehicle list?
Comments: To: Andrew <andrewaa@earthlink.net>
Comments: cc: ev@listproc.sjsu.edu
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Andrew,

No problem.

All the information on the EV list is located at
http://www.madkatz.com/ev/evlist.html

This is a busy and VERY informative list that can send out >100k of Emails
daily. It is also one of the most polite lists around . It compares very
favorably with the HP200lx list.

Joe




Andrew <andrewaa@earthlink.net> on 03/14/2002 06:06:47 AM

To:    joseph.e.buford@boeing.com, cpt_kludge@yahoo.com
cc:

Subject:  electric vehicle list?


Joseph
How are things at the lazy B ranch?
I'm interested in electric cars but not impressed by what seems to be
commercially available.
There's someone in town that is selling micro cars with a top speed of
35 mph which doesn't impress me. I'd like to trade range for speed, if I
could get 20 miles range at 50 mph I'd be happy.
I've about decided to build my own, there seem to be a number of
conversion kits for VW products.
Either that or try and find one of the Ford ranger electric pickups.
Could you send the EV list info?

Thanks
--
Andrew King
Ann Arbor Michigan
technology is the answer, what was the question?

I also am subscribed to an Electric Vehicle list that
usually has msg's >50K and I rarely have a problem rx
them.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 10:02:36 -0600
Reply-To:     John McCaskill <jmccask@POWERCHOKES.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John McCaskill <jmccask@POWERCHOKES.COM>
Subject:      Re: Recurring command to save and close all open apps in LX100
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
In-Reply-To:  <HPLX-L%2002031410423747@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I got an error at that address:
http://www.daniel-hertrich.de/lxbackup
error 404: Datei nicht gefunden!

However, it all seems to be explained pretty well at:
http://www.daniel-hertrich.de/backuplx/index.shtml

Thanks!!!

John

-----Original Message-----
From: HPLX Mailing List [mailto:HPLX-L@UConnVM.UConn.Edu]On Behalf Of
Daniel Hertrich
Sent: Thursday, March 14, 2002 8:44 AM
To: HPLX-L@UConnVM.UConn.Edu
Subject: Re: Recurring command to save and close all open apps in LX100


Hi friends

On Thu, 14 Mar 2002 06:42:55 -0800, Longden Loo <Longden_Loo@CANDLE.COM>
wrote:

> Maybe after Daniel's list mail troubles subside, he can elaborate on his
> methods which are much more detailed.

Actually, it is all described on
http://www.daniel-hertrich.de/lxbackup

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 17:17:19 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Recurring command to save and close all open apps in LX100
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Thu, 14 Mar 2002 10:02:36 -0600, "John McCaskill" <jmccask@powerchokes.com> wrote:

> I got an error at that address:
> http://www.daniel-hertrich.de/lxbackup
> error 404: Datei nicht gefunden!
>
> However, it all seems to be explained pretty well at:
> http://www.daniel-hertrich.de/backuplx/index.shtml

oops, sorry.
I mixed my own URL up with the name of the lx backup program on SUPER.
;-)

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 11:30:26 -0500
Reply-To:     Bob Penick <bnj@MYREALBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Penick <bnj@MYREALBOX.COM>
Subject:      Re: t2t drivers
Comments: To: Russel Brooks <rlbrooks@POBOX.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Russ,
I'm reading that your test shows your double speed to be almost twice as
SLOW?
I guess you got it backwards?
Or, did you end up with a rare half-speed crystal in your LX.  ;-)
bob

----- Original Message -----
From: "Russel Brooks"
Sent: Wednesday, March 13, 2002 7:51 PM
Subject: Re: t2t drivers


> Single speed was about 6 seconds.
> Double speed was about 10 seconds.
>
> Interesting the faster unit wasn't twice as fast.  (?)

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 09:59:51 -0700
Reply-To:     Michael Kopplin <kopplin@TECHNOIR.NU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Kopplin <kopplin@TECHNOIR.NU>
Subject:      Re: delivery problems
In-Reply-To:  <HPLX-L%2002031410260040@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Thu, 14 Mar 2002, Daniel Hertrich wrote:

> okay, I'm getting messages again, but this is only because Mike was so
> kind to set up an account for me on his machine, subscribed it to
> HPLX-L and lets it forward the messages to me.
>
> If it helps tracking down the problem:
>
> The messages arrive although they are forwarded by him to my new email
> address

They shouldn't be coming through as forwarded. I have configured
my mail server to relay email for a virtual address and rewrite
the envelope to your palmtop address. If you meant "forwarded"
as in an indirect route, yes, that is true.

> I hope the real problem can be found soon, as I don't want to annoy
> Mike longer than necessary with my problems.
>
> Thanks, Mike!
> I'll let you know when I get list message duplicates (because this will
> mean that normal delivery works again).

You're welcome, and it's no problem for me. It took 30 seconds
to set up, then a few minutes to figure out how to fool the
listserv into sending to a non-existent address since it sends
out a confirmation request. After that it takes no effort from
me, so it can stay setup as long as necessary.

But you are right that the problem should be found. A workaround
for you to get the list shouldn't be necessary.

Regards,
Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 12:18:18 -0500
Reply-To:     Eduardo Seudonimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudonimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: delivery problems
Comments: To: Michael Kopplin <kopplin@TECHNOIR.NU>
In-Reply-To:  <Pine.LNX.4.33.0203140946090.11121-100000@hal.technoir.nu>
MIME-Version: 1.0
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: quoted-printable

This sounds like it may be a networking problem. Perhaps Daniel's mail =
server and the list server simply cannot create a TCP connection?

> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@uconnvm.uconn.edu]On Behalf Of
> Michael Kopplin
> Sent: Thursday, March 14, 2002 12:00 PM
> To: HPLX-L@uconnvm.uconn.edu
> Subject: Re: delivery problems
>=20
>=20
> On Thu, 14 Mar 2002, Daniel Hertrich wrote:
>=20
> > okay, I'm getting messages again, but this is only because Mike was =
so
> > kind to set up an account for me on his machine, subscribed it to
> > HPLX-L and lets it forward the messages to me.
> >
> > If it helps tracking down the problem:
> >
> > The messages arrive although they are forwarded by him to my new =
email
> > address
>=20
> They shouldn't be coming through as forwarded. I have configured
> my mail server to relay email for a virtual address and rewrite
> the envelope to your palmtop address. If you meant "forwarded"
> as in an indirect route, yes, that is true.
>=20
> > I hope the real problem can be found soon, as I don't want to annoy
> > Mike longer than necessary with my problems.
> >
> > Thanks, Mike!
> > I'll let you know when I get list message duplicates (because this =
will
> > mean that normal delivery works again).
>=20
> You're welcome, and it's no problem for me. It took 30 seconds
> to set up, then a few minutes to figure out how to fool the
> listserv into sending to a non-existent address since it sends
> out a confirmation request. After that it takes no effort from
> me, so it can stay setup as long as necessary.
>=20
> But you are right that the problem should be found. A workaround
> for you to get the list shouldn't be necessary.
>=20
> Regards,
> Mike
>=20
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 18:08:31 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: t2t drivers *Correction*
Comments: To: Bob Penick <bnj@MYREALBOX.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Bob Penick wrote:
> I'm reading that your test shows your double speed to be almost twice as
> SLOW?
> I guess you got it backwards?
> Or, did you end up with a rare half-speed crystal in your LX.  ;-)
> bob

I think the half speed crystal is in my head.  :-)
Yeah, the timings are backward; so much for double checking
before hitting send.

The correct timing relationships are

  Single speed was about 10 seconds.
  Double speed was about  6 seconds.

Thanks for catching the error.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 20:43:33 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: 100LX to HP Jornada 568 conversion
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> Why don't they use a common file structure?

No, no, no, nooooo!
I do *not* want to be pressed into corsets just because Bill Gates finds it
convenient for virus purposes if everybodie's setup is exactly the same.
All I (and you) need, is a *documented* format, or ather one for each side.
A converter - and one accomodating every kinky kind of change you might
want to make to your adress book structure - is then a simple excercise in
BASIC or something.
From my database on the Atari (original or emulated on the games console) I
can write absolutely every format I know the specifications of. Haven't
been able to find something even near it on any other platform so far.

Just to give you a bit of the flavour:
To be able to cover all kinds of usage, I support three kinds of titles:
1) Dr. etc., put before the name or before the Chrisian name if present
2) von, de etc., part of the name but not to be sorted by
3) MP, Ph.D. etc., put after the name

The HP has just one field, name, which might hold the name of the company.
In that case the name might be put as Atn.Mr. J. Bloggs.

So that part of my export to HP reads:

IF LEN(fir$)<1
LET v01$=TRIM$(nam$+" "+ti3$)+", "+TRIM$(tit$+" "+TRIM$(vor$+" "+ti2$))
ELSE
LET v01$=fir$
ENDIF
'
IF zus$="z.Hd."
IF LEN(vor$)>0
LET v02$=LEFT$(vor$,1)+"."
ELSE
LET v02$=""
ENDIF
LET v02$=TRIM$(tit$+" "+TRIM$(v02$+" "+TRIM$(ti2$+" "+TRIM$(nam$+"
"+ti3$))))
IF INSTR(an2$,"Mr")>0
IF LEN(tit$)>0
LET v02$="Atn."+v02$
ELSE
LET v02$="Atn."+an2$+v02$
ENDIF
ELSE
IF an2$:"Frau"
LET v02$=zus$+"Fr. "+v02$
ELSE
LET v02$=zus$+"Hrn. "+v02$
ENDIF
ENDIF
ELSE
LET v02$=zus$
ENDIF
'
PRINT CHR$(34) v01$ CHR$(34) "," CHR$(34);
'
[phone number treatment omitted here]
'
PRINT v02$ CHR$(34) "," CHR$(34);
'

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 21:14:09 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: test
Comments: To: Sales@Systems-Consulting.com, Systems-Consulting
          <Sales@SYSTEMS-CONSULTING.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Paul

On Mon, 11 Mar 2002 11:04:12 -0500, Systems-Consulting <Sales@SYSTEMS-CONSULTING.COM> wrote:

> test
>
> Thanks,
>
> Paul Anderson, Pres, Systems-Consulting here since 1992

You're welcome. ;-)

Do you have problems receiving the list?
In case you haven't heard of it: Several German list members didn't get
any message for a few days, although most others didn't seem to have
any problem.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 09:15:16 +1300
Reply-To:     Roger Whitmarsh <lodger@NZ1.IBM.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Roger Whitmarsh <lodger@NZ1.IBM.COM>
Subject:      Software Carousel
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Hi Listers
I've never taken much notice of discussion of SC,
as I didn't think I'd ever need it, but now I find
I need to run a large application that takes max
memory, plus I need to refer to a database and
other LX applications.
Is SC what I need? Does it take much memory itself?
i.e. will it impact the memory requirements of the
big application?
Any other suggestions?

Cheers..Roger

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 15:31:37 -0500
Reply-To:     Bob Penick <bnj@MYREALBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Penick <bnj@MYREALBOX.COM>
Subject:      200lx System ROM differences
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I tested my single speed and double speed 200's and got approximately the
same times Russ did.  And then I noticed that the total byte count was
different on the two machines.  ????
Then I remembered that the single speed  I have is one of the earliest ones
released.  It's ROM is 1.00A  The double speed is 1.02A. (I think most of
the 200's out there are this version.)
Wondering about the differences, I did a "dir *.* /s>1x_rom.txt" on the
single and "dir *.* /s>2x_rom.txt" on the double.
started looking for the differences.  For whatever it is worth and for
whoever is interested, here they are:
Hope this displays OK.
In the 1.00A version all the directories in D: are dated 3/25/94 and in the
newer one they are dated 9/30/94

There are just 5 files that have any differences:
      CCMADE   EXM     50742 04-07-94   5:15p CCMADE   EXM     50742
05-23-94 3:13p

      MAZE     EXE     29669 02-17-94   9:34a
      MAZE     EXE     29779 05-06-94   9:11a

      CCMAIL   INI       781 06-07-93   3:46p CCMAIL   INI       781
05-06-94  12:09p

      CABUS    HLP     14323 03-08-94   3:10p CABUS    HLP     14323
05-26-94  11:14a
      QHPUS    HLP     52488 04-19-94   8:26p QHPUS    HLP     52488
09-22-94  11:40p


The only one that changed in file size is Maze.exe.  Wonder why that one
changed?
Does anyone out there have a ROM version 1.01A to see what differences that
are there?
What was the official release date of the 200lx?  I know it was before
9/30/94 because I purchased mine on 9/27/94..

In the Omnigo 700lx there are an extra 14 files and newer dates to many.
As I said, FWIW,
bob

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 21:54:47 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      HPLX Users Database (from "Around the world" thread)
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

thanks to the hard work of Bob Christopher, the HPLX users database is
now available for download.

This is a first version which is compiled from the "Around the world"
thread from January / February and from my former HPLX knowledge
database.

All list members are asked to do the following:

1. Download the ZIP file from
http://www.daniel-hertrich.de/hplxudb.zip
(no HTML page for it yet).

2. unzip it (you will need a password, I'll give this later)

3. Load the GDB file into the 200LX's database application,
scroll to your entry, if you are listed, and decide if it is okay.
Please consider especially if you would like to offer support to
others, if so, we will check the checkbox "offers support" of your
entry and add you skills profile (Category and comments).
Of course if you are not listed yet you are welcome to provide your
data!

3a. I have just added a new group of checkboxes, which should indicate
what kind of HPLX you use. All: please provide this information and
mail it to Bob!

4. If something should be changed, please write an email to Bob
(bob(at)palmtop.com). NOT TO ME, BOB IS THE MAINTAINER OF THE DATABASE!
If you want to be removed from the GDB, please
put "DO NOT LIST" into the subject. If something should be changed,
please put "HPLXUDB CHANGE" into the subject.
Don't forget to specify your name (how you are listed in the GDB) and
what should be changed.
To make it easier for Bob, please use the following form:

 Firstname Lastname:
        Corrections:
          LXs I use: [ ] 95LX  [ ] 100LX  [ ] 200LX
                     [ ] 700LX [ ] 1000CX [ ] others (Omnigo 100/120...)
 Offer Support? Y/N:
         Categories: (only from those already present in the GDB pls.)
             Skills:

If you want to be added to the "offers support" people, please provide
a skills profile related to the palmtop. See other "offers support"
entries as examples. You can press F6 (Subset) and choose the "offers
support" subset to get a list of all people who want to offer support.

The first entry in the database is a readme entry, just move the cursor
onto it and press F3 to read the README.

Well, I just wanted to make sure that you read everything carefully, so
I give you the unzip password now: It is hplxusers. Please also
consider that the database will publically downloadable, but always
scrambled with a password, so no Internet robots will grab any email
out of it for spamming. Your data is fairly safe.

We plan to make the final database available either on SUPER or on my
private homepage.

Bob is and will be the maintainer of the database.

Thanks

daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 21:58:30 +0100
Reply-To:     Laust Brock-Nannestad <laustbn@DIKU.DK>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Laust Brock-Nannestad <laustbn@DIKU.DK>
Subject:      Re: 200lx System ROM differences
In-Reply-To:  <017401c1cb97$3db7cb00$ae2d010a@penickrh40w>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Thu, 14 Mar 2002, Bob Penick wrote:

>       MAZE     EXE     29669 02-17-94   9:34a
>       MAZE     EXE     29779 05-06-94   9:11a
>
> The only one that changed in file size is Maze.exe.  Wonder why that one
> changed?

Perhaps it's compiled with a newer compiler or they fixed an obscure
bug? It would be fun to try and examine/compare the two files...


Regards,

Laust

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 15:53:49 -0700
Reply-To:     Michael Kopplin <kopplin@TECHNOIR.NU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Kopplin <kopplin@TECHNOIR.NU>
Subject:      Re: DHCP and LXTCP
In-Reply-To:  <Pine.OSF.4.33.0203140852040.13068-100000@worf.netins.net>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Thu, 14 Mar 2002, Theodore Heise wrote:
> On Thu, 14 Mar 2002, Michael Kopplin wrote:
> > So you're using dhcp.exe. I had thought about that, but what I
> > was really asking about is DHCP support built into the wattcp
> > component of LXTCP programs. I'll keep this in mind but I like
> > the simplicity of built-in support if I can get it to work.
>
> If you do, please let us know.

Works!! Turns out the problem was the DHCP server is configured
to verify mac addresses. Once my nics address was added it
worked fine.

WWW/LX works with dhcp.exe and ip-up.bat.

The LXTCP apps work with "my_ip=dhcp" in tcp.cfg.

Cheers,
Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 17:15:18 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: DHCP and LXTCP
In-Reply-To:  <Pine.LNX.4.33.0203141533040.12154-100000@hal.technoir.nu>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Thu, 14 Mar 2002, Michael Kopplin wrote:
>
> The LXTCP apps work with "my_ip=dhcp" in tcp.cfg.

Works here too--thanks for the info!

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 00:51:47 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: Software Carousel
Comments: To: Roger Whitmarsh <lodger@NZ1.IBM.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Roger Whitmarsh wrote:
> I've never taken much notice of discussion of SC,
> as I didn't think I'd ever need it, but now I find
> I need to run a large application that takes max
> memory, plus I need to refer to a database and
> other LX applications.
> Is SC what I need? Does it take much memory itself?
> i.e. will it impact the memory requirements of the
> big application?

My SC installation allows DOS sessions with 541,296 bytes of
memory; is that enough for your app?

SC's expense is a bit of memory (so you only have the 540k
above) and disk and/or EXM space to hold the paged out sessions.

I set aside 4M of T2T disk space for 255 TREMM 16k EXM pages
which is where I have SC swapping to (because it's faster that
way).

Is SC worth it?  YES!!!

It's a toss up whether SC or my 32M upgrade is more important.
(Either one is more important than the double speed upgrade.)

Cheers... Russ

200LX+T2T32M&2X+SC+WWW/LX+SecDev+FreeCell=Ideal Palmtop!

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 19:38:00 -0600
Reply-To:     Tim R <palmtop@N-LINK.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tim R <palmtop@N-LINK.COM>
Subject:      Re: Software Carousel
In-Reply-To:  <HPLX-L%2002031419504542@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

Hi Russel,

re:

On Fri, 15 Mar 2002, Russel Brooks wrote:
> I set aside 4M of T2T disk space for 255 TREMM 16k EXM pages
> which is where I have SC swapping to (because it's faster that
> way).

I may not be reading this correctly. Do you have these TREMM EXM pages
acting as a *big* "drive" for SC to hide its swap file, or are these LOTS
of little 16k pages that do something else?

--tim

PS. How do you make it work faster? <grin>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 03:52:58 +0000
Reply-To:     fjkaufman@WORLDNET.ATT.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "F. Kaufman" <fjkaufman@WORLDNET.ATT.NET>
Subject:      Re: One more test
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

> why don't I get ANY mail from the list???
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


As someone else mentioned, maybe your isp is applying some spam filter.
Since the hplist sends a series of messages, probably with the same
address, maybe your isp thinks it is redundant, spam and has started
rejecting it.

As you can see, your message has arrived so you can post to the list.
And your reply to Mike also made it to the list as did his initial
message to you (cc-ed to list).

I hope you figure it out - we do not want to lose you and your valuable
contributions.

Fred

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 00:23:01 -0500
Reply-To:     Keith Grider <k.grider@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Keith Grider <k.grider@EARTHLINK.NET>
Subject:      Re: DHCP and LXTCP
Comments: To: mike <kopplin@TECHNOIR.NU>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

This is a bit odd as Rod Whitby had incorporated it in the code fop some,
but not in all of the software he put together. This means that, yes, it
works with LXMTA, but does not work with LXtelnet (this still requires bootp
or a hard coded ip address). I find that some DHCP daemons are backwards
compatible with bootp (as bootp is a subset of DHCP). My SMC router here at
home is (maybe because it has an infinite lease). At work, I had to 'turn
on' bootp support with DHCPD on our linux server. It would be nice if
someone would 'fix' lxtelnet to have this feature. HINT HINT

I use lxtelnet in server mode to transfer files. It is fast, robust, and I
can use a graphical ftp program from my windows box to transfer files back
and forth via Ethernet instead of transfile over serial.

On a side note, has anyone ever gotten SMB to work with a win98 or win2k
network. I have spent unknown hours and tried BOTH of the suggestions on the
web and neither allow an SMB connection. I can either see the computer, but
cannot mount any shares or I cannot see any shares on the HP. If there is
anyone that does use this, please let us know.

KeithG
----- Original Message -----
From: "mike" <kopplin@TECHNOIR.NU>
Sent: Thursday, March 14, 2002 8:40 AM
Subject: DHCP and LXTCP


> Anyone using DHCP and LXTCP?
>
> It looks like I'll have to start using DHCP at work. I've never
> had to use it before so this is new to me. DHCP with WWW/LX
> seems straightforward enough, using dhcp.exe from dasoft. The
> LXTCP docs mention that DHCP is supported but undocumented.
> Looking at the source, it seems all I need is "my_ip=dhcp" in
> tcp.cfg. Is this correct?
>
> Regards,
> Mike
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 23:41:29 -0600
Reply-To:     Tim <palmtop@N-LINK.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tim <palmtop@N-LINK.COM>
Subject:      FLUFF: FA: More gadgets (one poss. of use <grin>).
In-Reply-To:  <HPLX-L%2002031419504542@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Hi all,

I had such luck w/ my last post, I thought I'd "do it again" ....

I've got a lot up for sale on eBay (mostly lenses), BUT am selling a "Flip
Disk" PCMCIA HDD.

I *NEVER* got it to work w/ an LX (I don't remember trying and don't want to
break anything now). It might be poss. *WITH* the right drivers; but I doubt
it ... It *can* be externally powered, so a talented LXer might be able to
make it work. But, it's prob. more for the folks who have an LX *and* a
laptop.

It's at:

http://cgi.ebay.com/ws/eBayISAPI.dll?ViewItem&item=2010011617

The "See All my Auctions" link at the bottom of that page will show you the
rest (including a Sony Clie). A straight link to "all my auctions" would be
too darn long.

Thanks for indulging me w/ the list space!

--tim

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 23:49:07 -0600
Reply-To:     Tim <palmtop@N-LINK.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tim <palmtop@N-LINK.COM>
Subject:      FS: KeyMate and Mini-Keyboard - "Take 2"
In-Reply-To:  <HPLX-L%2002031419504542@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I've "slept on" my idea for selling my KeyMate and Mini-Keyboard and think I
overpriced the keyboard.

I'd still like to sell it at the same time (the gear w/o the shipping is
only $95).


KeyMate -   58
Keyboard -  37
Shipping -   8
Total    - 102

(I'll use slow FEDEX for that shipping rate, IN the Continental U.S. ... We
can work something out, if you're outside CONUS).

The KB is a super-low power consumption, mini- KB, about 2/3 the size of a
regular KB. I can re-send the specs. to anyone who missed the first post.

TIA,

--tim

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 05:53:34 +0000
Reply-To:     fjkaufman@WORLDNET.ATT.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "F. Kaufman" <fjkaufman@WORLDNET.ATT.NET>
Subject:      Fluff: Conclusions
Comments: To: Nathalie Bugeaud <tps-seti@WANADOO.FR>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

> (E) Conclusion: Eat & drink what you like. It's speaking English that kills
> you. :)

GGGGGGGGG - thanks for a good chuckle.

> nat (in the process of fixing her bike to prevent having to drink red wine)

I just discovered last week that the top tube on my custom bike cracked
- from rust. (sigh) - which is why the chuckle helps with that pain!

I'm in the process of getting a new bike frame and drinking Port in the
mean time.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 14 Mar 2002 22:55:09 -0700
Reply-To:     Michael Kopplin <kopplin@TECHNOIR.NU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Kopplin <kopplin@TECHNOIR.NU>
Subject:      Re: DHCP and LXTCP
In-Reply-To:  <00f201c1cbe1$7a500830$2802a8c0@keith>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Fri, 15 Mar 2002, Keith Grider wrote:

> This is a bit odd as Rod Whitby had incorporated it in the code fop some,
> but not in all of the software he put together. This means that, yes, it

I posted in a followup that I had gotten it working, I just
needed to have my mac address added to the dhcp configuration
files.

> works with LXMTA, but does not work with LXtelnet (this still requires bootp
> or a hard coded ip address). I find that some DHCP daemons are backwards
> compatible with bootp (as bootp is a subset of DHCP). My SMC router here at
> home is (maybe because it has an infinite lease). At work, I had to 'turn
> on' bootp support with DHCPD on our linux server. It would be nice if
> someone would 'fix' lxtelnet to have this feature. HINT HINT

Yes, lxtelnet uses cutcp, the other lxtcp apps use wattcp. I
guess only wattcp has been updated to support dhcp.

Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 12:37:47 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      HPLXUDB
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

I have got some requests for the password for the HPLX users database.
;-)

For those who did NOT find it in my original posting: Please read it
once more (carefully!). And here the password goes once more:

hplxusers

For those who have problems unzipping the GDB, please use PKZIP /
PKUNZIP 2.04g and use the -s option.

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 12:31:40 +0100
Reply-To:     xmarc@free.fr
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marc BERLIOUX <xmarc@FREE.FR>
Subject:      Re: 100LX to HP Jornada 568 conversion
In-Reply-To:  <3C90FD65.9A84C506@NexGo.De>
Content-Type: text/plain; charset="iso-8859-1"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit

Le Jeudi 14 Mars 2002 20:43, Axel Berger a icrit :
> > Why don't they use a common file structure?
>
> No, no, no, nooooo!
> I do *not* want to be pressed into corsets just because Bill Gates
> finds it convenient for virus purposes if everybodie's setup is
> exactly the same. All I (and you) need, is a *documented* format,

i agree with you : All we need, is a *documented* format
but it's not always that simple.

Exemple :
It's now about 15 years i use computers. I've written documents in
formats .doc(MS word) .wps(MSworks) .cwk(Claris works) .sdw(Star
Office)....

I now use Linux and Star Office.

When i want to re-open old documents with Star Office, i can only
open .doc documents, but not Works and Claris documents.
If i send a document to someone using MS Word, i can't send him a
.sdw (Star Office) document.

I found that one of the common file format to all these
word-processors is RTF format. So when i create a new document i save
it also in .rtf format. If i change my mind next year and want to use
again Word i'll be able to reopen my jobs without re-installing a
word-processor (and sometimes the operating system)

For address-books, the problem is worst. I use HP95LX phone book, kab
(the KDE address-book), i have used outlook express, netscape. I
still use sometimes Pegasus Mail. There is no common file format you
can use between all these programs. The most common (and text-based)
are .LDIF and .CSV

If i could find a common file format to all those adress-books, i
will use it, do believe me...even if it's Bill Gates who creates it
!!!

My advice :
for text documents use .RTF or .HTML or plain text
for printable documents(not to be modified) use .PDF
for adress-books .LDIF or .CSV

Axel, if you don't like Bill Gates, why use Windows 98 ? ;o)

@+
--
Marc BERLIOUX
Win98 is called Win98 because after the system crashed 98 times, you
have to reinstall.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 12:51:13 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      HPLX Users Database (2nd time)
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

grrrrr - I have received about 10 password requests by now!
I post my original message once more. PLEASE READ IT CAREFULLY, then
you will also know the password for the HPLX users database full of
"hplxusers". !! ;-)

It was my intention to give the password LATE in that message, because I
wanted you all to read through the ENTIRE message. From the beginning
to the end. Because it is important. Okay?


========================= ORIGINAL MESSAGE =====================

Hi friends,

thanks to the hard work of Bob Christopher, the HPLX users database is
now available for download.

This is a first version which is compiled from the "Around the world"
thread from January / February and from my former HPLX knowledge
database.

All list members are asked to do the following:

1. Download the ZIP file from
http://www.daniel-hertrich.de/hplxudb.zip
(no HTML page for it yet).

2. unzip it (you will need a password, I'll give this later)

3. Load the GDB file into the 200LX's database application,
scroll to your entry, if you are listed, and decide if it is okay.
Please consider especially if you would like to offer support to
others, if so, we will check the checkbox "offers support" of your
entry and add you skills profile (Category and comments).
Of course if you are not listed yet you are welcome to provide your
data!

3a. I have just added a new group of checkboxes, which should indicate
what kind of HPLX you use. All: please provide this information and
mail it to Bob!

4. If something should be changed, please write an email to Bob
(bob(at)palmtop.com). NOT TO ME, BOB IS THE MAINTAINER OF THE DATABASE!
If you want to be removed from the GDB, please
put "DO NOT LIST" into the subject. If something should be changed,
please put "HPLXUDB CHANGE" into the subject.
Don't forget to specify your name (how you are listed in the GDB) and
what should be changed.
To make it easier for Bob, please use the following form:

 Firstname Lastname:
        Corrections:
          LXs I use: [ ] 95LX  [ ] 100LX  [ ] 200LX
                     [ ] 700LX [ ] 1000CX [ ] others (Omnigo 100/120...)
 Offer Support? Y/N:
         Categories: (only from those already present in the GDB pls.)
             Skills:

If you want to be added to the "offers support" people, please provide
a skills profile related to the palmtop. See other "offers support"
entries as examples. You can press F6 (Subset) and choose the "offers
support" subset to get a list of all people who want to offer support.

The first entry in the database is a readme entry, just move the cursor
onto it and press F3 to read the README.


>>>> (ATTENTION, NOW COMES THE IMPORTANT PARAGRAPH:) <<<<

Well, I just wanted to make sure that you read everything carefully, so
I give you the unzip password now: It is hplxusers. Please also
consider that the database will publically downloadable, but always
scrambled with a password, so no Internet robots will grab any email
out of it for spamming. Your data is fairly safe.

We plan to make the final database available either on SUPER or on my
private homepage.

Bob is and will be the maintainer of the database.

Thanks

daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 13:03:17 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Fluff: Spamfilter
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> Remote host said: 552 Message identified as spam....
> Return-Path: <cpt_kludge@yahoo.com>

Bad scheme: That tells the spammers "This is a valid and read address - try
again." which is not what I want them to get.

My main address's <Axel_Berger@Su2.Maus.De> BBS sysop offers filtering and
keeps filtered mail for about two days. And FWIW, yahoo.com is in that
filter too, try a reputable provider. I regularly scan the filter log with
<Ctrl><F> "subject:" and sometimes have to ask him for stuff but rarely.
This address is not filtered, which is why I will not and cannot ever use
it in newsgroups.

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 13:15:41 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: D&A ABC-LX and Kodak 1600mAH NiMH batteries
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> I can enter anything up to 1200mAH fine, but if I try and enter
> 1600, ABC-LX politely tells me to try again...

Don't worry about that, the capacity is only used to generate sensible
starting values anyway. After starting <Shift><F2> (auto-something) and
while it is already charging you can adjust them with <F2>. So just give it
a couple of tries with 600, 900, 1200 mAh and you'll have an idea, what
ABC-LX would consider sensible for 1600 mAh.
BTW I have found my ca. 900 mAh NiMH (as measured in another charger) a bit
difficult. They do not give any very clear indication of when they are full
and spend over two hours at a level several steps below the top one - and
that with them being far more sensitive to overcharging than NiCd are.

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 06:54:05 -0600
Reply-To:     TomSalwasser@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tom Salwasser <TomSalwasser@COMPUSERVE.COM>
Subject:      Re: Fluff: Spamfilter
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I'm using www.mailwasher.net. It bounces mail as having an invalid email
address. I don't know if it will reduce my spam but it makes me feel good when I
bounce an email!

Regards,
Tom Salwasser


>
> > Remote host said: 552 Message identified as spam....
> > Return-Path: <cpt_kludge@yahoo.com>
>
> Bad scheme: That tells the spammers "This is a valid and read address - try
> again." which is not what I want them to get.
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 15:39:18 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: Software Carousel
Comments: To: Tim R <palmtop@N-LINK.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Tim R wrote:
> On Fri, 15 Mar 2002, Russel Brooks wrote:
> > I set aside 4M of T2T disk space for 255 TREMM 16k EXM pages
> > which is where I have SC swapping to (because it's faster that
> > way).
>
> I may not be reading this correctly. Do you have these TREMM EXM pages
> acting as a *big* "drive" for SC to hide its swap file, or are these LOTS
> of little 16k pages that do something else?

No, I tell SC to swap to Expanded memory instead of a drive
specification.

Yes, it still ends up in that 4m TREMM space carved out of my C:
drive but the EMS driver is a bit faster than going thru DOS to
a swap space on the same drive.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 11:59:05 -0500
Reply-To:     Eduardo Seudonimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudonimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: Software Carousel
Comments: To: Roger Whitmarsh <lodger@NZ1.IBM.COM>
In-Reply-To:  <OFD7CF1B31.8A60199E-ONCC256B7C.006EB7F0@nz.ibm.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: quoted-printable

I used to use DosShell before I got software carousel. It works pretty =
well except for messing up graphics modes on PAL apps and appmgr when =
switching. It also swaps a whole lot slower than SC and may have a =
larger memory footprint but it still may be worthwhile given the cost =
(free). I would suggest you try dosshell first and then plunk down $ =
if/when you decide it sucks.

BTW: SC messes up graphics modes in app manager too but there's a little =
LX-specific trick built into it to circumvent it.



> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@uconnvm.uconn.edu]On Behalf Of
> Roger Whitmarsh
> Sent: Thursday, March 14, 2002 3:15 PM
> To: HPLX-L@uconnvm.uconn.edu
> Subject: Software Carousel
>=20
>=20
> Hi Listers
> I've never taken much notice of discussion of SC,
> as I didn't think I'd ever need it, but now I find
> I need to run a large application that takes max
> memory, plus I need to refer to a database and
> other LX applications.
> Is SC what I need? Does it take much memory itself?
> i.e. will it impact the memory requirements of the
> big application?
> Any other suggestions?
>=20
> Cheers..Roger
>=20
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 09:13:51 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: delivery problems
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Thu, 14 Mar 2002 16:27:15 +0200, Daniel Hertrich <daniel.hertrich@GMX.DE> wrote:

[snip]

> If it helps tracking down the problem:
>
> The messages arrive although they are forwarded by him to my new email
> address
>
> palmtop at daniel-hertrich dot de, this one forwards to
> daniel dot hertrich at gmx dot de and this one filters spam and forwards
> list messages to
> danielhertrich at compuserve dot de, where the messages finally appear.

Have you always used a "-" in your mailname? If that is new it
may be the problem. I have a - in my company domain and found
some Web sites that insisted that was an illegal character.

Or else, the listserver doesn't understand "at" and "dot".
Perhaps you should use "@" and "."?  <G>

Vic Roberts

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 20:11:49 -0000
Reply-To:     "Richard E. McEvoy" <remce@GOFREE.INDIGO.IE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Richard E. McEvoy" <remce@GOFREE.INDIGO.IE>
Subject:      Re: PLEASE EMAIL ME PRIVATELY
Comments: cc: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I got no mail from the list for three days. They resumed yesterday 14th.

Richard



----- Original Message -----
From: "Daniel Hertrich" <daniel.hertrich@GMX.DE>
Subject: PLEASE EMAIL ME PRIVATELY


> Hi friends,
>
> it seems that I have problems to get list emails. No list email since
> about 24h now, but Al Kind says the list server is okay.
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 20:40:51 -0000
Reply-To:     "Richard E. McEvoy" <remce@GOFREE.INDIGO.IE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Richard E. McEvoy" <remce@GOFREE.INDIGO.IE>
Subject:      Re: PLEASE EMAIL ME PRIVATELY
Comments: cc: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I got no mail from the list for three days. They resumed yesterday 14th.I
got 88 today.



Richard



----- Original Message -----
From: "Daniel Hertrich" <daniel.hertrich@GMX.DE>
Subject: PLEASE EMAIL ME PRIVATELY


> Hi friends,
>
> it seems that I have problems to get list emails. No list email since
> about 24h now, but Al Kind says the list server is okay.
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 15:21:18 -0600
Reply-To:     Tim Kelley <tpkelley@HOTMAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tim Kelley <tpkelley@HOTMAIL.COM>
Subject:      To Do's
Mime-Version: 1.0
Content-Type: text/plain; format=flowed

I am trying to find out how to display the to do's that have already been
checked off.  Is there anyway to do that?  Thanks.

Tim K



_________________________________________________________________
Send and receive Hotmail on your mobile device: http://mobile.msn.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 12:03:04 +1300
Reply-To:     Tony Kan <tony.kan@CLEAR.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Kan <tony.kan@CLEAR.NET.NZ>
Subject:      Re: To Do's
Comments: To: tpkelley@HOTMAIL.COM
MIME-version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding:  7bit

Presumably you are talking about the Appt application.  I thought the tasks
are just at the bottom of your list with a tick next to them...

> Date: Sat 16-Mar-2002 10:21
> To: HPLX-L@UConnVM.UConn.Edu (Tony Kan)
> From: tpkelley@HOTMAIL.COM (Tim Kelley)
> Subject: To Do's
>
> I am trying to find out how to display the to do's that have already
> been checked off.  Is there anyway to do that?  Thanks.
>
> Tim K
>
> _________________________________________________________________
> Send and receive Hotmail on your mobile device: http://mobile.msn.com
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 15 Mar 2002 17:10:48 -0600
Reply-To:     Tim Kelley <tpkelley@HOTMAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tim Kelley <tpkelley@HOTMAIL.COM>
Subject:      Re: To Do's
Comments: To: tony.kan@clear.net.nz
Mime-Version: 1.0
Content-Type: text/plain; format=flowed

Ok, it appears that you have to go from day to day to see the completed
items.  I was thinking that there might be a way to see all the tasks that
were accomplished in one fell swoop.
Yes I was talking about the appointment book.
Tim


>From: Tony Kan <tony.kan@clear.net.nz>
>To: tpkelley@HOTMAIL.COM, HPLX-L@UConnVM.UConn.Edu
>Subject: RE: To Do's
>Date: Sat, 16 Mar 2002 12:03:04 +1300
>
>Presumably you are talking about the Appt application.  I thought the tasks
>are just at the bottom of your list with a tick next to them...
>
> > Date: Sat 16-Mar-2002 10:21
> > To: HPLX-L@UConnVM.UConn.Edu (Tony Kan)
> > From: tpkelley@HOTMAIL.COM (Tim Kelley)
> > Subject: To Do's
> >
> > I am trying to find out how to display the to do's that have already
> > been checked off.  Is there anyway to do that?  Thanks.
> >
> > Tim K
> >
> > _________________________________________________________________
> > Send and receive Hotmail on your mobile device: http://mobile.msn.com
> >
> > ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
><< winmail.dat >>




_________________________________________________________________
Send and receive Hotmail on your mobile device: http://mobile.msn.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 06:11:22 +0100
Reply-To:     Nathalie Bugeaud <tps-seti@WANADOO.FR>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nathalie Bugeaud <tps-seti@WANADOO.FR>
Subject:      more tips for my XTGOLD users
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

1. tip:
use the "." key on the numeric side to switch between logged drives; on the
desktop version it is the  "<" and ">" key

2. tip:
tried automatic scrolling in "V" [view] mode? it supports 5 speeds and 3 LX
fonts!

Nathalie [ER and XTG specialist]

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 08:20:49 +0100
Reply-To:     "Helmuth E. Guenther" <h_e_guenther@ATTGLOBAL.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Helmuth E. Guenther" <h_e_guenther@ATTGLOBAL.NET>
Subject:      Re: more tips for my XTGOLD users
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Nathalie,

it is always a pleasure reading your tips. I use XTREE since version 1,
which I got in the eighties and later XTG. I also got a windows
version, which I unfortunately lost.

What do mean with "it supports 3 LX fonts"? Does this support automatic
wrap?

> 1. tip:
> use the "." key on the numeric side to switch between logged drives; on the
> desktop version it is the  "<" and ">" key
>
> 2. tip:
> tried automatic scrolling in "V" [view] mode? it supports 5 speeds and 3 LX
> fonts!
>
> Nathalie [ER and XTG specialist]
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 21:30:11 +1300
Reply-To:     Tony Hutchins <th@PARADISE.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Hutchins <th@PARADISE.NET.NZ>
Subject:      Re: ANN: CLOCKS
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Sat, 16 Mar 2002 13:12:24 +1300 (NZDT)

CLOCKS V4.3 is at:

http://homepages.paradise.net.nz/th/

A System Macro is provided to launch CLOCKS showing the clocks
for the "Custom Cities" subset in the palmtop WorldTime
database.

- Tony

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 09:36:32 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: To Do's
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Tim

On Fri, 15 Mar 2002 17:10:48 -0600, Tim Kelley <tpkelley@HOTMAIL.COM> wrote:

> Ok, it appears that you have to go from day to day to see the completed
> items.  I was thinking that there might be a way to see all the tasks that
> were accomplished in one fell swoop.
> Yes I was talking about the appointment book.
> Tim

PIM/PE makes all such things possible.

For your specific problem, you would have to go into PE, loading your
PIM file, press Ctrl-C, enter "+!" into the appearing mask, and you
would see all checked off items.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 09:36:38 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      To Jessica: SUPER95
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Sorry, folks, for the bandwidth.
I'm looking for Jessica Leah Lang (sorry if I misspelled your name).

Please contact me privately. I have a question about the maintenance of
the 95LX section of SUPER. David told me you are responsible now.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 12:47:10 +0200
Reply-To:     Nigel R <nigel@KEEPSMILING.CO.ZA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nigel R <nigel@KEEPSMILING.CO.ZA>
Organization: STRATEGIC ALLIANCE CONSULTING
Subject:      Re: HPLX Users Database (from "Around the world" thread)
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Howdy :-)

Errr, how can user only having access to a HP95LX access the data in GDB
format?  Is there a desk PC application we can use?  Did the idea of a PBK
or 1-2-3 format get abandoned?

All the best

Nigel R in sunny South Africa

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 13:28:31 +0100
Reply-To:     Josef Meyer <meyerjos@BLUEWIN.CH>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Josef Meyer <meyerjos@BLUEWIN.CH>
Subject:      Clocks
Comments: To: th@paradise.net.nz
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Tony,

I have installed clocks on my HPLX and I enjoy it very much. Much more
visible than the sysmgr program WORLD.

I have one remark: DST for Europe is LMLO (i.e. from last weekend in
march to last weekend in october), same as for Munich. You put a
different value to the example clock.cfg. For London I don't know if it
is the same, but according to WORLD it is LMLO as well.

Maybe the english (or scottish, ...) list members can confirm this?

Josef Meyer

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 19:58:17 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: HPLX Users Database (from "Around the world" thread)
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

yes .. there is a program (probably GDB4WIN)
for running under win9x and above to read
data in gdb format .. on the desktop ..
probably there on super or palmtop.net

if you don't find it there .. i have it somewhere
on my 6/7 hard disks .. (where is alladin's genie
so that he can 'one' day synchronise them all ?)

..pk


-----Original Message-----
From: Nigel R <nigel@KEEPSMILING.CO.ZA>
Date: Saturday, March 16, 2002 4:21 PM


>Errr, how can user only having access to a HP95LX access the data in GDB
>format?  Is there a desk PC application we can use?  Did the idea of a PBK
>or 1-2-3 format get abandoned?

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 07:38:08 -0700
Reply-To:     "Robert K. Meyer" <bmeyer@UNION-TEL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Robert K. Meyer" <bmeyer@UNION-TEL.COM>
Subject:      Running llrawin.exe Under Win 95
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Can it be done? In the Connectivity Pack there is
llrawin.exe (not llrawin.bat as created in some posts). I've
been searching the archives and Jorgen and cannot find how
to execute this program.

Does llrawin.exe only work in Win 3.1?

Are the previously posted batch solutions the only solution
in Win 95?

Bob
--
R.K. Meyer MSEE K7PPC bmeyer@union-tel.com Elk Mountain WY
http://w3.union-tel.com/~bmeyer/   His name...  Isaiah 9:6

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 09:16:28 -0800
Reply-To:     Joseph.Buford@HSC.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Joseph Buford <Joseph.Buford@HSC.COM>
Subject:      Re: Removing Icons under " More Applications"
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Owen,

Thanks for the links.

Joe

Reply to:
-----------------------------------------------------------------------------------------------------------------------------------
Date:    Thu, 14 Mar 2002 04:11:41 -0500
From:    Owen Samuelson <owensamuelson@COX.NET>
Subject: Re: Removing Icons under " More Applications"

See if this will help. http://www.palmtoppaper.com/ptphtml/45/45c00010.htm
And this: http://www.palmtoppaper.com/ptphtml/45/45c00011.htm
Best Regards,
Owen

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 18:44:31 +0100
Reply-To:     Tamas Feher <etomcat@FREEMAIL.HU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tamas Feher <etomcat@FREEMAIL.HU>
Subject:      From Japan: a serial to RS232 controller!?
MIME-Version: 1.0
Content-type: text/plain; charset=US-ASCII
Content-transfer-encoding: 7BIT

Hello all,

This looks like an RS-232 to Ethernet adapter, I guess it would be
nice for use with HPLX having a flashcard in its PCMCIA slot.

<http://elm-chan.org/tmp/avrea.jpeg>

(Note: above link does end in AVREA.JPEG, not .JPG as usual)

Sincerely: Tamas Feher.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 18:58:11 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Fwd: ANN: New version of PocketDOS available
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

From comp.sys.palmtops.
XT-CE will be discontinued.

--- begin of forwarded message ---

From: pocketdos@yahoo.co.uk (PocketDOS)
Subject: ANN: New version of PocketDOS available
Date: 13 Mar 2002 20:24:17 -0800

Q: What is PocketDOS?
A: PocketDOS is an MS-DOS 6.22 compatible DOS for your Microsoft Windows
CE or Psion/Symbian EPOC32 based Pocket Computer. In addition to a full
DOS, PocketDOS lets you install and run many DOS programs* on your
Pocket Computer. PocketDOS also lets you access devices such as
touchscreens, built-in and external modems, IR ports, flash disks,
network drives, printers and more from within DOS and DOS programs.
(* Intel 8086/80186 compatible using CGA, HP-LX or text display modes)

Q: What is new in this version?
A: This version:
- Superscedes XT-CE, which is now included in PocketDOS
- Adds a Windows CE file system driver to allow direct access to
  hard disk devices from DOS (eg. CompactFlash)
- Adds utilities to registered version to format and scan hard
  disk devices (eg. CompactFlash) for errors
- Adds support for Pocket PC devices that use a "landscape" mode
  display driver
- Adds facility to zoom display to a particular text size (eg.
  20x8) for industrial applications designed to run on non-
  standard DOS handhelds
- Adds PC speaker emulation
- Improved CPU performance (especially on ARM processors)
- Fixed bugs in CPU emulation which caused incompatibilities with
  PKUNZIP

Q: Which devices are compatible with PocketDOS?
A: All Windows CE (1.0 and later) and Pocket PC devices (including
Pocket PC 2002), in the Palm-sized, Pocket PC, Handheld PC, Handheld
PC Professional and Handheld PC 2000 formats with Hitachi SH3 or SH4,
MIPS-compatible, ARM and StrongARM processors.

Q: Where can I download a demo copy?
A: http://www.pocketdos.com

Q: What does PocketDOS cost?
A: PocketDOS costs 40USD which includes a license to Datalight's
ROM-DOS operating system.

Registered PocketDOS users will be sent an email detailing how to
upgrade (for free) to the latest version of PocketDOS.

Registered XT-CE users will be sent an email detailing how to upgrade
(for free) to the latest version of PocketDOS. XT-CE users will need
to continue using their existing DOS as they are not licensed to use
Datalight's ROM-DOS operating system.

Any queries should be addressed to:
demo "at" pocketdos.com
--
PocketDOS - An MS-DOS 6.22 compatible DOS for your Pocket Computer.
http://www.pocketdos.com
--- end of forwarded message ---

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 09:27:09 +1200
Reply-To:     Tony Hutchins <th@PARADISE.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
Comments:     RFC822 error: <W> Incorrect or incomplete address field found and
              ignored.
From:         Tony Hutchins <th@PARADISE.NET.NZ>
Subject:      Re: Clocks
Comments: To: Josef Meyer <meyerjos@bluewin.ch>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Sun, 17 Mar 2002 08:06:10 +1200 (NZT)

07h37m39s ago ...
On Sat, 16 Mar 2002 13:28:31 +0100 (added, Josef Meyer wrote:

> Tony,
>
> I have installed clocks on my HPLX and I enjoy it very
> much. Much more visible than the sysmgr program WORLD.

Thanks for your comments Jodef! What is WORLD? Is it
WORLD.EXM? I haven't seen that one.

> I have one remark: DST for Europe is LMLO (i.e. from last weekend in
> march to last weekend in october), same as for Munich. You put a
> different value to the example clock.cfg. For London I don't know if it
> is the same, but according to WORLD it is LMLO as well.

Thanks - I sure got that wrong - according to
www.worldtimezone.com/daylight.html nobody uses the LMFS that
I put in!! Probably nobody ever did either<G>.

The DST built in to CLOCKS is a bit simplified. But now CLOCKS
can interface with WorldTime, this is not such a problem, as
TIMEZONE.DAT can be adjusted from year to year.

Ah, I see, if D:\_SYS\TIMEZONE.DAT is copied to C:\_DAT then
new entries can be added and WorldTime picks them up! Hmm,
maybe I should use that TIMEZONE.DAT format for CLOCKS, even
when it runs standalone. Yup, especially as the DST can change
from year to year - we don't want to be changing them in too
many places.

Today it is "3M", the 3rd Sunday in March, and we have just
gone off Summer Time. Timely topic! :)

- Tony

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 16:05:03 -0800
Reply-To:     Joseph.Buford@HSC.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Joseph Buford <Joseph.Buford@HSC.COM>
Subject:      Fluff: Conclusions
Comments: cc: Nathalie Bugeaud <tps-seti@wanadoo.fr>
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Nathalie,

>Eat & drink what you like. It's speaking English that kills
you. :)

Perhaps I should learn french :-)

Joe

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 06:03:41 +0100
Reply-To:     Nathalie Bugeaud <tps-seti@WANADOO.FR>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nathalie Bugeaud <tps-seti@WANADOO.FR>
Subject:      Subject: HPLXUDB
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Daniel:
 >For those who have problems unzipping the GDB, please use PKZIP
 >/ PKUNZIP 2.04g and use the -s option.

ver. 2.04g seems the most commonly used one - it is also the one used for
XTGOLD v.3 which applies its excellent viewer program to zipped files
without extracting them.

personally i have never had problems, corrupt files etc, even if the zip
files contain 1000s of files and are as large as 500kb

what is the largest zip file ever created on the LX?

Nathalie, who is waiting for Norbert Giese to return my improved
MY-MONEY.WK1 to send to Leo at Fermilab

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 00:11:30 -0500
Reply-To:     John Alley <chia@ICX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John Alley <chia@ICX.NET>
Subject:      Re: XTREE Gold!!!??? Help!!!
In-Reply-To:  <20020317050127.EFFE683.fl-mta02@UConnVM.UConn.Edu>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

At 12:00 AM 3/17/2002 -0500, you wrote:

>it is always a pleasure reading your tips. I use XTREE since version 1,
>which I got in the eighties and later XTG. I also got a windows
>version, which I unfortunately lost.

         Wow... I forgot all about that software... what a blast from the
past... I Was soo mad when they quit supporting it or couldn't find it
again!! Wow.. the last one I had had support for compressed files as
well.... wow... that was great!! Now my next question.... where in the
world can I get a copy of it.. without trying to recover it off of this old
386 computer buried in a closet.....??? PLEASE help!!!

73 de KF4UAE
www.qsl.net/kf4uae
John R. Alley
kf4uae@arrl.net

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 16 Mar 2002 23:44:09 -0600
Reply-To:     Orin Keplinger <orink@IX.NETCOM.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Orin Keplinger <orink@IX.NETCOM.COM>
Subject:      Re: XTREE Gold!!!??? Help!!!
Comments: To: John Alley <chia@ICX.NET>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

John:

Have you tried Ztree? I believe that came out two or three years
ago. It was long filename compatible and written by someone who
was responding to the mass longing for an updated Xtree.

Links should pop up on a search for ztree windows.

As Ever,
Orin Keplinger
near Chicago
E) orink@ix.netcom.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 00:51:36 -0600
Reply-To:     Tim <palmtop@N-LINK.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tim <palmtop@N-LINK.COM>
Subject:      Re: Software Carousel
In-Reply-To:  <BMEDJPEHPGEIFEKEBFNOEELCCAAA.ohdamnthathurts@yahoo.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="US-ASCII"
Content-Transfer-Encoding: 7bit

I have an "odd" issue, w/ Software Carousel... Dunno if I should start a new
thread or not....

Whenever I have SC (actually Super SC7) running and the palmtop goes through
an auto shut-off to save power and I turn it on, it adds characters to some
text fields. This is most notable If I'm in the note field of a phone book
entry. I turn it back on and usually get an asterisk added to the text in
the note field.

What causes this?

It doesn't add characters to everything, and it sometimes adds two chars.
instead of one. I have the "typical" setup (pretty much default), running
SSC7, Buddy in the main session and the Andrew font set. It happens with a
DS and single speed (unmodified) LX; so it's not an issue w/ the DS or
memory expansion drivers...

Anyone else experience this? Since it doesn't always happen, it's hard to
troubleshoot, AND (on reflection) I think it only happens when the palmtop

Thanks,

--tim

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 11:43:10 +0100
Reply-To:     xmarc@free.fr
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marc BERLIOUX <xmarc@FREE.FR>
Subject:      Re: HPLX Users Database (from "Around the world" thread)
In-Reply-To:  <005401c1ccd8$1dc470e0$c35cef9b@co.za>
Content-Type: text/plain; charset="iso-8859-1"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit

Le Samedi 16 Mars 2002 11:47, Nigel R a icrit :
> Howdy :-)
>
> Errr, how can user only having access to a HP95LX access the data
> in GDB format?  Is there a desk PC application we can use?  Did the
> idea of a PBK or 1-2-3 format get abandoned?
>

At least could someone export the .gdb file in something
human-readable ?

--
Marc BERLIOUX
"Who is this General Failure and what is he doing in my PC ?"

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 12:38:34 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: HPLX Users Database (from "Around the world" thread)
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Nigel

On Sat, 16 Mar 2002 12:47:10 +0200, Nigel R <nigel@KEEPSMILING.CO.ZA> wrote:

> Errr, how can user only having access to a HP95LX access the data in GDB
> format?  Is there a desk PC application we can use?  Did the idea of a PBK
> or 1-2-3 format get abandoned?

You're right, we didn't care about the 95LX users. Sorry. ;-)

Well, of course 95LX users whould have access to the data as well,
so what do you think is the best option to convert the GDB to easily? I
think we should maintain only the GDB and everytime we release a new
version convert it to a 95LX-readable format and offer both versions
for download.

Can a GDB easily be converted to the PDB format in some way?

Easiest for us is of course to simply dump the data to an ASCII file.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 12:38:36 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: 200lx System ROM differences
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Bob

On Thu, 14 Mar 2002 15:31:37 -0500, Bob Penick <bnj@MYREALBOX.COM> wrote:

> I tested my single speed and double speed 200's and got approximately the
> same times Russ did.  And then I noticed that the total byte count was
> different on the two machines.  ????

> In the 1.00A version all the directories in D: are dated 3/25/94 and in the
> newer one they are dated 9/30/94
>
> There are just 5 files that have any differences:

In addition to the files, there may be differneces in the built-in
applications in ROM, which don't show up as files on D:.
Does anyone know what improvements have been made there?

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 16:22:21 +0100
Reply-To:     xmarc@free.fr
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marc BERLIOUX <xmarc@FREE.FR>
Subject:      Re: HPLX Users Database (from "Around the world" thread)
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
In-Reply-To:  <HPLX-L%2002031706502454@UCONNVM.UCONN.EDU>
Content-Type: text/plain; charset="iso-8859-1"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit

> You're right, we didn't care about the 95LX users. Sorry. ;-)
>
> Well, of course 95LX users whould have access to the data as well,
> so what do you think is the best option to convert the GDB to
> easily? I think we should maintain only the GDB and everytime we
> release a new version convert it to a 95LX-readable format and
> offer both versions for download.
>
> Can a GDB easily be converted to the PDB format in some way?
>
> Easiest for us is of course to simply dump the data to an ASCII
> file.

don't know if my 95lx can open .pdb files
plain text could be more simple for us too

--
          Marc BERLIOUX -- M.C.S.E
- Minesweeper Consultant & Solitaire Expert -

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 18:22:08 +0000
Reply-To:     Stefan.Peichl@T-ONLINE.DE
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Stefan Peichl <Stefan.Peichl@T-ONLINE.DE>
Subject:      Re: CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Daniel Hertrich wrote:

> On Sat, 9 Mar 2002 17:59:16 +0000, Stefan Peichl <Stefan.Peichl@T-ONLINE=
.DE> wrote:
>
> > LXCIC always only uses the socket number 1.
>
> Couldn't you simply modify LXCIC so that it also asks for info on
> socket 2? This way we could test that.

I can compile a test version which uses socket 2. After it
works with your hardware modifications, I should try to make
a variable socket version of LXCIC.

Stefan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 19:06:08 +0100
Reply-To:     hpstaber@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         HP Staber <hpstaber@COMPUSERVE.COM>
Subject:      Re: Fwd: ANN: New version of PocketDOS available
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Daniel Hertrich wrote:
>
> From comp.sys.palmtops.
> XT-CE will be discontinued.

I have upgraded.

The standard call of       www -d "!post"
POST/LX together with WWW/LX does not load - the GUI windows seem to
require too much memory.

HP Staber/Salzburg

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 12:52:45 -0700
Reply-To:     kwmiller@azbcs.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "ABCS INC." <kwmiller@AZBCS.COM>
Subject:      FW: 200lx ethernet adapter
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Thanks for all the reply's to my request for a source for Ethernet cards.  I
can report that I now have a new functioning 10mbit ethernet card working on
my 200lx thanks to Keith Grider from the list.  Here is a link to the
product information if anyone is curious.

Ethernet Card:
http://www.socketcom.com/product/ethernet_card.htm

I used the Ruggedized Low Power Ethernet PC Card Solution part #EA0914-337.
I used this one due to the mobile nature of the 200lx so I would not have to
buy a dongle when it breaks.  This card is ALSO CF compatible and uses a
PCMCIA adapter to work on PCMCIA machines.  The PCMCIA adapter ships with
these cards!  The card costs $106+shipping from CDW.COM

http://www.cdw.com/shop/products/default.asp?EDC=323951

The following drivers are used to operate the card.

LXCIC     <-- card services
LXEN2216  <-- ne2000 compatible driver
LXTCP     <-- tcpip network stack
WWW/LX    <-- web browser

I also use LXFTP, LXPING for network troubleshooting.

Thanks for all the help!

Kevin Miller

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 08:04:25 +1200
Reply-To:     Roger Whitmarsh <lodger@NZ1.IBM.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Roger Whitmarsh <lodger@NZ1.IBM.COM>
Subject:      Re: Software Carousel
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Thanks for your various responses. I've decided to buy SC.

Cheers...Roger

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 16:57:29 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: FW: 200lx ethernet adapter
In-Reply-To:  <BLENKJJKIJHGOGCHGNNNEEGAENAA.kwmiller@azbcs.com>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Sun, 17 Mar 2002, ABCS INC. wrote:

> I used the Ruggedized Low Power Ethernet PC Card Solution part #EA0914-337.

Thanks for the report!

Have you gotten a sense of the power requirements yet?  For example,
when you power on the LX after inserting the card do you get the
message "CARD BATTERY LOW - Press ESC"?

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 17 Mar 2002 17:55:14 -0700
Reply-To:     kwmiller@azbcs.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "ABCS INC." <kwmiller@AZBCS.COM>
Subject:      Re: 200lx ethernet adapter
In-Reply-To:  <Pine.OSF.4.33.0203171653130.4161-100000@worf.netins.net>
MIME-Version: 1.0
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: 7bit

>On Sun, 17 Mar 2002, Theodore Heise wrote:

>Have you gotten a sense of the power requirements yet?  For example,
>when you power on the LX after inserting the card do you get the
>message "CARD BATTERY LOW - Press ESC"?

When on batteries, I do not get that message.  I have run it on batteries to
access the network for approx 1/2 hour with no discernable power problem.  I
will let the list know my experience over time using the card.

Kevin Miller

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 05:48:28 +0100
Reply-To:     Nathalie Bugeaud <tps-seti@WANADOO.FR>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nathalie Bugeaud <tps-seti@WANADOO.FR>
Subject:      Re: more tips for my XTGOLD users
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

>-Guenther:
 >it is always a pleasure reading your tips. I use XTREE since
 >version 1, which I got in the eighties and later XTG. I also got
 >a windows version, which I unfortunately lost.

forget ver.1 for the LX .._._ Filer does a better job; the last XTREE ver.
for DOS is XTGOLD ver.3, and the 'LX reduced version' is also the best for
the palmtop. I run it on a Windoze98 PC just fine - hardly ever using dumb
Explorer/Navigator.

 >What do mean with "it supports 3 LX fonts"? Does this
 >support automatic wrap?

yes, typing "w" will wrap the text to the screen (in one font only). The LE
editor automatically wraps with 2 fonts but has no auto-scrolling.. I too
hate programs which don't wrap or wrap only after extensive formatting
procedures [like PalEdit - sorry Andreas :)]. On the other hand, the best
reading program for the LX is Andreas' READ.EXE!

Nathalie, finally getting MY-MONEY.ZIP on SUPER

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 08:21:16 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      Re: CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

I received a CF card for testing purposes (thanks to Alan),
already disassembled it and prepared for direct conection to 200lx board.
There seem to be no problem to connect it directly to motherboard. The space
between pins is enough. I will try it during this weekend.


Radek







                      Stefan Peichl
                      <Stefan.Peichl@T             To:  HPLX-L@UConnVM.UConn.Edu
                      -ONLINE.DE>                  cc:  (bcc: Radek Svagr/HRC/COMP/PHILIPS)
                      Sent by: HPLX                Subject:   Re: CF inside HP200LX  ( was: Re: HP collection
                      Mailing List
                      <HPLX-L@UConnVM.             Classification:
                      UConn.Edu>


                      2002-03-17 07:22
                      PM
                      Please respond
                      to Stefan.Peichl






Daniel Hertrich wrote:

> On Sat, 9 Mar 2002 17:59:16 +0000, Stefan Peichl <Stefan.Peichl@T-ONLINE.DE> wrote:
>
> > LXCIC always only uses the socket number 1.
>
> Couldn't you simply modify LXCIC so that it also asks for info on
> socket 2? This way we could test that.

I can compile a test version which uses socket 2. After it
works with your hardware modifications, I should try to make
a variable socket version of LXCIC.

Stefan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 13:00:22 +0100
Reply-To:     furlan@gmx.net
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Dr. Werner Furlan" <furlan@GMX.NET>
Organization: OE9FWV
Subject:      Motorolla Timeport GPRS
MIME-Version: 1.0
Content-type: text/plain; charset=US-ASCII
Content-transfer-encoding: 7BIT

hello,

a friend gave me his Motorolla Timeport GPRS Handy to try, and I
wanted to look if it works with the HP200. The IRDA Connect works,
but after this the modem Initialisation fails.
Does anybody know the Init-String for this phone?
I did not find informations on Daniels Homepage, just an email
address, that gave me an undeliverable message back.

TIA,
Werner
--
PGP-Key: <http://www.qsl.net/oe9fwv/furlan.asc>
SMS: <+436646340014@text.mobilkom.at>
Powered by Pegasus Mail - free at <http://www.pmail.com>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 13:33:48 +0100
Reply-To:     Dzon <dzon@SOFTHOME.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dzon <dzon@SOFTHOME.NET>
Subject:      atc for hplx?
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

Hello there,
I am looking for port of this superb game [linuxers know] for DOS and
hplx, did anyone meet one? It is pure ASCII textmode simulation of air
traffic, pretty tricky job to not let airplanes crash.

--
                                  -Dzon
                             dzon@softhome.net

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 14:46:59 +0200
Reply-To:     Nigel R <nigel@KEEPSMILING.CO.ZA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nigel R <nigel@KEEPSMILING.CO.ZA>
Organization: STRATEGIC ALLIANCE CONSULTING
Subject:      Re: XTREE Gold!!!??? Help!!!
Comments: To: Orin Keplinger <orink@IX.NETCOM.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Greetings from a sunny South Africa :-)

Apologies if I am duplicating information but noticed that another of my (in
addition to my trusty HP95LX) 'favourite' productivity tools is getting some
'air time',  XTGOLD!

I have original disks / copies of the application including ver 4 which
although supposedly 'Windows' based did a very good job of crashing more
times than it helped organise my massive (10 MB?) hard drive way back
...<grin>.  When trying to locate any service patches or releases I came
across the program referred to as ZTree.  WoW! If you liked XTREE then ZTREE
will blow your mind! It is a windows application that has been COMPLETELY
written to resemble the LOOK and FEEL of XTREE. There are DOZENS of
fantastic features and a session on my desk PC never go's by without ZTREE
being used!

Hope no objection to including some info taken from recent update here...
 ++++++++++++++++++++++++++++++++++++++++++++++++++++
A new beta of ZTreeWin - v1.48k - is now available.

Here's what's new in v1.48k:
----------------------------
Change- Alt-F10 - Page layout completely revised
Change- Alt-JFC - calls JFC command as specified in CO-1F
Change- Alt-Mirror - process branches collapsed by F5/F6
Change- DW - Backspace - jump to parent directory and finally root
Change- Log/Ctrl-Log - menus now more descriptive of function
Change- View - Ctrl-F3 replaces Alt-F3 for Auto-Reload
Added - /ROWS:MAX - start with window set to maximum height
Added - /COLS:MAX - start with window set to maximum width
Added - Alt-Attribute - DW -  F4 Apply to logged subdirectories (y/n)
Added - Alt-F10 - CO-1S - Swap Log and Ctrl-Log key assignments
Added - Alt-F10 - CO-2E - Kilobytes displayed as multiples of (1000/1024)
Added - Alt-F10 - CO-2R - Access to empty file windows
Added - Alt-F10 - CO-3L - F3 in File window retains cursor position
Added - Alt-F10 - CO-5D - Display archive list output
(View/Alt-View/Autoview)
Added - Batch parameters - %ja %jd %js - relate to other pane's current file
Added - F11 Bookmark history - Support for Del key
Added - F12 - support for keys SH_NUM1 - SH_NUM9
Added - F12 - support for NUM5 key
Added - FW - Backspace - switches to FW of parent directory (if permitted)
Added - View - HEX Edit - Display current byte in hex, oem, ascii, decimal
Fixed - /OD - command line option was broken
Fixed - Alt-F5 - Extract from spanned archive not displaying output
Fixed - Alt-F5 - .RAR - directory entries being logged as 0-byte files
Fixed - Alt-F9 - SFW - GPF toggling from largest size back to 25 lines
Fixed - Alt-F12 - File window - command unavailable when no files in list
Fixed - Alt-I - Version information not being initialized
Fixed - Alt-K - not showing branch totals when base directory empty
Fixed - Alt-K - Size - show 0k for directories containing only zero-byte
files
Fixed - Alt-K - Tagged - not refreshing after using Alt-C in DW
Fixed - Alt-Mirror - problem traversing branch when collapsed with F6
Fixed - Alt-Mirror - progress bar not initializing properly
Fixed - Alt-Mirror/Ctrl-Copy/Move - progress bar not updated for replace

<BIG SNIP>

Fixed - View - JUNK - buffer overrun at end of long file
Fixed - View - JUNK - Gather not capturing JUNK mode display
Fixed - View - JUNK - Gather causing GPF in certain cases
Fixed - View - JUNK - Search hits not being highlighted correctly
Fixed - View - Search hits with * not highlighted correctly when sub-hits
existed
-------------------------------------------------------------------

Please visit: http://www.ztree.com/html/beta.htm to download your copy.

This version can be installed over any release from v1.41 +.
+++++++++++++++++++++++++++++++++++++++++++++++++

Also from the same source are the following links:

Have you visited the ZTreeWin Unofficial Homepage recently?
http://www.vico1.com

Make sure you stop by Jeff Johnson's home page!
http://www.xtree.com

Don't forget to check out the XTree Fan page!
http://www.xtreefanpage.org

And for anyone looking for a good XTree clone for Linux, visit:
http://www.unixtree.org/

Last two points, 1) what / where is the versionof XTree for the palm and
where can a copy be found and 2) I have no commercial or any other
connection with ZTREE, just a VERY happy uisers!

Remember to KEEP SMILING!

Nigel R

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 14:45:55 +0200
Reply-To:     Nigel R <nigel@KEEPSMILING.CO.ZA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nigel R <nigel@KEEPSMILING.CO.ZA>
Organization: STRATEGIC ALLIANCE CONSULTING
Subject:      Re: HPLX Users Database (from "Around the world" thread)
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Me again!  (Sorry multiple posting to one digest...)

----- Original Message -----
From: "Daniel Hertrich" <daniel.hertrich@GMX.DE>
Sent: Sunday, March 17, 2002 12:38 PM
Subject: Re: HPLX Users Database (from "Around the world" thread)


> You're right, we didn't care about the 95LX users. Sorry. ;-)

No problem, I / (we?) 95LX users have VERY thick skins due to being around
as long as the 95! (with apologies to any users not meeting this criteria
<g>)

> Easiest for us is of course to simply dump the data to an ASCII file.

If the dump could be formatted as a csv with each record taking one line
this could then be imported into a spreadsheet OR opened in a easy to use
format directly on the 95 using supa 'Notepad' application (developed by
Charles Hayden). Could first line please contain 'header' details?  Tried
looking for GDB4WIN but unable to access SUPER so can't comment on using as
alternative.  My preference for the 95 will be the csv option.

As always, KEEP SMILING!

Nigel R in sunny South Africa

P.S. Daniel, any comments yet re the S35i cable query (sent direct)?

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 14:06:49 +0100
Reply-To:     castrobarco@wol.es
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Josi A. de Castro" <castrobarco@YAHOO.COM>
Subject:      Zcopy manual?
In-Reply-To:  <20020316212505.C3D6BD27BD@deborah.paradise.net.nz>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 8bit

I have got zcopy.com ver 1.21 for use with XFinder, but the manual is in
japonese :-).

Could someone give me any help?

________________________________________________

Josi Angel de Castro        castrobarco@yahoo.es
C/S.Lorenzo, 1-3:B
47001 VALLADOLID              Tfno: 983 36 30 42
________________________________________________

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 09:03:55 -0500
Reply-To:     Steve <novosad@SERVER030.FWB.SAIC.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Steve <novosad@SERVER030.FWB.SAIC.COM>
Subject:      Re: DHCP and LXTCP
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Keith Grider wrote:

> On a side note, has anyone ever gotten SMB to work with a win98 or win2k
> network. I have spent unknown hours and tried BOTH of the suggestions on the
> web and neither allow an SMB connection. I can either see the computer, but
> cannot mount any shares or I cannot see any shares on the HP. If there is
> anyone that does use this, please let us know.
>
> KeithG

Keith,

   I guess a question of whether you are using a NetBIOS or
NetBIOS over TCP/IP network comes up.  I got my 200LX to access
a LAN Server network using NetBIOS.  I never tried any TCP/IP
stuff though.  Not all that practical, due to the small C: drive
when using a network card.

Steve

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 16:12:20 +0100
Reply-To:     Dzon <dzon@SOFTHOME.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dzon <dzon@SOFTHOME.NET>
Subject:      Re: CF inside HP200LX
In-Reply-To:  <OFF12C0289.A40AF698-ONC1256B80.0025E3D5@diamond.philips.com>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

> I received a CF card for testing purposes (thanks to Alan),
> already disassembled it and prepared for direct conection to 200lx board.
> There seem to be no problem to connect it directly to motherboard. The space

There are rumours that the compact flash medium's life is not as long as I
thought, ie neverending :). How long can I count the CF card survives when
used regularly as a hard drive?

--
                                  -Dzon
                             dzon@softhome.net

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 11:47:34 -0800
Reply-To:     j_vanderstel@JUNO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John J Vander Stel <j_vanderstel@JUNO.COM>
Subject:      Re: HPLX-L Digest - 16 Mar 2002 to 17 Mar 2002 (#2002-83)
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Hi Daniel,

>Well, of course 95LX users would have access to the data as well,
>so what do you think is the best option to convert the GDB to easily? I
>think we should maintain only the GDB and everytime we release a new
>version convert it to a 95LX-readable format and offer both versions
>for download.
>
>Can a GDB easily be converted to the PDB format in some way?
>
>Easiest for us is of course to simply dump the data to an ASCII file.

I don't have a 95LX, but I don't use the built-in database program in my
200LX, either.  It would be really helpful if the database was also made
available in a password protected zipped up ASCII file.

This would even work for those who don't actually have an LX and
subscribe to this list for the hard to find DOS info.

Even better.. is there a simple standalone DOS based utility freely
available that can convert a GDB file to an ASCI file?

Cheers!

John Vander Stel
Grand Rapids, Michigan

________________________________________________________________
GET INTERNET ACCESS FROM JUNO!
Juno offers FREE or PREMIUM Internet access for less!
Join Juno today!  For your FREE software, visit:
http://dl.www.juno.com/get/web/.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 23:47:00 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      GDB4WIN
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

i've located it GDB4WIN .. dunno if
this list allows attachment .. but its
very very useful to view the gdb files
under win9x and above .. 122kb zip file

..pk

(daniel .. if you put it on super .. where do
i send it .. so that you can do it ?)


-----Original Message-----
From: Nigel R <nigel@KEEPSMILING.CO.ZA>
To: HPLX-L@UConnVM.UConn.Edu <HPLX-L@UConnVM.UConn.Edu>
Date: Monday, March 18, 2002 6:22 PM
Subject: Re: HPLX Users Database (from "Around the world" thread)


>Me again!  (Sorry multiple posting to one digest...)
>
>----- Original Message -----
>From: "Daniel Hertrich" <daniel.hertrich@GMX.DE>
>Sent: Sunday, March 17, 2002 12:38 PM
>Subject: Re: HPLX Users Database (from "Around the world" thread)
>
>
>> You're right, we didn't care about the 95LX users. Sorry. ;-)
>
>No problem, I / (we?) 95LX users have VERY thick skins due to being around
>as long as the 95! (with apologies to any users not meeting this criteria
><g>)
>
>> Easiest for us is of course to simply dump the data to an ASCII file.
>
>If the dump could be formatted as a csv with each record taking one line
>this could then be imported into a spreadsheet OR opened in a easy to use
>format directly on the 95 using supa 'Notepad' application (developed by
>Charles Hayden). Could first line please contain 'header' details?  Tried
>looking for GDB4WIN but unable to access SUPER so can't comment on using as
>alternative.  My preference for the 95 will be the csv option.
>
>As always, KEEP SMILING!
>
>Nigel R in sunny South Africa
>
>P.S. Daniel, any comments yet re the S35i cable query (sent direct)?
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 12:26:45 -0600
Reply-To:     Tim <palmtop@N-LINK.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tim <palmtop@N-LINK.COM>
Subject:      Software Carousel and "odd" character insertion....
In-Reply-To:  <000b01c1cd80$2f17c740$6401a8c0@gadgetbase>
MIME-Version: 1.0
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: 7bit

I have an "odd" issue, w/ Software Carousel...

Whenever I have SC (actually Super SC7) running and the palmtop goes through
an auto shut-off to save power and I turn it on, it adds characters to some
text fields. This is most notable If I'm in the note field of a phone book
entry. I turn it back on and usually get an asterisk added to the text in
the note field.

What causes this?

It doesn't add characters to everything, and it sometimes adds two chars.
instead of one. I have the "typical" setup (pretty much default), running
SSC7, Buddy in the main session and the Andrew font set. It happens with a
DS and single speed (unmodified) LX; so it's not an issue w/ the DS or
memory expansion drivers...

Anyone else experience this? Since it doesn't always happen, it's hard to
troubleshoot, AND (on reflection) I think it only happens when the palmtop

Thanks,

--tim

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 13:28:23 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: 200lx ethernet adapter
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

An ethernet card like this gets my vote as a prime candidate for occupying
an internal "Slot2", if one is possible. Having ethernet built in, with the
regular card slot still open for a big Flash card, would be most useful.

Bob

-----Original Message-----
From: ABCS INC. [mailto:kwmiller@azbcs.com]
Sent: Sunday, March 17, 2002 1:53 PM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: FW: 200lx ethernet adapter

<snip>

Ethernet Card:
http://www.socketcom.com/product/ethernet_card.htm

I used the Ruggedized Low Power Ethernet PC Card Solution part #EA0914-337.
I used this one due to the mobile nature of the 200lx so I would not have to
buy a dongle when it breaks.  This card is ALSO CF compatible and uses a
PCMCIA adapter to work on PCMCIA machines.

<snip>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 22:32:51 -0000
Reply-To:     =?iso-8859-1?Q?Paulo_Cust=F3dio?= <psfgc@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         =?iso-8859-1?Q?Paulo_Cust=F3dio?= <psfgc@YAHOO.COM>
Subject:      Re: GDB4WIN
Comments: To: pksharma <pksharma@CAL.VSNL.NET.IN>
In-Reply-To:  <011101c1cea9$1a0032a0$986dc5cb@q20>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 8bit

It is already available in SUPER at
http://www.palmtop.net/cgi-bin/search.pl?Case=Yes&Query=gdbwin&Cat=All&Type=
Words&Allmatch=No&Sort=Alpha

Paulo


-----Original Message-----
From: HPLX Mailing List [mailto:HPLX-L@UConnVM.UConn.Edu]On Behalf Of
pksharma
Sent: Segunda-feira, 18 de Margo de 2002 18:17
To: HPLX-L@UConnVM.UConn.Edu
Subject: GDB4WIN


i've located it GDB4WIN .. dunno if
this list allows attachment .. but its
very very useful to view the gdb files
under win9x and above .. 122kb zip file

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 00:06:29 +0100
Reply-To:     Jan Brandt <jebrandt@XS4ALL.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jan Brandt <jebrandt@XS4ALL.NL>
Subject:      IR connection to Ericsson T39
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I have recently purchased an Ericsson T39m mobile phone, and I am now trying
to connect to the phone from my HP200LX via infrared.
First I tried with www/lx, but in the end gave up (for now) to find a proper
setup in the config file to make it work.
I then thought I'd try and take it step by step. I downloaded ir.exe from
D&A and was hoping I could at least get a connection with the phonemodem.
But ir.exe reports:

 Opening IrDA for Interactive session...
 Talking with "T39"...
then it sits there for some seconds and then apparently fails because it
comes out with:
 IrDA connect failed
 Cannot establish LMP connection.

So apparently it sees the phone, but doesn't succeed in making a proper
connection. I am pretty much clueless about these things so I would
appreciate any help.

Jan.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 19:26:23 -0500
Reply-To:     Bob Newins <bnew@ATTBI.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Newins <bnew@ATTBI.COM>
Subject:      Re: Software Carousel and "odd" character insertion....
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Tim,

I am running a similiar setup, but I am not using Buddy.  I am not
having any problems. The font I am using is one I designed called
Bobfont(G) which is also similiar to Andrew font.  Try removing Buddy
and see if anything changes.  Buddy is a great program, but I stopped
using it because of the big lower DOS memory hit.    =Bob=

Tim wrote:
>
> I have an "odd" issue, w/ Software Carousel...
>
> Whenever I have SC (actually Super SC7) running and the palmtop goes through
> an auto shut-off to save power and I turn it on, it adds characters to some
> text fields. This is most notable If I'm in the note field of a phone book
> entry. I turn it back on and usually get an asterisk added to the text in
> the note field.
>
> What causes this?
>
> It doesn't add characters to everything, and it sometimes adds two chars.
> instead of one. I have the "typical" setup (pretty much default), running
> SSC7, Buddy in the main session and the Andrew font set. It happens with a
> DS and single speed (unmodified) LX; so it's not an issue w/ the DS or
> memory expansion drivers...
>
> Anyone else experience this? Since it doesn't always happen, it's hard to
> troubleshoot, AND (on reflection) I think it only happens when the palmtop
>
> Thanks,
>
> --tim
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 06:03:04 +0100
Reply-To:     Nathalie Bugeaud <tps-seti@WANADOO.FR>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nathalie Bugeaud <tps-seti@WANADOO.FR>
Subject:      HPLX312.GDB
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

  >-Daniel wrote-:
 >Please note that changes to the master datafile are uploaded
 >to Daniel every week or two depending on the number of changes.
 >So your changes may not appear on Daniel's site for awhile but
 >they are made in the only database that counts - the master.

i was going to watch TV after work and write to Bob tomorrow  :) ... but i
decided instead to write to you all .._._ re. DB engines:

there usually are 2 reasons for having DBs:
 1. find something accurately, and 2. quickly!

Bob's "master" HPLX_Listmembers DB can be made to maximise those 2 in the
following way:

1. remove the checkbox "[x] offers support" and use the space for "skills"

reason: there is noone listed who has skills but does not want to offer
support, and the space can be used for 2 rows (edit smart clip definition),
and is not wasted in the datacard. Bob Lowe shows a cross in his checkbox
but then states "skills not specified" (rather confusing)

2. remove the 2 "00" in front of README and replace with a space; rename in
subsets the German "Alle Eintraege" to "All Database Items"

reason: looks better, and not everyone speaks German

3. edit the subset "People offering support" list (non-data card) by
removing the column "e-mail" and replacing it with "skills", then resize the
two remaining colums to 10% for "name" and 90% for "skills"

reason: it makes it easier scrolling for skills needed, especially for
HPLX100 users without a data card

4. Modify the whole database (filer F) to remove the [x] checkbox and extend
the e-mail box to accomodate up to 3 e-mail addresses; rename the "location"
item to "interests"; put a & before the "S" in skills to easily get to

reason: the checkbox is useless; Ken Hansen is mentioned twice and  Stuart
Grey's 2nd e-mail address is in the notes F3 "comments"; there is no
"location" entry for anyone, but entries for "interest" can easily be
found - everyone has a hobby! tab 10 times to get to skills is tiring

5. delete 2 of the 3 versions of the skills "database programming/LX basics"
(take care that all are connected to the remaing version) and replace the 2
with "EXM programming" and "Carousel"; remove the "skills not specified" and
replace with "misc.skills"

reason: let the Japanese get some credit, and get some support from Ed Keefe
and Hal Goldstein, and last not least let the doctors and mechanics fix your
ailing mobility and moving equipment. :)
----

If dear Bob has no time i am willing to 'borrow' the "master" for a day and
return it 'improved' .._._ wie steht's Daniel - kannst Du dem Bob mir
vertrauen? :) :) :)

Nathalie - grabbing the 'Remocon' to fall asleep in front of the box

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 23:32:55 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: HPLX312.GDB
In-Reply-To:  <004901c1cf04$c596d5a0$c5170950@oemcomputer>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Tue, 19 Mar 2002, Nathalie Bugeaud wrote:

> ...rename in subsets the German "Alle Eintraege" to "All Database Items"

I thought the German was sort of cute.  <grin>

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 17:51:33 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: CF inside HP200LX
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Dzon

On Mon, 18 Mar 2002 16:12:20 +0100, Dzon <dzon@SOFTHOME.NET> wrote:

> There are rumours that the compact flash medium's life is not as long as I
> thought, ie neverending :). How long can I count the CF card survives when
> used regularly as a hard drive?

If you use it for a non-multitasking system like the DOS on the 200LX,
you can consider it to be immortal, if you buy a modern CF card.
I think they are rated at about 1.000.000-10.000.000 write cycles
(and unlimited read cycles) per memory cell, so calculate yourself:
if it should die after 100 years, you must do at least 1.000.000/100 =
10.000 writes per year per cell, this is 27 writes per day or about 1
write per hour PER memory CELL. A 128 MB CF card has 128 * 1024 * 1024
* 8 = 1.073.741.824 memory cells.....
Since you are usually not writing periodically to one specific cell,
but you fill up your card with a few programs, so the first half of the
card is only written once a yer maybe, and the rest is written far more
often, but never as much as required to wear it out, I think this limit
is not so important anymore.

Differently however if you use such a card as a harddrive in Linux or
Windows systems, since there a specific range on the drive, usually
even a specific partition under Linux, is used as RAM swap space, and
this is written very often under some circumstances, the limit can
become very important there.

So the best you can do for your card is in all cases to make sure that
write cycles are applied to different ranges on the card. This can be
caused for example if you sometimes copy a large program folder to
another location and delete the original folder. Then a large amount of
space becomes free for your data files which you work on and newer
copies of these data files are written into that space instead of where
they have been written before. The new copy of the large program folder
will block the range where data files may have been written before.

This is all a statistical thing, and you can never be sure, a memory
cell may even fail after the 10th write or it may fail not before the
100.000.000.000th write, but as always, we must use and work with the
statistical numbers.

Personally, I never care about this limit in the way I described above
(moving large fixed data blocks), I also never care about using my
rechargeables efficiently, because I think the amount of work and
thinking which is necessary for this kind of maintenance is far more
than the amount of money and maybe time to simply replace the dead CF
card or battery.

Of course, this is only true if you always have a recent backup!

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 22:45:50 -0800
Reply-To:     bobv <bobv@SOS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         bobv <bobv@SOS.NET>
Subject:      Nokia 3285
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Does anyone know of a phonebook manager for the HPLX (or even a windows
laptop) for maintining the Nokia 3285 phone book?

I think it is the same as the 6185.

TIA

Bob

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 19:08:22 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      GDB to ASCII
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi John

On Mon, 18 Mar 2002 11:47:34 -0800, John J Vander Stel <j_vanderstel@JUNO.COM> wrote:

> I don't have a 95LX, but I don't use the built-in database program in my
> 200LX, either.  It would be really helpful if the database was also made
> available in a password protected zipped up ASCII file.

Okay .We will include an ASCII file with the next version.

> Even better.. is there a simple standalone DOS based utility freely
> available that can convert a GDB file to an ASCI file?

Sure. Look for GDBIO on SUPER. There are others, a Japanese program
called "convert" I think... I think it's not yet on SUPER, but I'll put
it there soon.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 09:48:42 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Radek

On Mon, 18 Mar 2002 08:21:16 +0100, Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM> wrote:

> I received a CF card for testing purposes (thanks to Alan),
> already disassembled it and prepared for direct conection to 200lx board.
> There seem to be no problem to connect it directly to motherboard. The space
> between pins is enough. I will try it during this weekend.

Great! I'm very curious if this will work.
If it doesn't work on the first try, please also try it with the
Accurite Doubleslot driver. This may be necessary to make it possible
for software to speak with the 2nd socket.

If I had the time I would also do this test, but unfortunately, I
really cannot afford the time. :-(

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 08:03:03 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      partitioned memory card in 200lx!
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Maybe I just discovered america but...

I succesfully partitioned memory card so it was readable in 200lx as A: and B:
BUT it was SRAM car not CF:-( I was not able to partition CF.

Radek

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 08:41:57 +0100
Reply-To:     Dzon <dzon@SOFTHOME.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dzon <dzon@SOFTHOME.NET>
Subject:      Re: atc for hplx?
In-Reply-To:  <Pine.LNX.4.10.10203181329120.1766-100000@dzon>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

> Hello there,
> I am looking for port of this superb game [linuxers know] for DOS and
> hplx, did anyone meet one? It is pure ASCII textmode simulation of air
> traffic, pretty tricky job to not let airplanes crash.

I've found some, check out http://168.216.219.18/pub/IBM/MegaGames3/ for
some of good old things. But none of the two atc's there is what I'm
looking for. Anyway, try atc2.zip, run atc 1 4 to get best graph mode on
LX. Cool thing, but the airplanes's number is limited even in registered
version :(

--
                                  -Dzon
                             dzon@softhome.net

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 02:41:08 -0500
Reply-To:     Martin Bergvill <hplx@BERGVILL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Martin Bergvill <hplx@BERGVILL.COM>
Subject:      Re: IR connection to Ericsson T39
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Tue, 19 Mar 2002 00:06:29 +0100, Jan Brandt wrote:

Hi Jan

> I have recently purchased an Ericsson T39m mobile phone, and I am now trying
> to connect to the phone from my HP200LX via infrared.

Works well here for both HSCSD and GPRS

> First I tried with www/lx, but in the end gave up (for now) to find a proper
> setup in the config file to make it work.

My setup is

[ISP_Telenor]
Port=-1
Baud=38400
Modem=1
PPP=1
Login=
Password=
Modeminit=ATZ+cbst=0,0,1;+chsn=4,2,0,12
Dial=
DNS_IP=
DNS2_IP=
Script=CHAP_Script
OmniGo=0
My_IP=0.0.0.0


Not sure if the modeminit is the best one. I think Daniel knows the one
that are the best to use.

[ISP_Gprs]
Magic=0
Port=-1
OmniGo=1
PPP=1
Modem=1
Baud=38400
My_IP=0.0.0.0
DNS_IP=
DNS2_IP=
Script=CHAP_Script
Login=T39
ModemInit=AT+cgdcont=1,"IP","internet"
Password=Something
Dial=*99***1#

For GPRS you need a special version of Www.exe. You have to talk to D&A
to get it.

> I then thought I'd try and take it step by step. I downloaded ir.exe from
> D&A and was hoping I could at least get a connection with the phonemodem.
> But ir.exe reports:
>
>  Opening IrDA for Interactive session...
>  Talking with "T39"...
> then it sits there for some seconds and then apparently fails because it
> comes out with:
>  IrDA connect failed
>  Cannot establish LMP connection.

I use T39 ad HPLX for Vcards too. It works well. Look at
http://www.daniel-hertrich.de/mob_hplx/

>
> So apparently it sees the phone, but doesn't succeed in making a proper
> connection. I am pretty much clueless about these things so I would
> appreciate any help.

We will get you trhough this.

For a regular connection (HSCSD or justplain 9600) you do not need a
special version of WWW.exe. But if you would like to use GPRS you need
one.

The T39/T68 has a bug in the implementition of PPP in GPRS thats why
you need a special Www.exe. NOTHING wrong with Www/LX but it is the
Ericsson.

I hope this helped.

Regards

--
Martin Bergvill ,Narvik Norway

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 09:14:23 +0100
Reply-To:     Etienne Lemaire <etienne.lemaire@pandora.be>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Etienne Lemaire <etienne.lemaire@PANDORA.BE>
Subject:      Re: Running llrawin.exe Under Win 95
Comments: To: "Robert K. Meyer" <bmeyer@UNION-TEL.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

http://www.mydocsonline.com/pub/trial1/laplink.doc

Download this file, (too large to post) and start with the
bottom part "tip from Pete Jordan". A long time ago, I tried
successfully at least one of his methods

Oh,  and if you care to read the rest and transform all these
little notes into something more readable, you are welcome!
:-))

HTH

Etienne
----- Original Message -----
From: "Robert K. Meyer" <bmeyer@UNION-TEL.COM>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Saturday, March 16, 2002 03:38 PM
Subject: Running llrawin.exe Under Win 95


| Can it be done? In the Connectivity Pack there is
| llrawin.exe (not llrawin.bat as created in some posts).

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 10:52:24 +0100
Reply-To:     Feher Tamas <feher.tamas@2FKFT.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Feher Tamas <feher.tamas@2FKFT.COM>
Subject:      Re: 200lx ethernet adapter
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-2"
Content-Transfer-Encoding: 7bit

Hello,

>>SocketCom Ruggedized Low Power Ethernet
>>PC Card Solution part #EA0914-337
>
>An ethernet card like this gets my vote as a prime
>candidate for occupying an internal "Slot2", if one is
>possible. Having ethernet built in, with the regular card
>slot still open for a big Flash card, would be most useful.

Indeed, sarting the first day, when antimatter-alkaline batteries in
size AA format become commercially available. The flashcard+LANcard
combo would suck dry Li-ions in an hour. LANcards need power even when
offline!

I think an external solution, a serial-attached ethernet 10TX card would
be a better solution, especially with its own 9V cell, kind of a
"pocket-modem" for LAN. I know RS232 is limited to 115kbps, but I guess
it's enough bandwidth, considering the palmtop's weak CPU. You just
cannot utilize 10mbps.

Sincerely: Tamas Feher.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 14:52:25 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: From Japan: a serial to RS232 controller!?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Tamas

On Sat, 16 Mar 2002 18:44:31 +0100, Tamas Feher <etomcat@FREEMAIL.HU> wrote:

> This looks like an RS-232 to Ethernet adapter, I guess it would be
> nice for use with HPLX having a flashcard in its PCMCIA slot.
>
> <http://elm-chan.org/tmp/avrea.jpeg>

Yes, looks really as RS232<->ethernet.
I don't know the components used, so I cannot say anything about th
functionality, but at least you will need a software driver to make
this thing work, I guess.
And the jack at the top shows you need an external power supply.

I could not find any description of this circuit on the elm-chan.org
homepage. Did you?

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 09:19:30 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: IR connection to Ericsson T39
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Jan

On Tue, 19 Mar 2002 00:06:29 +0100, Jan Brandt <jebrandt@XS4ALL.NL> wrote:

> I have recently purchased an Ericsson T39m mobile phone, and I am now trying
> to connect to the phone from my HP200LX via infrared.

No problem.
Here on the list are at least 3 people doing this daily. One of those
is me.

> First I tried with www/lx, but in the end gave up (for now) to find a proper
> setup in the config file to make it work.
> I then thought I'd try and take it step by step. I downloaded ir.exe from
> D&A and was hoping I could at least get a connection with the phonemodem.
> But ir.exe reports:
>
>  Opening IrDA for Interactive session...
>  Talking with "T39"...
> then it sits there for some seconds and then apparently fails because it
> comes out with:
>  IrDA connect failed
>  Cannot establish LMP connection.
>
> So apparently it sees the phone, but doesn't succeed in making a proper
> connection. I am pretty much clueless about these things so I would
> appreciate any help.

Okey. To track down the problem, please
1. read http://www.daniel-hertrich.de/mob_hplx carefully,
2. read http://www.daniel-hertrich.de/ir_dev carefully,
3. if you still have problems, please give us the www.cfg setup section
you use.

This as a start, more to come later.

GTX
daniel




--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 12:50:43 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      test
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

seems I have some problem with e-mail

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 09:19:31 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Nokia 3285
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Bob

On Mon, 18 Mar 2002 22:45:50 -0800, bobv <bobv@SOS.NET> wrote:

> Does anyone know of a phonebook manager for the HPLX (or even a windows
> laptop) for maintining the Nokia 3285 phone book?

There is no phone book manager.
But there is Robot/LX and the robot script "phone.scr", which enables
you to download or upload the whole phone book via WWW/LX and Robot/LX.

So you can download it, maintain it with a text editor and upload it
again. Or you can use the 200LX built-in phonebook as the "master"
phone book and let my program PDB2PHN create a phone book which you can
then upload to the phone. This is what I do.

http://www.daniel-hertrich.de/pdb2x

Or you can write an own phonebook maintenance program in the Robot/LX
scripting language. Since all phnone book maintenance can be done voa
AT commands through a cable or IrDA interface, this is theoretically
possible.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 05:08:11 -0800
Reply-To:     Ian Butler <ianb@HPLX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ian Butler <ianb@HPLX.NET>
Subject:      Re: 200lx ethernet adapter
In-Reply-To:  <003e01c1cf2b$c549dc60$162fa8c0@2fkft.com>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Tue, 19 Mar 2002, Feher Tamas wrote:

> I think an external solution, a serial-attached ethernet 10TX card
> would be a better solution, especially with its own 9V cell, kind of a
> "pocket-modem" for LAN. I know RS232 is limited to 115kbps, but I
> guess it's enough bandwidth, considering the palmtop's weak CPU. You
> just cannot utilize 10mbps.

Actually, a PCMCIA network card in a double-speed 200LX can do around
450-500kbps.  Not THAT much faster than the serial port, but definitely
noticeable.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 07:20:11 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: partitioned memory card in 200lx!
MIME-Version: 1.0
Content-Type: text/plain

HOW????

-----Original Message-----
From: Radek Svagr [mailto:radek.svagr@LGPHILIPS-DISPLAYS.COM]
Sent: Tuesday, March 19, 2002 1:03 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: partitioned memory card in 200lx!


Maybe I just discovered america but...

I succesfully partitioned memory card so it was readable in 200lx as A: and
B:
BUT it was SRAM car not CF:-( I was not able to partition CF.

Radek

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 13:14:47 +0000
Reply-To:     Stefan.Peichl@T-ONLINE.DE
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Stefan Peichl <Stefan.Peichl@T-ONLINE.DE>
Subject:      Re: CF inside HP200LX  ( was: Re: HP collection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Radek Svagr wrote:

> I received a CF card for testing purposes (thanks to Alan),
> already disassembled it and prepared for direct conection to 200lx =
board.

Please note: LXCIC is only an I/O card enabler, not a memory
card enabler. Don't expect LXCIC to recognize a memory card
at socket 2.

Stefan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 09:25:27 -0500
Reply-To:     Francois Gurin <matrix@SHOT.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Francois Gurin <matrix@SHOT.ORG>
Subject:      Re: 200lx ethernet adapter
In-Reply-To:  <003e01c1cf2b$c549dc60$162fa8c0@2fkft.com>; from Feher Tamas on
              Tue, Mar 19, 2002 at 10:52:24AM +0100
Mime-Version: 1.0
Content-Type: text/plain; charset=us-ascii

On Tue, Mar 19, 2002 at 10:52:24AM +0100, Feher Tamas wrote:
> >>SocketCom Ruggedized Low Power Ethernet
> >>PC Card Solution part #EA0914-337
> >
> Indeed, sarting the first day, when antimatter-alkaline batteries in
> size AA format become commercially available. The flashcard+LANcard
> combo would suck dry Li-ions in an hour. LANcards need power even when
> offline!
>
> I think an external solution, a serial-attached ethernet 10TX card would
> be a better solution, especially with its own 9V cell, kind of a
> "pocket-modem" for LAN. I know RS232 is limited to 115kbps, but I guess
> it's enough bandwidth, considering the palmtop's weak CPU. You just
> cannot utilize 10mbps.

FWIW, Socket Communications no longer directly sells the LPE in a PCMCIA
form, which uses about 65ma peak.  It now sells it's compact flash LPE
with cf->pcmcia adapter.  Peak power consumption on this card is rated at
19ma (if i remember right) which makes it very light on the batteries, and
I believe lxcic has the capabilities to turn off the power to the pcmcia
slot as it is.
What does this add up to?  A quick search brings up the following maximum
typical power consumption for cf memory cards @5v/@3.3v during a write:
115/115ma http://www.longshin.com.tw/Company/Products/Download/FLASHMEMCARD.PDF
32/20ma http://www.emjembedded.com/products/flash/compact.html
25/25ma http://www.evalue-tech.com/evalueweb/products/specifications/ACC-CFC.cfm

Socket lists the power consumption of the lpe (ea0914-337 et al) @3.3v active:
19ma ftp://ftp.socketcom.com/ea/lpepcdatasheet.pdf

So the ethernet card is just about the same as the average cf card doing
nothing but writes.  Even with both active, you're likely to get more than
an hour of battery life.

Anyone have power specs on the ds & ram upgrades?

--francois

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 07:32:17 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: 200lx ethernet adapter
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-2"

Yes, power use might be a consideration. However, some modification of the
case would be necessary to get the LAN connection out, so you could also add
a small slide switch to manually turn the ethernet card on and off.

Another possible alternative would be to combine two CF cards in a single
PCMCIA card. I think the dimensions are OK, but some additional electronics
and software probably would be needed.

One can dream.

-----Original Message-----
From: Feher Tamas [mailto:feher.tamas@2FKFT.COM]
Sent: Tuesday, March 19, 2002 3:52 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: 200lx ethernet adapter


Hello,

>>SocketCom Ruggedized Low Power Ethernet
>>PC Card Solution part #EA0914-337
>
>An ethernet card like this gets my vote as a prime
>candidate for occupying an internal "Slot2", if one is
>possible. Having ethernet built in, with the regular card
>slot still open for a big Flash card, would be most useful.

Indeed, sarting the first day, when antimatter-alkaline batteries in
size AA format become commercially available. The flashcard+LANcard
combo would suck dry Li-ions in an hour. LANcards need power even when
offline!

I think an external solution, a serial-attached ethernet 10TX card would
be a better solution, especially with its own 9V cell, kind of a
"pocket-modem" for LAN. I know RS232 is limited to 115kbps, but I guess
it's enough bandwidth, considering the palmtop's weak CPU. You just
cannot utilize 10mbps.

Sincerely: Tamas Feher.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 08:43:40 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: atc for hplx?
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Dzon wrote:
>I am looking for port of this superb game
> [linuxers know] for DOS and hplx, did
> anyone meet one? It is pure ASCII textmode
> simulation of air traffic, pretty tricky job to not
> let airplanes crash.

I have ATC on my 200lx.  I haven't played it for a while but
I've been playing it for years.  It probably pre-dates linux.
What's on my 200lx is just the executable if I remember right.
I'll have to locate the original zip if I still have it.

if you'll send me a private email at barry AT fbtc DOT net I'll
be happy to send it in a reply when I find it.

If this isn't on the Super site it probably should be.  It's a
fun game and it works perfectly on the 200lx.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 15:52:43 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      Re: partitioned memory card in 200lx!
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Using MEMCARD.EXE which is in Olivetti Quaderno mininotebook (386 version). I made 2 partitions on this 512 kB SRAM card, one 255 and one 256 kB.
Both were then acessible on 200lx as A: and B:. What is funny that Olivetti quaderno itself didn't recognize the second partition. But this could be due to wrong settings of its drivers.

Then I tried the same with CF card, but MEMCARD.EXE refused to partition it.

Radek







                      "Feldman, Robert"
                      <Robert_Feldman@JDE             To:  HPLX-L@UConnVM.UConn.Edu
                      DWARDS.COM>                     cc:  (bcc: Radek Svagr/HRC/COMP/PHILIPS)
                      Sent by: HPLX                   Subject:   Re: partitioned memory card in 200lx!
                      Mailing List
                      <HPLX-L@UConnVM.UCo             Classification:
                      nn.Edu>


                      2002-03-19 03:20 PM
                      Please respond to
                      "Feldman, Robert"






HOW????

-----Original Message-----
From: Radek Svagr [mailto:radek.svagr@LGPHILIPS-DISPLAYS.COM]
Sent: Tuesday, March 19, 2002 1:03 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: partitioned memory card in 200lx!


Maybe I just discovered america but...

I succesfully partitioned memory card so it was readable in 200lx as A: and
B:
BUT it was SRAM car not CF:-( I was not able to partition CF.

Radek

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 10:01:00 -0500
Reply-To:     flora@MINPOST.NU
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Rolf Aronsson <flora@MINPOST.NU>
Subject:      PostLx......
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

17-Mar-02

Hi, all!

Are there possibilities to extract readable files from
Postlx' boxes? I mean a *.doc file for example.

Thanks for this HPLX-community, going over the world! So
many tips and trix, so many themes.........


Regards Rolf Aronsson, Sweden.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 08:59:20 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: CF inside HP200LX
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Dzon wrote:
> There are rumours that the compact flash medium's
> life is not as long as I thought, ie neverending :). How
> long can I count the CF card survives when used
> regularly as a hard drive?

I have one of the early 10 meg Sundisk (now Sandisk) cards and
it came with a program called wear that looks for any sectors
that are slowing down on writes (that's how they wear out) and
swaps the contents of those sectors with the contents of fast
sectors, letting the card wear evenly.  It's called wear
levelling.

Anyway I've run it once or twice a year and each time it checks
and says that the card doesn't need wear leveling yet.  I
suppose that means nothing has slowed down yet.

This is one of the early technology cards that was rated at
something like 200,000 writes.  Or maybe it was 400,000.  I
forget.  Todays cards are rated at 4,000,000 writes.

I used this card heavily for a number of years and then about 2
or 3 years ago I moved it to the 200lx I keep by my desktop
computer to remember websites, passwords, software registration
codes, etc.  Also phone numbers.  I guess it's had only light to
moderate use since then.  As far as I know it's still perfect.

In recent years I do grit my teeth everytime I run wear.exe.
Someday it'll give me bad news. :)

As I understand it, when they do wear out they lose their
ability to write to the worn out sectors.  But they can still be
read and the rest of the card can still be written to.  So, with
a little tinkering with Norton's editor the card should still be
safely usable for years after it begins to wear out.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 11:41:16 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: CF inside HP200LX
In-Reply-To:  <16nIVM-1BkPEOC@fwd02.sul.t-online.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Tis could make the thaddeus memory upgrades somewhat obsolete. Flash mem =
is cheaper and all that really costs is the labor for installing the =
card internally. The flash mem is not as fast but, hey, if had a built =
in 512MB CF card, I would not care. I wonder if you can install a built =
in flash card and still use an external one? Has anyone yet laid claim =
to a 1-Gigbyte 200LX? I know the 1 gig cards are abundant now.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 09:59:44 -0700
Reply-To:     Michael Kopplin <kopplin@TECHNOIR.NU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Kopplin <kopplin@TECHNOIR.NU>
Subject:      Re: partitioned memory card in 200lx!
In-Reply-To:  <OF8258F035.6209969E-ON41256B81.0050D6B9@diamond.philips.com>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Tue, 19 Mar 2002, Radek Svagr wrote:

> Using MEMCARD.EXE which is in Olivetti Quaderno mininotebook
> (386 version). I made 2 partitions on this 512 kB SRAM card,
> one 255 and one 256 kB. Both were then acessible on 200lx as
> A: and B:. What is funny that Olivetti quaderno itself
> didn't recognize the second partition. But this could be due
> to wrong settings of its drivers.

What kind of partitions? Primary? Extended? Were they made
active?

Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 18 Mar 2002 19:24:43 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: GDB4WIN
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi PK

On Mon, 18 Mar 2002 23:47:00 +0530, pksharma <pksharma@CAL.VSNL.NET.IN> wrote:

> (daniel .. if you put it on super .. where do
> i send it .. so that you can do it ?)

to super@palmtop.net

But - is it the same as "GDBWIN"? That's already on SUPER....

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 17:34:19 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: atc for hplx?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Barry

On Tue, 19 Mar 2002 08:43:40 -0600, Barry <barry@FBTC.NET> wrote:

> If this isn't on the Super site it probably should be.  It's a
> fun game and it works perfectly on the 200lx.

As always, please send it to super at palmtop.net and I will put it on
SUPER.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 17:34:21 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: PostLx......
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Rolf

On Tue, 19 Mar 2002 10:01:00 -0500, Rolf Aronsson <flora@MINPOST.NU> wrote:

> Are there possibilities to extract readable files from
> Postlx' boxes? I mean a *.doc file for example.

I am not sure what you mean.
Do you mean converting Post/LX EMAILS to DOC format, or are you
speaking of email attachments in DOC format?

You can save attachments with "menu / file / save attachment".

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 19:06:10 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: CF inside HP200LX
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Daniel Hertrich wrote:
> If you use it for a non-multitasking system like the DOS on the 200LX,
> you can consider it to be immortal, if you buy a modern CF card.

There is another issue which I think will extend a CF's life.
DOS, starting with release 3 (I think), started selecting where
it would next write on a drive by searching for free space from
where it last looked.  Previously it always started from the
front of the drive.  The purpose of this change was to keep from
over writing deleted files right away and therefore allowing
un-erase to have a higher chance of success.

I remember reading about this change but I never looked into the
details to confirm it actually does as I described.  If it does
work this way it will assist in prolonging a flash card's life
by not always writing to those available sectors near the front
of the drive.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 21:18:35 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      [Fwd: Re: HPLX-L Digest - 16 Mar 2002 to 17 Mar 2002 (#2002-83)]
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Did it again, thanks John for telling me:

-------- Original Message --------
Subject: Re: HPLX-L Digest - 16 Mar 2002 to 17 Mar 2002 (#2002-83)
Date: Tue, 19 Mar 2002 00:48:10 +0100
From: Axel Berger <Axel-Berger@NexGo.De>
Reply-To: Axel.Berger@NexGo.De
To: j_vanderstel@JUNO.COM
References: <20020318.120249.-190297.0.j_vanderstel@juno.com>

> who don't actually have an LX

I won't advocate theft here - never have, never will. But does anyone here
have connections to anyone with a little authority at HP?
Neither the LX nor as far as I am aware the connectivity kit software is
sold anymore and there is absolutely no more support. So might they be
persuaded to do the decent thing and declare it abandonware?
To cite an example, GEM for DOS is so declared and the rights holders have
made it freely distributable - in that case including all sources that
could and can still be found.

I have a kit and like the ability to run 200 apps on the big games console
very much.

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 21:33:18 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      SUPER update
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

another SUPER update. The 200LX user's manual PDF file is now publicly
available. Check out the "new additions" page and find a few
interesting new things! :-)

GTX
daniel

* 03/19/02
IPCALC.PL zipped to avoid "internal server error" due to execution of pl
LXORAN added
HP200LX.PDF added (HP 200LX manual)
DOSGUI added
COM2LPT added
CZECH PACKAGE added
MY-MONEY.WK1 added
PDF2TXT added
SYSLOG "screenshot" added
TSBAT added
LXPIC updated to Version 7.1


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 15:38:32 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Rayovac Unveils New Quick Recharge Battery
In-Reply-To:  <HPLX-L%2002031912380154@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Rayovac Unveils New Quick Recharge Battery


http://story.news.yahoo.com/news?tmpl=3Dstory&u=3D/nm/20020319/tc_nm/manu=
facturing_rayovac_dc_1&cid=3D581

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 22:43:48 +0100
Reply-To:     Jan Brandt <jebrandt@XS4ALL.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jan Brandt <jebrandt@XS4ALL.NL>
Subject:      Re: IR connection to Ericsson T39
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

As far as I can see I am using a similar setup to yours. See my other note
in this pass.
I am not going to be using GPRS, just GSM.

Jan.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 22:37:58 +0100
Reply-To:     Jan Brandt <jebrandt@XS4ALL.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jan Brandt <jebrandt@XS4ALL.NL>
Subject:      Re: IR connection to Ericsson T39
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

> Okey. To track down the problem, please
> 1. read http://www.daniel-hertrich.de/mob_hplx carefully,
> 2. read http://www.daniel-hertrich.de/ir_dev carefully,
> 3. if you still have problems, please give us the www.cfg setup section
> you use.

Thanks Daniel. I had already studied your pages, but I still can't make it
work.
I include below the relevant parts of my www.cfg file.
It may very well be that I'm doing something fundamentally wrong with
www/lx. I used to use it together with Post/LX daily, but the last year or
so I haven't been using it and have forgotten all the setup details.
That's why I thought it might be a better idea to try to see if I can
establish an IrDA connection at all with my phone, and then move on to
www/lx once I get that working. So I downloaded the IR.EXE program and tried
it out, just to see if I can send an AT command or perhaps send or receive a
VCARD. But I can't make that work either, so perhaps my phone setup is
wrong, although I can't find other settings for the IR in the phone except
to switch it on or off.
The LX does see the phone, because it reports it is "Talking with T39", but
after a few seconds it reports "IrDA connection failed".

************** www.cfg start *******************
; Configuration file for WWW
; A. Garzotto, February 1998

; *** NOTE THAT LINES STARTING WITH ; ARE COMMENTS! ***

[Global]
Command=a:\wwwlx\HV.EXE
Cache=a:\wwwlx\cache
Setup=Ericsson
; uncomment to create a log file
;Log=a:\_DAT\WWW.LOG
UserName=Jan Brandt
RegID=************

[Setup]
Ericsson=Ericsson T39

[Script]
CIS_Script=Compuserve dial up
IBM_Script=IBM dial up script
Pipex_Script=PIPEX dial up script
CHAP_Script=PPP dial up using CHAP or PAP
ISP_SLIP_Script=Generic SLIP (needs to be modified)
Direct_Script=Direct line (needs to be modified)

[CHAP_Script]
e=Initializing modem
m=
s=\r
w=5 OK
e=Dialing
d=
s=\r
w=75 CONNECT

[Ericsson]
Port=-1
OmniGo=0
PPP=1
Modem=0
Baud=19200
My_IP=0.0.0.0
DNS_IP=0.0.0.0
DNS2_IP=0.0.0.0
Script=CHAP_Script
Login=***********
ModemInit=at+cbst=71,0,1;+chsn=1,1,0,4
Dial=atdt0102997505
Password=*********

************** www.cfg end *******************

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 23:05:20 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      [Fwd: Rejected posting to HPLX-L@UCONNVM.UCONN.EDU]
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

It didn't quite work out as I wanted it to, but it was not Going postal at
fault here. So scroll down for the good news and hurray for real
programmers, able to do it in less than gigahertz on hundreds of megabytes.

-------- Original Message --------
Subject: Rejected posting to HPLX-L@UCONNVM.UCONN.EDU
Date: Tue, 19 Mar 2002 16:55:49 -0500
From: "L-Soft list server at U. of Connecticut (1.8d)"
<LISTSERV@UConnVM.UConn.Edu>
To: Berger.mobil@WEB.DE

You  are   not  authorized  to  send   mail  to  the  HPLX-L   list  from
your Berger.mobil@WEB.DE account. You  might be authorized to send to  the
list from another of  your accounts,  or perhaps  when using  another mail
program which generates slightly  different addresses, but  LISTSERV has no
way  to associate this other account or address with yours. If you need
assistance or if you have any question regarding  the policy of the HPLX-L
list,  please contact the list owners: HPLX-L-request@UCONNVM.UCONN.EDU.

------------------------ Rejected message (30 lines)
--------------------------
Return-Path: <Berger.mobil@WEB.DE>
Received: from UCONNVM (NJE origin SMTP4@UCONNVM) by UCONNVM.UCONN.EDU
(LMail V1.2d/1.8d) with BSMTP id 4015; Tue, 19 Mar 2002 16:55:49 -0500
Received: from smtp.web.de [217.72.192.151] by UConnVM.UConn.Edu (IBM VM
SMTP Level 310) via TCP with SMTP ; Tue, 19 Mar 2002 16:55:48 EST
Received: from [212.211.74.53] (helo=212.211.74.53)
        by smtp.web.de with smtp (WEB.DE(Exim) 4.41 #2)
        id 16nRb6-0006CY-00
        for HPLX-L@UConnVM.UConn.Edu; Tue, 19 Mar 2002 22:56:50 +0100
From: Axel Berger <Berger.mobil@Web.De>
To: HPLX-L@UConnVM.UConn.Edu
Date: Tue, 19 Mar 2002 22:51:38 +0100 (MEZ)
X-Mailer: Goin' Postal - HP 100/200LX (v5.01) (Freeware)
Mime-Version: 1.0
Content-Type: text/plain; charset=iso-8859-1
Content-Transfer-Encoding: 8bit
Message-Id: <E16nRb6-0006CY-00@smtp.web.de>
Sender: Berger.mobil@Web.De

If this works, I have been able to set up Going Postal, use it over the GSM
network with CompuServe Classic and access the smtp server of my mail
provider (Web.De) by using the "smtp after pop" method. Which means nothing
less than that GP fulfils all my requirements and all my wishlist and is
hereby thoroughly recommended - not least for ease of setup.

Axel

--
This account is for mobile use only and messages will be retrieved
over a very expensive GSM connection. Please send short and pure
ASCII text only. Anything else to be sent to <Axel-Berger@NexGo.De>
and a short notification here, please.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 17:14:38 -0500
Reply-To:     palmtop@warp.nfld.net
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tom Rowsell <palmtop@WARP.NFLD.NET>
Subject:      Re: Nokia 3285

** Reply to note from Daniel Hertrich <daniel.hertrich@GMX.DE>         Tue, 19 Mar 2002 09:19:31 +0200

I read in a Nokia FAQ that the 3285 is supposed to work with Fonesync using the 6185 driver. Fonesync was bundled with
Microsoft Works Suite 2001. It looks to be as close to a "Phone Book Manager" as you can get. I can't get it to work
though. I have a "cheap" data cable for my 3285. I don't know how to get a PC (or the 200lx) to communicate with the
phone. Are there any commands that I could try (in Datacomm for example) to see if the cable is ok ?

Tom


> Hi Bob
>
> On Mon, 18 Mar 2002 22:45:50 -0800, bobv <bobv@SOS.NET> wrote:
>
> > Does anyone know of a phonebook manager for the HPLX (or even a windows
> > laptop) for maintining the Nokia 3285 phone book?
>
> There is no phone book manager.
> But there is Robot/LX and the robot script "phone.scr", which enables
> you to download or upload the whole phone book via WWW/LX and Robot/LX.
>
> So you can download it, maintain it with a text editor and upload it
> again. Or you can use the 200LX built-in phonebook as the "master"
> phone book and let my program PDB2PHN create a phone book which you can
> then upload to the phone. This is what I do.
>
> http://www.daniel-hertrich.de/pdb2x
>
> Or you can write an own phonebook maintenance program in the Robot/LX
> scripting language. Since all phnone book maintenance can be done voa
> AT commands through a cable or IrDA interface, this is theoretically
> possible.
>
> GTX
> daniel
>
> --
> http://www.daniel-hertrich.de/contact
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 19 Mar 2002 17:44:13 -0700
Reply-To:     Bob Christopher <bob@PALMTOP.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Christopher <bob@PALMTOP.COM>
Subject:      CF inside HP200LX
Mime-Version: 1.0
Content-Type: text/plain; charset=iso-8859-1
Content-Transfer-Encoding: 8bit

Since you're already tinkering under the hood :) see if you can
squeeze in a white LED that could illuminate the screen. Before
you ask, no I am not kidding. Maybe remove the blue Pocket
Quicken key (the least used key for most of us I'm sure) and
replace it with a small LED. Maybe power it with a single AA
housed in an adapter that could plug into the serial port. Just
wishing...

Bob
 Bob Christopher . Littleton, Colorado USA . bob@palmtop.com
  Palmtop Computers . Minox Cameras . All The Small Stuff

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 04:30:30 +0100
Reply-To:     Nathalie Bugeaud <tps-seti@WANADOO.FR>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nathalie Bugeaud <tps-seti@WANADOO.FR>
Subject:      Re: HPLX Users Database (from "Around the world" thread)
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

two HPLX-L digests in a row the same question was asked:

 >John J Vander Stel <j_vanderstel@JUNO.COM>:
 >Even better.. is there a simple standalone DOS based
 >utility freely available that can convert a GDB file to an ASCI file?

i hope i am not the <10th to give out this info:
 Module: GDBIO.EXE  Author: Craig Payne, Imports and exports quoted,
comma-delimited data to and from HP 100LX database files.

GDBIO is free and can import and export all fields to and from 100LX *.GDB
database files and phonebook (*.PDB) files.

Nathalie who dreamt she was stopped for speeding her LX

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 05:56:44 +0100
Reply-To:     hpstaber@COMPUSERVE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         HP Staber <hpstaber@COMPUSERVE.COM>
Subject:      Re: PostLx......
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Rolf Aronsson wrote:
>
> Are there possibilities to extract readable files from
> Postlx' boxes? I mean a *.doc file for example.

Hitting Shift-F10 will open a dialog with which you can save the whole
message (excl. attachments) into an ASCII textfile.

Ctrl-M opens a dialog to  save attachments.

HP Staber/Salzburg

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 05:48:06 +0000
Reply-To:     fjkaufman@WORLDNET.ATT.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "F. Kaufman" <fjkaufman@WORLDNET.ATT.NET>
Subject:      Re: partitioned memory card in 200lx!
Comments: To: radek.svagr@LGPHILIPS-DISPLAYS.COM
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

> Maybe I just discovered america but...
>
> I succesfully partitioned memory card so it was readable in 200lx as A: and B:
> BUT it was SRAM car not CF:-( I was not able to partition CF.

Interesting.  Maybe that's the secret - that the a: b: was intended for
the original SRAM cards which are different than the "newer" pcmcia
flash cards

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 05:48:16 +0000
Reply-To:     fjkaufman@WORLDNET.ATT.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "F. Kaufman" <fjkaufman@WORLDNET.ATT.NET>
Subject:      Re: partitioned memory card in 200lx!
Comments: To: Michael Kopplin <kopplin@TECHNOIR.NU>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

> On Tue, 19 Mar 2002, Radek Svagr wrote:
>
> > Using MEMCARD.EXE which is in Olivetti Quaderno mininotebook
> > (386 version). I made 2 partitions on this 512 kB SRAM card,
> > one 255 and one 256 kB. Both were then acessible on 200lx as
> > A: and B:. What is funny that Olivetti quaderno itself
> > didn't recognize the second partition. But this could be due
> > to wrong settings of its drivers.
>
> What kind of partitions? Primary? Extended? Were they made
> active?


Hmmm.  Wonder if the partitioning information could be moved (using
norton or similar) to a flash card.  But it is probably the nature of
sram versus flash that accounts for the working partitions.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 07:40:52 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      Re: partitioned memory card in 200lx!
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Nothing like this: create and format new partition - 100%? - NO - two times and that's it. No making active or primary/extended partition.

Radek






                      Michael Kopplin
                      <kopplin@TECHNOI             To:  HPLX-L@UConnVM.UConn.Edu
                      R.NU>                        cc:  (bcc: Radek Svagr/HRC/COMP/PHILIPS)
                      Sent by: HPLX                Subject:   Re: partitioned memory card in 200lx!
                      Mailing List
                      <HPLX-L@UConnVM.             Classification:
                      UConn.Edu>


                      2002-03-19 05:59
                      PM
                      Please respond
                      to Michael
                      Kopplin






On Tue, 19 Mar 2002, Radek Svagr wrote:

> Using MEMCARD.EXE which is in Olivetti Quaderno mininotebook
> (386 version). I made 2 partitions on this 512 kB SRAM card,
> one 255 and one 256 kB. Both were then acessible on 200lx as
> A: and B:. What is funny that Olivetti quaderno itself
> didn't recognize the second partition. But this could be due
> to wrong settings of its drivers.

What kind of partitions? Primary? Extended? Were they made
active?

Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 19:44:22 +1200
Reply-To:     Tony Hutchins <th@PARADISE.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Hutchins <th@PARADISE.NET.NZ>
Subject:      ANN: CLOCKS v5.0
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Wed, 20 Mar 2002 19:38:35 +1200 (NZT)

Now at http://homepages.paradise.net.nz/th

Interfaces better with WorldTime.
Does moon phases and equinoxes/solstices.
Finished now :)

- Tony

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 11:14:43 +0100
Reply-To:     Dzon <dzon@SOFTHOME.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dzon <dzon@SOFTHOME.NET>
Subject:      one-purpose switch speaker off
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

I was looking for something to let me not to disturb others with my loud
LX speaker. There probably are plenty of tools, but I like several
one-purpose programs rather than one big [it's unix :)]. If you feel like
me, open hex editor and create speakoff.com with:
B8 00 48 CD 15 B8 00 4C CD 21
and yep, no need of hardware hacking :)
You can create speakon.com changing the _first_ zero byte with 01 to 03
[03 is loudest].

--
                                  -Dzon
                             dzon@softhome.net

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 06:46:23 -0600
Reply-To:     Tim <palmtop@N-LINK.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tim <palmtop@N-LINK.COM>
Subject:      FLUFF: (really fluff) .... Did I overprice my eBay HDD?
In-Reply-To:  <200203200103.g2K13Qx17319@ez0.ezlink.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Hi all,

Since this is a list of "gadget experts," thought I'd ask if you folks
thought I overpriced this:

http://cgi.ebay.com/ws/eBayISAPI.dll?ViewItem&item=2010011617

I started it at $199 and am wondering why no one bid on it..... Maybe I
messed up the description(?).

OK, No more wasted bandwidth w/ this one.... Just wondering.

TIA,

--tim

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 06:39:30 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: partitioned memory card in 200lx!
MIME-Version: 1.0
Content-Type: text/plain

MEMCARD requires the Microsoft Flash File System Driver (MS-FLASH.SYS) in
order to work with Flash cards. (This information is in the text in MEMCARD,
which can be read using Notepad on an Windows machine, or Debug or other
programs under DOS. I use DR.COM, an old PC Magazine file utility.) MS-FLASH
probably needs some other card and/or socket drivers to work, but I haven't
tried it out you. BTW, I was able to download an OB450 version of MEMCARD
from http://24.237.160.4/files/omnibook/ob425/Software/ROMcard/. I also have
versions of MEMCARD and MS-FLASH from a Toshiba laptop I also have.

MEMCARD looks a lot like FDISK when you run it: you can view, change or
delete partitions, which can be MS-DOS or MS-FLASH. On an SRAM card, you are
limited to MS-DOS partitions.

If I have time today, I plan to try out MS-FLASH, as well as some Phoenix
Card Manager software from the Toshiba. The PCM suite includes an ATA card
driver that looks promising.

Bob

-----Original Message-----
From: Radek Svagr [mailto:radek.svagr@LGPHILIPS-DISPLAYS.COM]
Sent: Tuesday, March 19, 2002 8:53 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: partitioned memory card in 200lx!


Using MEMCARD.EXE which is in Olivetti Quaderno mininotebook (386 version).
I made 2 partitions on this 512 kB SRAM card, one 255 and one 256 kB.
Both were then acessible on 200lx as A: and B:. What is funny that Olivetti
quaderno itself didn't recognize the second partition. But this could be due
to wrong settings of its drivers.

Then I tried the same with CF card, but MEMCARD.EXE refused to partition it.

Radek







                      "Feldman, Robert"
                      <Robert_Feldman@JDE             To:
HPLX-L@UConnVM.UConn.Edu
                      DWARDS.COM>                     cc:  (bcc: Radek
Svagr/HRC/COMP/PHILIPS)
                      Sent by: HPLX                   Subject:   Re:
partitioned memory card in 200lx!
                      Mailing List
                      <HPLX-L@UConnVM.UCo             Classification:
                      nn.Edu>


                      2002-03-19 03:20 PM
                      Please respond to
                      "Feldman, Robert"






HOW????

-----Original Message-----
From: Radek Svagr [mailto:radek.svagr@LGPHILIPS-DISPLAYS.COM]
Sent: Tuesday, March 19, 2002 1:03 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: partitioned memory card in 200lx!


Maybe I just discovered america but...

I succesfully partitioned memory card so it was readable in 200lx as A: and
B:
BUT it was SRAM car not CF:-( I was not able to partition CF.

Radek

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 15:26:50 +0100
Reply-To:     Michel Bel <michel.bel@ZONNET.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michel Bel <michel.bel@ZONNET.NL>
Subject:      Re: partitioned memory card in 200lx!
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Subject: Re: partitioned memory card in 200lx!


> MEMCARD requires the Microsoft Flash File System Driver (MS-FLASH.SYS) in
> order to work with Flash cards. (This information is in the text in
MEMCARD,
> which can be read using Notepad on an Windows machine, or Debug or other


Memcard (and MS-FLASH) expects 'Linear' cards, e.g. either Sram or Flash
disk with a simple linear adressing scheme. It does not expect, nor work on
ATA cards, and the LX uses different drivers to address these cards. ATA
cards use a PCMCIA ATA driver, and copies sectors to buffer memory, linear
cards are mapped into memory ( a bit like EMS), and directly addressed,
almost exactly like the internal C: RAM disk. Totally different drivers.
Hence, if the 'memory disk'driver can map/page internal memory as C:, and a
Sram partition as A:, it may very easily map another Sram partition as B - .
This is totally different from ATA mapping.

Michel
- MS-Flash if you want older addressing, TFFS for newer drivers.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 08:47:00 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: partitioned memory card in 200lx!
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

Unfortunately, the Phoenix ATA driver (PCMATA.SYS) from my Toshiba requires
at least an 80286.

Using CSMAPPER.SYS and CARDDRV.EXE in my CONFIG.SYS, I was able to get
MEMCARD to wipe out the partition on a 10MB SunDisk card (which is some
progress, I guess), but I could not get MEMCARD to partition the flash card.

Anyone know what the available switches are for the built-in FDISK100?
"FDISK100 /?" gives a terse message, and other things I have tried, such as
"/2" give an "Invalid switch" message. The standard FDISK from an MS-DOS 5.0
disk I have does not see any fixed disks on the 200LX, so it can't be used.

-----Original Message-----
From: Michel Bel [mailto:michel.bel@ZONNET.NL]
Sent: Wednesday, March 20, 2002 8:27 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: partitioned memory card in 200lx!


Subject: Re: partitioned memory card in 200lx!


> MEMCARD requires the Microsoft Flash File System Driver (MS-FLASH.SYS) in
> order to work with Flash cards. (This information is in the text in
MEMCARD,
> which can be read using Notepad on an Windows machine, or Debug or other


Memcard (and MS-FLASH) expects 'Linear' cards, e.g. either Sram or Flash
disk with a simple linear adressing scheme. It does not expect, nor work on
ATA cards, and the LX uses different drivers to address these cards. ATA
cards use a PCMCIA ATA driver, <snip>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 07:59:11 -0600
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: D&A ABC-LX and Kodak 1600mAH NiMH batteries
Comments: To: Philip Pemberton <philpem@ZETNET.CO.UK>
In-Reply-To:  <01a301c1cac5$1d710a00$0100005a@phoenix>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Hi Philip (and others):

Re ABC/LX parameters:  Just enter the highest value you can. The value is
used to generate a "reasonable" set of starting values, and it is CERTAINLY
not cast in stone, rock, or any other hard mineral. I believe this is also
explained in the manual (I am not sure any more...)

Regarding "Autotune": This is an APPROXIMATE process - just _something_ to
START with. You can BYPASS it altogether and use other values which people
have had reasonable experiences with and you will still get good results
even without autotuning.

E.g. Stop charging when voltage hits 2.95V, or when you charged 15 hours,
or when the voltage has not changed in 3 hours. Start charging at 2.50V (my
favorite. You can go lower, but that means you deplete the battery more
before beginning to charge it up again.)

If you find that these values do not give optimal results (whatever
"optimal" is!) then tweak these values and learn from your own experience
which is the best setting for YOUR set of batteries (did anyone mention
that batteries change? Any pair can display VERY different behaviour from
another pair! And they even change over time!)

Lastly, so many people perceive that ABC/LX is TOTALLY accurate and that it
can produce 100% accurate results with batteries.  That is not so.  People
sometimes think this program will make their batteries work 100%
consistently from charge cycle to another. That is not so - the batteries
are chemical "factories" and they are affected by so many variables: Temp,
rate of discharge, manufacturing inconsistencies, and so on.  And then I
have this "pet" gripe: I see people spend hours on research (I do not know
that you did this). They will measure batteries: charging, discharging.
They will devise scientific-level experiments and demand accuracy of 1
minute per whatever. They spend huge amounts of time chasing another peak
voltage, another 5 minutes per discharge cycle. In truth: We designed
ABC/LX so it REMOVES all this nonsensical waste of time (Sorry Battery
researchers - I really feel that this pursuit of another minute, or even 20
is simply a waste.)

The point of the program is to give you a tool that will do your work for
you. It will sit in the background and monitor the status of the battery.
When it deems that recharging is needed, it will do so.  Otherwise nothing.
It will provide you with GOOD OR BETTER results. Sometimes even EXCELLENT.
But mostly it will give you good service and save you time and take out one
item OUT OF YOUR LIFE that you need to worry about.  All you need to do is
monitor it for awhile, decide what is a reasonable set of parameters, and
let go! Maybe once every 6 months re-visit your parameters, watch the
battery for awhile and decide if a change is needed.  Consider all this
time NOT SPENT on tweaking the parameters daily, or several times per day
as our gift to you - a valuable gift of time! <G>

Take the dog for a walk on the beach, maybe read a story to your child, or
take you beloved to a concert, a movie, or just a walk.

So this is how to use ABC/LX: Monitor briefly to see that you get
reasonable time from the batteries. If it is 11hrs and 10 minutes, or 10hrs
57 minutes is just not worth tracking in detail (IMHO). Set up the
parameters (or use the values above). Use your palmtop in good health. When
you see an adapter, plug it in. ABC/LX will decide for you if it should be
actively charging or not. You can use your time to DO WORK on the palmtop.


    Avi


At 3/13/02 03:27 PM, Phillip Pemberton wrote:
>Hi,
>     I've just put a pair of 1600mAH Kodak "PhotoLife" NiMHs in my 700LX and
>I'm having some trouble getting ABC-LX to let me enter the battery capacity.
>I can enter anything up to 1200mAH fine, but if I try and enter 1600, ABC-LX
>politely tells me to try again...
>
>I know some D&A reps frequent HPLX-L, so can any of them (or anyone else for
>that matter) please tell me how to fix this so I can use my NiMHs? It would
>be a great shame to have to use my old Uniross 700mAH NiCads again,
>especially when I've got these NiMHs...
>
>Thanks.
>--
>Phil.
>philpem@bigfoot.com
>http://www.philpem.btinternet.co.uk/
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 08:11:23 -0600
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: Fluff: Conclusions
Comments: To: Joseph.Buford@HSC.COM
In-Reply-To:  <OF4270440F.2EEFCBDA-ON88256B7F.00000CBF@hughes.com>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

I'd like to hear you recite some poems in French! <VBG>

    Avi
(from Cool Minnesota - today 20 Mar, it is lovely skies and no snow, but
plenty on unmelted stuff on the side of streets and on Lake O'Leary - ask
me if you do not know about Lake O'Leary.)

At 3/16/02 06:05 PM, you wrote:
>Nathalie,
>
> >Eat & drink what you like. It's speaking English that kills
>you. :)
>
>Perhaps I should learn french :-)
>
>Joe
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 09:09:59 -0600
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: Fluff: Spamfilter
Comments: To: TomSalwasser@COMPUSERVE.COM
In-Reply-To:  <001a01c1cc20$7e74fb20$1f98c0d8@oemcomputer>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Tried it too today. It seems to work well, and can even fire up my Eudora
(and presumably even my Post/LX on the desktop. My Palmtop broke
physically) two-tree weeks ago and I am reduced to Eudora on the desktop
(which I like a lot.) (I will eventually also set up POST/LX on the desktop
for some fast email runs.

What I have been doing in Eudora is very strong filtering: If any header
contains "mortgage" or "insurance" or "domain names" etc - then delete that
email item on the server, and the copy on the machine move to folder
"??TRASH??".

There are several other such very broad filters, such as words used by
porno sites, casinos, viagra and other pharmaceuticals dealers, and things
like "DVD copy", "targeted mailing", and so on.

Of the 200 emails daily received in all the email accounts, about 150-190
are trash. They end up in the ??TRASH?? folder.

I use the ??TRASH?? folder as my last resort: I go over it fairly quickly
once a day in case a real email got filtered by mistake, then I delete the
entire batch at once.

This seems to work out well to stave off the assault of spam without adding
much time.

I have long been looking at some way to send back an indication to the
spammer that my email address is a dead one, and MAILWASHER seems to be the
tool for this. I just wonder if that bounce somehow reveals that it was
created by Mailwasher.

I like that it lets me check emails up front, even see the whole text, if
necessary.

Nice tool. Thanks for the tip.

    Avi (from sunny, really, very sunny Minnesota)


At 3/15/02 06:54 AM, you wrote:
>I'm using www.mailwasher.net. It bounces mail as having an invalid email
>address. I don't know if it will reduce my spam but it makes me feel good
>when I
>bounce an email!
>
>Regards,
>Tom Salwasser
>
>
> >
> > > Remote host said: 552 Message identified as spam....
> > > Return-Path: <cpt_kludge@yahoo.com>
> >
> > Bad scheme: That tells the spammers "This is a valid and read address - try
> > again." which is not what I want them to get.
> >
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 09:18:09 -0600
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: FW: 200lx ethernet adapter
Comments: To: Theodore Heise <theise@NETINS.NET>
In-Reply-To:  <Pine.OSF.4.33.0203171653130.4161-100000@worf.netins.net>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

At 3/17/02 04:57 PM, you wrote:
>On Sun, 17 Mar 2002, ABCS INC. wrote:
>
> > I used the Ruggedized Low Power Ethernet PC Card Solution part #EA0914-337.
>
>Thanks for the report!
>
>Have you gotten a sense of the power requirements yet?

I did not use the card, but checked the Website. They claim 19mW when
active, and the general gist is that these cards are very low power cards.
Looks interesting.




>For example,
>when you power on the LX after inserting the card do you get the
>message "CARD BATTERY LOW - Press ESC"?
>
>--
>Ted Heise      <theise@netins.net>      West Lafayette, IN, USA
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 09:21:37 -0600
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: FW: 200lx ethernet adapter
Comments: To: kwmiller@azbcs.com
In-Reply-To:  <BLENKJJKIJHGOGCHGNNNEEGAENAA.kwmiller@azbcs.com>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Thank you for the info! Can you kindly also elaborate more how you set up
the Palmtop and the order of the software etc. Also, what did you have to
do on the connecting component in the network? Did you connect to a
desktop? What did you do there?

I hope this is not too much to ask.

Avi

At 3/17/02 01:52 PM, kwmiller@azbcs.com wrote:
>Thanks for all the reply's to my request for a source for Ethernet cards.  I
>can report that I now have a new functioning 10mbit ethernet card working on
>my 200lx thanks to Keith Grider from the list.  Here is a link to the
>product information if anyone is curious.
>
>Ethernet Card:
>http://www.socketcom.com/product/ethernet_card.htm
>
>I used the Ruggedized Low Power Ethernet PC Card Solution part #EA0914-337.
>I used this one due to the mobile nature of the 200lx so I would not have to
>buy a dongle when it breaks.  This card is ALSO CF compatible and uses a
>PCMCIA adapter to work on PCMCIA machines.  The PCMCIA adapter ships with
>these cards!  The card costs $106+shipping from CDW.COM
>
>http://www.cdw.com/shop/products/default.asp?EDC=323951
>
>The following drivers are used to operate the card.
>
>LXCIC     <-- card services
>LXEN2216  <-- ne2000 compatible driver
>LXTCP     <-- tcpip network stack
>WWW/LX    <-- web browser
>
>I also use LXFTP, LXPING for network troubleshooting.
>
>Thanks for all the help!
>
>Kevin Miller
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 10:26:33 -0600
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: mail web interface
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
In-Reply-To:  <HPLX-L%2002030305250211@UCONNVM.UCONN.EDU>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

It does not work because of other reasons. It seems to rely on some
information to be passed from the Palmtop (and I think it is some info it
places in cookies!) and thus it can show the list of emails, but fails on
reading them for display :-(  ...

Sorry I brought this up so late....

   Avi



At 3/3/02 05:27 AM, Daniel Hertrich wrote:
>Hi friends
>
>I have found a universal web interface for email which might work on
>the palmtop.
>It is a derivate of the service mail2web.com.
>
>Go to www.mail2pda.com and have a look. I just tried it with Netscape,
>and the pages look as they could be displayed by HV. Only the URLs are
>very long and thus might limit the usablilty.
>
>Maybe Arachne/LX will support long URLs.
>
>GTX
>daniel
>
>--
>http://www.daniel-hertrich.de/contact
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 10:41:53 -0600
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: PostLx......
Comments: To: flora@MINPOST.NU
In-Reply-To:  <HPLX-L%2002031910010046@UCONNVM.UCONN.EDU>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Rolf,

The files where messages andattachments are stored (such as mail.i) are
essentially readable because they are ASCII. However, there is a separator
between messages containing binary characters.

I routinely open the .I files in editors such as PE and MEMO, as well as
Word, Notepad, etc.

I am not sure what the last part is - what do you mean extracting .DOC
files from the message files? If you mean attachments, then yes, just press
CTRL-M and the attachment will be saved as the file name it was attached
with and you can then process it with whatever opens .DOC files. (I presume
you do not mean MEMO-style .DOC files.) There is a program called VIEW
which will open .DOC files and strip the formatting and just show the
contents and it can be directly activated to view .DOC files - see the
www.dasoft.com webpage for the trick on this.

If I made too many assumptions and missed your meaning, let me know.

    Avi (from sunny, really, Minnesota!)
At 3/19/02 09:01 AM, you wrote:
>17-Mar-02
>
>Hi, all!
>
>Are there possibilities to extract readable files from
>Postlx' boxes? I mean a *.doc file for example.
>
>Thanks for this HPLX-community, going over the world! So
>many tips and trix, so many themes.........
>
>
>Regards Rolf Aronsson, Sweden.
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 18:04:45 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: partitioned memory card in 200lx!
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

another idea on this topic:
ATA (compact) flash cards can be accessed via a, IDE-to-PCMCIA (or -CF)
adapter. So, they are acting just as a hard disk.
This is done for example in the earlier Omnibooks (300-600).
Does the hornet chip in the 200LX have an IDE interface?  8-)

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 11:17:48 -0600
Reply-To:     Tim Kelley <tpkelley@HOTMAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tim Kelley <tpkelley@HOTMAIL.COM>
Subject:      Re: FW: 200lx ethernet adapter
Mime-Version: 1.0
Content-Type: text/plain; format=flowed

I looked at the website as well and saw they have a low power wireless card
as well!  Perhaps this would be a wireless option for the HP.
Tim K

>From: A Meshar <hplxmail@YAHOO.COM>
>Reply-To: hplxmail@YAHOO.COM
>To: HPLX-L@UConnVM.UConn.Edu
>Subject: Re: FW: 200lx ethernet adapter
>Date: Wed, 20 Mar 2002 09:18:09 -0600
>
>At 3/17/02 04:57 PM, you wrote:
>>On Sun, 17 Mar 2002, ABCS INC. wrote:
>>
>> > I used the Ruggedized Low Power Ethernet PC Card Solution part
>>#EA0914-337.
>>
>>Thanks for the report!
>>
>>Have you gotten a sense of the power requirements yet?
>
>I did not use the card, but checked the Website. They claim 19mW when
>active, and the general gist is that these cards are very low power cards.
>Looks interesting.
>
>
>
>
>>For example,
>>when you power on the LX after inserting the card do you get the
>>message "CARD BATTERY LOW - Press ESC"?
>>
>>--
>>Ted Heise      <theise@netins.net>      West Lafayette, IN, USA
>>
>>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>
>_________________________________________________________
>Do You Yahoo!?
>Get your free @yahoo.com address at http://mail.yahoo.com
>
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>




_________________________________________________________________
Chat with friends online, try MSN Messenger: http://messenger.msn.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 11:25:55 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: atc for hplx?
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Dzon wrote:
> I've found some, check out
http://168.216.219.18/pub/IBM/MegaGames3/ for
> some of good old things. But none of the two atc's there is
what I'm
> looking for. Anyway, try atc2.zip, run atc 1 4 to get best
graph mode on
> LX. Cool thing, but the airplanes's number is limited even in
registered
> version :(

At that site, ATC10 is the one I was using on my 200lx.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 12:34:05 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: FLUFF: (really fluff) .... Did I overprice my eBay HDD?
Comments: To: Tim <palmtop@N-LINK.COM>
In-Reply-To:  <000b01c1d00d$3e92b9c0$6401a8c0@gadgetbase>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

I guess that all depends... supply and demand and all that jazz. You'll =
know at the end of your auction.=20

A lot of people don't like to place initial bids on high priced items =
until the auction is winding down. I personally do not bid on things =
until the last 24 hours. I also sometimes use a service like Esnipe to =
place last second bids. This prevents you from falling into the bidding =
war trap. I sit there and decide how much I am willing to pay then tell =
Esnipe to bid that amount a few seconds before the auction ends. If it =
was not high enough then 'so be it'. It's better to stick to the =
original 'how much is it worth to me' mentality than to overpay.

Maybe someone wills snipe your auction at the end.

BTW: Read the ebay 'selling tips' secion. There they say that it's =
better to list your item with a low price and place a reserve on it as =
the low price will attract attention (and hopefully ignite a bidding =
war... it's good for the seller, after all.).=20


> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@uconnvm.uconn.edu]On Behalf Of
> Tim
> Sent: Wednesday, March 20, 2002 7:46 AM
> To: HPLX-L@uconnvm.uconn.edu
> Subject: FLUFF: (really fluff) .... Did I overprice my eBay HDD?
>=20
>=20
> Hi all,
>=20
> Since this is a list of "gadget experts," thought I'd ask if you folks
> thought I overpriced this:
>=20
> http://cgi.ebay.com/ws/eBayISAPI.dll?ViewItem&item=3D2010011617
>=20
> I started it at $199 and am wondering why no one bid on it..... Maybe =
I
> messed up the description(?).
>=20
> OK, No more wasted bandwidth w/ this one.... Just wondering.
>=20
> TIA,
>=20
> --tim
>=20
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 09:32:58 -0800
Reply-To:     Sandra Wambold <wambold@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Sandra Wambold <wambold@POBOX.COM>
Subject:      Want a Lotus 1-2-3 manual?
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

I have a Lotus-1-2-3 Manual, Release 2.01 that I'm willing to give to
anyone who'll pay shipping on it.  It has reference, tutorial, getting
started, quick reference and the original 5.25" disks.  (It'll ship
from San Jose, California)

-sew

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 22:10:59 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Fw: Re: CF inside HP200LX
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

-----Original Message-----
From: pksharma <pksharma@cal.vsnl.net.in>
To: Russel Brooks <rlbrooks@POBOX.COM>
Date: Wednesday, March 20, 2002 8:32 AM
Subject: Re: Re: CF inside HP200LX


>
>-----Original Message-----
>From: Russel Brooks <rlbrooks@POBOX.COM>
>To: HPLX-L@UConnVM.UConn.Edu <HPLX-L@UConnVM.UConn.Edu>
>Date: Wednesday, March 20, 2002 2:24 AM
>Subject: Re: CF inside HP200LX
>
>
>>DOS, starting with release 3 (I think), started selecting where
>>it would next write on a drive by searching for free space from
>>where it last looked.  Previously it always started from the
>>front of the drive.  The purpose of this change was to keep from
>>over writing deleted files right away and therefore allowing
>>un-erase to have a higher chance of success.
>>
>>I remember reading about this change but I never looked into the
>>details to confirm it actually does as I described.
>
>
>yes .. it does .. all later versions of dos use the unallocated
>clusters of the harddisk .. and don't overwrite the 'once
>used' clusters .. this i know from the experience of reading
>clusters/sectors/physical areas of the hard disk umpteen
>number of times (including MBR and BRs, Dir area and Fat1
>Fat2 areas) .. only when the harddisk becomes full .. it starts
>'overwriting' .. meaning re alloting those 'already' used
>sectors/clusters for writing data !
>
>But .. and this is important .. a check needs to be done for
>floppies .. very easy for all .. not for me .. i don't use floppies
>at all .. intentionally .. avoid lots of virus problems from my
>family and staff (intensive gamers) ..
>
>one could .. format a new floppy .. write a small file .. delete
>it .. and write another small file .. and THEN .. check the
>floppy areas .. even with the dos debug .. if one knows exactly
>where to look, of course !
>
>if the cf is not going to be A or B .. the above experiment
>is not at all necessary !
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 14:25:32 -0500
Reply-To:     wally@theblackmoor.net
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Walter Francis <wally@THEBLACKMOOR.NET>
Organization: Linux is organization enough..
Subject:      Re: Nokia 3360
Comments: To: hplxmail@YAHOO.COM
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii; format=flowed
Content-Transfer-Encoding: 7bit

A Meshar wrote:


> Except: 3360 has an internal modem, and 8260 does not. 3360
> has an IR and 8260 does not.
>
> My very basic question is if anyone used 3360 with WWW/LX over the IR.

I'm a little behind getting back to you, but I have connected to my ISP
using my 3360 in Linux, but it would connect and never get past the
authentication stage.  So I have something odd software wise.

My copy of WWW/LX doesn't do IRDA so I can't say about it, but using ir.exe
I can definately talk to the phone, make a connection, etc..

I hope your 3360 will have a newer firmware than mine, I have trouble with
my phone locking up sometimes..  Mostly when I'm playing games tho.  :)
Happens occationally in WAP too.  BTW, whoever designed the interface to WAP
was an idiot, it's SO SLOW to browse around and such.  Oh well.

--
Walter Francis
http://theblackmoor.net                  Powered by Red Hat Linux 7.2

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 07:51:35 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      Re: partitioned memory card in 200lx!
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

If anyone wants to play with it... I can send memcard.exe. It is also available somewhere on Olivetti quaderno pages, but I don't know where.
Please note that I used the one form Quaderno C33 /386 version /not from V30 /xt version/ - this one hanged my 200lx.
I also experimented with card enabler from Quaderno. It saw two sockets and one card in 200lx, when card was installed.


Radek




                      "F. Kaufman"
                      <fjkaufman@WORLDN             To:  HPLX-L@UConnVM.UConn.Edu
                      ET.ATT.NET>                   cc:  (bcc: Radek Svagr/HRC/COMP/PHILIPS)
                      Sent by: HPLX                 Subject:   Re: partitioned memory card in 200lx!
                      Mailing List
                      <HPLX-L@UConnVM.U             Classification:
                      Conn.Edu>


                      2002-03-20 06:48
                      AM
                      Please respond to
                      fjkaufman






> On Tue, 19 Mar 2002, Radek Svagr wrote:
>
> > Using MEMCARD.EXE which is in Olivetti Quaderno mininotebook
> > (386 version). I made 2 partitions on this 512 kB SRAM card,
> > one 255 and one 256 kB. Both were then acessible on 200lx as
> > A: and B:. What is funny that Olivetti quaderno itself
> > didn't recognize the second partition. But this could be due
> > to wrong settings of its drivers.
>
> What kind of partitions? Primary? Extended? Were they made
> active?


Hmmm.  Wonder if the partitioning information could be moved (using
norton or similar) to a flash card.  But it is probably the nature of
sram versus flash that accounts for the working partitions.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 14:36:39 -0500
Reply-To:     amusse@mediaim.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Alfredo Musse T." <amusse@MEDIAIM.COM>
Subject:      Owner's Manual HP200LX
In-Reply-To:  <3C98E22C.2010907@theblackmoor.net>
MIME-Version: 1.0
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: 7bit

Hi,

Does anyone knows where I can download the Owner's or User's Manual for the
HP200LX ??

Thanks in advance


Alfredo Musse T.
media improvement - solutions for the digital world
Tel. (511) 562-0216
amusse@mediaim.com
http://www.mediaim.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 21:04:08 +0100
Reply-To:     furlan@gmx.net
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Dr. Werner Furlan" <furlan@GMX.NET>
Organization: OE9FWV
Subject:      Motorola Timeport T 260 and GPRS connection
MIME-Version: 1.0
Content-type: text/plain; charset=US-ASCII
Content-transfer-encoding: 7BIT

I am still trying to find out the right parameters for the Motorola
Timeport T260 to use it with the HP200 and IRDA.
What I am looking for now is an explanation of the Modem Init String.
In Martin Bergvill's example for the Ericson phone there was the
line:
ModemInit=AT+cgdcont=1,"IP","internet"

This line is maybe also valid for the Motorola Phone. What means
"IP", "internet" ?

Is there anybody on the list who got this phone to connect over GPRS?

cheers,
Werner

--
Powered by Pegasus Mail - free at <http://www.pmail.com>
Homepage: <http://www.qsl.net/oe9fwv>
SMS:<+436646340014@text.mobilkom.at>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 13:12:34 -0700
Reply-To:     Donald Puscher <dpuscher@QUALCOMM.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Donald Puscher <dpuscher@QUALCOMM.COM>
Subject:      OT: Windows command prompt tab completion tip
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Thought there might be some folks who would benefit from this tip from a
coworker. I haven't tried it but I haven't heard anyone complain about it
either :) As always when working with the Windows registry, be careful and
make a backup first!

Don

============TIP========================
Do you ever wish the command prompt in Windows could perform completion
when you hit tab, similar to many UNIX shells?  Well, you can.  Here's how:

Run the registry editor:
Start->Run->regedit

Edit the following key:
My Computer\HKEY_CURRENT_USER\Software\Microsoft\Command
Processor\CompletionChar

Set the key value to 9 (ASCII for TAB).

exit the registry editor and restart your command prompt window(s).  The
setting will take effect when the program is started.

This only works for Windows NT and Windows 2000.  I haven't tried ME or XP.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 15:37:13 -0500
Reply-To:     Martin Bergvill <hplx@BERGVILL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Martin Bergvill <hplx@BERGVILL.COM>
Subject:      Re: Motorola Timeport T 260 and GPRS connection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Wed, 20 Mar 2002 21:04:08 +0100, Dr. Werner Furlan wrote:

> I am still trying to find out the right parameters for the Motorola
> Timeport T260 to use it with the HP200 and IRDA.
> What I am looking for now is an explanation of the Modem Init String.
> In Martin Bergvill's example for the Ericson phone there was the
> line:
> ModemInit=AT+cgdcont=1,"IP","internet"
>
> This line is maybe also valid for the Motorola Phone. What means
> "IP", "internet" ?

Well here is What I know about this:

AT+CGDCONT =this is a code to configure CID(Context identification)
parameters in your phone.

=1 means that you choose account 1 in your phone.

"IP" is the Packet data protocol. It tells what type of protocol will
be used. Internet protocol)

Not sure about the "internet"

AT+CGDCONT=<CID>,<PDP_TYPE>,<APN>, PDP_ADDR>

But it is he Apn I think that you indicate with "Internet"?

PDP_ADDR is not used when operator gives you the ip address.


> Is there anybody on the list who got this phone to connect over GPRS?

You should probably check out:

<http:/telenormobil.no/kundeservice/teknisk/brukerveiledning/oppsettgprs/motorolat260/index.jsp>

You can probably get some help ther eeventhough it is in norwegians.

Hope this helped

Regards

--
Martin Bergvill ,Narvik Norway

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 22:18:55 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: FW: 200lx ethernet adapter
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Avi

On Wed, 20 Mar 2002 09:18:09 -0600, A Meshar <hplxmail@YAHOO.COM> wrote:

> I did not use the card, but checked the Website. They claim 19mW when
> active, and the general gist is that these cards are very low power cards.
> Looks interesting.

milli WATTs? not milli Amperes?

19mW would mean only 3.8mA at 5V. That's almost nothing! The 150mA
limit at the PCMCIA slot would allow to drive 40 of these cards
simultanously!

So, if it would ever be possible to build one of these cards directly
into the LX (using PCMCIA socket 2), it would at least never be a big
power-related problem. :-)

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 22:18:56 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: FW: 200lx ethernet adapter
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Tim

On Wed, 20 Mar 2002 11:17:48 -0600, Tim Kelley <tpkelley@HOTMAIL.COM> wrote:

> I looked at the website as well and saw they have a low power wireless card
> as well!  Perhaps this would be a wireless option for the HP.
> Tim K

How much exactly?

If it follows the full 802.11b standard (wireless LAN), it cannot be so
little power consumption that it can be driven in the LX (because the
TX power of 802.11b is already higher than the power the LX can
provide). But if this card implements something like a "light" 802.11b,
it could be interesting!
Or, is it another technology, such as Bluetooth?

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 22:18:57 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Owner's Manual HP200LX
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Alfredo

On Wed, 20 Mar 2002 14:36:39 -0500, "Alfredo Musse T." <amusse@MEDIAIM.COM> wrote:

> Does anyone knows where I can download the Owner's or User's Manual for the
> HP200LX ??

Just yesterday I announced that it is now available in the SUPER
archive. (http://www.palmtop.net).

http://www.palmtop.net/cgi-bin/query.pl?Query=hp200lx.zip

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 14:25:53 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: FW: 200lx ethernet adapter
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

19 mA, 63mW

-----Original Message-----
From: Daniel Hertrich [mailto:daniel.hertrich@GMX.DE]
Sent: Wednesday, March 20, 2002 2:19 PM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: FW: 200lx ethernet adapter


Hi Avi

On Wed, 20 Mar 2002 09:18:09 -0600, A Meshar <hplxmail@YAHOO.COM> wrote:

> I did not use the card, but checked the Website. They claim 19mW when
> active, and the general gist is that these cards are very low power cards.
> Looks interesting.

milli WATTs? not milli Amperes?

19mW would mean only 3.8mA at 5V. That's almost nothing! The 150mA
limit at the PCMCIA slot would allow to drive 40 of these cards
simultanously!

So, if it would ever be possible to build one of these cards directly
into the LX (using PCMCIA socket 2), it would at least never be a big
power-related problem. :-)

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 22:57:08 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Putting atc on super
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Barry,
to the list, because peronal mail to you got bounced:

=============

Hi Barry

On Wed, 20 Mar 2002 11:33:07 -0600, "Barry" <barry@fbtc.net> wrote:

> How do I upload something to Super?  It's been years since I did
> and it's all changed.
>

Please send it to super@palmtop.net. Then I'll get it (and also Ian,
David and all the other SUPER people. I'll then add it to the next
SUPER update.

Please provide program name, version, author, author's email, and a
short description.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 22:08:15 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: CF inside HP200LX
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Bob Christopher wrote:
>  Maybe remove the blue Pocket
> Quicken key (the least used key for most of us I'm sure) and

I use to agree with you but not any more.  I've stopped using my
desktop Quicken and now use Pocket Quicken only.  I wish I'd
done this years ago when I first got my LX.

Blue keys I don't use:  Filer, Memo, Lotus123

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 22:08:18 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: one-purpose switch speaker off
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Dzon wrote:
> I was looking for something to let me not to disturb others with my loud
> LX speaker. There probably are plenty of tools, but I like several

I use LXPRO.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 17:23:27 -0500
Reply-To:     Bob Penick <bnj@MYREALBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Penick <bnj@MYREALBOX.COM>
Subject:      Fluff  Re: CF inside HP200LX
Comments: To: Russel Brooks <rlbrooks@POBOX.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

----- Original Message -----
From: "Russel Brooks"
Sent: Wednesday, March 20, 2002 5:08 PM
Subject: Re: CF inside HP200LX


> I use to agree with you but not any more.  I've stopped using my
> desktop Quicken and now use Pocket Quicken only.  I wish I'd
> done this years ago when I first got my LX.
>
I Completely agree with you here Russ.

> Blue keys I don't use:  Filer, Memo, Lotus123
>
Blue keys I don't use:   NONE!!!
Don't think we agree on this one though.
Later,
bob

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 12:39:35 -0800
Reply-To:     bobv <bobv@SOS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         bobv <bobv@SOS.NET>
Subject:      Re: Nokia 3285
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Thanks Daniel

Bob

---------------------
Hi Bob

On Mon, 18 Mar 2002 22:45:50 -0800, bobv <bobv@SOS.NET> wrote:

> Does anyone know of a phonebook manager for the HPLX (or even a windows
> laptop) for maintining the Nokia 3285 phone book?

There is no phone book manager.
But there is Robot/LX and the robot script "phone.scr", which enables
you to download or upload the whole phone book via WWW/LX and Robot/LX.

So you can download it, maintain it with a text editor and upload it
again. Or you can use the 200LX built-in phonebook as the "master"
phone book and let my program PDB2PHN create a phone book which you can
then upload to the phone. This is what I do.

http://www.daniel-hertrich.de/pdb2x

Or you can write an own phonebook maintenance program in the Robot/LX
scripting language. Since all phnone book maintenance can be done voa
AT commands through a cable or IrDA interface, this is theoretically
possible.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 12:47:24 -0800
Reply-To:     bobv <bobv@SOS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         bobv <bobv@SOS.NET>
Subject:      Re: Nokia 3285
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Tom,

I bought a cheap data cord for the 3285 on e-bay, and it DOESN'T work.
The one purchased from Nokia (DLR-3P) does work. It requires
installation of the Nokia modem on your laptop, for your laptop to be
able to communicate via that cable. (or some other software to drive
it).

I will see if I can find fonesync and report.

Thanks,

bob

----------------
Tom Rowsell <palmtop@WARP.NFLD.NET> wrote:

** Reply to note from Daniel Hertrich <daniel.hertrich@GMX.DE>
Tue,
19 Mar 2002 09:19:31 +0200

I read in a Nokia FAQ that the 3285 is supposed to work with Fonesync
using
the 6185 driver. Fonesync was bundled with
Microsoft Works Suite 2001. It looks to be as close to a "Phone Book
Manager" as you can get. I can't get it to work
though. I have a "cheap" data cable for my 3285. I don't know how to get
a
PC (or the 200lx) to communicate with the
phone. Are there any commands that I could try (in Datacomm for example)
to
see if the cable is ok ?

Tom

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 18:00:58 -0500
Reply-To:     Eduardo Seudonimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudonimo <ohdamnthathurts@YAHOO.COM>
Subject:      OT:RE: Windows command prompt tab completion tip
Comments: To: Donald Puscher <dpuscher@QUALCOMM.COM>
In-Reply-To:  <5.1.0.14.2.20020320130857.00ab6848@smtphost-co.qualcomm.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: quoted-printable

Also look for 'xteq systems x-setup' if you're nervous about registry =
munging. It's like TeakUI on steroids. It has an option for command line =
completion and a whole load of other stuff and it's free.




> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@uconnvm.uconn.edu]On Behalf Of
> Donald Puscher
> Sent: Wednesday, March 20, 2002 3:13 PM
> To: HPLX-L@uconnvm.uconn.edu
> Subject: OT: Windows command prompt tab completion tip
>=20
>=20
> Thought there might be some folks who would benefit from this tip from =
a
> coworker. I haven't tried it but I haven't heard anyone complain about =
it
> either :) As always when working with the Windows registry, be careful =
and
> make a backup first!
>=20
> Don
>=20
> =
=3D=3D=3D=3D=3D=3D=3D=3D=3D=3D=3D=3DTIP=3D=3D=3D=3D=3D=3D=3D=3D=3D=3D=3D=3D=
=3D=3D=3D=3D=3D=3D=3D=3D=3D=3D=3D=3D
> Do you ever wish the command prompt in Windows could perform =
completion
> when you hit tab, similar to many UNIX shells?  Well, you can. =20
> Here's how:
>=20
> Run the registry editor:
> Start->Run->regedit
>=20
> Edit the following key:
> My Computer\HKEY_CURRENT_USER\Software\Microsoft\Command
> Processor\CompletionChar
>=20
> Set the key value to 9 (ASCII for TAB).
>=20
> exit the registry editor and restart your command prompt window(s).  =
The
> setting will take effect when the program is started.
>=20
> This only works for Windows NT and Windows 2000.  I haven't tried=20
> ME or XP.
>=20
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 17:05:19 -0700
Reply-To:     kwmiller@azbcs.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "ABCS INC." <kwmiller@AZBCS.COM>
Subject:      Re: FW: 200lx ethernet adapter
Comments: To: hplxmail@yahoo.com
In-Reply-To:  <5.1.0.14.2.20020320091904.00a235f0@pop.mail.yahoo.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="US-ASCII"
Content-Transfer-Encoding: 7bit

The Palmtop was setup in the exact order listed below.

Drivers used and sequence loaded to enable TCPIP communication.  All drivers
were downloaded from the below web sites.

http://sourceforge.net/project/showfiles.php?group_id=3765

http://www.palmtop.net/super4.html

1. LXCIC     <-- card services to enable the card services
2. LXEN2216  <-- ne2000 compatible driver to activate the card (originally
for the Accton EN2216-1 card.)
3. LXTCPCFG  <-- tcpip network stack using DHCP
4. WWW/LX    <-- web browser

I also use LXFTP, LXPING for network troubleshooting.

I connected the ethernet cable from the PCMCIA/CF card directly to a 16 port
10/100 Switch.  This switch inturn connects to a Linksys DSL/Cable modem 4
port router and this connects to my cable modem.  No PC was used to connect
to the internet.

Kevin Miller

-----Original Message-----
From: hplxmail@yahoo.com [mailto:hplxmail@yahoo.com]
Sent: Wednesday, March 20, 2002 8:22 AM
To: kwmiller@azbcs.com; hplx-l@uconnvm.uconn.edu
Subject: Re: FW: 200lx ethernet adapter


Thank you for the info! Can you kindly also elaborate more how you set up
the Palmtop and the order of the software etc. Also, what did you have to
do on the connecting component in the network? Did you connect to a
desktop? What did you do there?

I hope this is not too much to ask.

Avi

At 3/17/02 01:52 PM, kwmiller@azbcs.com wrote:
>Thanks for all the reply's to my request for a source for Ethernet cards.
I
>can report that I now have a new functioning 10mbit ethernet card working
on
>my 200lx thanks to Keith Grider from the list.  Here is a link to the
>product information if anyone is curious.
>
>Ethernet Card:
>http://www.socketcom.com/product/ethernet_card.htm
>
>I used the Ruggedized Low Power Ethernet PC Card Solution part #EA0914-337.
>I used this one due to the mobile nature of the 200lx so I would not have
to
>buy a dongle when it breaks.  This card is ALSO CF compatible and uses a
>PCMCIA adapter to work on PCMCIA machines.  The PCMCIA adapter ships with
>these cards!  The card costs $106+shipping from CDW.COM
>
>http://www.cdw.com/shop/products/default.asp?EDC=323951
>
>The following drivers are used to operate the card.
>
>LXCIC     <-- card services
>LXEN2216  <-- ne2000 compatible driver
>LXTCP     <-- tcpip network stack
>WWW/LX    <-- web browser
>
>I also use LXFTP, LXPING for network troubleshooting.
>
>Thanks for all the help!
>
>Kevin Miller
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 16:31:39 -0600
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: FW: 200lx ethernet adapter
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
In-Reply-To:  <HPLX-L%2002032016173452@UCONNVM.UCONN.EDU>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Easy to check on their Website if I made a mistake. I do not have the URL
handy... As I wrote - I DO NOT HAVE the card, and all the info I got was
the website. I am really not the expert on this product.  I am known to
have made a mistake or two before <G> ... Sorry if I mislead anyone...

At 3/20/02 02:18 PM, you wrote:
>Hi Avi
>
>On Wed, 20 Mar 2002 09:18:09 -0600, A Meshar <hplxmail@YAHOO.COM> wrote:
>
> > I did not use the card, but checked the Website. They claim 19mW when
> > active, and the general gist is that these cards are very low power cards.
> > Looks interesting.
>
>milli WATTs? not milli Amperes?
>
>19mW would mean only 3.8mA at 5V. That's almost nothing! The 150mA
>limit at the PCMCIA slot would allow to drive 40 of these cards
>simultanously!
>
>So, if it would ever be possible to build one of these cards directly
>into the LX (using PCMCIA socket 2), it would at least never be a big
>power-related problem. :-)
>
>GTX
>daniel
>
>--
>http://www.daniel-hertrich.de/contact
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 16:33:09 -0600
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: FW: 200lx ethernet adapter
Comments: To: "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
In-Reply-To:  <D8020D6F0DB8D211B99A0008C7C59CFE0FD8F775@cormails1.jdedwar
              ds.com>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Thanks for correcting my numbers, Robert...


At 3/20/02 03:25 PM, you wrote:
>19 mA, 63mW
>
>-----Original Message-----
>From: Daniel Hertrich [mailto:daniel.hertrich@GMX.DE]
>Sent: Wednesday, March 20, 2002 2:19 PM
>To: HPLX-L@UCONNVM.UCONN.EDU
>Subject: Re: FW: 200lx ethernet adapter
>
>
>Hi Avi
>
>On Wed, 20 Mar 2002 09:18:09 -0600, A Meshar <hplxmail@YAHOO.COM> wrote:
>
> > I did not use the card, but checked the Website. They claim 19mW when
> > active, and the general gist is that these cards are very low power cards.
> > Looks interesting.
>
>milli WATTs? not milli Amperes?
>
>19mW would mean only 3.8mA at 5V. That's almost nothing! The 150mA
>limit at the PCMCIA slot would allow to drive 40 of these cards
>simultanously!
>
>So, if it would ever be possible to build one of these cards directly
>into the LX (using PCMCIA socket 2), it would at least never be a big
>power-related problem. :-)
>
>GTX
>daniel
>
>--
>http://www.daniel-hertrich.de/contact
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 16:34:26 -0600
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: Nokia 3360
Comments: To: wally@theblackmoor.net
In-Reply-To:  <3C98E22C.2010907@theblackmoor.net>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Hi Walter:

Thanks for the post, even late. This last weekend I actually got one to
hold and I am now sure - it is not for me.


At 3/20/02 01:25 PM, you wrote:
>A Meshar wrote:
>
>
>>Except: 3360 has an internal modem, and 8260 does not. 3360
>>has an IR and 8260 does not.
>>
>>My very basic question is if anyone used 3360 with WWW/LX over the IR.
>
>I'm a little behind getting back to you, but I have connected to my ISP
>using my 3360 in Linux, but it would connect and never get past the
>authentication stage.  So I have something odd software wise.
>
>My copy of WWW/LX doesn't do IRDA so I can't say about it, but using ir.exe
>I can definately talk to the phone, make a connection, etc..
>
>I hope your 3360 will have a newer firmware than mine, I have trouble with
>my phone locking up sometimes..  Mostly when I'm playing games tho.  :)
>Happens occationally in WAP too.  BTW, whoever designed the interface to WAP
>was an idiot, it's SO SLOW to browse around and such.  Oh well.
>
>--
>Walter Francis
>http://theblackmoor.net                  Powered by Red Hat Linux 7.2
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 16:49:37 -0800
Reply-To:     Joseph.Buford@HSC.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Joseph Buford <Joseph.Buford@HSC.COM>
Subject:      Re: Fluff: Conclusions
Comments: To: hplxmail@yahoo.com
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

" There once was a lady of Paris........" <grin back>

Avi,

Been cool here (mid 60's). Ha Ha :-)

How is the culture shock going?

Joe




hplxmail@yahoo.com on 03/20/2002 06:11:23 AM

To:    Joseph.Buford@HSC.COM, hplx-l@uconnvm.uconn.edu
cc:

Subject:  Re: Fluff: Conclusions


I'd like to hear you recite some poems in French! <VBG>

    Avi
(from Cool Minnesota - today 20 Mar, it is lovely skies and no snow, but
plenty on unmelted stuff on the side of streets and on Lake O'Leary - ask
me if you do not know about Lake O'Leary.)

At 3/16/02 06:05 PM, you wrote:
>Nathalie,
>
> >Eat & drink what you like. It's speaking English that kills
>you. :)
>
>Perhaps I should learn french :-)
>
>Joe
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 19:58:02 -0500
Reply-To:     Bob Newins <bnew@ATTBI.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Newins <bnew@ATTBI.COM>
Subject:      Re: CF inside HP200LX
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Russ,

I agree.  I use Pocket Quicken all the time.    =Bob=

Russel Brooks wrote:
>
> Bob Christopher wrote:
> >  Maybe remove the blue Pocket
> > Quicken key (the least used key for most of us I'm sure) and
>
> I use to agree with you but not any more.  I've stopped using my
> desktop Quicken and now use Pocket Quicken only.  I wish I'd
> done this years ago when I first got my LX.
>
> Blue keys I don't use:  Filer, Memo, Lotus123
>
> Cheers... Russ
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 20:05:23 -0800
Reply-To:     bobv <bobv@SOS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         bobv <bobv@SOS.NET>
Subject:      Re: one-purpose switch speaker off
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

That looks like sending a binary to the list to me! :)

Cool - thanks


Dzon <dzon@SOFTHOME.NET> wrote:

I was looking for something to let me not to disturb others with my loud
LX speaker. There probably are plenty of tools, but I like several
one-purpose programs rather than one big [it's unix :)]. If you feel
like
me, open hex editor and create speakoff.com with:
B8 00 48 CD 15 B8 00 4C CD 21
and yep, no need of hardware hacking :)
You can create speakon.com changing the _first_ zero byte with 01 to 03
[03 is loudest].

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 00:29:36 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      FW: Important Yahoo! Mail Service Announcement
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

oh, well. It was fun while it lasted....

-------------


Hello,
Important service announcement regarding your POP3 or Mail Forwarding =
service. Please read on.

Effective April 24, 2002, Yahoo! Mail will no longer provide free POP3 =
Access or Auto Mail Forwarding to Yahoo! Delivers subscribers.=20
If you would like to continue using Mail Forwarding or POP3 Access, =
please subscribe to our improved package that allows you to:=20
Use Outlook, Eudora, or another POP3 client to access and manage your =
Yahoo! Mail.=20
Automatically forward your Yahoo! Mail to another email account -- even =
another Yahoo! address!=20
Send larger attachments, now up to 5MB instead of the free 1.5MB limit.=20
Send email without the Yahoo! promotional text at the bottom.* =20
Sign up today and SAVE 33%=20


Subscribe before April 24th and get the first year of service for just =
$19.99. That's 33% off the regular service fee of $29.99.=20
Remember, if you do not subscribe by April 24, 2002, you will no longer =
be able to access your Yahoo! Mail messages by POP or at another email =
address.
Sincerely,
The Yahoo! Mail Team
For further information, please read our frequently asked questions. =
Please note that your Yahoo! Delivers settings will not be affected.=20
*Applies only to email sent through the Yahoo! SMTP servers.=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 11:26:02 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

all good things must come to an end ..
the gooder they are .. the faster they end !
(from pk's book of quotable quotes)
(the book exists in ether, of course !)

..pk

> Effective April 24, 2002, Yahoo! Mail will no longer
provide free POP3 Access or
> Auto Mail Forwarding to Yahoo! Delivers subscribers.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 20 Mar 2002 21:57:29 -0800
Reply-To:     Marta Pierce <Marta1@attbi.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marta Pierce <Marta1@ATTBI.COM>
Organization: Family
Subject:      Barbie Design Center  With Pen Mouse
In-Reply-To:  <20020315050211.KIOB10334.rwcrgwc51.attbi.com@UConnVM.UConn.Edu>
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Hello Listers,

Okay, I just recived my barbie mouse. Now someone on this list has
been using it.  Could you please give me the specifics on how to get
it to work?

TIA

--
Best regards,
 Marta                            mailto:Marta1@attbi.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 01:46:00 -0500
Reply-To:     Francois Gurin <matrix@SHOT.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Francois Gurin <matrix@SHOT.ORG>
Subject:      The saddest day in my life
Mime-Version: 1.0
Content-Type: text/plain; charset=us-ascii

Today, while mildly dizzy from this aweful flu, I took the M11 bus in ny, ny,
going downtown.  At about 6pm Eastern time, I got off the bus and walked into
the company colo facility, when suddenly I realized, My Bag Was Still on the
Bus!

The only thing of importance in the bag was some banking papers and my main
HP 200LX!!  I was so absolutely heartbroken!

There's still hope for recovery of my bag, but I think the chances are slim.
Lesson: when you're not feeling well, make sure everything is firmly attached
to your body at all times, or just stay home and wait it out.

And should anyone happen to come across a 4mb 200lx with a 48mb sandisk
flashcard, please let me know.  I have a feeling if it doesn't show up at
the bus depot, it will be listed on ebay.

Thanks for listening,
--francois

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 07:57:53 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: partitioned memory card in 200lx!
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Radek Svagr wrote:
> Using MEMCARD.EXE which is in Olivetti
> Quaderno mininotebook (386 version). I made
> 2 partitions on this 512 kB SRAM card, one 255
> and one 256 kB. Both were then acessible on
> 200lx as A: and B:. What is funny that Olivetti
> quaderno itself didn't recognize the second
> partition. But this could be due to wrong settings
> of its drivers.

There are a lot of differences in the way a PC handles a floppy
drive and a hard drive.  The Oliveti BIOS expects to find the
floppy drive(s) in a certain place.  The BIOS is probably just
like any other PC BIOS and expects what it finds there to be an
actual floppy drive.

Since the flash card presents itself as an ATA device the BIOS
probably treats it automatically as a hard drive.  A: and B: are
reserved for floppy drives.  That's why the first hard drive is
C: whether there are 1 or 2 floppies.

The 200lx, on the other hand, is designed to treat the PCMCIA
slot as a floppy drive.  That was probably it's primary intended
purpose and the BIOS was probably designed with that in mind.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 07:02:39 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: Barbie Design Center  With Pen Mouse
MIME-Version: 1.0
Content-Type: text/plain

If you have the HP connectivity cables, use the regular cable (HP to DE9
female) and the DE9-DE9 null modem connector. You need the null modem
connector because the cable is meant to connect the HP to another computer,
so the send and receive lines are switched from what you need for the mouse.
Next, plug the mouse into the null modem connector. Unfortunately, this
cable combination is a bit unwieldy, but is necessary unless you can make a
short regular serial cable (HP to DE9 male).

I load the supplied mouse driver (APMOUSE.SYS) in my Config.sys file. Add
the following line to your config.sys file, adjusting the "C:\" to match the
path were you have APMOUSE.SYS:

DEVICE=C:\APMOUSE.SYS

Note that there are no spaces in the line.

Make sure that the serial port is turned on. If you use Buddy, make sure it
is also unlocked in Buddy. Reboot the computer with the mouse connected.
During the boot process, you will get a screen message that the driver has
or has not been installed properly. You can use the test program that also
comes with the mouse to verify that it is working.

-----Original Message-----
From: Marta Pierce [mailto:Marta1@attbi.com]
Sent: Wednesday, March 20, 2002 11:57 PM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Barbie Design Center With Pen Mouse


Hello Listers,

Okay, I just recived my barbie mouse. Now someone on this list has
been using it.  Could you please give me the specifics on how to get
it to work?

TIA

--
Best regards,
 Marta                            mailto:Marta1@attbi.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 08:23:33 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: FLUFF: (really fluff) .... Did I overprice my eBay HDD?
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Tim wrote:
> Since this is a list of "gadget experts," thought I'd
> ask if you folks thought I overpriced this:
> http://cgi.ebay.com/ws/eBayISAPI.dll?ViewItem&item=2010011617
> I started it at $199 and am wondering why no one
> bid on it..... Maybe I messed up the description(?).
> OK, No more wasted bandwidth w/ this one.... Just
> wondering.

Most laptops today have USB ports and USB portable hard drives
prices start around $199.  I just checked J and R Computer World
and for $199 or less you can choose from a number of drives.
They even have 40 gig drives at $179 and $189.  These are new
prices.

I have a 6 gig Archos Jukebox which is a good mp3 player with a
hard drive and it also works fine as a portable hard drive.  J
and R doesn't carry the 6 gig model but they have the 10 gig
model for $219.  And that's for a pocket size (barely) AA
battery operated unit that makes a first rate feature filled MP3
player as well as a portable hard drive.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 08:55:44 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: The saddest day in my life
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

Francois Gurin wrote about losing his HP200LX.

I know exactly how you feel.  Last spring I flew into Boston
to attend a conference.  My flight arrived late in the evening.
I was exhausted, but tried reading e-mail on my 32M HP200LX
during the cab ride to the hotel.  Finding the light too low,
I set the palmtop on the seat next to me, intending to look
at it as soon as there was more light.  Well, you guessed it.
I was tired enough that I didn't think about picking it up,
and didn't realize what had happened until I was checking in
at the hotel and the cab had left.

I called the Boston taxi lost and found and posted a reward
for the unit, but I never heard anything back.  The three
days of that conference were a nightmare--I ended up with
a fistful of handwritten notes to be trancribed later.  The
worst was being without contact information and e-mail.  I
called Thaddeus from Boston and had a new unit the day I
returned home.  Luckily I had a recent backup, so I only lost
about a week's worth of work.

Hang in there, and good luck!

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 09:18:38 -0600
Reply-To:     John McCaskill <jmccask@POWERCHOKES.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John McCaskill <jmccask@POWERCHOKES.COM>
Subject:      Re: The saddest day in my life
In-Reply-To:  <Pine.OSF.4.33.0203210846490.7498-100000@worf.netins.net>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I know what you mean. In late 1992 I was traveling from Germany to
Switzerland via rail, and left my 95LX on the train! I had reached
Winterthur before I discovered my loss. I panicked, took a train back to the
border, and found that, since the train had crossed the country's border,
they had done a search of the entire train, and found my palmtop. I got it
back from lost & found! Only 4 hours of anxiety for me, though.

John McCaskill
Houston, TX, USA
Who doesn't even have a 200LX... just a 1 mB 100LX.

-----Original Message-----
From: HPLX Mailing List [mailto:HPLX-L@UConnVM.UConn.Edu]On Behalf Of
Theodore Heise
Sent: Thursday, March 21, 2002 8:56 AM
To: HPLX-L@UConnVM.UConn.Edu
Subject: Re: The saddest day in my life


Francois Gurin wrote about losing his HP200LX.

I know exactly how you feel.  Last spring I flew into Boston
to attend a conference.  My flight arrived late in the evening.
I was exhausted, but tried reading e-mail on my 32M HP200LX
during the cab ride to the hotel.  Finding the light too low,
I set the palmtop on the seat next to me, intending to look
at it as soon as there was more light.  Well, you guessed it.
I was tired enough that I didn't think about picking it up,
and didn't realize what had happened until I was checking in
at the hotel and the cab had left.

I called the Boston taxi lost and found and posted a reward
for the unit, but I never heard anything back.  The three
days of that conference were a nightmare--I ended up with
a fistful of handwritten notes to be trancribed later.  The
worst was being without contact information and e-mail.  I
called Thaddeus from Boston and had a new unit the day I
returned home.  Luckily I had a recent backup, so I only lost
about a week's worth of work.

Hang in there, and good luck!

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 12:10:05 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      FLUFF: E-Books (was:  Important Yahoo! Mail Service Announcement
Comments: To: pksharma <pksharma@CAL.VSNL.NET.IN>
In-Reply-To:  <015801c1d09d$161b1100$2aadc8cb@q20>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

> (from pk's book of quotable quotes)
> (the book exists in ether, of course !)

<off topic>
That reminds me of Kurt Vonnegut's 'Galapagos'. The narrator is writing =
the book but he doubts that anyone will ever read it. This is because he =
is writing it in thin air with his finger... oh, yeah, he's also a ghost =
so even his finger is not really.. real. ;^> A must read for those who =
appreciate dark perverse humor. This is true of all his books that I've =
read.=20
</off topic>

<Semi-on topic>
I wonder if you can get these books in E format. I find that I read more =
and more Ebooks as time goes by. I no longer use the LX tho as I have =
found that my Nino 200 does a much better job (not good for much else =
tho :^/ ). I've even paid for a few SciFi books from www.baen.com=20



=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 11:52:05 -0600
Reply-To:     palmtop@n-link.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tim <palmtop@N-LINK.COM>
Subject:      Re: FLUFF: (really fluff) .... Did I overprice my eBay HDD?
In-Reply-To:  <000b01c1d0e4$0fc0d0a0$a60d22d1@oemcomputer>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Hi all. THANKS for the input. I reduced the price (sadly to less than 1/4 of
what I paid for it) and added "no bad sectors" and other info to the
description.

With luck, that should draw the bidders out. Thanks to all (again) who sent
me advice!

--tim

-----Original Message-----
From: HPLX Mailing List [mailto:HPLX-L@UCONNVM.UCONN.EDU]On Behalf Of
Barry
Sent: Thursday, March 21, 2002 8:24 AM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: Re: FLUFF: (really fluff) .... Did I overprice my eBay HDD?


Tim wrote:
> Since this is a list of "gadget experts," thought I'd
> ask if you folks thought I overpriced this:
> http://cgi.ebay.com/ws/eBayISAPI.dll?ViewItem&item=2010011617
> I started it at $199 and am wondering why no one
> bid on it.....

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 23:45:58 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: FLUFF: E-Books (was:  Important Yahoo! Mail Service
              Announcement
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

this is urgent, immediate, necessry response to
Eduardo's <off topics>
.. (thank god .. on topic wud've been a serious matter) :

"those who appreciate dark perverse humor"
guys ! this doesn't apply to my book !

..pk

(mine is lite inverse humor)

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 00:30:33 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: FLUFF: (really fluff) .... Did I overprice my eBay HDD?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

-----Original Message-----
From: Tim <palmtop@N-LINK.COM>
To: HPLX-L@UConnVM.UConn.Edu <HPLX-L@UConnVM.UConn.Edu>
Date: Thursday, March 21, 2002 11:35 PM
Subject: Re: FLUFF: (really fluff) .... Did I overprice my
eBay HDD?


> ... I reduced the price (sadly to less than 1/4 of
>what I paid for it)

my 380MB hdd cost me 27,000/- .. i'll be lucky to
get 270/- .. its down to 1% .. time destroys demand

btw what is the kind of hdd ? 2.5" or 3.5" ?

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 23:09:35 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: The saddest day in my life
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Francois Gurin wrote:
> Today, while mildly dizzy from this aweful flu, I took the M11 bus in ny, ny,
> going downtown.  At about 6pm Eastern time, I got off the bus and walked into
> the company colo facility, when suddenly I realized, My Bag Was Still on the
> Bus!

B-I-G loss!  I am constantly afraid I'll lose my LX and it has
had the positive effect of forcing me to make better and more
frequently backup.

> And should anyone happen to come across a 4mb 200lx with a 48mb sandisk
> flashcard, please let me know.  I have a feeling if it doesn't show up at
> the bus depot, it will be listed on ebay.

Care to post the serial number we should watch out for?

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 17:13:35 -0700
Reply-To:     "Robert K. Meyer" <bmeyer@UNION-TEL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Robert K. Meyer" <bmeyer@UNION-TEL.COM>
Subject:      Re: Fluff: Spamfilter
Comments: To: TomSalwasser@COMPUSERVE.COM
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

I have also been using MailWasher on Tom's recommendation.
The website indicates that bounced email appears exactly as
if bounced by your email server, no indication of MailWasher
intervention. I think it is good enough that I may even
register the program.

Previously I've been forwarding mail to "abuse@...,
postmaster@..., fraud@..., spam@...," wasting time and
probably does no good. A couple of clicks with MailWasher
and it is done. Probably even easier in some automated mode.

Bob

Tom Salwasser wrote:
>
> I'm using www.mailwasher.net. It bounces mail as having an invalid email
> address. I don't know if it will reduce my spam but it makes me feel good when I
> bounce an email!
>
> Regards,
> Tom Salwasser
>
> >
> > > Remote host said: 552 Message identified as spam....
> > > Return-Path: <cpt_kludge@yahoo.com>
> >
> > Bad scheme: That tells the spammers "This is a valid and read address - try
> > again." which is not what I want them to get.
> >
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

--
R.K. Meyer MSEE K7PPC bmeyer@union-tel.com Elk Mountain WY
http://w3.union-tel.com/~bmeyer/   His name...  Isaiah 9:6

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 22:03:09 -0500
Reply-To:     Francois Gurin <matrix@SHOT.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Francois Gurin <matrix@SHOT.ORG>
Subject:      Happy Ending (Was: The saddest day in my life)
In-Reply-To:  <20020321014559.A20538@shot.org>; from Francois Gurin on Thu,
              Mar 21, 2002 at 01:46:00AM -0500
Mime-Version: 1.0
Content-Type: text/plain; charset=us-ascii

Thank you for all the support.  Fortunately this story has a happy ending.
Earlier today I spoke with someone at the mta and the driver had brought my
bag to the bus depot.   Much to the surprise of the mta employees who helped
get the bag back to me, nothing was at all was missing!  My main hplx is home
again and I will be sure to take better care of it in the future.

Aside from a warm fuzzy feeling knowing there are many good people out there,
I'm also taking with me the realization that I did not have information
such as the serial numbers of the hplx and card et al.

Hopefully I'll never need all the information, but if it's ever necessary I'm
going to have it available!

Thanks!
--francois

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 19:12:19 -0800
Reply-To:     Gary Jacek <gary-jacek@SHAW.CA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Gary Jacek <gary-jacek@SHAW.CA>
Organization: @Shaw
Subject:      ILGRadio Shortwave Database in GDB Format
MIME-version: 1.0
Content-type: text/plain; charset=us-ascii
Content-transfer-encoding: 7BIT

Hey gang.

One of my other interests is Shortwave Radio.

I recently happened upon the ILGRadio site.
HTTP://www.ilgradio.com/

ILGRadio has a database of Shortwave broadcasters, worldwide.

ILGSTLAN.ZIP at this site, contains individual databases in
LINUX text format, for broadcasts
in English, French / Creole, German, Arabic, Italian, Dutch /
Afrikaans, Portuguese,                        Russian /
Ukrainian, Spanish and "Nordic" (Danish Icelandic, Norwegian,
Swedish, and Finnish).

You guessed it.  I just had to have the English broadcast
database in my palmtop for on-the-go listening.

I have written a program that converts the ILGRadio LINUX format
databases into something that
GDBLOAD can accept.  I used my program and GDBLOAD (available on
SUPER) to convert the
ILGSTENG.TXT English broadcast database into ILGSTENG.GDB.

There is a catch here.  In order to get the ILGRadio database,
you need to register at
the ILGRadio site.  The bad news is that it takes a few days to
get a Userid/Password for
download.  The good news is that it is free for noncommercial
use.

I can't give away the ILGSTENG.GDB database, but I can give away
the tools to create it.

If there are any other shortwave listeners on the HPLX list that
would find this of benefit,
I can clean it up and make it available.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 11:39:24 +0800
Reply-To:     Adrian Ho <aho-hplx@03S.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Adrian Ho <aho-hplx@03S.NET>
Subject:      Re: Happy Ending (Was: The saddest day in my life)
In-Reply-To:  <20020321220308.C20538@shot.org>; from matrix@SHOT.ORG on Thu,
              Mar 21, 2002 at 10:03:09PM -0500
Mime-Version: 1.0
Content-Type: text/plain; charset=us-ascii

On Thu, Mar 21, 2002 at 10:03:09PM -0500, Francois Gurin wrote:
> Much to the surprise of the mta employees who helped get
> the bag back to me, nothing was at all was missing!

Goodness, the first four words are quite a comment on the
general level of personal integrity in your area.

Nevertheless, I'm happy for you.

> Aside from a warm fuzzy feeling knowing there are many good
> people out there, I'm also taking with me the realization
> that I did not have information such as the serial numbers
> of the hplx and card et al.

You might want to take pictures of them as well.  It's easier
to show them to the people you talk to, than try to describe
them when possibly in a state of panic, semi-coherent, or
(when in a foreign country) don't speak the language.

Heck, most parents do so with their kids -- not primarily to
aid in searching for them when they go missing, but it's useful
that way too.  I'm sure you love your LX just as much.  8-)

- Adrian

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 06:27:21 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: Happy Ending (Was: The saddest day in my life)
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

LET'S ALL REMEBER .. GOOD PEOPLE DO
EXIST .. ALL IS NOT LOST ..

i dedicate a full ONE minute today .. to thank
good .. for creating good people too .. who light
up our lives .. and we survive the darkenss/badness

guys .. wanna join me .. then we'll have so many
good people of this list .. giving one minute each
for the so many other good people other than
this list  :)

..pk


-----Original Message-----
From: Francois Gurin <matrix@SHOT.ORG>
Date: Friday, March 22, 2002 8:39 AM


>Thank you for all the support

> Much to the surprise of the mta employees who helped
>get the bag back to me, nothing was at all was missing!

(the impossible is possible too !)
(from the pk's book of quoteable
quotes .. which is still in ether)
(this is quote number 20020322 :-D)

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 20:01:43 -0800
Reply-To:     Qman <qman@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Qman <qman@EARTHLINK.NET>
Subject:      Re: Happy Ending (Was: The saddest day in my life)
Comments: To: pksharma <pksharma@CAL.VSNL.NET.IN>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Amen!

Incase you all did know, I'm also a Transit Operator (Las Vegas, NV). (:-0)


Regards,
Qman...


----- Original Message -----
From: "pksharma" <pksharma@CAL.VSNL.NET.IN>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Thursday, March 21, 2002 4:57 PM
Subject: Re: Happy Ending (Was: The saddest day in my life)


> LET'S ALL REMEBER .. GOOD PEOPLE DO
> EXIST .. ALL IS NOT LOST ..
>
> i dedicate a full ONE minute today .. to thank
> good .. for creating good people too .. who light
> up our lives .. and we survive the darkenss/badness
>
> guys .. wanna join me .. then we'll have so many
> good people of this list .. giving one minute each
> for the so many other good people other than
> this list  :)
>
> ..pk
>
>
> -----Original Message-----
> From: Francois Gurin <matrix@SHOT.ORG>
> Date: Friday, March 22, 2002 8:39 AM
>
>
> >Thank you for all the support
>
> > Much to the surprise of the mta employees who helped
> >get the bag back to me, nothing was at all was missing!
>
> (the impossible is possible too !)
> (from the pk's book of quoteable
> quotes .. which is still in ether)
> (this is quote number 20020322 :-D)
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 05:23:51 +0100
Reply-To:     Nathalie Bugeaud <tps-seti@WANADOO.FR>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nathalie Bugeaud <tps-seti@WANADOO.FR>
Subject:      Re: Fluff: Conclusions
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 8bit

 >I'd like to hear you recite some poems in French! <VBG>
 >ask me if you do not know about Lake O'Leary.)

i don't ! so who is this O'Leary ?

 >I'm using www.mailwasher.net. It bounces mail

how do i 'use' it here in France?

nat

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 11:01:20 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      strange behaviour of DS 200lx
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

I' am observing strange behavior of my DS 200lx.
Disk operations /C drive/ are much slower when CF card is not inserted. If I insert a CF card back, the execution of programs from C: drive is much faster.
I have no path  assigned to a: so it cannot be caused by acesing not acessible A: drive. My 200lx is completely independent form A: drive.


Any suggestions?



Radek

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 11:47:59 +0100
Reply-To:     xmarc@free.fr
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marc BERLIOUX <xmarc@FREE.FR>
Subject:      palmtop.net down ?
Content-Type: text/plain; charset="iso-8859-1"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit

i can't connect to http://www.palmtop.net
is it normal

--
Marc BERLIOUX
"A force de vouloir faire la lumihre sur tout,
 on ne distingue plus rien" R.Devos

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 13:26:21 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: strange behaviour of DS 200lx
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Radek

On Fri, 22 Mar 2002 11:01:20 +0100, Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM> wrote:

> I' am observing strange behavior of my DS 200lx.
> Disk operations /C drive/ are much slower when CF card is not inserted. If I insert a CF card back, the execution of programs from C: drive is much faster.
> I have no path  assigned to a: so it cannot be caused by acesing not acessible A: drive. My 200lx is completely independent form A: drive.

hmmm - did you already solder around at the PCMCIA slot? ;-)

Otherwise I would suggest a hard reset. Maybe jsut some software has
chained into the disk access. Any drivers loaded?

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 14:17:48 +0100
Reply-To:     furlan@gmx.net
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Dr. Werner Furlan" <furlan@GMX.NET>
Organization: OE9FWV
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
Comments: To: Eduardo Seudsnimo <ohdamnthathurts@yahoo.com>
MIME-Version: 1.0
Content-type: text/plain; charset=ISO-8859-15
Content-transfer-encoding: Quoted-printable

hi Eduardo and company,

Eduardo Seudsnimo schrieb =FCber FW: Important Yahoo! Mail Service=20
Announcement:

> oh, well. It was fun while it lasted....
>=20
> -------------
>=20
>=20
> Hello,
> Important service announcement regarding your POP3 or Mail Forwarding =
service. Please read
> on.
>=20
> Effective April 24, 2002, Yahoo! Mail will no longer provide free =
POP3 Access or Auto Mail
> Forwarding to Yahoo! Delivers subscribers.=20
> If you would like to continue using Mail Forwarding or POP3 Access, =
please subscribe to
> our improved package that allows you to:=20
> Use Outlook, Eudora, or another POP3 client to access and manage your =
Yahoo! Mail.=20
> Automatically forward your Yahoo! Mail to another email account -- =
even another Yahoo!
> address!=20
> Send larger attachments, now up to 5MB instead of the free 1.5MB =
limit.=20
> Send email without the Yahoo! promotional text at the bottom.* =20
> Sign up today and SAVE 33%=20

There is no need to stick with yahoo at all.
I am a content user of GMX. The provide a free mail service with=20
forwarding to 2 mail addresses of your choice, web interface,=20
POP3/SMTP acces, 10 MB mailbox volume. And to stay on topic:
it works very well with my HP200 and WWW/LX.

Sign up today and SAVE 100% ;-)

cheers,
Werner=20


-- =20
PGP-Key: <http://www.qsl.net/oe9fwv/furlan.asc>
SMS: <+436646340014@text.mobilkom.at>
Powered by Pegasus Mail - free at <http://www.pmail.com>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 14:39:46 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      Re: strange behaviour of DS 200lx
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Not soldered yet:-)
What I load is doublespeed driver end EMS driver. But the same behaviour is when I plug it into the DC adaptor!
I think some kind of interference around crystal, which is grounded via CF card or DC adapter;-))))
It will need further analysis, when I open it for soldering of CF inside...



Radek

P.S. Of course I have one spare unit. I am not so crazy to solder to the only one:-) I received a special version of lxcic from Stefan (for socket 2) so I will
try to install something inside 200lx this weekend.






                      Daniel Hertrich
                      <daniel.hertrich             To:  HPLX-L@UConnVM.UConn.Edu
                      @GMX.DE>                     cc:  (bcc: Radek Svagr/HRC/COMP/PHILIPS)
                      Sent by: HPLX                Subject:   Re: strange behaviour of DS 200lx
                      Mailing List
                      <HPLX-L@UConnVM.             Classification:
                      UConn.Edu>


                      2002-03-22 12:26
                      PM
                      Please respond
                      to Daniel
                      Hertrich






Hi Radek

On Fri, 22 Mar 2002 11:01:20 +0100, Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM> wrote:

> I' am observing strange behavior of my DS 200lx.
> Disk operations /C drive/ are much slower when CF card is not inserted. If I insert a CF card back, the execution of programs from C: drive is much faster.
> I have no path  assigned to a: so it cannot be caused by acesing not acessible A: drive. My 200lx is completely independent form A: drive.

hmmm - did you already solder around at the PCMCIA slot? ;-)

Otherwise I would suggest a hard reset. Maybe jsut some software has
chained into the disk access. Any drivers loaded?

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 14:46:19 +0100
Reply-To:     Juergen Korthof <hplx@0800CALLING.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Juergen Korthof <hplx@0800CALLING.DE>
Subject:      CEBIT2002 still nothing compares to our HPLX
In-Reply-To:  <HPLX-L%2002032207250295@UCONNVM.UCONN.EDU>
Mime-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Hello Listmembers,

recently I visited the CeBIT in Hannover.
There are some new PDA. But i found nothing what can be called
a real successor for our LX.

It is always the same:
If they have Color
- they have no acceptable battery-stand time.
If they are capable of sending and receiving email.
- they are fixed to GPRS (or to O2, former E2 VIAG Intercom)
  with not yet acceptable reachability in germany.
If they have a keyboard
- they have too small keys for typing a letter (e.g. an
average email)

The only comparable Mobile-PCs are still in the size of a
paperback book and
suffer with much more wheight than you want to have in your
pocket.

It seems to me, the developers are from outerspace, unmovable
if they find a mains-source or battery-depot and good
aerialsignal.
They must have spiderfingers (or no fingers at all),
medium-pizza-sized "palm"
and jacketpockets like magicians hats, wherein you can store
10 pigeons,
5 hares, 20 sparebatteries and even an average sized modern
"Palmtop-Computer".:-)

Furthermore i will be very carefully to my LX - it is the
most valuable Computer, I can use in these days.


Happy LXing
Juergen.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 15:24:44 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: CEBIT2002 still nothing compares to our HPLX
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Juergen

On Fri, 22 Mar 2002 14:46:19 +0100, Juergen Korthof <hplx@0800CALLING.DE> wrote:

> recently I visited the CeBIT in Hannover.
> There are some new PDA. But i found nothing what can be called
> a real successor for our LX.

The most promising machine is IMO the Sharp Zaurus thing (palm sized,
but with keyboard, Linux OS). Did you see that one on Cebit? I would be
very interested in having a look at this machine.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 08:55:35 -0800
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Need a Thaddeus 56K Modem Driver
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

I have one of Thaddeus' 56KB modems (it says "56K Fax Modem" on the front).

I believe it had a diskette with a driver on it when I got the modem from
Thaddeus. Does anyone know?

I am rebuilding an OB800CT and Win95b in it does not recognize the modem as
a 56K, only as a standard 28.8 modem.

Anyone has a better driver for it? If you do, please send it to me, or let
me know a URL where I can d/l it (Thaddeus' site maybe?)

Thanks in advance


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 10:15:28 -0500
Reply-To:     Eduardo Seudonimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudonimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: Happy Ending (Was: The saddest day in my life)
Comments: To: Francois Gurin <matrix@SHOT.ORG>
In-Reply-To:  <20020321220308.C20538@shot.org>
MIME-Version: 1.0
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: quoted-printable

Many people thing that New York is a place filled with dis-honorable =
people but I always beg to differ. In a place with so many people =
there's bound to be a few bad ones. Those are the ones everyone =
remembers.  I've had similar experinces losing things on the subway and =
getting them back (and this was before the good will created after =
9/11... nowadays New Yorkers are so polite it's ... eerie.)



> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@uconnvm.uconn.edu]On Behalf Of
> Francois Gurin
> Sent: Thursday, March 21, 2002 10:03 PM
> To: HPLX-L@uconnvm.uconn.edu
> Subject: Happy Ending (Was: The saddest day in my life)
>=20
>=20
> Thank you for all the support.  Fortunately this story has a happy =
ending.
> Earlier today I spoke with someone at the mta and the driver had=20
> brought my
> bag to the bus depot.   Much to the surprise of the mta employees=20
> who helped
> get the bag back to me, nothing was at all was missing!  My main=20
> hplx is home
> again and I will be sure to take better care of it in the future.
>=20
> Aside from a warm fuzzy feeling knowing there are many good=20
> people out there,
> I'm also taking with me the realization that I did not have =
information
> such as the serial numbers of the hplx and card et al.
>=20
> Hopefully I'll never need all the information, but if it's ever=20
> necessary I'm
> going to have it available!
>=20
> Thanks!
> --francois
>=20
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 10:03:47 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Eduardo Seudsnimo wrote:
> Effective April 24, 2002, Yahoo! Mail will no
> longer provide free POP3 Access or Auto Mail
> Forwarding to Yahoo! Delivers subscribers.

CNN's website has started charging to view a number of things.
You have to subscribe for $4.95 a month to be able to see a lot
of their columns and any of their video or audio segments.

I heard about this on NPR radio the other day.  They said that a
lot of other sites are considering this as well.

I think in a few years we'll think of the old internet as
Camelot.  And when we're gone it'll just be a legend.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 10:13:49 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: The saddest day in my life
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

John McCaskill wrote:
> I know what you mean. In late 1992 I was traveling
> from Germany to Switzerland via rail, and left my
> 95LX on the train! I had reached Winterthur before
> I discovered my loss. I panicked, took a train back
> to the border, and found that, since the train had
> crossed the country's border, they had done a search
> of the entire train, and found my palmtop. I got it back
> from lost & found! Only 4 hours of anxiety for me, though.

I guess Houston is a lucky city for LX users.  I left mine in a
doctor's waiting room twice (different doctors) and didn't
realize it till that evening when it was too late to do
anything.  Both times I called first thing the next morning.
Both times it was still there and they held it till I retrieved
it.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 17:56:52 +0100
Reply-To:     Juergen Korthof <hplx@0800CALLING.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Juergen Korthof <hplx@0800CALLING.DE>
Subject:      AW: CEBIT2002 still nothing compares to our HPLX
In-Reply-To:  <HPLX-L%2002032209232168@UCONNVM.UCONN.EDU>
Mime-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Hi Daniel,

> Daniel Hertrich
> The most promising machine is IMO the Sharp Zaurus
> thing (palm sized,
> but with keyboard, Linux OS). Did you see that one
> on Cebit? I would be
> very interested in having a look at this machine.

There are at least two websites, where you get more
Information:
http://www.sharp.de/php/p.php?par=3D17_no_no_107

and
http://www.zaurus.de

It is a wonderful machine, but to me it is like
driving a Porsche with only a few liters Fuel-Tank-capacity.

It has a 950mAh LiIon-Battery. With permanent Color-TFT,
if won=B4t give enough mobility-time to me.

Happy LXing
Juergen.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 11:08:47 -0600
Reply-To:     John McCaskill <jmccask@POWERCHOKES.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John McCaskill <jmccask@POWERCHOKES.COM>
Subject:      CF inside HP100LX
In-Reply-To:  <000201c1d036$b600c640$b7acc8cb@q20>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I got a 16MB Sandisk CF & PCMCIA adapter for my 100LX. Works fine in the LX
and in my Antec USB PCMCIA reader attached to my desktop PC. I got a generic
128 MB FC from Fry's for $45.00 which works fine in my PCMCIA reader,
transfers files to & from my PC OK, but when I put it in the HP100LX I get a
"card not ready" error. I tried both the Antec and Sandisk PCMCIA adapters.

What am I missing here? What do I need to do to get this to work in my
100LX?

John

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 12:47:21 -0500
Reply-To:     amusse@mediaim.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Alfredo Musse T." <amusse@MEDIAIM.COM>
Subject:      WINCE: HP320LX
In-Reply-To:  <NFBBIDBHCLHDDBEKCHHDOEABCNAA.jmccask@powerchokes.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Dear friends,

I have a ericsson mc12 running WinCE 1.0, I read is just like the hp320lx.
Is there a way to connect this device to a LAN using a PCMCIA Lan Adapter
otherwise that changing the ROM first?
By the way does anyone knows where to find the WinCe 2.0 ROM Upgrade for the
hp320lx.

Thanks,


Alfredo Musse T.
media improvement - solutions for the digital world
Tel. (511) 562-0216
amusse@mediaim.com
http://www.mediaim.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 22 Mar 2002 19:41:33 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: AW: CEBIT2002 still nothing compares to our HPLX
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Juergen

On Fri, 22 Mar 2002 17:56:52 +0100, Juergen Korthof <hplx@0800CALLING.DE> wrote:

> It is a wonderful machine, but to me it is like
> driving a Porsche with only a few liters Fuel-Tank-capacity.
>
> It has a 950mAh LiIon-Battery. With permanent Color-TFT,
> if won4t give enough mobility-time to me.

So it seems to be time to collect all our hardware skills and use it
not longer for upgrading the HPLX, but for downgrading newer machines.
;-)

For example dimming the backlight, making processors slower, replacing
color with b/w screens, replacing WinCE ROMs with DOS ROMs....

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 07:17:24 +0800
Reply-To:     Oliver Chua <bud@MINDGATE.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Oliver Chua <bud@MINDGATE.NET>
Subject:      Dictionary pcmcia
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Hi Everyone,

I struck gold yesterday rummaging in the local second hand store.  I found
an HP dictionary / thesaurus (F1005A) pcmcia card for almost nothing.  Its
got a dictionary, a cool text pad and hangman game.

I tried copying the whole content into the internal memory (drive c) and to
my CF card (drive a) but it would not run from either.  It would always ask
for the original pcmcia card to be inserted.

Has anyone found a hack around this problem so that I don't have to keep
swapping cards everytime I want to use the dictionary or text pad?  Any ideas?

Thanks,

Oliver Chua

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 11:06:43 +1200
Reply-To:     Tony Hutchins <th@PARADISE.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Hutchins <th@PARADISE.NET.NZ>
Subject:      ANN: CLOCKS 5.5
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Sat, 23 Mar 2002 10:52:32 +1200 (NZT)

Yes, there is, as always <G>, a new verson of CLOCKS at
http://homepages.paradise.net.nz/th - the main new item is the
"E" key - this shows the sun/moon on the clock faces. Makes it
easy to quickly see if it is day/night for a clock, and where
the moon is. F1 shows help screens. "S" makes it tick like a
dripping tap<G>. "P" changes colours (VGA only). "Q" jumps to
next moon quarter phase, and "A" to the next solstice/equinox.
Also it now runs off the same DST data as in the WorldTime
file "timezone.dat", and can be synched with the WorldTime
"Custom Cities".

- Tony

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 08:30:39 +0100
Reply-To:     Josef Meyer <meyerjos@BLUEWIN.CH>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Josef Meyer <meyerjos@BLUEWIN.CH>
Subject:      Re: WINCE: HP320LX
Comments: To: "Alfredo Musse T." <amusse@MEDIAIM.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Alfredo,

evtl. this product might work:

CF Ethternet Adapter made by Socket
(http://www.socketcom.com, if I am right)

I bought one of those 2 years ago and it came with a setup and driver
for WinCE, but I can't remember if for 1.0 or 2.0.

Josef


Alfredo Musse T. wrote:
> Dear friends,
>
> I have a ericsson mc12 running WinCE 1.0, I read is just like the hp320lx.
> Is there a way to connect this device to a LAN using a PCMCIA Lan Adapter
> otherwise that changing the ROM first?

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 11:51:57 -0600
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
Comments: To: pksharma <pksharma@CAL.VSNL.NET.IN>
In-Reply-To:  <015801c1d09d$161b1100$2aadc8cb@q20>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

The Yahoo announcement means only that: IF you opted to get their
(occasional) junk email and in return be able to login and use their SMTP
and POP3 - that privilege is no longer free. You will still be able to get
Yahoo email via Web, and so on.

You will be able to receive and send email from your Yahoo email box by
using POST/LX - but only if you pay them for the privilege.

It is the way of many free things on the internet. Just recently ONEBOX.COM
which provided a free unified messaging and even using a toll-free number,
withdrew their free offer - it now costs, albeit modestly.

We will see a lot of these things. What worries me are not the services
with the "wow" value, but the barring of access to information for free.

Avi


At 3/20/02 11:56 PM, PKSHARMA wrote:
>all good things must come to an end ..
>the gooder they are .. the faster they end !
>(from pk's book of quotable quotes)
>(the book exists in ether, of course !)
>
>..pk
>
> > Effective April 24, 2002, Yahoo! Mail will no longer
>provide free POP3 Access or
> > Auto Mail Forwarding to Yahoo! Delivers subscribers.
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 21 Mar 2002 11:53:05 -0600
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: Fluff: Conclusions
Comments: To: Joseph.Buford@HSC.com
In-Reply-To:  <OF55F79691.D5DEF341-ON88256B83.00043ECF@hughes.com>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

<ROFL> ...


At 3/20/02 06:49 PM, you wrote:

>" There once was a lady of Paris........" <grin back>
>
>Avi,
>
>Been cool here (mid 60's). Ha Ha :-)
>
>How is the culture shock going?
>
>Joe
>
>
>
>
>hplxmail@yahoo.com on 03/20/2002 06:11:23 AM
>
>To:    Joseph.Buford@HSC.COM, hplx-l@uconnvm.uconn.edu
>cc:
>
>Subject:  Re: Fluff: Conclusions
>
>
>I'd like to hear you recite some poems in French! <VBG>
>
>     Avi
>(from Cool Minnesota - today 20 Mar, it is lovely skies and no snow, but
>plenty on unmelted stuff on the side of streets and on Lake O'Leary - ask
>me if you do not know about Lake O'Leary.)
>
>At 3/16/02 06:05 PM, you wrote:
> >Nathalie,
> >
> > >Eat & drink what you like. It's speaking English that kills
> >you. :)
> >
> >Perhaps I should learn french :-)
> >
> >Joe
> >
> >** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>
>_________________________________________________________
>Do You Yahoo!?
>Get your free @yahoo.com address at http://mail.yahoo.com


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 14:42:52 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: Dictionary pcmcia
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

if in dos5 .. try using the subst command

susbt a: c:\<SubDirName>

os will think its looking at A: instead of c:\<SubDirName>

(SubDirName is the name where you copied the files!)

..pk


-----Original Message-----
From: Oliver Chua <bud@MINDGATE.NET>
Date: Saturday, March 23, 2002 4:30 AM


>I tried copying the whole content into the internal memory
(drive c) and to
>my CF card (drive a) but it would not run from either.  It
would always ask
>for the original pcmcia card to be inserted.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 12:59:26 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
MIME-Version: 1.0
Content-Type: text/plain; charset=iso-8859-1
Content-Transfer-Encoding: quoted-printable

> It is the way of many free things on the internet.

Well, let`s be honest about one thing: None of those people was ever
planning to run a public service, they were out to make money - yours and
mine. Anf if they did not try to take it directly it was by far more
pernicious ways, selling addresses and details or some such. I never like=
d
that "free" attitude. Years ago, when you could access Compuserve via an
ASCII terminal, nothing was free but most of it was well worth the money.
Now nobody lets me pay them, but OTOH all I can get is worthless and
tedious junk.
To put it bluntly and succinctly: I still prefer to sit in a restaurant a=
nd
pay for having a meal served, even if McDonalds officially allow me to ra=
id
their waste pails for free. And from what I have so far found in that
brightly coloured web playground that comparison is unfortunately a rathe=
r
apt one.
And I=B4d me most delighted to be charged for every single mail if they c=
ould
ensure that the same held for all those spammers.

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 16:41:30 -0600
Reply-To:     hplx@TWU.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jessica Blank <hplx@TWU.NET>
Subject:      NO luck getting online. :/
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

Hi all.

Sorry I've been gone so long. Been super-busy with work!

I am trying to get my 200LX online via PPP. ALL I NEED IS TELNET. Period.
I need to be able to get online via PPP and TELNET OUT to my shell on
twu.net. That is IT. I do not need to do e-mail, FTP, Web, etc. on the
LX-- ONLY TELET. However, this goal seems elusive!

I have had great success via NetTamer on my laptop-- with the SAME copy of
NetTamer and the SAME PCMCIA modem (Noteworthy 14.4 xjack) I am trying on
the LX. It works on the laptop-- on the LX, it dials out, connects,
logs in, then FREEZES (I need to
ctrl-alt-del to get out of it) when it sets up the nameserver's IP
address.

If anyone could help me with this NetTamer problem, it'd be much
appreciated. I already e-mailed the nettamer people.

----------

I have also tried using the DOS PPPD/chat package (the one that is a port
of the Linux PPPD and chat). I can get it to dial out, but the chat
package is (as always) a bitch to configure; that, however, is not my
problem. I can manually log in using COMTOOL, then ctrl-C out of it and
run EPPPD.EXE. It loads into memory, resident at the 0x60 vector.

I then try running:

* NCSA Telnet's "TELBIN.EXE" (which crashes with a math error, and says
"Cannot find command interpreter - COMMAND.COM not found". I then must
reboot, obviously.)

* NCSA Telnet's "TELPKT.EXE", which freezes the machine. No error, it just
freezes.

* Minuet, which tries gathering Network info and then does nothing. It
does NOT freeze-- however, it also does not telnet, or do anything else
useful. :P

* IBM's old "MS-Kermit" Kermit program, which seems worthless. It
supposedly has a telnet client built in, but hell if I can figure it out.
I try the 'CONNECT' command, and help under that section of the program
mentions several things about telnet; however, I cannot seem to telnet
into twu.net!

PLEASE, can SOMEONE help me, SOMEHOW, dial into the Net via PPP and use
telnet!!??


=========================================
  J e s s i c a    L e a h    B l a n k
-----------------------------------------
  Programmer * Unix Sysadmin * Web Geek
 jessica@twu.net * http://www.JessL.org/
=========================================

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 15:47:12 -0800
Reply-To:     Ian Butler <ianb@HPLX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ian Butler <ianb@HPLX.NET>
Subject:      Re: NO luck getting online. :/
Comments: cc: Jessica Blank <hplx@twu.net>
In-Reply-To:  <Pine.LNX.4.40.0203231633430.8696-100000@twu.net>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Sat, 23 Mar 2002, Jessica Blank wrote:

> I am trying to get my 200LX online via PPP. ALL I NEED IS TELNET.
> Period. I need to be able to get online via PPP and TELNET OUT to my
> shell on twu.net. That is IT. I do not need to do e-mail, FTP, Web,
> etc. on the LX-- ONLY TELET. However, this goal seems elusive!

Have you tried LXTelnet (and, for SSH on the 200LX, SSHDOS)?  LXTelnet was
modified by Rod Whitby specifically for use on the 200LX, and is part of
the LXTCP package.  It's available at http://lxtcp.hplx.net.  Once you've
gotten LXTelnet working, you can substitute the SSHDOS program for the
LXTelnet program, keeping the same PPP setup, and have secure shell access
as well.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 18:07:42 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: NO luck getting online. :/
In-Reply-To:  <Pine.LNX.4.33.0203231542320.32419-100000@hplx.net>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Sat, 23 Mar 2002, Ian Butler wrote:

> Have you tried LXTelnet (and, for SSH on the 200LX, SSHDOS)?  LXTelnet was
> modified by Rod Whitby specifically for use on the 200LX, and is part of
> the LXTCP package.  It's available at http://lxtcp.hplx.net.  Once you've
> gotten LXTelnet working, you can substitute the SSHDOS program for the
> LXTelnet program, keeping the same PPP setup, and have secure shell access
> as well.

I have written a brief set of instructions for setting up LXTCP.
Have a look at:  http://heise.nu/LXTCP.html

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 20:20:07 -0600
Reply-To:     "Timothy P. Kelley" <tpkelley@HOUSTON.RR.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Timothy P. Kelley" <tpkelley@HOUSTON.RR.COM>
Subject:      Other Uses for 200lx
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Even though I use the 200LX for a nnumber of things,
I feel like I am under utilizing it in my daily life.

When I get to work I plug in my ac adapter and keep the
LX going by my desktop to record things to do etc.

I have suddenly gotten very busy at work, and have found that the
appointment book to do's are helping me to maintain
my sanity.

I am also having to charge back my time in my new job,
so I am using TT/LX for that.

QuickLX is helping me to quickly compose memos etc.

I have been using MM/LX on my project to help validate plans
and try to think outside the box.

I also use WWW/LX for my email needs.  I connect to my
cable modem via the Accton ethernet card for this.

I have developed a couple databases for recording desktop
service calls, and profiles.

Is there some common use that I am missing?

I do have an Ipaq.  But I found that it is only useful if
it has a wireless lan card.  And even then, the battery life is so
bad that it is hard to make it through a meeting.
I use it mainly to be able to support others with ipaqs.

Thanks,
Tim K

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 21:23:18 -0600
Reply-To:     hplx@TWU.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jessica Blank <hplx@TWU.NET>
Subject:      Re: NO luck getting online. :/
Comments: To: Ian Butler <ianb@hplx.net>
In-Reply-To:  <Pine.LNX.4.33.0203231542320.32419-100000@hplx.net>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

I will check that out! I hope it is not part of that expensive WWW/Lx
package. :)


=========================================
  J e s s i c a    L e a h    B l a n k
-----------------------------------------
  Programmer * Unix Sysadmin * Web Geek
 jessica@twu.net * http://www.JessL.org/
=========================================


On Sat, 23 Mar 2002, Ian Butler wrote:

> On Sat, 23 Mar 2002, Jessica Blank wrote:
>
> > I am trying to get my 200LX online via PPP. ALL I NEED IS TELNET.
> > Period. I need to be able to get online via PPP and TELNET OUT to my
> > shell on twu.net. That is IT. I do not need to do e-mail, FTP, Web,
> > etc. on the LX-- ONLY TELET. However, this goal seems elusive!
>
> Have you tried LXTelnet (and, for SSH on the 200LX, SSHDOS)?  LXTelnet was
> modified by Rod Whitby specifically for use on the 200LX, and is part of
> the LXTCP package.  It's available at http://lxtcp.hplx.net.  Once you've
> gotten LXTelnet working, you can substitute the SSHDOS program for the
> LXTelnet program, keeping the same PPP setup, and have secure shell access
> as well.
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 21:27:52 -0600
Reply-To:     hplx@TWU.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jessica Blank <hplx@TWU.NET>
Subject:      Re: NO luck getting online. :/
Comments: To: Theodore Heise <theise@NETINS.NET>
In-Reply-To:  <Pine.OSF.4.33.0203231806270.7997-100000@worf.netins.net>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

INSTRUCTIONS! Someone took the time to write INSTRUCTONS! You are a
goddess! Ah, err, god. Sorry, most of my friends are female. :>

Thank you! This should help me. I might toy with this after I do some
chores.

Now I will share my own instructions with you folks, in case anyone here
is a Unixhead (and I bet a bunch of you are). Here is my collection of
miscellaneous solutions to miscellaneous Unix annoyances:

http://fox.twu.net/tech/writing/tutorials/arghanswers.shtml

Yes, I like writing documentation too! :) ((I am a published author too)

Again THANK YOU!!! :)

Ah YES!! It is freeware. Thanks!

                                                --Jessica

=========================================
  J e s s i c a    L e a h    B l a n k
-----------------------------------------
  Programmer * Unix Sysadmin * Web Geek
 jessica@twu.net * http://www.JessL.org/
=========================================


On Sat, 23 Mar 2002, Theodore Heise wrote:

> On Sat, 23 Mar 2002, Ian Butler wrote:
>
> > Have you tried LXTelnet (and, for SSH on the 200LX, SSHDOS)?  LXTelnet was
> > modified by Rod Whitby specifically for use on the 200LX, and is part of
> > the LXTCP package.  It's available at http://lxtcp.hplx.net.  Once you've
> > gotten LXTelnet working, you can substitute the SSHDOS program for the
> > LXTelnet program, keeping the same PPP setup, and have secure shell access
> > as well.
>
> I have written a brief set of instructions for setting up LXTCP.
> Have a look at:  http://heise.nu/LXTCP.html
>
> --
> Ted Heise      <theise@netins.net>      West Lafayette, IN, USA
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 21:36:03 -0600
Reply-To:     hplx@TWU.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jessica Blank <hplx@TWU.NET>
Subject:      Re: NO luck getting online. :/
Comments: To: Theodore Heise <theise@NETINS.NET>
In-Reply-To:  <Pine.OSF.4.33.0203231806270.7997-100000@worf.netins.net>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

Err, I hate to be a pest when you have been helpful, but--

I cannot seem to reach that URL. I can't seem to connect to heise.nu.


=========================================
  J e s s i c a    L e a h    B l a n k
-----------------------------------------
  Programmer * Unix Sysadmin * Web Geek
 jessica@twu.net * http://www.JessL.org/
=========================================


On Sat, 23 Mar 2002, Theodore Heise wrote:

> On Sat, 23 Mar 2002, Ian Butler wrote:
>
> > Have you tried LXTelnet (and, for SSH on the 200LX, SSHDOS)?  LXTelnet was
> > modified by Rod Whitby specifically for use on the 200LX, and is part of
> > the LXTCP package.  It's available at http://lxtcp.hplx.net.  Once you've
> > gotten LXTelnet working, you can substitute the SSHDOS program for the
> > LXTelnet program, keeping the same PPP setup, and have secure shell access
> > as well.
>
> I have written a brief set of instructions for setting up LXTCP.
> Have a look at:  http://heise.nu/LXTCP.html
>
> --
> Ted Heise      <theise@netins.net>      West Lafayette, IN, USA
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 03:40:49 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: Other Uses for 200lx
Comments: To: "Timothy P. Kelley" <tpkelley@HOUSTON.RR.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Timothy P. Kelley wrote:
> Even though I use the 200LX for a nnumber of things,
> I feel like I am under utilizing it in my daily life.
...
> Is there some common use that I am missing?

Balance your checkbook with Quicken?  Also use it to track your
credit cards.

Spend a few free minutes playing a Curtis Cameron game.  You
don't have to complete a game in one setting if you devote a
Software Carousel session to it; just switch to it as you want.

Use Secure Device to create a small encrypted logical drive.
In this drive keep sensitive info like account numbers, pin
codes, userids and their passwords, etc.  I use a small bat file
to LOGIN to the drive then it edits my pw file and when I leave
the editor it locks the drive back up again.

I'm sure there are many other tasks.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 19:42:54 -0800
Reply-To:     Ian Butler <ianb@HPLX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ian Butler <ianb@HPLX.NET>
Subject:      Re: NO luck getting online. :/
Comments: cc: Jessica Blank <hplx@TWU.NET>
In-Reply-To:  <Pine.LNX.4.40.0203232123000.8696-100000@twu.net>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Sat, 23 Mar 2002, Jessica Blank wrote:

> I will check that out! I hope it is not part of that expensive WWW/Lx
> package. :)

No, WWW/LX's telnet client is called Telnet/LX, and is written
specifically for WWW/LX's TCP/IP stack.  LXTelnet is an open-source
modification of a pre-existing WatTCP telnet client, IIRC.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 21:45:46 -0600
Reply-To:     hplx@TWU.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jessica Blank <hplx@TWU.NET>
Subject:      Re: NO luck getting online. :/
Comments: To: Ian Butler <ianb@hplx.net>
In-Reply-To:  <Pine.LNX.4.33.0203231939450.2434-100000@hplx.net>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

Ah. With the names, t is easy to confuse 'em.


=========================================
  J e s s i c a    L e a h    B l a n k
-----------------------------------------
  Programmer * Unix Sysadmin * Web Geek
 jessica@twu.net * http://www.JessL.org/
=========================================


On Sat, 23 Mar 2002, Ian Butler wrote:

> On Sat, 23 Mar 2002, Jessica Blank wrote:
>
> > I will check that out! I hope it is not part of that expensive WWW/Lx
> > package. :)
>
> No, WWW/LX's telnet client is called Telnet/LX, and is written
> specifically for WWW/LX's TCP/IP stack.  LXTelnet is an open-source
> modification of a pre-existing WatTCP telnet client, IIRC.
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 22:09:49 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: NO luck getting online. :/
In-Reply-To:  <Pine.LNX.4.40.0203232135330.8696-100000@twu.net>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Sat, 23 Mar 2002 hplx@twu.net wrote:

> Err, I hate to be a pest when you have been helpful, but--
>
> I cannot seem to reach that URL. I can't seem to connect to heise.nu.

You can try http://www.heise.nu/LXTCP.html , but it's possible my
firewall is too restrictive.  Another place is:
http://showcase.netins.net/web/twheise/LXTCP.html

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 05:08:03 +0100
Reply-To:     Nathalie Bugeaud <tps-seti@WANADOO.FR>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nathalie Bugeaud <tps-seti@WANADOO.FR>
Subject:      Re: Happy Ending (Was: The saddest day in my life)
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 8bit

 >Adrian:
 >You might want to take pictures of them as well.  It's easier to
 >show them to the people you talk to, than try to describe

'one' of my underworld fiends who sells Mary-Jane sent me his pic of his
LX200 he says he needs it to track production and customers with 'secure
device'.._._ the LX is srrounded by $100000 in real 100 and 50 dollar-notes!

 >Qman:
 >Incase you all did know, I'm also a Transit Operator (Las Vegas,
 >NV). (:-0)

on the subject of 'trust' and Las Vegas i want to share a message from an
anonymous list member who sent money to an e-bay seller after winning a bit
on a palmtop:

 -insert start-
Still no palmtop! :( It's been a week since it was supposedly shipped from
Nevada on {snip} [the seller is working in a casino]. I'm not sure about
this.......... :(( This is the part about eBay that I don't like. :((( The
purchaser has to send money in an irrevocable form like a cashier's check or
money order, the seller cashes the check, and then supposedly the seller
sends the product. The only aspect to all of this is that it would be hard
to rip off more than a few people before the eBay controls catch up with the
seller. Nevertheless, there is much more protection for the seller than for
the buyer. I do know a couple buyers who were defrauded on eBay, but they
had used PayPal and were eventually protected by the credit card company
that was used with PayPal, but not by PayPal itself. eBay gives the buyer no
protection - "let the buyer beware". Oh well, we'll keep hoping. I don't
think that I will do this again, at least not with someone who has only 2
sales on eBay like this guy. One always hears stories like "I found it on
eBay - good price", but I wonder what the fraud rate is.  -insert end-
nat

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 23 Mar 2002 23:12:34 -0800
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: Need a Thaddeus 56K Modem Driver
In-Reply-To:  <5.1.0.14.2.20020322085132.00a86e30@pop.mail.yahoo.com>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Thanks to William for a fast response. The driver he sent worked well.

Avi



At 3/22/02 -0800, you wrote:
>I have one of Thaddeus' 56KB modems (it says "56K Fax Modem" on the front).
>
>I believe it had a diskette with a driver on it when I got the modem from
>Thaddeus. Does anyone know?
>
>I am rebuilding an OB800CT and Win95b in it does not recognize the modem as
>a 56K, only as a standard 28.8 modem.
>
>Anyone has a better driver for it? If you do, please send it to me, or let
>me know a URL where I can d/l it (Thaddeus' site maybe?)
>
>Thanks in advance
>
>
>_________________________________________________________
>Do You Yahoo!?
>Get your free @yahoo.com address at http://mail.yahoo.com
>
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 18:11:38 +0800
Reply-To:     Oliver Chua <bud@MINDGATE.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Oliver Chua <bud@MINDGATE.NET>
Subject:      dictionary pcmcia
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Pk,

Will not work.  That is the same as me putting the files in the root
directory of my CF card.  It seems before the dictionary exm program runs,
it makes a checksum check to make sure the dictionary pcmcia card is the
one inserted.

Oliver

>if in dos5 .. try using the subst command
>
>susbt a: c:\<SubDirName>
>
>os will think its looking at A: instead of c:\<SubDirName>
>
>(SubDirName is the name where you copied the files!)
>
>..pk

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 10:56:09 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      FA: 95LX and 200LX on ebay
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

I have currently two palmtops on ebay for sale.
One is a defective 95LX (mainboard OK, screen has with a loose
contact, needs pressure to begin to work, but is otherwise OK,
hinge defective, case defective). Only good as a spare part holder.

The other one is a 200LX with 3 MB RAM (upgraded, original 1MB) in good
condition, with only two little problems: The latch springs are broken,
I have fixed that with a little piece of foam stuffed under the latch,
and the screen has 4 missing pixel columns, which I have tried to fix,
but was unable, because it was the first screen which I _tried_ to fix
and I made a mistake... :-( now a few pins of one of the screen ICs
are unusable. See pictures. The effect of the 4 missing columns is not
_that_ bad, the LX is still well usable.

For you list members, I also ship within Europe, not only to Germany,
as the auction says.

Auction numbers:
95LX:  1340802273
200LX: 1341494616

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 12:20:47 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: NO luck getting online. :/
MIME-Version: 1.0
Content-Type: text/plain; charset=iso-8859-1
Content-Transfer-Encoding: quoted-printable

I am surprised NT doesn't work for you. Did you give it all the RAM and t=
ry
to run it without 200.com loaded? If run from PIM did you use the inverte=
d
exclamation mark?
I have found it more bulky and cumbersome than going postal for my email
needs, but apart from that I had it working faultlessly.

I did have some problems with hangups in the beginning though and as I am
too old to remember well I just looked it up. This is what I wrote to Dav=
id
Colston about it:

--------------------------------------------------------------------
I have found two things you might want to pass on in the doc or faq:

The hangups weren=B4t there at first so it must have been something I did=
 -
and it was. The 700 comes with a smart charge utility in ROM, named
smartchg.com but started by call like a batch - no doc whatever. I called
that before nt as I might use a cardmodem with external power and that di=
d
it - so leave it off!

My standard autoexec.bat is on drive A:. Drive C: is only used for data
transfer where the slot may be needed for a modem. So on C: there are:

autoexec.bat:
prompt $p$g
path c:\dos;d:\;d:\bin;d:\dos
c:
cic100 /gen 1

and for using the ROM programs
hp.bat:
call smartchg.com
d:\bin\lamptsr.com /l /i
d:\bin\comtsr.com /L
if exist d:\bin\700.com goto omni
200
goto end
:omni
700
:end

(If you do not have both a 200 and the 700 this can of course be cleaned =
up
a bit.)
--------------------------------------------------------------------

Hope this helps. By the way if you and Ian go on quoting each other in fu=
ll
your mails will soon be too big to fit on an LX. Please do not introduce
windumb misbehaviour into a group for sensible machines.

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 08:56:18 -0500
Reply-To:     Martin Bergvill <hplx@BERGVILL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Martin Bergvill <hplx@BERGVILL.COM>
Subject:      Re: Nokia 3360
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Wed, 20 Mar 2002 14:25:32 -0500, Walter Francis wrote:

> I hope your 3360 will have a newer firmware than mine, I have trouble with
> my phone locking up sometimes..  Mostly when I'm playing games tho.  :)
> Happens occationally in WAP too.  BTW, whoever designed the interface to WAP
> was an idiot, it's SO SLOW to browse around and such.  Oh well.

I never used wap when I had a Nokia 7110 and 6210. Now I have Ericsson
T39 and wap over gprs. It works okey. Much faster than with 7110/6210.

Regards

--
Martin Bergvill ,Narvik Norway

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 09:37:38 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Axel Berger wrote:
> Well, let`s be honest about one thing:
> None of those people was ever planning to run
> a public service, they were out to make money
> - yours and mine. Anf if they did not try to take it
> directly it was by far more pernicious ways,
> selling addresses and details or some such.
> I never liked that "free" attitude. Years ago,
> when you could access Compuserve via an
> ASCII terminal, nothing was free but most of it
> was well worth the money. Now nobody lets me
> pay them, but OTOH all I can get is worthless and
> tedious junk.

I can't actually disagree with you but a lot of us remember
that, while you were paying the high price for Compuserve (so
did I) we were also using the not very well known internet.
There was no WWW then.  There wasn't anything you could pay for.
But there was a lot of really good content provided by people
who worked hard on their own time to put it there.

It wasn't commercial content.  You couldn't buy things on the
internet.  But there was good solid access to information.

Now everybody thinks the internet is the WWW but all the real
meat is still there.  There are newsgroups (still the best
information source on the internet), listserves like this one,
email.  There is gopher, a menu system that linked everything on
the net like the WWW does except that it was just a text
roadmap, not a lot of  hype.  There is archie that can find
files anywhere they might exist on the internet so you can find
what you're looking for.  There are games like MUDs that are
probably more elaborate than anything you'll find on the web or
in a computer store.  Not more flashy but far more intricate and
feature filled.  And all you need to access this stuff is an
ascii terminal.

Free stuff done by people who had no interest in making money
was what built the internet.  It truly brought people from all
over the world together, person to person.  Just like this
listserve does.  Anyone who wanted to could join a group or form
their own group to create something new for the internet.  And a
LOT of people did.  It was all created by the people using it.

It's all still there but what will eventually kill it is the
commercial success of the WWW.  More and more controls will be
needed to protect that and our access to the internet will be
controled and reduced and confined, eventually, to the point
that we won't be able to acces those things that nobody today is
being told about anyway.

I enjoy the commercial uses of the internet and it's happening
and nothing will stop it.  So there's no point in complaining
about it.  Except that one of the most beautiful things in human
history is being turned into one of the most successful things.
That's painful and lamentable.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 07:56:09 -0800
Reply-To:     patrick@west.net
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Patrick West <francis_patrick_west@YAHOO.COM>
Subject:      1993 IBM New Bible Library with softcopy nav
In-Reply-To:  <00b601c1c0ba$92893480$077dfea9@downeast>
Mime-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Folks,

Back in 1993 IBM partnered with Ellis Enterprises to produce
the New Bible Library using the Softcopy Nav program, a version=
 of
their Bookmanager Read program. (ISSC)

If anyone happens across a copy please tell me. I'd love to get a=
 copy of it.
It uses an old DOS based program that runs fine on my dos based=
 palmtop.

I recently setup the "Revised English Bible" from my Old dos=
 based "Oxford
Reference Library" on my palmtop and it works nicely.
--
Patrick West, patrick@west.net on 03/23/2002

--
Patrick West, francis_patrick_west@yahoo.com on 03/24/2002



_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 11:44:24 -0500
Reply-To:     Tom <tom.hornberger@VERIZON.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tom <tom.hornberger@VERIZON.NET>
Subject:      Docking cradle for 200LX
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Does any one know where I could obtain 1 or 2 of the old Sparcom(?)
docking cradles for the 100/200?  I want set up a permanent connection
to my desktop machines at home and at work.  I remember a post about a
year ago for a source for the cases only.  Anybody happen to have that
info?

TIA,
Tom

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 12:40:30 -0600
Reply-To:     hplx@TWU.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jessica Blank <hplx@TWU.NET>
Subject:      Re: NO luck getting online. :/
Comments: To: Axel.Berger@NexGo.De
In-Reply-To:  <3C9DB68F.856901D0@NexGo.De>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

Oh! I am sorry. I didn't realize people on the list actually read the list
FROM 200LXes.

I use PINE on Linux for my e-mail, for the record. And always have, for
the past 5+ years. :)

                                                        --Jessica

=========================================
  J e s s i c a    L e a h    B l a n k
-----------------------------------------
  Programmer * Unix Sysadmin * Web Geek
 jessica@twu.net * http://www.JessL.org/
=========================================

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 10:42:32 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      MochaPPP
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Those of you on this list who know me also know I am always
behind the curve. I let others test the "bleeding edge" and
then I learn from your experience.<G>

Well, I was way behind reading messages so I didn't learn
about MochaPPP until yesterday. I installed it today,
configured my copy of WWW/LX 2.2 per Avi's message of December
19, 2001 and it works just great! The only difference in
method is that I created the MochaPPP section and the
MochaPPP_Script section in www.cfg by hand, and was able to
get MochaPPP to install in \Program Files\MochaPPP by creating
the empty directory before I ran Setup (for the second time -
since it failed when the directory did not exist.)

My host machine is an IBM X21 laptop running Win98SE. The X21
is connected to the Inet via Ethernet and a cable modem. My ISP
is Earthlink and, while I do have both hardware and software
firewalls on my home network, I do not have a proxy server.

This shareware seems to be worth far more than the $9.95
registration price.

Vic Roberts

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 19:55:48 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Fluff: WWW vs. Usenet
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> There are newsgroups (still the best information source on the internet

I'd love to agree with you, unfortunately I can't and may, after years of
use decide to quit usenet completely some time soon. With all those
illiterate yobs crowding in and writing two lines of irrelevant comment
completely hidden in several pages of quotes, mostly many stages deep, it
is no more worth reading but fill the address I use there with spam to the
brim. (All other addresses are completely clean, at least when not counting
unsolicited commercials from the mailbox providers.) I will not and never
stoop so low as post using a munged reply address and so will have to
leave. All this elctronic data exchange used to be so nice and useful once
...

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 20:10:07 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      charging system
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

I need help fromthose experinced with the power system. My only 200 LX
nearly (but funnily not quite) always shows the following symptoms:
Plugging the charger in (and a regulated lab power supply at 10.5 V, so
that isn't the reason) drives the diplay completely black. It also the
totally ruins voltage measurement. A voltage of 2.7 V is read as something
as low as 2.2 V which becomes visible for a short time on pulling the plug
out. Also if left in that state unobserved for a time, the voltage graph in
ABC looks terrible.
Is there an obvious place to start looking?

Danke
        Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 20:20:50 +0100
Reply-To:     Klaus Reinhardt <K.Rdt@TU-BERLIN.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Klaus Reinhardt <K.Rdt@TU-BERLIN.DE>
Subject:      Re: Fluff: Spamfilter
In-Reply-To:  <3C9A772F.9395BE11@union-tel.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Am 22.03.02 01:13:35, schrieb "Robert K. Meyer" <bmeyer@UNION-TEL.COM>:

>I have also been using MailWasher on Tom's recommendation.
>The website indicates that bounced email appears exactly as
>if bounced by your email server, no indication of MailWasher
>intervention. I think it is good enough that I may even
>register the program.
----------------- mailto:K.Rdt@TU-Berlin.DE start -------------------
Hi
Thank you so much for this tip!
                K@Rdt
----------------- mailto:K.Rdt@TU-Berlin.DE !end! -------------------

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 20:36:03 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: charging system
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Addendum:

As the condition throws voltage measurement out of kilter it naturally also
results in spurious "backup battery low" warnings.
And I just managed to cure it (for the time being):
With the screen black I drove the volage (from the regulated supply) right
up to nearly 14 V and everthing suddenly righted itself. I was then able to
take it back to 10.5 V again and can now unplug it and plug it in again,
manually stop and strt charging and do what I want to. Of course that
"cure" is not one I want to repeat nor is that a very practical
proposition, but perhaps it tells one of you something about what is wrong
inside.

Danke
        Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 20:39:54 +0100
Reply-To:     Zoran Vignjevic <zoranv@GOV.YU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Zoran Vignjevic <zoranv@GOV.YU>
Subject:      One my old game for my new 200lx...
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Hi,
I am the new owner of 200lx and last 30 years I am in IT...
I've found one of my old old games:
for given 5 (possible more) numbers, max 255 (posible more) players can
substract any number from just one given number of 5...
Winer is first one who get all (5) zero's...
I put gwbasic onto 200lx and tiped basic program to show algorithm...
With your 200lx you can play simultaniously with lot of players...
Because comp gives stable state and the other player only make it
unstable.
If the first player give you the stable state 5 nubmers stay the same
and you can substract just one from bigest number and wait the other
player to make mistake...
Trivial stable state is x,x,0,0,0 because if the other player makes it
x-n,x,0,0,0 you make x-n,x-n,0,0,0
The other trivial stable state is x,y,x,y,0...

If you want to play just rem all prints except 60,450 and 490 (there are
few remed prints from debugging also...)
As you will see stable state is when all columns of binary presentations
of the 5 numbers has even numbers of 1's (test line shows it).
There is no the end of program, just CtrlC... If you don't know it and
like it make it finished :)

10 CLEAR
20 DEFINT A-Z
30 OPTION BASE 1
40 DIM D(5),B(40),T(8)
50 INPUT D(1),D(2),D(3),D(4),D(5)
60 PRINT D(1);D(2);D(3);D(4);D(5)
70 GOSUB 90
80 GOTO 290
90 REM
100 FOR I=1 TO 5
110 FOR J=1 TO 8
120 B((I-1)*8+J)=(D(I) AND 2^(8-J))/2^(8-J)
130 PRINT B((I-1)*8+J);
140 NEXT J
150 PRINT D(I)
160 NEXT I
170 PRINT
180 FOR J=1 TO 8
190 T(J)=0
200 FOR I=1 TO 5
210 T(J)=T(J) + B((I-1)*8+J)
220 NEXT I
230 TT=T(J)/2
240 T(J)=ABS(T(J)-TT*2)
250 PRINT T(J);
260 NEXT J
270 PRINT "test"
280 RETURN
290 FOR J=1 TO 8
300 PRINT
310 IF T(J)=0 THEN 480
320 REM PRINT J
330 FOR I=1 TO 5
340 IF B((I-1)*8+J)=0 THEN 470
350 REM PRINT I
360 FOR K=J TO 8
370 IF T(K) = 1 THEN B((I-1)*8+K)=1-B((I-1)*8+K)
380 REM PRINT ((I-1)*8+K); B((I-1)*8+K)
390 NEXT K
400 D(I)=0
410 FOR K=1 TO 8
420 D(I)=D(I)+B((I-1)*8+K)*2^(8-K)
430 NEXT K
440 GOSUB 90
450 PRINT D(1);D(2);D(3);D(4);D(5)
460 GOTO 10
470 NEXT I
480 NEXT J
490 PRINT D(1);D(2);D(3);D(4);D(5)
500 GOTO 10

Regards,
Zoran

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 21:35:59 +0100
Reply-To:     Juergen Korthof <hplx@0800CALLING.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Juergen Korthof <hplx@0800CALLING.DE>
Subject:      AW: charging system
In-Reply-To:  <3C9E2AA3.EFEA9130@NexGo.De>
Mime-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Hello Axel,

> up to nearly 14 V and everthing suddenly righted
> itself. I was then able to
> take it back to 10.5 V again and can now unplug it
> and plug it in again,

I want to mention, I use a 12V-Adapter! - And it makes no
problems.
On the Back of my LX is a print that tells me to use 12V.

Are you really using a _rare_ LX that uses 10,5V ???


Happy LXing
Juergen

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 16:14:30 EST
Reply-To:     HiLill@AOL.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Harb Lill <HiLill@AOL.COM>
Subject:      Sandisk 64Mb CF not recognized
MIME-Version: 1.0
Content-Type: text/plain; charset="US-ASCII"
Content-Transfer-Encoding: 7bit

Hello all,

I have enjoyed lurking for years, but now find myself in need of a list
assist.  I couldn't log onto the HPLX.net for faq assistance and my attempts
to search the archives proved overwhelming -- I guess I can't build decent
query.

I have a 4Mb doublespeed HP200LX.  It works flawlessly with a variety of
PCMCIA cards, most recently a Sandisk 20Mb.

At a recent computer show, I impulsively bought a Sandisk CompactFlash PC
card adaptor and a Sandisk 64Mb CF card.

I popped the adaptor and new CF card into my 200LX.  Filer did not detect the
card, and when I attempted to select the A: drive, I was notified "Drive not
ready".  I went to the DOS C: prompt and attempted to format the new card.  I
was prompted to put a new card into the a: drive and hit enter.  I was
notified that "format not supported on drive A:, format terminated"

I inserted the adaptor and new CF card into my laptop.  It was recognized as
an unformated Sandisk 64Mb card.  When prompted, I formatted the card using
FAT (not FAT 32).  The laptop subsequently recognized and read the card,
however, the 200LX still does not.

I also put my "old" Sandisk card into the laptop and it had no trouble
reading my files.

Am I overlooking something...or have I wasted $29 on the card?

Thanks for your help.

Best, Harb

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 16:38:30 -0500
Reply-To:     Bill Sprague <eugarps@MINDSPRING.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bill Sprague <eugarps@MINDSPRING.COM>
Subject:      Re: Fluff: WWW vs. Usenet
Comments: To: Axel.Berger@NexGo.De
In-Reply-To:  <3C9E2134.7B6330D4@NexGo.De>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Axel wrote:

<snip> With all those illiterate yobs crowding in and writing two lines of
irrelevant comment completely hidden in several pages of quotes, mostly many
stages deep, it is no more worth reading but fill the address I use there
with spam to the brim. <snip>

Axel,

I agree with your analysis of usenet news.  I logged on to the Nissan
vehicle newsgroup with a valid question and got a bunch of folks responding
who obviously didn't know the answer to my question but that didn't keep
them from making fun of my question.  I never did get the answer from there.
So much for community!

The usenet news groups seem to be populated by a bunch of people who now
know each other and really don't want anyone else to crash their party.

Best,

Bill

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 14:31:39 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: Sandisk 64Mb CF not recognized
Comments: To: HiLill@AOL.COM
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Sun, 24 Mar 2002 16:14:30 EST, Harb Lill <HiLill@AOL.COM> wrote:

[snip]

> At a recent computer show, I impulsively bought a Sandisk CompactFlash PC
> card adaptor and a Sandisk 64Mb CF card.
>
> I popped the adaptor and new CF card into my 200LX.  Filer did not detect the
> card, and when I attempted to select the A: drive, I was notified "Drive not
> ready".  I went to the DOS C: prompt and attempted to format the new card.  I
> was prompted to put a new card into the a: drive and hit enter.  I was
> notified that "format not supported on drive A:, format terminated"
>
> I inserted the adaptor and new CF card into my laptop.  It was recognized as
> an unformated Sandisk 64Mb card.  When prompted, I formatted the card using
> FAT (not FAT 32).  The laptop subsequently recognized and read the card,
> however, the 200LX still does not.
>
> I also put my "old" Sandisk card into the laptop and it had no trouble
> reading my files.
>
> Am I overlooking something...or have I wasted $29 on the card?

Well, it seems you have done all the right things. I use a
192MB Sandisk CF card in my 200LX, so we know the card size is
not a problem.

There used to be some issue with the Master Boot Record on
flash cards used in the LX. You may want to use FDISK100 to
set up the card. FDISK100 is located in D:\bin on your 200KX.

Vic Roberts

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 24 Mar 2002 16:20:23 -0800
Reply-To:     Longden_Loo@CANDLE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Longden Loo <Longden_Loo@CANDLE.COM>
Subject:      Re: dictionary pcmcia
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

I've never heard of a hack to get the HP dictionary card software working
off another flash card (or in RAM), tho that doesn't mean there isn't one.

It may be better to just put the card on your "collectibles" shelf, and
spend the $36 for the Collins software from Thaddeus if you really need a
dictionary on your main flash card.

My $.36

- Longden

> Will not work.  That is the same as me putting the files in the root
> directory of my CF card.  It seems before the dictionary exm program
runs,
> it makes a checksum check to make sure the dictionary pcmcia card is the
> one inserted.
>
> Oliver
>
> >if in dos5 .. try using the subst command
> >susbt a: c:\<SubDirName>
> >os will think its looking at A: instead of c:\<SubDirName>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 00:27:58 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: NO luck getting online. :/
Comments: To: hplx@TWU.NET
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Jessica Blank wrote:
> Oh! I am sorry. I didn't realize people on the list actually read the list
> FROM 200LXes.

I use WWW/LX on my 200LX to do all my personal email and
newsgroups.  This includes several lists and rec.guns (@1000
posts/week).

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 10:39:10 -0800
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: dictionary pcmcia
MIME-Version: 1.0
Content-Type: multipart/alternative;
              boundary="----=_NextPart_000_007F_01C1D3E9.4C3B9B20"

This is a multi-part message in MIME format.

------=_NextPart_000_007F_01C1D3E9.4C3B9B20
Content-Type: text/plain;
        charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

u r right .. using exm means not in pure dos ..
wont work

..pk

(i learn too .. each day :-D )

----- Original Message -----
From: "Oliver Chua" <bud@MINDGATE.NET>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Sunday, March 24, 2002 2:11 AM
Subject: dictionary pcmcia


> Pk,
>
> Will not work.  That is the same as me putting the files
in the root
> directory of my CF card.  It seems before the dictionary
exm program runs,
> it makes a checksum check to make sure the dictionary
pcmcia card is the
> one inserted.




------=_NextPart_000_007F_01C1D3E9.4C3B9B20
Content-Type: text/html;
        charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0 Transitional//EN">
<HTML><HEAD>
<META http-equiv=3DContent-Type content=3D"text/html; =
charset=3Diso-8859-1">
<META content=3D"MSHTML 5.50.4134.600" name=3DGENERATOR>
<STYLE></STYLE>
</HEAD>
<BODY bgColor=3D#ffffff>
<DIV><FONT face=3D"Comic Sans MS" size=3D2><FONT face=3D"Times New =
Roman" size=3D3>u r=20
right .. using exm means not in pure dos ..<BR>wont =
work<BR><BR>..pk<BR><BR>(i=20
learn too .. each day :-D )<BR><BR>----- Original Message -----<BR>From: =
"Oliver=20
Chua" &lt;</FONT><A href=3D"mailto:bud@MINDGATE.NET"><FONT face=3D"Times =
New Roman"=20
size=3D3>bud@MINDGATE.NET</FONT></A><FONT face=3D"Times New Roman"=20
size=3D3>&gt;<BR>To: &lt;</FONT><A =
href=3D"mailto:HPLX-L@UConnVM.UConn.Edu"><FONT=20
face=3D"Times New Roman" =
size=3D3>HPLX-L@UConnVM.UConn.Edu</FONT></A><FONT=20
face=3D"Times New Roman" size=3D3>&gt;<BR>Sent: Sunday, March 24, 2002 =
2:11=20
AM<BR>Subject: dictionary pcmcia<BR><BR><BR>&gt; Pk,<BR>&gt;<BR>&gt; =
Will not=20
work.&nbsp; That is the same as me putting the files<BR>in the =
root<BR>&gt;=20
directory of my CF card.&nbsp; It seems before the dictionary<BR>exm =
program=20
runs,<BR>&gt; it makes a checksum check to make sure the =
dictionary<BR>pcmcia=20
card is the<BR>&gt; one =
inserted.</FONT><BR><BR><BR></FONT></DIV></BODY></HTML>

------=_NextPart_000_007F_01C1D3E9.4C3B9B20--

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 10:39:13 -0800
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: dictionary pcmcia
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

u r right .. using exm means not in pure dos ..
wont work

..pk

(i learn too .. each day :-D )

----- Original Message -----
From: "Oliver Chua" <bud@MINDGATE.NET>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Sunday, March 24, 2002 2:11 AM
Subject: dictionary pcmcia


> Pk,
>
> Will not work.  That is the same as me putting the files
in the root
> directory of my CF card.  It seems before the dictionary
exm program runs,
> it makes a checksum check to make sure the dictionary
pcmcia card is the
> one inserted.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 00:21:07 -0500
Reply-To:     John Alley <chia@ICX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John Alley <chia@ICX.NET>
Subject:      A question on compact flash cards......
In-Reply-To:  <20020325050142.LQII683.fl-mta02@UConnVM.UConn.Edu>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

        Ok, I have a HP100LX that I use daily... and I finally got a PCMIA-->CF
adaptor card (SanDisk) that works great with the 16Meg CF card I have. Now
I got a 32Meg Lexar card from a friend. It will not work... I know it was
used in a digital camera and was wondering if there is something that I can
do to get it to work.. or is the limit about 16Megs on the CF usage in the
HPLX pamltops....? Any info is greatly apprecaited. Thanks...

73 de KF4UAE
www.qsl.net/kf4uae
John R. Alley
kf4uae@arrl.net

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 17:45:05 +1200
Reply-To:     Tony Hutchins <th@PARADISE.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Hutchins <th@PARADISE.NET.NZ>
Subject:      ANN: POSTPDU & CLOCKS
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Mon, 25 Mar 2002 16:33:32 +1200 (NZT)

Just to say POSTPDU version 1.28 and CLOCKS version 7.0 are
now at http://homepages.paradise.net.nz/th

POSTPDU has a trap for long lines in a message. Previously a
line of over 508 characters, without a CR/LF, caused an
"unknown command" error report. Now, this is reported a little
more explicitly.

CLOCKS 7.0 can now do not only the sun/moon, but also can put 5
other planets on the rim of the clocks. So, now you can tell
whether Mercury/Venus will be a "morning star" or an "evening
star", and if you think you see Jupiter or Mars, you will be
able to confirm it with CLOCKS :) Also in effect it does a rough
horoscope which is surpringly accurate, although the ascendant
etc shown are only valid at latitude zero. Examples included -
a horoscope can be stored in a one line .BAT file and replayed
easily. F1 does help now, and only one key quits (ESC).

- Tony

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 08:09:31 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      Re: strange behaviour of DS 200lx
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

So I "found" the problem. BREAK=ON in config.sys. After removing this line strange behaviour was gone. I really have no
idea how this could have some connection with a card inserted or AC adaptor plugged. I would except such strange
things from a windows machine not from dos:-)

Radek





                      Daniel Hertrich
                      <daniel.hertrich             To:  HPLX-L@UConnVM.UConn.Edu
                      @GMX.DE>                     cc:  (bcc: Radek Svagr/HRC/COMP/PHILIPS)
                      Sent by: HPLX                Subject:   Re: strange behaviour of DS 200lx
                      Mailing List
                      <HPLX-L@UConnVM.             Classification:
                      UConn.Edu>


                      2002-03-22 12:26
                      PM
                      Please respond
                      to Daniel
                      Hertrich






Hi Radek

On Fri, 22 Mar 2002 11:01:20 +0100, Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM> wrote:

> I' am observing strange behavior of my DS 200lx.
> Disk operations /C drive/ are much slower when CF card is not inserted. If I insert a CF card back, the execution of programs from C: drive is much faster.
> I have no path  assigned to a: so it cannot be caused by acesing not acessible A: drive. My 200lx is completely independent form A: drive.

hmmm - did you already solder around at the PCMCIA slot? ;-)

Otherwise I would suggest a hard reset. Maybe jsut some software has
chained into the disk access. Any drivers loaded?

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 08:29:41 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      CF catd inside 200lx - RESULTS:-(
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

So here are the results of my experiments: for these who don't like long explanations - didn't  work.

Now somethig longer:

First I soldered all 50 wires to CF card (uff)
then I started to solder it to 200lx, but realized that it is really dangerous because mean time my soldering device
became dead and I dindn't want to kill 200lx with a spare soldering device.
So I took one my many Olivetti quaderno spare motherboards and unsoldered a PCMCIA slot from it.
Then I disassembled a PCMCIA-CF card adaptor and connected this PCMCIA slot to it (soldering 2*68
wires - uff uff)
Finally I had a PCMCIA to CF and PCMCIA adaptor.

Now the test:

CF card first modem last: no sucess. CF card was sometimes readable sometime 200 lx freezed
Modem first CF card last: no sucess modem was detected by lxcic, after an isertion of CF card
a CF card taken over a socket one (detected by LXCIC) but nothing was aceessible.
Similar results with CF - SRAM combination and CF - FLASH card combination.
I also tried LXCIC2 and DSLOT.SYS. LXCIC2 never detected a card in a socket 2

Conclusion: 2 cards cannot work in paralel in 200lx. It may need some additional hardware which is in ACCURITECH
double slot adaprtor, or  different connections of some signals. Please note that card detect 1 and 2 signals are according
to what I have seen connected together and grounded in every card.

BTW: any owner of accuritech doubleslot adaptor willing to look what is inside?;-)


Radek

I appologize for possible worse readability of this text. I use lotus notes 5.0 which i a real shit and has a very special way of text formating.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 10:15:33 +0100
Reply-To:     Lillebjorn Nilsen <bjni@ONLINE.NO>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Lillebjorn Nilsen <bjni@ONLINE.NO>
Subject:      Re: Sandisk 64Mb CF not recognized
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

On Sun, 24 Mar 2002 16:14:30 EST, Harb Lill <HiLill@AOL.COM> wrote:
>
> At a recent computer show, I impulsively bought a Sandisk CompactFlash =
PC
> card adaptor and a Sandisk 64Mb CF card.
>
> I popped the adaptor and new CF card into my 200LX.  Filer did not =
detect the
> card, and when I attempted to select the A: drive, I was notified =
"Drive not
> ready".  I went to the DOS C: prompt and attempted to format the new =
card.  I
> was prompted to put a new card into the a: drive and hit enter.  I was
> notified that "format not supported on drive A:, format terminated"

Strange. I have a Sandisk 64MB working
with no problems in my HP200LX. I don't
think I even had to format it. It is in
the slot. Could your card adaptor be the
problem?

 -----------------
 Lillebjorn Nilsen, Oslo Norway
 http://home.online.no/~bjni/lillebjorn.html
 http://bjni.home.online.no

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 14:12:39 +0100
Reply-To:     Zoran Vignjevic <zoranv@GOV.YU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Zoran Vignjevic <zoranv@GOV.YU>
Subject:      Re: Sandisk 64Mb CF not recognized
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

On Sun, 24 Mar 2002 16:14:30 EST, Harb Lill <HiLill@AOL.COM> wrote:
>
> At a recent computer show, I impulsively bought a Sandisk CompactFlash
PC
> card adaptor and a Sandisk 64Mb CF card.
>
> I popped the adaptor and new CF card into my 200LX.  Filer did not
detect the
> card, and when I attempted to select the A: drive, I was notified
"Drive not
> ready".  I went to the DOS C: prompt and attempted to format the new
card.  I
> was prompted to put a new card into the a: drive and hit enter.  I was

> notified that "format not supported on drive A:, format terminated"

Strange. I have a Sandisk 64MB working
with no problems in my HP200LX. I don't
think I even had to format it. It is in
the slot. Could your card adaptor be the
problem?

 -----------------
 Lillebjorn Nilsen, Oslo Norway
=============================================

Maybe Harb has to push PCMCIA adapter just 1 or 2mm more...
This happened to me with PCMCIA adapter for Smartmedia cards...
At first, nothing,but when I pushed litle more I can read/write all
sizes of my SM cards, 32-128MB, (size is critical with SM and not so
much with CF).PCMCIA adapter for CF is pasive circuit because ATA flash
card and CompactFlash card are the same logical andpin layout format,
CFis just more compact...
If it is not so, error is in some pin connection between input for CF
and ATA output to comp...

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 14:21:56 +0100
Reply-To:     Zoran Vignjevic <zoranv@GOV.YU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Zoran Vignjevic <zoranv@GOV.YU>
Subject:      Re: Sandisk 64Mb CF not recognized
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

But, before new trial, it is good to make reset of 200lx, cause info about
"A: FAILED" maybe stays somewhere and prevent further accessto A: ...
Anyhow I've done it, and afterwords when push litle bit more,everything was
ok.
Regards,
Zoran

Zoran Vignjevic wrote:

> Maybe Harb has to push PCMCIA adapter just 1 or 2mm more...
> This happened to me with PCMCIA adapter for Smartmedia cards...
> At first, nothing,but when I pushed litle more I can read/write all
> sizes of my SM cards, 32-128MB, (size is critical with SM and not so
> much with CF).PCMCIA adapter for CF is pasive circuit because ATA flash
> card and CompactFlash card are the same logical andpin layout format,
> CFis just more compact...
> If it is not so, error is in some pin connection between input for CF
> and ATA output to comp...
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 08:28:39 EST
Reply-To:     HiLill@AOL.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Harb Lill <HiLill@AOL.COM>
Subject:      Re: Sandisk 64Mb CF not recognized
MIME-Version: 1.0
Content-Type: text/plain; charset="US-ASCII"
Content-Transfer-Encoding: 7bit

Thanks to all who have responded!

Vic - thanks for reminding me about FDISK100.  I tried to FDISK, but
naturally was advised it was a bad command.  I quickly and successfully
partitioned the disk using FDISK100, but I now get a different error message
("insufficient memory") when I attempt to format the card.  I performed a MEM
and my little LX indicated that 651 Kb were available for use.

Lilebjorn - I might have also suspected the CF adaptor, but fortunately I was
able to test it in my Dell laptop.  I successfully transferred a spreadsheet
to the CF card (within the adaptor) and subsequently read the file.  Seemed
to work just fine in the laptop.  Still using the laptop, I then copied a
text file to the card and then tried the card in the LX, but I got an I/O
device error in Filer.  When I tried to DIR the A: drive I got the following
message "Invalid media type reading drive A:"   For a moment I thought that
perhaps I put the CF card into the adaptor upside down (I can be a klutz at
times), but the grooves along the side prevent it from being inserted
incorrectly.

John - The CF is indeed a Sandisk, but thank you the offer to experiment with
an ACE driver.  I'd like to try it.

For all - thanks again for the responses.

Best, Harb

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 08:37:10 EST
Reply-To:     HiLill@AOL.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Harb Lill <HiLill@AOL.COM>
Subject:      Re: Sandisk 64Mb CF not recognized
MIME-Version: 1.0
Content-Type: text/plain; charset="US-ASCII"
Content-Transfer-Encoding: 7bit

Hello Zoran,

I just tried the CTL-ALT-DEL reboot, but alas, it had no affect.  I'm still
unable to format or read the card.  Is there a "better" way to reset the LX?

Thanks, Harb

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 14:44:11 +0100
Reply-To:     Michel Bel <michel.bel@ZONNET.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michel Bel <michel.bel@ZONNET.NL>
Subject:      Re: CF catd inside 200lx - RESULTS:-(
Comments: To: radek.svagr@LGPHILIPS-DISPLAYS.COM
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

> So here are the results of my experiments: for these who don't like long
explanations - didn't  work.
>

Well, so I assumed, you assert the Card Enable (CE1 and CE2) of both cards
simultaneously, so this ought not to work. Essentially, this is the only
place where the access to PCMCIA slots differs. All else is parallell.

I am getting a 700LX soon (tomorrow) , and will try to find out what the CE1
and CE2 of the second (Nokia Card) slot are connected to on the Hornet chip.

It may be that there are CE for the second slot somewhere connected to
official PCMCIA NC (not connected) pins on the first slot of a 200LX, and
that these are rewired in the Accurite, but I guess that the Accurite uses
address lines, as these use identical timing as CE lines.

Michel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 14:55:41 +0100
Reply-To:     Zoran Vignjevic <zoranv@GOV.YU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Zoran Vignjevic <zoranv@GOV.YU>
Subject:      Re: Sandisk 64Mb CF not recognized
Comments: To: HiLill@AOL.COM
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

I make a "HW" reset - pull out all bateries, but I dont have anything in RAM
what already not in ROM (because I was new owner of 200lx,and haven't done
anything inportant before I got PCMCIA adapter for my SM cards what were used
with my digicams...
But there is much smoother HW reset, see it in User Guide...I don't have it here
now.
Regards,
Zoran
P.S. Have you tried to push PCMCIA adapter a litle bit more into 200lx?


Harb Lill wrote:

> Hello Zoran,
>
> I just tried the CTL-ALT-DEL reboot, but alas, it had no affect.  I'm still
> unable to format or read the card.  Is there a "better" way to reset the LX?
>
> Thanks, Harb
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 09:00:39 -0500
Reply-To:     "William T. Hole" <wth@NLM.NIH.GOV>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "William T. Hole" <wth@NLM.NIH.GOV>
Subject:      dictionary pcmcia and food analyst card hack?
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii" ; format="flowed"

A long time ago, I copied my Personal Food Analyst to my flash card,
which then still insisted on the original card.  I examined the code with debug
and changed the explicit references to the drive and directory, which then
let me put the files where I want except, as I recall, the path
length in the old
references couldn't be change and that restricted where I could put the files.

Not for the faint of heart!

--Bill
--

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 09:12:18 EST
Reply-To:     HiLill@AOL.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Harb Lill <HiLill@AOL.COM>
Subject:      Re: Sandisk 64Mb CF not recognized
MIME-Version: 1.0
Content-Type: text/plain; charset="US-ASCII"
Content-Transfer-Encoding: 7bit

Zoran,

Yes, the card appears to be fully seated in the LX.  It fits in just as
smoothly as my other 20Mb Type II card and appears to be fully flush with the
exterior of the case.  The CF also appears to fit well within the adaptor.

Unfortunately, I'm on the road and 2,700 miles from my manual, so I'll have
to backup files and remove primary and backup batteries...overnight?...for a
reset.

Perhaps I can find a local friend who would allow me to try their camera's CF
card just for camparison.

Again, thanks for the interest.

Best, Harb

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 15:17:49 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      Re: Sandisk 64Mb CF not recognized
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

You said you have a DS 200lx? I had the same problem when I upgraded my 200lx to DS. Try it on normal 200lx.
 It can be caused by this. In my case it was 128MB card made by Apacer, which was giving the same results in DS 200lx.
I don't believe that Sundisk card has this problem, but if everything else fails...

Radek




                      Harb Lill
                      <HiLill@AOL.COM>             To:  HPLX-L@UConnVM.UConn.Edu
                      Sent by: HPLX                cc:  (bcc: Radek Svagr/HRC/COMP/PHILIPS)
                      Mailing List                 Subject:   Re: Sandisk 64Mb CF not recognized
                      <HPLX-L@UConnVM.
                      UConn.Edu>                   Classification:


                      2002-03-25 02:28
                      PM
                      Please respond
                      to HiLill






Thanks to all who have responded!

Vic - thanks for reminding me about FDISK100.  I tried to FDISK, but
naturally was advised it was a bad command.  I quickly and successfully
partitioned the disk using FDISK100, but I now get a different error message
("insufficient memory") when I attempt to format the card.  I performed a MEM
and my little LX indicated that 651 Kb were available for use.

Lilebjorn - I might have also suspected the CF adaptor, but fortunately I was
able to test it in my Dell laptop.  I successfully transferred a spreadsheet
to the CF card (within the adaptor) and subsequently read the file.  Seemed
to work just fine in the laptop.  Still using the laptop, I then copied a
text file to the card and then tried the card in the LX, but I got an I/O
device error in Filer.  When I tried to DIR the A: drive I got the following
message "Invalid media type reading drive A:"   For a moment I thought that
perhaps I put the CF card into the adaptor upside down (I can be a klutz at
times), but the grooves along the side prevent it from being inserted
incorrectly.

John - The CF is indeed a Sandisk, but thank you the offer to experiment with
an ACE driver.  I'd like to try it.

For all - thanks again for the responses.

Best, Harb

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 06:27:59 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: A question on compact flash cards......
Comments: To: John Alley <chia@ICX.NET>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Mon, 25 Mar 2002 00:21:07 -0500, John Alley <chia@ICX.NET> wrote:

>         Ok, I have a HP100LX that I use daily... and I finally got a PCMIA-->CF
> adaptor card (SanDisk) that works great with the 16Meg CF card I have. Now
> I got a 32Meg Lexar card from a friend. It will not work... I know it was
> used in a digital camera and was wondering if there is something that I can
> do to get it to work.. or is the limit about 16Megs on the CF usage in the
> HPLX pamltops....? Any info is greatly apprecaited. Thanks...

I use a 48MB Sandisk CF card in my 100LX, so 32MB is not too
large. However, there are some brands of CF cards that do not
work as well as others with the 100LX. I don't know if that is
the problem. Or, perhaps the CF card has to be set up with
D:\BIN\FDISK100 and then formatted in the 100LX to work in the
100LX.

Vic Roberts

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 06:43:30 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: Sandisk 64Mb CF not recognized
Comments: To: HiLill@AOL.COM
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Harb,

How are you going to DOS? If you press CRTL-123 you get only
the amount allocated in Setup to the DOS Box. For maximum DOS
memory you should terminate System Manager.

Vic Roberts

On Mon, 25 Mar 2002 08:28:39 EST, Harb Lill <HiLill@AOL.COM> wrote:

> Thanks to all who have responded!
>
> Vic - thanks for reminding me about FDISK100.  I tried to FDISK, but
> naturally was advised it was a bad command.  I quickly and successfully
> partitioned the disk using FDISK100, but I now get a different error message
> ("insufficient memory") when I attempt to format the card.  I performed a MEM
> and my little LX indicated that 651 Kb were available for use.

[snip]

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 09:51:49 -0500
Reply-To:     Dario Draiman <dario200@MAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dario Draiman <dario200@MAIL.COM>
Subject:      Re: A question on compact flash cards......
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: 7bit
MIME-Version: 1.0

I use a Lexar 48MB without problems. Try reformating the CF inside the LX.

----- Original Message -----
From: John Alley <chia@ICX.NET>
Date:         Mon, 25 Mar 2002 00:21:07 -0500
To: HPLX-L@UConnVM.UConn.Edu
Subject:      A question on compact flash cards......


>         Ok, I have a HP100LX that I use daily... and I finally got a PCMIA-->CF
> adaptor card (SanDisk) that works great with the 16Meg CF card I have. Now
> I got a 32Meg Lexar card from a friend. It will not work... I know it was
> used in a digital camera and was wondering if there is something that I can
> do to get it to work.. or is the limit about 16Megs on the CF usage in the
> HPLX pamltops....? Any info is greatly apprecaited. Thanks...
>
> 73 de KF4UAE
> www.qsl.net/kf4uae
> John R. Alley
> kf4uae@arrl.net
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

--

_______________________________________________
Sign-up for your own FREE Personalized E-mail at Mail.com
http://www.mail.com/?sr=signup

Win the Ultimate Hawaiian Experience from Travelocity.
http://ad.doubleclick.net/clk;4018363;6991039;n?http://svc.travelocity.com/promos/winhawaii/

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 10:07:36 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: Fluff: WWW vs. Usenet)
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Axel Berger wrote:
> I'd love to agree with you, unfortunately I can't and may,
> after years of use decide to quit usenet completely some
> time soon. With all those illiterate yobs crowding in and
> writing two lines of irrelevant comment completely hidden
> in several pages of quotes, mostly many stages deep, it
> is no more worth reading but fill the address I use there
> with spam to the brim. (All other addresses are completely
> clean, at least when not counting unsolicited commercials
> from the mailbox providers.) I will not and never stoop so
> low as post using a munged reply address and so will have
> to leave. All this elctronic data exchange used to be so
> nice and useful once

I have to agree about the spam.  I have an email address that I
use just for usenet so that minimizes the problem for me.  I
still get plenty of spam in my regular email but that's from
other sources.

I'm more bothered by the spam in the newsgroups themselves.

As for the long belabored messages, that's always been there.
It's nothing new.  Maybe you're in groups where that's become
more common.  The groups I frequent are mostly about programming
and old computers and a couple concerned with using graphics
programs.  I also sometimes read some literary newgroups.  These
are as good as ever.  Better in some ways.  A lot of the people
on them have been on them for years and have more to contribute.

Alt.lang.asm is one of my favorites.  There is a continual
discussion of "proper" programming methods and how they're
affected by the various tools.  And sometimes it bogs down with
everyone repeating the same things in different ways.   But then
it gets fresh again.  There is also a LOT of help given to young
programmers learning asm and I find that fun.

Comp.lang.forth covers the same ground over and over a lot but
with new approaches and there are always new topics and ideas.
All in all I think this might be the most intelligent group of
people I've ever encountered.  (other than thos one, of course).
My interest in forth is marginal but I've been reading and
enjoying this group for years because of the quality and depth
of a lot of the discussion.

The sloppiest newsgroup on usenet is probably
alt.folklore.computers.  The discussions get silly.  They drift
off topic.  Some get very lengthy.  But I was a  programmer for
over 30 years and a lot of people on that group were programming
years and even decades before I started and there are
discussions of computer history that are just beautiful, very
often by people who were there.

I'd say that 60% or 70% of my time spent on the internet is in
usenet.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 11:17:38 EST
Reply-To:     HiLill@AOL.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Harb Lill <HiLill@AOL.COM>
Subject:      Success! -- was Re: Sandisk 64Mb CF not recognized
MIME-Version: 1.0
Content-Type: text/plain; charset="US-ASCII"
Content-Transfer-Encoding: 7bit

Vic,

I believe you put me right on target, though I did stumble a bit.  I
terminated the System Manager, but didn't know how to get from the start-up
screen to Dos.  I ended up activating Filer, then looked through each menu to
see if I had inadvertantly toggled some setting which would prevent me from
formatting the card.  I noticed that one of the Filer options was to format a
card...so I tried it...and to my happy surprise the LX started the slow
formatting process.  I've now test the CF card on both the LX and laptop and
it works exceptionally well in both!!!

My humble thanks to Vic, Zoran, Radek, Lillebjorn, John and Bill for your
patience, knowledge and friendly helpfulness.

Warm regards, Harb

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 10:28:09 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: Fluff: WWW vs. Usenet
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Bill Sprague wrote:
> The usenet news groups seem to be populated
> by a bunch of people who now know each other
> and really don't want anyone else to crash their
> party.

A few years ago I bought a very old Mac at a garage sale.  I
know nothing about Macs.  I went to a Mac newsgroup and asked if
anyone knew how I could upgrade the OS since I couldn't find
software that worked on the old OS I had.  The computer had no
terminal program so downloading a new OS wasn't one of the
options.

I got pretty much the same reaction you did.  I don't care if a
few jerks want to laugh at me but they wouldn't even talk about
my question.  So I went to a Mac IRC channel and again I got the
same reaction.  Even though I stayed polite they kicked me out
and banned me from the channel.

That exists.  No question about it.  But there are good
newsgroups, too.  Lots and lots of them.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 19:03:16 +0100
Reply-To:     Axel.Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: AW: charging system
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> Are you really using a _rare_ LX that uses 10,5V ???

Well no, not really. The adapter that was with it when I bought it has a
nominal 9 V 400 mA, but is admittedly not genuine HP - I never saw one of
those.

The
       http://www.hplx.net/faq.power.html
says:

> I have an adapter that is 9V, 300mA, and another that is 12V,
> 500mA, and both work fine.

So I had a range of 9-12 to start with and as my 700 LXs use the Nokia
charger which at a nominal 12 V is regulated to a constant 10.8 V I chose
something near that on the lab supply.

But you are probably right - I'll keep the lead and plug from the 9V supply
and look round the spares box for one with better suited values.

Danke
        Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 20:03:50 +0100
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: AW: charging system
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

I have now tried my second 200 LX (bought as defective with screen
problems, but it seems to be nothing but dodgy contacts - we'll see how
much cleaning has helped) but otherwise (well there is a bad hinge crack)
flawless.
For the time being both show the same behaviour which is consistent with
what the faq led me to expect:
Turning the supply down whnen charging will make them toggle charge on and
off continuously at around 9.3 V. But neither is the screen affected nor
the voltage reading in the bottom left corner. With charging off and in the
config screen I can make them switch from adaptor to battery power and back
by lowering votage slightly below and above 9.0 V.

So the blackening of the screen and knocking voltage metering out of kilter
(I presume the latter is the reason and the first the result of some
automatic contrast adjustment) may be triggered by an adaptor with rather
low voltage but it does seem to be a fault rather than a normal reaction.
As long as I can avoid it I won't mind too much but it is a bit of a worry.

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 20:24:30 +0100
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Datacomm
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Using modems I usually have little setup scripts for each, something of the
kind:

send AT&F
send some configs
send AT&W1
send some other configs
send AT&W0

When I tried it in datacomm I found something curious:
Although other scripts like CIS loging work perfectly (not that having
logged in I can do anything there anymore) with this one

{OK}  (wait for OK)

does nothing. A workaround are pauses, though with the long time some take
especially after ATZ it may need four ~~~~ in a row for reliability. Has
anyone got an idea, and if not, take this as a tip. An example for my dayna
14400 is this:

ATZ|
~~~AT&F|
~~ATTM2|
~~AT&W0|
~~AT&C1&D3&G2Y1|
~~ATS6=1S7=85S11=120|
~~AT&Y1|
~~AT&W1|
~~~ATZ1|
~~~~AT&V|

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 11:27:52 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: Success! -- was Re: Sandisk 64Mb CF not recognized
Comments: To: HiLill@AOL.COM
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Harp,

Congratulations on your success. You found a way to format the
card that I had forgotten about.

To get the maximum amount of DOS memory on the 200LX, you can
turn it into a pure DOS machine by stopping System Manager.
This is more than just closing it and going to the Top Card
screen.

To terminate System Manager, close all your applications. Then
press the "&... MORE" key to open Application Manager. Then
press Menu and then the A key and then the T key. Read the
warning screen and then press ENTER. This will make your 200LX
a "pure" DOS machine. To restart System Manager, type 200
<ENTER> at the DOS prompt.

Vic Roberts


On Mon, 25 Mar 2002 11:17:38 EST, Harb Lill <HiLill@AOL.COM> wrote:

> Vic,
>
> I believe you put me right on target, though I did stumble a bit.  I
> terminated the System Manager, but didn't know how to get from the start-up
> screen to Dos.  I ended up activating Filer, then looked through each menu to
> see if I had inadvertantly toggled some setting which would prevent me from
> formatting the card.  I noticed that one of the Filer options was to format a
> card...so I tried it...and to my happy surprise the LX started the slow
> formatting process.  I've now test the CF card on both the LX and laptop and
> it works exceptionally well in both!!!

[snip]

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 15:46:30 -0500
Reply-To:     eugarps@mindspring.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bill Sprague <eugarps@MINDSPRING.COM>
Subject:      Re: Success! -- was Re: Sandisk 64Mb CF not recognized
Comments: To: HiLill@AOL.COM

Harb,

Glad you got it sorted out.

Bill

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 20:55:44 -0000
Reply-To:     "Richard E. McEvoy" <remce@GOFREE.INDIGO.IE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Richard E. McEvoy" <remce@GOFREE.INDIGO.IE>
Subject:      OT, WindozeXP
MIME-Version: 1.0
Content-Type: multipart/alternative;
              boundary="----=_NextPart_000_0015_01C1D43F.6EAFAEC0"

This is a multi-part message in MIME format.

------=_NextPart_000_0015_01C1D43F.6EAFAEC0
Content-Type: text/plain;
        charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

This is a follow-up to my post of Feb. 25 about a disastrous system =
crash, after which I settled initially for a parallel installation. =
Eventually I backed up everything, reformatted the drive and reinstalled =
everything plus some which would not install on the original Dell =
factory setup. The new USB  ATA card reader I had just bought from PSISM =
(psism.com) resisted all attempts at installation, giving a variety of =
error messages depending on which route I took -wizard or manual. It =
kept telling me that I should only use "signed software", warning me of =
dangers to come if I persisted. I persisted, and it worked after a =
fashion, but gave trouble. Then I looked in Device manager and found the =
problem. To enable use of "Unsigned software" in XP just proceed as =
follows:-

In My Computer, rt.click Properties, then click Device  Manager, Driver =
Signing, and you find three options. The ticked one that is the default =
selection is "Never install unsigned driver software". Untick that and =
tick "Ignore - install the software anyway and don't ask for my =
approval".

The card reader works perfectly now. So does my Collins French =
dictionary and  other applications which would not install before.

Richard


------=_NextPart_000_0015_01C1D43F.6EAFAEC0
Content-Type: text/html;
        charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0 Transitional//EN">
<HTML><HEAD>
<META http-equiv=3DContent-Type content=3D"text/html; =
charset=3Diso-8859-1">
<META content=3D"MSHTML 6.00.2600.0" name=3DGENERATOR>
<STYLE></STYLE>
</HEAD>
<BODY bgColor=3D#ffffff>
<DIV><FONT face=3DArial size=3D2>This is a follow-up to my post of Feb. =
25 about a=20
disastrous system crash, after which I settled initially for a parallel=20
installation. Eventually I backed up everything, reformatted the drive =
and=20
reinstalled everything plus some which would not install on the original =

Dell&nbsp;factory setup. The new USB&nbsp; ATA card reader I had just =
bought=20
from PSISM (psism.com) resisted all attempts at installation, giving a =
variety=20
of error messages depending on which route I took -wizard or manual. It =
kept=20
telling me that I should only use "signed software", warning me of =
dangers to=20
come if I persisted. I persisted, and it worked after a fashion, but =
gave=20
trouble. Then I looked in Device manager and found the problem. To =
enable use of=20
"Unsigned software" in XP just proceed as follows:-</FONT></DIV><FONT =
face=3DArial=20
size=3D2></FONT><FONT face=3DArial size=3D2>
<DIV><BR>In My Computer, rt.click Properties, then click Device&nbsp; =
Manager,=20
Driver Signing, and you find three options. The ticked one that is the =
default=20
selection is "Never install unsigned driver software". Untick that and =
tick=20
"Ignore - install the software anyway and don't ask for my=20
approval".<BR><BR>The&nbsp;card reader works perfectly now. So does my =
Collins=20
French dictionary and&nbsp;&nbsp;other applications which would not =
install=20
before.</DIV>
<DIV>&nbsp;</DIV>
<DIV>Richard<BR></DIV></FONT></BODY></HTML>

------=_NextPart_000_0015_01C1D43F.6EAFAEC0--

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 15:15:54 -0600
Reply-To:     Curtis Cameron <curtc@AIRMAIL.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Curtis Cameron <curtc@AIRMAIL.NET>
Organization: None
Subject:      Please don't use "reply" for new subject
Comments: cc: Axel-Berger@NEXGO.DE
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

If you're starting a new subject for the group, I (and others) would
appreciate it if you would start with a blank message, and not just
hit "reply" to an existing message.

For those of us using threading mail readers, your message shows up
under the thread that you reply to, and in my case, I can't see the
subject of your message unless I actually click on it to read it (and
if it's in a thread I don't care about, that won't happen).

thanks,

Curtis Cameron

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 22:17:24 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      MindMap/LX
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

there is no undo feature in MM/LX, right? Or have I just overlooked it?

Attention: If you accidentally delete an item or even a whole branch of
a map, DON't HIT ESC (as it would be the intuitive reaction)! This
could cause MM/LX to save the map and your item or branch is lost if
you haven't a backup file!

Use Ctrl-A to Abort MM without saving!
Even if you "save as" your map after the error, it will ALSO save the
map with its original file name! I just ran into this problem with a
fairly huge MindMap I'm currently creating about telecommunicaiton
networks.

BTW: Anyone interested in that map (about almost all aspects of
telecommunication networks, from POTS and ISDN over Ethernet, xDSL, all
the used protocols, ISO-OSI reference model, Routing, Bridging......)
let me know - I'll gladly share it with you. It's in German, and the
final size will probably be around 45-50 kB.

GTX
daniel



--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 16:46:46 -0500
Reply-To:     Bruce_Martin@MANULIFE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bruce Martin <Bruce_Martin@MANULIFE.COM>
Subject:      Re: CEBIT2002 still nothing compares to our HPLX
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

>> recently I visited the CeBIT in Hannover.
>> There are some new PDA. But i found nothing what can be called
>> a real successor for our LX.
>>
> The most promising machine is IMO the Sharp Zaurus thing (palm sized,
> but with keyboard, Linux OS). Did you see that one on Cebit? I would be
> very interested in having a look at this machine.
>
I agree about the Zaurus. But what I *really* want, to replace my 200LX, is
a pocket wireless terminal.

Being a terminal, it would have no real OS. Instead, it would work with any
platform for which the open-source host software has been compiled
(Windows, DOS, Mac, OS X, Linux etc. etc.) and to which a base station
tranceiver has been attached. So, for example, you could dial in to your
Mac at home and run the applications that are on that machine, then later
dial into your office PC running Windows. Also, it would have no local file
storage, because any changes would be made directly to files on the host
machine. So, no need to synchronize your pocket machine with your desktop
machine!

It would have a greyscale screen that echoes what is displayed on the host
machine's monitor. It would have a thumb-operable keyboard and some kind of
pointing mechanism, any manipulation of which would be echoed to the host
machine.

Specifically, this device would be have a size and weight somewhere between
a Palm and a 200LX. It would get at least 10 days of heavy use from
commonly-available batteries, which could be recharged inside the unit
overnight.

And, of course, I want it *now*!  ;-)

Bruce in Toronto

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 22:48:06 +0100
Reply-To:     "Helmuth E. Guenther" <h_e_guenther@ATTGLOBAL.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Helmuth E. Guenther" <h_e_guenther@ATTGLOBAL.NET>
Subject:      Re: MindMap/LX
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Daniel,

> there is no undo feature in MM/LX, right? Or have I just overlooked it?
>
> Attention: If you accidentally delete an item or even a whole branch of
> a map, DON't HIT ESC (as it would be the intuitive reaction)! This
> could cause MM/LX to save the map and your item or branch is lost if
> you haven't a backup file!

And what happens if you press <Paste>?

Here it puts back the deleted part.

> Use Ctrl-A to Abort MM without saving!
> Even if you "save as" your map after the error, it will ALSO save the
> map with its original file name! I just ran into this problem with a
> fairly huge MindMap I'm currently creating about telecommunicaiton
> networks.

I am glad you proceed with your work <g>.

> BTW: Anyone interested in that map (about almost all aspects of
> telecommunication networks, from POTS and ISDN over Ethernet, xDSL, all
> the used protocols, ISO-OSI reference model, Routing, Bridging......)
> let me know - I'll gladly share it with you. It's in German, and the
> final size will probably be around 45-50 kB.

Yes I am looking forward to receiving your map. Did you already send
it? It didn't arrive here. I am not in a hurry ;-)))

Kind regards

Helmuth

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 23:17:43 +0100
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: CEBIT2002 still nothing compares to our HPLX
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> Being a terminal, it would have no real OS.

Don't know if you are old enaugh to remember, but that was the way we did
it in the goodold days when you still got real work done on computers at a
minimum of effort. The problem with that: 1200 baud is enaugh to transfer
text faster than I can read but graphics is tediously slow even at my ISDNs
64 kbps.

> It would get at least 10 days of heavy use from
> commonly-available batteries

While continuously sending and receiving at high speed over a wireless
connection?
It would be nice, that much I'll grant you - then OTOH lorry starter
batteries are commonly available, aren't they?

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 06:51:56 +0800
Reply-To:     Oliver Chua <bud@MINDGATE.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Oliver Chua <bud@MINDGATE.NET>
Subject:      dictionary pcmcia
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Longden,

Thank you for the info.  I guess I might just have to do that if I want the
dictionary that bad.

Oliver

>I've never heard of a hack to get the HP dictionary card software working
>off another flash card (or in RAM), tho that doesn't mean there isn't one.
>
>It may be better to just put the card on your "collectibles" shelf, and
>spend the $36 for the Collins software from Thaddeus if you really need a
>dictionary on your main flash card.
>
>My $.36
>
>- Longden

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 17:39:03 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
In-Reply-To:  <3C9C6E1E.BB37226E@NexGo.De>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

Now, you will pay for the privledge of having ads and personal =
information sold. It sounds like the same service but now they charge =
for it. They will still sell your info. Nowadys the best bet is to get =
broadband, a registered domain and a linux server to do DNS,mail,WWW, =
etc. for you. I got a linux server running that is even running as a =
gnutella server.


BTW:
Here's another great option for the money: www.freeshell.org. They have =
cheap lifetime memberships and the moderator will occasionally bug you =
for donations to enhance the service. He's just one guy with a few Linux =
boxes and most of the cost of the service comes out of his pocket. I =
usually send in a few extra bucks 'cause it's worth it. This is great if =
you're a unix geek as Freeshell let's you have up to 300MB storage, =
telnet and ssh shell access, ftp, www, mail and a bunch of other stuff =
for a basic membership (I think it's $35 for lifetime). It's a great =
option for 200LX users as all you really need is telnet access to the =
server.




> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@uconnvm.uconn.edu]On Behalf Of
> Axel Berger
> Sent: Saturday, March 23, 2002 6:59 AM
> To: HPLX-L@uconnvm.uconn.edu
> Subject: Re: FW: Important Yahoo! Mail Service Announcement
>=20
>=20
> > It is the way of many free things on the internet.
>=20
> Well, let`s be honest about one thing: None of those people was ever
> planning to run a public service, they were out to make money - yours =
and
> mine. Anf if they did not try to take it directly it was by far more
> pernicious ways, selling addresses and details or some such. I never =
liked
> that "free" attitude. Years ago, when you could access Compuserve via =
an
> ASCII terminal, nothing was free but most of it was well worth the =
money.

snipt

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 17:46:06 -0800
Reply-To:     j_vanderstel@JUNO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John J Vander Stel <j_vanderstel@JUNO.COM>
Subject:      Re: Docking cradle for 200LX
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Hi Tom,

>Does any one know where I could obtain 1 or 2 of the old Sparcom(?)
>docking cradles for the 100/200?  I want set up a permanent connection
>to my desktop machines at home and at work.  I remember a post about a
>year ago for a source for the cases only.  Anybody happen to have that
>info?

That was me.  I still have one of those shells, but I don't think I could
find my notes about it, anymore.  Those dusty cases were probably thrown
out long ago since I didn't end up taking them off their hands, but you
might be able to find that info by querying the database of historical
HPLX-L posts.

I have only one shell and no other hardware for it.  I was going to use
it, along with some odd hardware laying around, to make a docking
station, but never did follow through with the project since the simple
serial cable worked just as well.

I don't remember what I paid for the shell, but its been gathering dust
for quite a while now.  If you would like it, just send me your snail
mail address in a private email and I'll send you mine in a reply.  How
does a $5 bill + postage sound?  I would really like to see *someone*
make good use of it.

Cheers!

John Vander Stel
Grand Rapids, Michigan

________________________________________________________________
GET INTERNET ACCESS FROM JUNO!
Juno offers FREE or PREMIUM Internet access for less!
Join Juno today!  For your FREE software, visit:
http://dl.www.juno.com/get/web/.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 18:13:40 -0500
Reply-To:     Jack Schudel <schudel@UFL.EDU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jack Schudel <schudel@UFL.EDU>
Subject:      SSH for WWW/LX
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Does anyone know of an SSH client that will work with the WWW/LX TCPIP
stack?

Every once in a while my pop3 connection to the mail host gets "lost,"
and the only way I can get back on is to telnet to the server, and kill
the
pop3 thread.  However, telnet has been disabled in favor of ssh,
so now I am stuck.

Any ideas?

/jack

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 15:22:07 -0800
Reply-To:     Patrick West <francis_patrick_west@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Patrick West <francis_patrick_west@YAHOO.COM>
Subject:      Re: Please don't use "reply" for new subject
Comments: To: Curtis Cameron <curtc@AIRMAIL.NET>
In-Reply-To:  <5l4v9ukdfmhh8dssrsvjgnie50ojin35dh@4ax.com>
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii

I understand but sometimes that is not an option.
For some reason some of my new messages to hplx get
bounced regardless of what email address I use.

When I have time I spend a few minutes looking for the
problem, other times I don't.

--- Curtis Cameron <curtc@AIRMAIL.NET> wrote:
> If you're starting a new subject for the group, I
> (and others) would
> appreciate it if you would start with a blank
> message, and not just
> hit "reply" to an existing message.
>
> For those of us using threading mail readers, your
> message shows up
> under the thread that you reply to, and in my case,
> I can't see the
> subject of your message unless I actually click on
> it to read it (and
> if it's in a thread I don't care about, that won't
> happen).
>
> thanks,
>
> Curtis Cameron
>
> ** HPLX-L LIST Info at
> http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>


__________________________________________________
Do You Yahoo!?
Yahoo! Movies - coverage of the 74th Academy Awards.
http://movies.yahoo.com/

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 00:20:07 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Is 2X worth it?  Maybe, Maybe Not.
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

I've been a vocal odd man out on the list several times in the
past when the question of double speed came up and I would speak
in favor of SINGLE speed.

...and then I didn't take my own adice.  My old single speed is
now my backup and I'm using a double speed as my primary LX.

So, how do I like it?  Was I wrong?  (Were you right?)

..Maybe..

I must say I like the quicker sorts and packing within wwwlx.  I
do several email lists and a couple of newsgroups (1 VERY
active) so sorting and repacking is something I end up doing
often.

However, I can't think of anything else that is REALLY GREAT
about the extra speed.  I can notice a few other things running
faster but either not enough faster to rate as GREAT or they're
tasks like backup that I tend to start and let run while I do
something else.

On the negative side I think I have noticed a bit of reduced
battery life.  (I use throw aways.)  I haven't had it long
enough to have a good feel for battery life yet though so final
evaluations are still on hold.

Another, more important negative, is the display.  With the
double speed it seems I can't make the contrast high enough
without also making the display seem dark.  I'm having to settle
for semi-washed out but not too dark.  It works but is less than
GREAT.

I'll continue using my 2X and refining my reaction to 2X speed.
Maybe after a couple of months I'll try switching back to my 1X
to see how the loss of speed will affect me.  I'll let the list
know if/when I try.  My feeling now is it isn't worth it; I
think I could switch back now without feeling as I lost
something important.

To be continued (in a few months)...

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 16:41:07 -0800
Reply-To:     "Martin G. Ramirez" <mramirez@LMU.EDU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Martin G. Ramirez" <mramirez@LMU.EDU>
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
In-Reply-To:  <HPLX-L%2002032519190409@UCONNVM.UCONN.EDU>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Why does the DISPLAY act differently in a 2X system?  Is this a given?  I'd
like to get my 200LX a 2X upgrade some day, but maybe not if the display
quality is not so great as a result.

Martin G. Ramirez


>Another, more important negative, is the display.  With the
>double speed it seems I can't make the contrast high enough
>without also making the display seem dark.  I'm having to settle
>for semi-washed out but not too dark.  It works but is less than
>GREAT.
>

============================
Dr. Martin G. Ramirez
Department of Biology
Loyola Marymount University
One LMU Drive, MS 8220
Los Angeles, CA  90045-2659, U.S.A.
(310) 338-5120
FAX: (310) 338-4479
e-mail: mramirez@lmu.edu
=============================




NTMail K12 - the Mail Server for Education

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 19:13:29 -0700
Reply-To:     Michael Kopplin <kopplin@TECHNOIR.NU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Kopplin <kopplin@TECHNOIR.NU>
Subject:      Re: SSH for WWW/LX
In-Reply-To:  <008801c1d452$b39c8270$bcd4e380@schudel2.nerdc.ufl.edu>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Mon, 25 Mar 2002, Jack Schudel wrote:

> Does anyone know of an SSH client that will work with the WWW/LX TCPIP
> stack?

Unless Andreas is working on one, the answer is no.

> Any ideas?

There is SSHDOS by Daniel Nagy that works on the WATTCP TCP/IP
stack. Available at http://sshdos.sourceforge.net/ I use it
regularly over ethernet, and my cell phone.

You'll need a ppp packet driver such as DOS_PPP which includes a
dialer. You can get this at lxtcp.hplx.net.

Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 18:21:44 -0800
Reply-To:     Ian Butler <ianb@HPLX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ian Butler <ianb@HPLX.NET>
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
In-Reply-To:  <4.1.20020325163719.00ba2e70@lmumail.lmu.edu>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Mon, 25 Mar 2002, Martin G. Ramirez wrote:

> Why does the DISPLAY act differently in a 2X system?  Is this a given?
> I'd like to get my 200LX a 2X upgrade some day, but maybe not if the
> display quality is not so great as a result.

I've never heard of this problem before, and none of the palmtops I've
ever seen have had any difference in display quality with the 2x upgrade ,
except for the well-known problems that occur without the speed driver
installed, which results in the screen being shifted two columns to the
right and, on some models, becoming completely unreadable.  But those
problems only exist when the driver isn't running.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 02:27:39 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: Sandisk 64Mb CF not recognized
Comments: To: HiLill@AOL.COM
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Harb Lill wrote:
> I just tried the CTL-ALT-DEL reboot, but alas, it had no affect.  I'm still
> unable to format or read the card.  Is there a "better" way to reset the LX?

Left Shift-Ctrl-ON.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 02:27:42 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: Sandisk 64Mb CF not recognized
Comments: To: HiLill@AOL.COM
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Harb Lill wrote:
> For all - thanks again for the responses.

I have 2 64M and 2 128M Sandisk CF cards I use without any
problems or drivers in my 200LX.  I have tested them with 3
different CF adapters.  I have used them with 1X and 2X 200LX.
I didn't have to anything to get them recognized in the LX but I
also haven't used them in any other computer.

Have you tried booting using the ROM Config.sys and Autoexec.bat
to see if the CF is recognized?  If it is then something started
in your r/w versions of those files may be affecting the pcmcia
slot.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 21:44:32 -0800
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: SSH for WWW/LX
Comments: To: Michael Kopplin <kopplin@TECHNOIR.NU>
In-Reply-To:  <Pine.LNX.4.33.0203251902580.20554-100000@hal.technoir.nu>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

At 3/25/02 -0700, you wrote:
>On Mon, 25 Mar 2002, Jack Schudel wrote:
>
> > Does anyone know of an SSH client that will work with the WWW/LX TCPIP
> > stack?
>
>Unless Andreas is working on one, the answer is no.

He is not AFAIK.


> > Any ideas?
>
>There is SSHDOS by Daniel Nagy that works on the WATTCP TCP/IP
>stack. Available at http://sshdos.sourceforge.net/ I use it
>regularly over ethernet, and my cell phone.

Bingo - I recalled something when I read Jack's request, but could not
conjure up the name... Thanks for having a better memory <G>...

Jack was looking for something to work with www/lx API, but unfortunately,
there is not one of those.

Avi


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 25 Mar 2002 22:17:34 -0700
Reply-To:     Ace Frehley <alaskan@V-WAVE.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ace Frehley <alaskan@V-WAVE.COM>
Organization: test
Subject:      Consumer Broadband and Digital Television Promotion Act
MIME-version: 1.0
Content-type: text/plain; charset=us-ascii
Content-transfer-encoding: 7BIT

As we are all aware, this is not a forum to discuss political issues
or laws. However, with the continued government pressure and attempts
to reform and regulate the hardware and software industries, readers
should be informed and aware of these new laws which will no doubt
impact all of us.


Senator Hollings is attempting to regulate hardware and software
development. The bill can be reviewed here:
http://cryptome.org/broadbandits.htm

Concerned software developers can submit comments here:
http://judiciary.senate.gov/special/input_form.cfm?comments=1

You can review other peoples comments here:
http://judiciary.senate.gov/special/input_form.cfm

The following senators also support this Bill:
Ted Stevens (R-Alaska), Daniel Inouye (D-Hawaii),
John Breaux (D-Louisana) and Dianne Feinstein (D-California).

There is a mailing list discussing these issues here:
http://lists.microshaft.org/mailman/listinfo/dmca_discuss


----- Forwarded message from Declan McCullagh <declan@well.com> -----


As a bonus, here's a section-by-section summary of the bill:
http://www.wired.com/news/politics/0,1283,51275,00.html

And a collection of info on the Consumer Broadband and Digital
Television Promotion Act (CBDTPA):
http://www.politechbot.com/docs/cbdtpa/

-Declan

---

http://www.wired.com/news/politics/0,1283,51274,00.html

   Anti-Copy Bill Slams Coders
   By Declan McCullagh (declan@wired.com)

1:25 p.m. March 22, 2002 PST
WASHINGTON -- America's programmers, engineers and sundry bit-heads
have not yet figured out how much a new copyright bill will affect
their livelihood.

When they do, watch for an angry Million Geek March to storm Capitol
Hill.

A bill introduced this week by Sen. Fritz Hollings (D-South Carolina)
would roil the electronics industry by forcibly embedding copy
protection into all digital devices, from MP3 players to cell phones,
fax machines, digital cameras and personal computers.

But the Consumer Broadband and Digital Television Promotion Act
(CBDTPA) would also wreak havoc on programmers and software companies
-- both those distributing code for free and those selling it.

No more than two years and seven months after the bill becomes law,
the only code programmers and software firms will be able to
distribute must have embedded copy-protection schemes approved by the
federal government.

To put this in perspective: The CBDTPA would, if enacted in its
current form, have the electrifying effect on computer professionals
that the Supreme Court's decision in Bush v. Gore did to some
Democratic Party members.

Legal experts said on Friday that the CBDTPA regulates nearly any
program, in source or object code, that runs on a PC or anything else
with a microprocessor.

That's not just Windows media players and their brethren, as you might
expect. The CBDTPA's sweeping definition of "any hardware or software"
includes word processors, spreadsheets, operating systems, compilers,
programming languages -- all the way down to humble Unix utilities
like "cp" and "cat."

"The definition will cover just about anything that runs on your
computer -- except maybe the clock," said Tom Bell, a professor at
Chapman University School of Law who teaches intellectual property
law.

   [...]



-------------------------------------------------------------------------
POLITECH -- Declan McCullagh's politics and technology mailing list
You may redistribute this message freely if you include this notice.
Declan McCullagh's photographs are at http://www.mccullagh.org/
To subscribe to Politech:
http://www.politechbot.com/info/subscribe.html
This message is archived at http://www.politechbot.com/
-------------------------------------------------------------------------


----- End forwarded message -----

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 01:48:06 -0500
Reply-To:     John J Vanderstel <j_vanderstel@JUNO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John J Vanderstel <j_vanderstel@JUNO.COM>
Subject:      Re: CEBIT2002 still nothing compares to our HPLX
MIME-Version: 1.0
Content-Type: text/plain
Content-Transfer-Encoding: 7bit

Hi Bruce,

>I agree about the Zaurus. But what I *really* want, to replace my 200LX,
is
>a pocket wireless terminal.
>
>Being a terminal, it would have no real OS. Instead, it would work with
any
>platform for which the open-source host software has been compiled
>(Windows, DOS, Mac, OS X, Linux etc. etc.) and to which a base station
>tranceiver has been attached. So, for example, you could dial in to your
>Mac at home and run the applications that are on that machine, then
later
>dial into your office PC running Windows. Also, it would have no local
file
>storage, because any changes would be made directly to files on the host
>machine. So, no need to synchronize your pocket machine with your
desktop
>machine!

That would be cool, indeed.  I know where you are coming from, Bruce. :-)

I used to run a one line BBS long ago and I used to be able to do that
from any computer with a modem and terminal program with doorway mode.
It worked great when I had a DOS program running in a full screen on my
home computer.  I requires a dedicated phone line only for that computer.

It did not work when my computer was running something in a normal
Window, though.

I did figure out a way to reboot my computer at home from a remote
terminal if it was not running DOS or a DOS program in a full screen
window at the time.  (My home computer was setup to reboot to a full
screen DOS window, where I could launch any DOS program I wanted to run
on my home computer.)

Unfortunately, to access and use a Windows program in a window remotely
on a home computer requires much more than just a simple terminal
program.

Also, I'm afraid that a wireless unit would require far too much energy
to run for 10 days like that on a single charge.  Even for one using a
modem and phone line, that would be a rather tall order to fill.

I would have a great time with a wireless hand held plain terminal that
could be operated for 10 days on a single charge.  For that kind of
access, I would gladly find, install and use only DOS programs on an old
home PC dedicated as a host for that very purpose.  I already have a DOS
program that competes pretty well with almost all of the Windows programs
I use.

Cheers!

John Vander Stel
Grand Rapids, Michigan


________________________________________________________________
GET INTERNET ACCESS FROM JUNO!
Juno offers FREE or PREMIUM Internet access for less!
Join Juno today!  For your FREE software, visit:
http://dl.www.juno.com/get/web/.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 15:53:22 +0800
Reply-To:     Adrian Ho <aho-hplx@03S.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Adrian Ho <aho-hplx@03S.NET>
Subject:      Re: CEBIT2002 still nothing compares to our HPLX
In-Reply-To:  <OF1BEC5C0D.9311C712-ON85256B87.006E0FF3@manulife.com>; from
              Bruce_Martin@MANULIFE.COM on Mon, Mar 25, 2002 at 04:46:46PM -0500
Mime-Version: 1.0
Content-Type: text/plain; charset=us-ascii

On Mon, Mar 25, 2002 at 04:46:46PM -0500, Bruce Martin wrote:
> I agree about the Zaurus. But what I *really* want, to
> replace my 200LX, is a pocket wireless terminal.
> [description deleted]

Sounds like a wireless VNC terminal (for those who have no idea
what I'm talking about, <http://www.uk.research.att.com/vnc/>'s
the place to look).

> And, of course, I want it *now*!  ;-)

You can already put it together, for the most part -- the VNC
client has been ported to almost every PDA platform out there
(excluding, alas, the LX).  The tricky part is selecting
a suitable power-miser wireless technology for your chosen
platform that meets your connectivity needs, yet still gives
you your 10 days of operation.

- Adrian

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 09:00:29 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Russ

On Tue, 26 Mar 2002 00:20:07 +0000, Russel Brooks <rlbrooks@POBOX.COM> wrote:

> However, I can't think of anything else that is REALLY GREAT
> about the extra speed.  I can notice a few other things running
> faster but either not enough faster to rate as GREAT or they're
> tasks like backup that I tend to start and let run while I do
> something else.

But isn't it nice that the palmtop is ready for something else much
quicker than before? I really don't like it when the palmtop does its
backup and I am not able to look up something in PIM/PE or the
dictionary...

> On the negative side I think I have noticed a bit of reduced
> battery life.  (I use throw aways.)  I haven't had it long
> enough to have a good feel for battery life yet though so final
> evaluations are still on hold.

That's true. Battery life decreases. But if you do a lot of
CPU-intensive tasks, the gain in performance is higher than the loss in
battery life, so you end up in the same or even less dollars for
batteries per task.

> Another, more important negative, is the display.  With the
> double speed it seems I can't make the contrast high enough
> without also making the display seem dark.  I'm having to settle
> for semi-washed out but not too dark.  It works but is less than
> GREAT.

Are you sure the double speed upgrade made the difference? Have you
seen this upgraded palmtop before the upgrade? Some screens are simply
worse than others, mainly in contrast. Maybe swapping the screens (ir
the motherboards, that's easier) is the thing you need in order to
combine the good screen with the fast motherboard.
Another thing you could try: Mack's double speed driver allows
adjusting the refresh rate with a hotkey. Try to switch throught the
rates, maybe you find one which lets you adjust the contrast better.

> To be continued (in a few months)...

I'm curious!

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 09:15:47 +0100
Reply-To:     Juergen Korthof <hplx@0800CALLING.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Juergen Korthof <hplx@0800CALLING.DE>
Subject:      Re: CEBIT2002 still nothing compares to our HPLX
Comments: To: Daniel Hertrich <daniel.hertrich@gmx.de>
In-Reply-To:  <HPLX-L%2002032213401079@UCONNVM.UCONN.EDU>
Mime-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Hi Daniel,

you had a fine Idea with downgrading newer machines! :-)

> -----Original Message-----
> Daniel Hertrich
> So it seems to be time to collect all our hardware
> skills and use it > not longer for upgrading the HPLX, but
for
> downgrading newer machines.
> ;-)

I just bought a HP360LX on ebay to see what could be done with
downgrading.

For the one who not knows the 360LX: It has 8MB RAM, 1
CF-Slot, 1 PCMCIA, IRDA, Touchscreen 640x240, VGA-Greyscale,
switchable Backlight.
Good-sized Keyboard ...No NumKey-Block:-(
It has marginable acceptable size, wheight and
batteryconsumption.

>
> For example dimming the backlight, making
> processors slower, replacing
> color with b/w screens, replacing WinCE ROMs with
> DOS ROMs....

The first exploration will be to make it boot to pure DOS,
...perhaps to Linux.
Then connectivity pack, PAL...


Happy LXing
Juergen

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 10:46:36 +0100
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
MIME-Version: 1.0
Content-Type: text/plain; charset=iso-8859-1
Content-Transfer-Encoding: quoted-printable

> Another, more important negative, is the display.

Can others confirm this? While undoubtedly good, with its size the displa=
y
is marginal for my eyes, I'd not wnat it made worse ever so slightly.
OTOH there is so far only one thing where I have found my LX to be slow:
After changing up from the Portfolio I found I could now keep my whole 70=
0
entry address list with acceptable load times instead of just a selection
of about 100. But searching in that list (F4) now really takes patience.
Everything else is just fine, 123 tables have to be kept smallish for oth=
er
reasons, so they are fast enaugh.

Tsch=F6 wa
                Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 12:58:07 +0000
Reply-To:     Stefan.Peichl@T-ONLINE.DE
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Stefan Peichl <Stefan.Peichl@T-ONLINE.DE>
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Russel Brooks wrote:

> Another, more important negative, is the display.  With the
> double speed it seems I can't make the contrast high enough

if you have time, just try the DSPEED.COM doublespeed driver and
see if it makes any difference. IMHO the screen looks "crisper"
with DSPEED.

http://peichl.hplx.net/dspeed.zip

or download from S.U.P.E.R.

Stefan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 10:23:11 -0500
Reply-To:     Bruce_Martin@MANULIFE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bruce Martin <Bruce_Martin@MANULIFE.COM>
Subject:      Pocket wireless terminal? (Was: Re: CEBIT2002 still nothing
              compares to our HPLX)
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

>> Being a terminal, it would have no real OS.
>>
> Don't know if you are old enaugh to remember, but that was the way we did
> it in the goodold days when you still got real work done on computers at
a
> minimum of effort. The problem with that: 1200 baud is enaugh to transfer
> text faster than I can read but graphics is tediously slow even at my
ISDNs
> 64 kbps.
>
Absolutely!  I am so old (drum roll) I wrote my first program in COBOL - on
punchcards - for the IBM 370 mainframe at McGill University in Montreal. I
also communicated remotely with the Sir George Williams maniframe (I forget
what kind) via a lineprinter terminal - no monitor, kids!

To better understand what I'd like to see in a pocket wireless terminal,
think of a 200LX with a built-in cellular modem and higher resolution
display, running something like PC Anywhere or Timbuktu to control a
desktop host. What you see on your pocket screen is what's displayed on the
desktop, and what the desktop does is in response to commands you key in on
your pocket machine.

Bruce in Toronto

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 13:16:18 -0500
Reply-To:     Steve <novosad@SERVER030.FWB.SAIC.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Steve <novosad@SERVER030.FWB.SAIC.COM>
Subject:      Re: Fluff: WWW vs. Usenet)
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Barry wrote:

> Alt.lang.asm is one of my favorites.

   Hmm.  How does it compare to comp.lang.asm.x86 (if you
follow both)?


Steve

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 21:09:33 -0000
Reply-To:     Chris Randle <chris@AMLOG.CO.UK>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Chris Randle <chris@AMLOG.CO.UK>
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
In-Reply-To:  <4.1.20020325163719.00ba2e70@lmumail.lmu.edu>
MIME-Version: 1.0
Content-Type: text/plain; charset="us-ascii"
Content-Transfer-Encoding: quoted-printable

> -----Original Message-----
> Behalf Of Martin G. Ramirez
> Sent: 26 March 2002 00:41

> Why does the DISPLAY act differently in a 2X system?  Is this=20
> a given?  I'd
> like to get my 200LX a 2X upgrade some day, but maybe not if=20
> the display
> quality is not so great as a result.

I've had three 200LXs; two SS, one DS. In each case the screen had
noticably different characteristics in terms of colo(u)r and clarity. My
double-speed (the newest machine) had, IMO, the most legible screen, so
it may just be a bit of luck with the donor machine. The best authority
would be someone who has had a known machine upgraded who could comment
on whether or not the contrast was affected.

--=20
Chris Randle

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 15:36:49 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
In-Reply-To:  <000801c1d50a$8eac2480$0100a8c0@dell>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Tue, 26 Mar 2002, Chris Randle wrote:

> > Behalf Of Martin G. Ramirez
> > Sent: 26 March 2002 00:41
>
> > Why does the DISPLAY act differently in a 2X system?  Is this
> > a given?
>
> I've had three 200LXs; two SS, one DS. In each case the screen had
> noticably different characteristics in terms of colo(u)r and clarity. My
> double-speed (the newest machine) had, IMO, the most legible screen, so
> it may just be a bit of luck with the donor machine. The best authority
> would be someone who has had a known machine upgraded who could comment
> on whether or not the contrast was affected.

I've had four 200LXs; two were new SS, one was new DS, and one was a
used DS.  One of the new SS units had a noticeably sharper display
than the other three.  I had it upgraded to 32M and DS by Times2Tech
and did not notice any change in the display.  After upgrade it was
still better looking.  By better, I mean it had higher contrast.
The other three are all pretty comparable.

Unfortunately, the one with the best display is the one I lost in
Boston last year.  :(

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 22:39:41 +0100
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> The best authority would be someone who has had
> a known machine upgraded

Are there comprehensive instructions about on how to do that? I have looked
at the Thaddeus site, and while admittedly I don't think anyone could offer
what they do commercially for less, it is a lot of money for me and I have
soldered the off part or two in the past.

I have just looked at my address database in the address book of the
connectivity software on the games console and searching with F4 the answer
flashed up in an instant - amazing, though admittedly my database on the 16
MHz Atari does the same.

Is there any known reason why HP didn't use the higher speed in the first
place?

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 22:25:51 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: Fluff, Consumer Broadband and Digital Television Promotion Act
Comments: To: Ace Frehley <alaskan@V-WAVE.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Ace Frehley wrote:
> As we are all aware, this is not a forum to discuss political issues
> or laws. However, with the continued government pressure and attempts
> to reform and regulate the hardware and software industries, readers
...

If you want to fight all the stupid laws affecting the net then
go here  -->   http://www.eff.org

The Electronic Frontier Foundation has proven itself willing to
go to court to fight for internet freedoms.

They also have a good news letter you can subscribe to (if you
don't already get too much email).

I support EFF with $$$ (and matching $$$ from my employer).

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 23:50:56 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Daniel Hertrich wrote:
> Are you sure the double speed upgrade made the difference? Have you
> seen this upgraded palmtop before the upgrade? Some screens are simply
> worse than others, mainly in contrast. Maybe swapping the screens (ir
> the motherboards, that's easier) is the thing you need in order to
> combine the good screen with the fast motherboard.
> Another thing you could try: Mack's double speed driver allows
> adjusting the refresh rate with a hotkey. Try to switch throught the
> rates, maybe you find one which lets you adjust the contrast better.

Daniel & others,

My DS LX is a 2M LX I purchased used from a post on this list
from Floyd Smithberg when he decided to give up the LX because
of his eyes.  While I tested it to be sure it was Ok I never
really used it before sending it in (many months later) for the
32M + DS upgrade.

To start with I don't think the display was as good as my other
LXs.  I don't think the DS upgrade helped it any either but
since I have little experience with this unit before the upgrade
I am probably blaming the upgrade far too much; expecially since
so many others have DS units with good displays.

So... ignore my display comments but the rest of what I posted
still stands.  It'll be interesting to see if I become as
fanatical as the rest of you DS owners over time.

I'll try playing with Mack's driver keystroke options and I've
also downloaded Stefan's DSPEED drive to try it too.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 13:09:48 -0500
Reply-To:     theise@netins.net
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: CEBIT2002 still nothing compares to our HPLX

Daniel Hertrich writes:
> > So it seems to be time to collect all our hardware
> > skills and use it not longer for upgrading the HPLX, but
> > for downgrading newer machines.
> > ;-)

Juergen Korthof writes:
>
> you had a fine Idea with downgrading newer machines! :-)

I agree.  It may not be feasible to do, but the idea certainly shows
creative thinking.

--
Ted Heise     <theise@netins.net>     West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 19:01:19 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
Comments: To: Barry <barry@FBTC.NET>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Sun, 24 Mar 2002 09:37:38 -0600, Barry <barry@FBTC.NET> wrote:

[snip]

> I can't actually disagree with you but a lot of us remember
> that, while you were paying the high price for Compuserve (so
> did I) we were also using the not very well known internet.
> There was no WWW then.  There wasn't anything you could pay for.
> But there was a lot of really good content provided by people
> who worked hard on their own time to put it there.

[snip]

I disagree. The Internet was never "free". It just seemed that
way to the small group of us that had access at no cost to us.
The Internet was initially designed to connect government,
university and industrial research labs. Almost every person
associated with one of these organizations had "free" access
but the Internet backbone was paid for by the US Government
and each university and industrial lab had to pay for their
own connection. So, our "free" use was being subsidized by our
government, university or employer.

There are few things of value in this world that are totally
free. I would suggest that instead of looking for "free" ISPs
and "free" e-mail services, we all find competent providers and
pay them a fair fee to insure that they can stay in business.

Victor Roberts

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 21:58:23 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
Comments: To: Victor Roberts <RobertsV@earthlink.net>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

----- Original Message -----
From: "Victor Roberts" <RobertsV@earthlink.net>
To: "Barry" <barry@FBTC.NET>; <HPLX-L@UCONNVM.UCONN.EDU>
Sent: Tuesday, March 26, 2002 9:01 PM
Subject: Re: FW: Important Yahoo! Mail Service Announcement


> I disagree. The Internet was never "free". It just seemed that
> way to the small group of us that had access at no cost to us.
> The Internet was initially designed to connect government,
> university and industrial research labs. Almost every person
> associated with one of these organizations had "free" access
> but the Internet backbone was paid for by the US Government
> and each university and industrial lab had to pay for their
> own connection. So, our "free" use was being subsidized by our
> government, university or employer.
>
> There are few things of value in this world that are totally
> free. I would suggest that instead of looking for "free" ISPs
> and "free" e-mail services, we all find competent providers
and
> pay them a fair fee to insure that they can stay in business.

I realize that.  I did have free access a long time ago before I
even knew there was an internet, thanks to my room-mate's
brother. I didnt know what it was.  It was just a lot of email
and newsgroups on an Amdahl in Canada.  The university always
posted the bill as I signed off but I never had to pay for it.
It was usually in the hundreds of dollars.

Ever since that I've had access that I paid for.

I was referring to things on the internet being free.  I paid to
get on but that was it.  There was no way to spend money on the
internet.  At least I didn't know of any.

It was a big wide open world full of things to do and things to
learn.  There weren't many fences.  I was free to roam.

Maybe you like it better when everybody pays his way.  I like
that too, in principle.  But I remember how nice the internet
used to be.  It's more important now but not nearly as nice.

I kept a shell account for a few years after I got my first SLIP
account.  But the graphics and the color and the mouse lured me
away.  Nobody to blame but me.  It's the way things go and I
went with it.  By the time they shut down the shell server at my
ISP I wasn't using it that much anyway.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 12:02:50 +0800
Reply-To:     Wee-Meng Lee <leewm@ANAKIN.SGP.HP.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Wee-Meng Lee <leewm@ANAKIN.SGP.HP.COM>
Subject:      200LX display
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Hi,

Saw some posts about screen quality of the 200LX, DS and non DS.

I have with me two non-DS 200LX 2MB and am comparing the screen
contrast. One is clearer than the other despite playing with the
contrast (ON -/+) on the dimmer one.  The dimmer one is
slightly more brownish. The clearer one is more light green.

So it could be some screen batch quality thing. But they're
still usable, so no, I'm not selling my spare :)

Rgds,
weemeng

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 20:18:06 -0800
Reply-To:     Gary Spiers <garys@LIDAR.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Gary Spiers <garys@LIDAR.COM>
Subject:      Re: ILGRadio Shortwave Database in GDB Format
Comments: To: Gary Jacek <gary-jacek@SHAW.CA>
In-Reply-To:  <3C9AA113.3D403B18@shaw.ca>
Content-Type: text/plain; charset="iso-8859-1"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit

Gary,

The  Dos version of the ILGRadio program runs on the palmtop. Additionally
the dbase format of the ILG database should be readable by a number of
database programs that will run on the palmtop (haven't tried).

GaryS (Owner of an aging Drake R8)

On Thursday 21 March 2002 07:12 pm, you wrote:
> Hey gang.
>
> One of my other interests is Shortwave Radio.
>
> I recently happened upon the ILGRadio site.
> HTTP://www.ilgradio.com/
>
> ILGRadio has a database of Shortwave broadcasters, worldwide.
>
> ILGSTLAN.ZIP at this site, contains individual databases in
> LINUX text format, for broadcasts
> in English, French / Creole, German, Arabic, Italian, Dutch /
> Afrikaans, Portuguese,                        Russian /
> Ukrainian, Spanish and "Nordic" (Danish Icelandic, Norwegian,
> Swedish, and Finnish).
>
> You guessed it.  I just had to have the English broadcast
> database in my palmtop for on-the-go listening.
>
> I have written a program that converts the ILGRadio LINUX format
> databases into something that
> GDBLOAD can accept.  I used my program and GDBLOAD (available on
> SUPER) to convert the
> ILGSTENG.TXT English broadcast database into ILGSTENG.GDB.
>
> There is a catch here.  In order to get the ILGRadio database,
> you need to register at
> the ILGRadio site.  The bad news is that it takes a few days to
> get a Userid/Password for
> download.  The good news is that it is free for noncommercial
> use.
>
> I can't give away the ILGSTENG.GDB database, but I can give away
> the tools to create it.
>
> If there are any other shortwave listeners on the HPLX list that
> would find this of benefit,
> I can clean it up and make it available.
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 23:13:55 -0600
Reply-To:     Curtis Cameron <curtc@AIRMAIL.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Curtis Cameron <curtc@AIRMAIL.NET>
Organization: None
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
Comments: To: Russel Brooks <rlbrooks@POBOX.COM>
In-Reply-To:  <HPLX-L%2002032519190409@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

On Tue, 26 Mar 2002 00:20:07 +0000 Russel Brooks wrote:
>Another, more important negative, is the display.

Here's another data point. My 200LX, which I got when they were
brand-new, has a sharp, crisp display.

I got my wife a 100LX from a friend who didn't use his anymore, and
that display was very much worse than my 200LX. I posted to this list
once that I thought the 200LXs had better displays than the 100LXs,
and David Sargent replied that the displays didn't seem to be split by
which model you have, it's just that some had the good displays and
some had the bad.

I think I've noticed that the bad ones are a silvery-gray background
color, and the good ones are a greenish-gray color. I have a pair of
greenish-gray slacks, and my 200LX's screen is the exact same color.

--
Curtis Cameron

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 17:54:25 +0800
Reply-To:     Wee-Meng Lee <leewm@ANAKIN.SGP.HP.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Wee-Meng Lee <leewm@ANAKIN.SGP.HP.COM>
Subject:      Can 200LX print to 82240B Infrared Printer?
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Hi,

I'm looking for a battery powered printer that's real small to
work with the 200LX and I came across this HP 82240B Infrared
Printer.

Can anyone tell me if I can use the InfraRed port to print to it?

Thank you,
weemeng

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 12:04:29 +0100
Reply-To:     Jacques Belin <jbelin@ALTERN.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jacques Belin <jbelin@ALTERN.ORG>
Subject:      Re: Can 200LX print to 82240B Infrared Printer?
In-Reply-To:  <200203270954.RAA14416@anakin.sgp.hp.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="ISO-8859-1"
Content-Transfer-Encoding: 8bit

Le Wed, 27 Mar 2002 17:54:25 +0800
Wee-Meng Lee <leewm@ANAKIN.SGP.HP.COM> a icrit:

> Can anyone tell me if I can use the InfraRed port to print to it?

Check for IR-Print, on the Super page :

   http://www.palmtop.net/super3.html


Jacques.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 14:11:19 +0100
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Victor Roberts wrote:
> I would suggest that instead of looking for "free" ISPs
> and "free" e-mail services, we all find competent providers and
> pay them a fair fee to insure that they can stay in business.

Quoting someone at length and adding no maore than "me too" is rightly
considered bad form and I normally don't do it - this is the one exception
though:
"Hear hear" <knocking on table>

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 14:38:58 +0100
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: Datacomm
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

I'm still having problems. Trying to run scripts in datacomm completely
freezes the card. It got so bad that I first thought the card drew too much
current to work and then that I had fried the port so that even the other
wouldn't work anymore. But then both cards worked perfectly with going
postal and after that could be talked to in datacomm as well - until I
tried running a script again, when all was back to un-normal.
Is there any workaround? Scripts do work while being connected.

Or alternatively (and additionally for the desktop) can you suggest a slim
and simple terminal with good and well documented scripting? W98 Hyperterm
is too braindead as is the W31 terminal and big packages like crosspost are
too complicated for me.

Danke
        Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 14:45:37 +0100
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> But I remember how nice the internet used to be.

Me too. It is so no more. One reason seems to be that too many newbies have
been led to think of "the internet" as a huge anonymous machine spewing out
answers insead of a huge bunch of individual people quite willing to help
if you ask nicely.
The second is that with the advent of colour all notions of netiquette have
gone down the drain. In sci.energy, which used to be very worthwhile and
sometimes still can be, two thirds of all posts show me a full screen - or
several down - of all quote with no content. I have mostly given up
scrolling down, although sometimes what follws might be worth reading. It
goes against the grain, but if people insist on full untrimmed quoting
(including the quotes included, which include ...) then (and only then) top
posting is the lesser evil. MausNet, my old-style BBS network and gateway
to usenet (this way I can at least use a decent reader) used to be
different, but by now there is a huge brain drain and dieing of boxes and
the chances of actually finding someone knowing more about the questions I
have than myself are getting lower every day.

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 05:47:44 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
Comments: To: Barry <barry@FBTC.NET>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Tue, 26 Mar 2002 21:58:23 -0600, Barry <barry@FBTC.NET> wrote:

[snip]

> I was referring to things on the internet being free.  I paid to
> get on but that was it.  There was no way to spend money on the
> internet.  At least I didn't know of any.
>
> It was a big wide open world full of things to do and things to
> learn.  There weren't many fences.  I was free to roam.
>
> Maybe you like it better when everybody pays his way.  I like
> that too, in principle.  But I remember how nice the internet
> used to be.  It's more important now but not nearly as nice.

[snip]

I think we both agree that it is reasonable for us to each pay
for basic access to the Internet. As for the types of services
available on the Internet, I would argue that much of the free
and creative stuff we both remember is still there. It may not
be as visible due to all the commercial activity, but creative
people are still writing and posting free or low cost software
and the newsgroups are all still free. The fact that newsgroups
have become populated by too many thoughtless people is, I
believe, due more to the huge increase in the number of people
on the Inet then to commercial activity.

Vic Roberts

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 05:59:38 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: Datacomm
Comments: To: Axel-Berger@NexGo.De
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Wed, 27 Mar 2002 14:38:58 +0100, Axel Berger <Axel-Berger@NEXGO.DE> wrote:

[snip]

> Or alternatively (and additionally for the desktop) can you suggest a slim
> and simple terminal with good and well documented scripting?

I don't know why your Datacomm scripts do not work, but the old
DOS version of Kermit runs well on the 95LX, 100LX and 200LX. I
am referring to the Kermit terminal emulation and file transfer
program, not just to the Kermit file transfer protocol that is
built into many other COMM programs.

Kermit used to be freeware produced by Columbia University. In
the old 95LX days I posted a version of Kermit 2.2 on the
HPHAND forum on Compuserve. It was so small it ran well on my
original 512KB 95LX. It has a great and configurable VT100
terminal emulator and good scripting. I then moved on to Kermit
3.1 for my 100LX because the scripting was a bit easier to use.

If you can't find Kermit 2.2 or Kermit 3.1 on SUPER or
elsewhere, contact me at VicRoberts@earthlink.net and I will
send you copies of each.

Vic Roberts

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 08:52:42 -0600
Reply-To:     Jens Siffring <jsiffrin@SIEMENS-EMIS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jens Siffring <jsiffrin@SIEMENS-EMIS.COM>
Subject:      Re: 200LX display
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Hi,

HP changed the display on the 4MB units. The 4MB ones
had noticable better contrast then the 2MB unit machines.

Thanks,

Jens

--
Jens G. Siffring
Project Lead
Solace  -  The Siemens EMIS service and support department
7225 Northland Drive, Brooklyn Park, MN 55428-1540
phone: 214-743-6746
jsiffrin@siemens-emis.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 08:54:50 -0600
Reply-To:     Jens Siffring <jsiffrin@SIEMENS-EMIS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jens Siffring <jsiffrin@SIEMENS-EMIS.COM>
Subject:      Re: Can 200LX print to 82240B Infrared Printer?
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Hi  Wee-Meng!

if you are looking for a battery powered printer with IR interface
you should also consider the Citizen PN60i. It's a pretty small
printer, can be used with a black and white cartridge and a color
one. Never tried the color one but I had the IR-port working on the
HP200LX. Printing quality was good, they promissed 'laser like'
on the box, but it was just 'good'.
My one is just sitting somewhere, I hardly use it anymore....
if you are interested.

Thanks,

Jens

Wee-Meng Lee <leewm@ANAKIN.SGP.HP.COM>@UCONNVM.UCONN.EDU> on 03/27/2002
03:54:25 AM

Please respond to Wee-Meng Lee <leewm@ANAKIN.SGP.HP.COM>

Sent by:    HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>


To:    HPLX-L@UCONNVM.UCONN.EDU
cc:
Subject:    Can 200LX print to 82240B Infrared Printer?


Hi,

I'm looking for a battery powered printer that's real small to
work with the 200LX and I came across this HP 82240B Infrared
Printer.

Can anyone tell me if I can use the InfraRed port to print to it?

Thank you,
weemeng

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


--
Jens G. Siffring
Project Lead
Solace  -  The Siemens EMIS service and support department
7225 Northland Drive, Brooklyn Park, MN 55428-1540
phone: 214-743-6746
jsiffrin@siemens-emis.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 09:43:51 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: 200LX display
In-Reply-To:  <200203271452.IAA37532@dingo.empros.com>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Wed, 27 Mar 2002, Jens Siffring wrote:

> HP changed the display on the 4MB units. The 4MB ones
> had noticable better contrast then the 2MB unit machines.

The 200LX I had with better display was a 4MB unit.  My current
working 200LX has a poorer display.  It's a 32MB upgrade ftom
Thaddeus with "4MB" printed above the display, but I suppose
it's possible the screen and overlay were not from the same
original source.

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 09:48:08 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: Fluff: WWW vs. Usenet)
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Steve wrote:
> Barry wrote:
>>
>> Alt.lang.asm is one of my favorites.
>
>   Hmm.  How does it compare to comp.lang.asm.x86
> (if you follow both)?

They're similar.  A lot of the same people are on both.  Each
has a few different people.  On alt.lang.asm they sometimes try
to keep it general and not centered around the x86 cpu but for
the most part the people there are x86 programmers and examples
are usually given in x86 code.  The difference is small.

There are some long winded discussions about the "proper" way to
code and the proper way to organize a program.  I usually enjoy
these for a while and then ignore them when they get repetitive.
A lot of the discussion, on both groups, is about how to get
some particular thing done.

Randy Hyde is on both groups and his no longer so new HLA
assembler (High Level Assembler) becomes a topic from time to
time and that gets interesting.  It's not just the usual "how
much should an assembler do for you" discussion but that's
usually it's starting point.

What keeps both groups interesting is the knowlegable people
that frequent it.  A few jerks participate now and then and
sometimes one is so loquacious that I'll stop reading till he
goes away.  But not usually.  It's normally a pretty polite
group.  Not as polite as this list, but then not many lists are
this polite either.

I do follow both, but not all the time.  I'll read one or the
other for a while and then drift away and then come back and
follow them again.  The only groups I read every day are the
Tandy group (I have some model 100/102/200s) and and the HP48
group and most of the time, comp.lang.forth and comp.os.cpm.
All in all I probably read the asm groups about half the time.

Comp.os.msdos.programmer and alt.msdos.programmer are also
pretty good sometimes.  I don't follow them but I read them and
get involved in a thread or two sometimes.

Every couple of weeks I'll read comp.graphics.algorithms, which
is often over my head since my math is limited, but I learn a
lot every time.  Not that I do much programming anymore but I
still enjoy learning about new things.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 09:58:03 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: Fluff, Consumer Broadband and Digital Television Promotion Act
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Russel Brooks wrote:
> Ace Frehley wrote:
>> As we are all aware, this is not a forum to discuss political
issues
>> or laws. However, with the continued government pressure and
attempts
>> to reform and regulate the hardware and software industries,
readers
>
> If you want to fight all the stupid laws affecting the net
then
> go here  -->   http://www.eff.org
>
> The Electronic Frontier Foundation has proven itself willing
to
> go to court to fight for internet freedoms.

While the CDDTPA will have a pretty big effect on the net,
that's not really what it's about.  This is about every
computer, connected or not.  It's about DVD players and, if
they're computer controlled, cars and washing machines.  And
it's about programmers.

I sure hope the EFF gets involved in this but if they're the
only ones or even the main ones, we're in trouble.  This is a
lot bigger problem than that.  The whole electronics industry
and everyone who uses electronics should get involved in this.

I do agree this isn't a forum for political issues and
discussing it here won't accomplish much.  But I think some
small discussion of it from time to time to keep everyone aware
of it is probably worthwhile.  This law will definitely affect
200lx users.

I hope others agree.  Others, do you agree?

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 10:10:35 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: 200LX display
MIME-Version: 1.0
Content-Type: text/plain; charset="Windows-1252"
Content-Transfer-Encoding: 7bit

Wee-Meng Lee:
> I have with me two non-DS 200LX 2MB and am
> comparing the screen contrast. One is clearer
> than the other despite playing with the contrast (ON -/+)
> on the dimmer one.  The dimmer one is slightly more
> brownish. The clearer one is more light green.

I have 3 200LXs and a 100lx and 2 95LXs and I used to have
another 95lx which my nephew now has.  None are DS or modified
in any way.

Each has a different looking screen.  I have green and brown, as
you do.  The 100lx color tends more toward gold.  It has the
best contrast.

But the best of all was the 95lx that my nephew now has.  It has
a beautiful bright golden screen with great contrast.

One of mine has little enough contrast that I prefer not to use
it except in very good light.  It was my first 200lx.  I finally
got tired of the screen and bought another one.  The third one
was just a good deal I found in a pawn shop.  ($95 for a good as
new 2 meg 6 years ago).

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 17:22:36 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Chris

On Tue, 26 Mar 2002 21:09:33 -0000, Chris Randle <chris@AMLOG.CO.UK> wrote:

> it may just be a bit of luck with the donor machine. The best authority
> would be someone who has had a known machine upgraded who could comment
> on whether or not the contrast was affected.

When I upgraded my machine (one of the really well readable screens
from the 1998 made series SG8...), I haven't noticed any effect in
screen readability.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 10:38:50 -0600
Reply-To:     n2vip@VERIZON.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ken Hansen <n2vip@VERIZON.NET>
Subject:      Yahoo email (sorry out of thread)
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 7bit

Faced with the same Yahoo email change, I have decided to setup my own mailserver (Linux/Solaris box hanging off my DSL line with a dynamic DNS domain name - see http://www.dyndns.org/)...

To be honest, I have seen a marked increase in the amount of "spam" (is it still spam if I agree to it?) I get to compensate Yahoo for my POP access, so I won't really mind giving up the account by April 24th...

Just another data point, sorry if others previously suggested same, as I have been "out of the loop" for a week or two...

Ken

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 11:55:06 -0500
Reply-To:     Bob Newins <bnew@ATTBI.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Newins <bnew@ATTBI.COM>
Subject:      Re: 200LX display
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Best display I ever had was on a 100LX which I later upgraded to DS and
5 megs.  Wish I still had it.   =Bob=

Jens Siffring wrote:
>
> Hi,
>
> HP changed the display on the 4MB units. The 4MB ones
> had noticable better contrast then the 2MB unit machines.
>
> Thanks,
>
> Jens
>
> --
> Jens G. Siffring
> Project Lead
> Solace  -  The Siemens EMIS service and support department
> 7225 Northland Drive, Brooklyn Park, MN 55428-1540
> phone: 214-743-6746
> jsiffrin@siemens-emis.com
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 11:00:24 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
Comments: To: Victor Roberts <RobertsV@earthlink.net>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

----- Original Message -----
From: "Victor Roberts" <RobertsV@earthlink.net>
To: "Barry" <barry@FBTC.NET>; <HPLX-L@UCONNVM.UCONN.EDU>
Sent: Wednesday, March 27, 2002 7:47 AM
Subject: Re: FW: Important Yahoo! Mail Service Announcement


> I think we both agree that it is reasonable for us to each pay
> for basic access to the Internet. As for the types of services
> available on the Internet, I would argue that much of the free
> and creative stuff we both remember is still there. It may not
> be as visible due to all the commercial activity, but creative
> people are still writing and posting free or low cost software
> and the newsgroups are all still free. The fact that
newsgroups
> have become populated by too many thoughtless people is, I
> believe, due more to the huge increase in the number of people
> on the Inet then to commercial activity.

The good stuff is still there and I still use it.  But it's days
are numbered.  So are mine so I guess that's ok. :)

I do think the huge increase in the number of people in the net
and commercial activity go hand in hand.  They're the same
thing.  More people makes commerce possible and potentially
profitable and commerce draws more people.

Change happens.  This is the way of the world.  I'm not
complaining.  I don't argue with thunderstorms, either.  But it
saddens me to see some of the changes.  It saddened me when the
high winds in a thunderstorm blew down the shed in my back yard
last summer.  But I'm not really angry at the thunderstorm.

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 09:56:55 -0700
Reply-To:     Getz <jgetz@WCENET.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Getz <jgetz@WCENET.COM>
MIME-Version: 1.0
Content-Type: multipart/alternative;
              boundary="----=_NextPart_000_00D6_01C1D575.BA535D40"

This is a multi-part message in MIME format.

------=_NextPart_000_00D6_01C1D575.BA535D40
Content-Type: text/plain;
        charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

SIGNOFF HPLX-L=20

------=_NextPart_000_00D6_01C1D575.BA535D40
Content-Type: text/html;
        charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

<!DOCTYPE HTML PUBLIC "-//W3C//DTD HTML 4.0 Transitional//EN">
<HTML><HEAD>
<META http-equiv=3DContent-Type content=3D"text/html; =
charset=3Diso-8859-1">
<META content=3D"MSHTML 6.00.2600.0" name=3DGENERATOR>
<STYLE></STYLE>
</HEAD>
<BODY bgColor=3D#ffffff>
<DIV>SIGNOFF HPLX-L </DIV></BODY></HTML>

------=_NextPart_000_00D6_01C1D575.BA535D40--

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 10:41:05 -0800
Reply-To:     Qman <qman@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Qman <qman@EARTHLINK.NET>
Subject:      "Let there be (Revo)light!"
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

NEWS
Revoworld has a report on a successful modification of a Revo Plus. A South
Korean enthusiast has put a backlight on his Revo, complete with discrete
on-and-off switch.
http://www.geek.com/news/geeknews/2002mar/bpd20020314010724.htm

Now, you can read the backlight modification guidance in English at
http://www.kpsiug.net/
and look under "TIP&TECH"



Later,
Qman...

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 11:52:29 -0700
Reply-To:     "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
Subject:      Re: "Let there be (Revo)light!"
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"

The problem with adding a backlight to the LX is not that it couldn't be
done, it couldn't be done _consistently_ (i.e., without sometimes destroying
the LCD panel).

-----Original Message-----
From: Qman [mailto:qman@EARTHLINK.NET]
Sent: Wednesday, March 27, 2002 12:41 PM
To: HPLX-L@UCONNVM.UCONN.EDU
Subject: "Let there be (Revo)light!"


NEWS
Revoworld has a report on a successful modification of a Revo Plus. A South
Korean enthusiast has put a backlight on his Revo, complete with discrete
on-and-off switch.
<snip>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 20:03:50 +0100
Reply-To:     "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Subject:      Re: "Let there be (Revo)light!"
In-Reply-To:  <000e01c1d5be$f3eafa10$24637818@qmanibk3cv8u7t>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

> Revoworld has a report on a successful modification of a Revo
> Plus. A South
> Korean enthusiast has put a backlight on his Revo, complete with discrete
> on-and-off switch.

Looks interresting. I'd like to see an english translation of that page (and
later on some comments if this can be done with a HPLX).
Is there a korean listmember who can supply translation of the important
parts (and if its a crack or a scratch you can see on the two pictures taken
after re-assembly...)

regards,
Oliver

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 13:31:47 -0500
Reply-To:     John J Vanderstel <j_vanderstel@JUNO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         John J Vanderstel <j_vanderstel@JUNO.COM>
Subject:      Re: FW: Important Yahoo! Mail Service Announcement
MIME-Version: 1.0
Content-Type: text/plain
Content-Transfer-Encoding: 7bit

> There was no WWW then.  There wasn't anything you could pay for.
> But there was a lot of really good content provided by people
> who worked hard on their own time to put it there.

At a time when the general population could not get private internet
access from the island of Oahu Hawaii, a group of us pulled together and
eventually found access to the internet through the University of
Hawaii's free online library system.

We found a way to tunnel through the endless maze of menus within UH Carl
system and then on to most of the nation's freenets from where we could
do almost anything and access almost anything in text mode... all from a
little island in the middle of the Pacific.  It left all of us in awe!

We were never able to download anything with Kermit though that
connection, though.  I think it had something to do with a marginal 7 bit
connection somewhere down the line.

That didn't stop us from doing massive screen captures from various
newsgroups and other interesting places. ;-)  I used to post my screen
captures on my BBS for all to check out.

I paid for only one thing that I found while online at that time, and
that was a transcript for a specific television show.  I don't know if
that was located in the UH's local library or somewhere else on the
internet, though.

Later, when a lucky few actually got more direct (although long distance)
access to the internet, I setup a multi-user soup reader on my BBS and
regularly got copies of current soup packets from friends.  That allowed
anyone on the island with the simple terminal program "Banana Com" (with
doorway mode) could remotely use their account on that  soup reader and a
small amount of tightly controlled storage space on my hard drive to
follow a small select group of newsgroups.

As a feeble attempt to relate this thread back to the HP200LX, if I had
known about the HP200LX back then, I would have been able to access all
of that from a HP200LX.

Sorry.  I couldn't help jumping into this thread one last time.  This
string just brings back such good memories! :-)

Cheers!

John Vander Stel
Grand Rapids, Michigan


________________________________________________________________
GET INTERNET ACCESS FROM JUNO!
Juno offers FREE or PREMIUM Internet access for less!
Join Juno today!  For your FREE software, visit:
http://dl.www.juno.com/get/web/.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 11:12:11 -0800
Reply-To:     Qman <qman@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Qman <qman@EARTHLINK.NET>
Subject:      Re: "Let there be (Revo)light!"
Comments: To: "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I was able to read the English translation by going to
http://www.kpsiug.net/  look under Tips Tech.
Note: IE had to install the need fonts first though..



Later,
Qman...
----- Original Message -----
From: "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Wednesday, March 27, 2002 11:03 AM
Subject: Re: "Let there be (Revo)light!"


> > Revoworld has a report on a successful modification of a Revo
> > Plus. A South
> > Korean enthusiast has put a backlight on his Revo, complete with
discrete
> > on-and-off switch.
>
> Looks interresting. I'd like to see an english translation of that page
(and
> later on some comments if this can be done with a HPLX).
> Is there a korean listmember who can supply translation of the important
> parts (and if its a crack or a scratch you can see on the two pictures
taken
> after re-assembly...)
>
> regards,
> Oliver
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 11:18:17 -0800
Reply-To:     Qman <qman@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Qman <qman@EARTHLINK.NET>
Subject:      Re: "Let there be (Revo)light!"
Comments: To: "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I only need it done once,  getting the kit is the problem. (:-o)
Do you know of a sourse?



Later,
Qman...


----- Original Message -----
From: "Feldman, Robert" <Robert_Feldman@JDEDWARDS.COM>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Wednesday, March 27, 2002 10:52 AM
Subject: Re: "Let there be (Revo)light!"


> The problem with adding a backlight to the LX is not that it couldn't be
> done, it couldn't be done _consistently_ (i.e., without sometimes
destroying
> the LCD panel).
>
> -----Original Message-----
> From: Qman [mailto:qman@EARTHLINK.NET]
> Sent: Wednesday, March 27, 2002 12:41 PM
> To: HPLX-L@UCONNVM.UCONN.EDU
> Subject: "Let there be (Revo)light!"
>
>
> NEWS
> Revoworld has a report on a successful modification of a Revo Plus. A
South
> Korean enthusiast has put a backlight on his Revo, complete with discrete
> on-and-off switch.
> <snip>
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 21:26:36 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      OT: Re: Important Yahoo! Mail Service Announcement
Comments: To: Victor Roberts <RobertsV@EARTHLINK.NET>,
          Victor Roberts <RobertsV@EARTHLINK.NET>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Vic

On Tue, 26 Mar 2002 19:01:19 -0800, Victor Roberts <RobertsV@EARTHLINK.NET> wrote:

> There are few things of value in this world that are totally
> free. I would suggest that instead of looking for "free" ISPs
> and "free" e-mail services, we all find competent providers and
> pay them a fair fee to insure that they can stay in business.

I like these systems where the provider offer a basic service for free
but if you want more, you have to pay. So they win because they reach a
lot of people, and we win because we can have a lot of small services
for free.

In that case it is not the government whi pays, but these people who
want to use the advanced services.

Typical example is my email provider GMX. The basic services they offer
for free are more than enough for me. Okay, no large attachments
accepted, but for that purpose I have another mailnox at a provider
where I PAY for the service (and email is only a secondary service of
them, main service is the DSL access and web hosting).

Of course these free basic services are all on a best-effort basis, no
guaranteed services. But usually it works.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 21:26:38 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Datacomm
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Axel

Sorry, no idea about your problem, but..

On Wed, 27 Mar 2002 14:38:58 +0100, Axel Berger <Axel-Berger@NEXGO.DE> wrote:

> Or alternatively (and additionally for the desktop) can you suggest a slim
> and simple terminal with good and well documented scripting? W98 Hyperterm

have you tried Conex? It is a very flexible teminla emulation, and I'm
pretty sure it supports scripting.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Tue, 26 Mar 2002 23:13:57 +0100
Reply-To:     Michel Bel <michel.bel@ZONNET.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michel Bel <michel.bel@ZONNET.NL>
Subject:      Ohming out the 700LX PCMCIA socket 2 - Re: CF card inside 200LX
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

yesterday I wrote

> Well, so I assumed, you assert the Card Enable (CE1 and CE2) of both cards
> simultaneously, so this ought not to work. Essentially, this is the only
> place where the access to PCMCIA slots differs. All else is parallell.
>
> I am getting a 700LX soon (tomorrow) , and will try to find out what the
CE1
> and CE2 of the second (Nokia Card) slot are connected to on the Hornet
chip.
>

Results:

In the 700LX the CE1 and 2 are NOT connected to the hornet at all - so
either there are no extra pins for second PCMCIA slot use on the hornet, or
they are not used in the 700LX.

The other pins on the Nokia card slot are not matched with pins on the
PCMCIA 1 slot, except ground. So this appears a dead end.

So what is possible:

a) Assuming that the LX's use word access on all PCMCIA cards - Mux A0, CE1
and CE2 s.t. A0=0  asserts CE1,2 on the first slot, A0=1 asserts CE1,2 on
the second slot, and link a driver accordingly. You need to handle requests
to both PCMCIA socket 1 and PCMCIA socket 2

b) Abuse (as previously hinted) A24 and E25 as CE1 and CE2 for a second
card. This means thou canst not use linear memory cards over 16MB in the
first slot... ( or, not use more than 16MB linear). Use a small driver
which, when requesting a slot 2 access, raises A25 and A25 as well. You only
need to catch request to PCMCIA socket 2.

Michel


Michel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 09:31:47 +1200
Reply-To:     Roger Whitmarsh <lodger@NZ1.IBM.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Roger Whitmarsh <lodger@NZ1.IBM.COM>
Subject:      ASIC Registration
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

Folks, I am using ASIC quite heavily, and want to
register it, but when trying to contact the author,
David Visti at 73065.1302@compuserve.com I get an
"undeliverable" message from Compuserve.
Does anyone have another email address for David or
80/20 software?

Cheers...Roger Whitmarsh

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 22:44:28 +0100
Reply-To:     Frank LOUWERS <efflept@irfl.8m.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Frank LOUWERS <efflept@IRFL.8M.COM>
Subject:      Re: "Let there be (Revo)light!"
Comments: To: "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
In-Reply-To:  <NGBBIMAAPPDKFBDCKKACAEFICEAA.Oliver@Compuseum.de>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

On Wed, 27 Mar 2002 20:03:50 +0100, Oliver W. Leibenguth wrote:


>Looks interresting. I'd like to see an english translation of that page (and
>later on some comments if this can be done with a HPLX).
>Is there a korean listmember who can supply translation of the important
>parts (and if its a crack or a scratch you can see on the two pictures taken
>after re-assembly...)

Yes, you can read an English translation on
http://www.kpsiug.net/  and click Tip & Tech (on the left) and then
click article 91
You can/will be asked (several times) to install Korean Language pack
but I ignored that.

Regarding the HPLX, under photo 10 he speaks twice of a 200LX backlight
kit, interesting isn't it?

Best regards

Frank Louwers (Belgium)

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 23:04:25 +0100
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: Datacomm
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> have you tried Conex?

No, not yet. As I may have mentioned before I come from the Atari and still
do not use the games console as my main machine - will have to some day
soon though. I shall try it out, if google can find it for me, and thanks
for the hint.

As long as W98 supports full and complete not emulated DOS support I may
still get some useful work done.

Danke
        Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 10:14:13 +1200
Reply-To:     Tony Kan <tony.kan@CLEAR.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Kan <tony.kan@CLEAR.NET.NZ>
Subject:      Re: 200LX display
Comments: To: jsiffrin@SIEMENS-EMIS.COM
MIME-version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding:  7bit

Strangely my experience is more similar to Curtis Cameron's i.e. my 2Mb
version has the slightly green/yellow background and my 4Mb machine has a
silvery gray background.  I use the 2Mb machine and assigned the 4Mb as a
backup because of the better contrast.

>
> HP changed the display on the 4MB units. The 4MB ones had noticable
> better contrast then the 2MB unit machines.
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 09:54:11 +1100
Reply-To:     Russell Hemery <rhemery@POWERUP.COM.AU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russell Hemery <rhemery@POWERUP.COM.AU>
Subject:      Sega AC adapter perfect for LX
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Hi all

I just found an AC adapter at a garage sale that is a perfect match for the
LX.

Its an adapter for use with the Sega megadrive. Listed as 10 Volts 1.2 amps
voltage actual is 12.25V with the right size plug and correct polarity
(negative tip).

Hope this helps someone

Regards

Russell

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 20:02:57 -0500
Reply-To:     stan.hplx@VERIZON.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Stanley Dobrowski <stan.hplx@VERIZON.NET>
Subject:      Re: Around The World Info
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

If it is not too late:

I grew up in New Jersey, USA and currenly live in Rutherford, NJ.

My father is 100% Polish because both of his parents came to
this country throught Ellis Island from Poland.  On my mother's
side, I am a mixture of English, German and Irish that has been
living in the USA for many generations.


Stan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 17:22:54 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: Nicads in a 95lx
Comments: To: Barry <barry@FBTC.NET>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Sorry for another late reply. (and the long quote. But the
message is so old I thought it should be repeated.)

I certainly do not mind. In fact, the situation is worse than
indicated in my note below. I can state from first hand
experience <G> that if you insert NiCad batteries backwards
into a 95LX (easy to do because of the non-standard layout of
the spring contacts with respect to the positive battery
terminals) you will burn out the reverse battery protection
circuit. One weekend morning many years ago I had smoke pouring
out of my 95LX when I did just that.

NiCad and NiMH batteries have lower internal resistance than
alkaline batteries. If short circuited they will provide higher
current than an alkaline, even though their open circuit
voltage is lower. The reverse battery protection circuit in the
95LX is not designed to withstand this higher current.

Vic Roberts


On Sat, 5 Jan 2002 09:24:59 -0600, Barry <barry@FBTC.NET> wrote:

>
> This was on the Palmtop Paper site.  Victor, I hope you don't
> mind me posting it.
>
> This isn't what I remember from the discussions in HPHAND but
> it's what I can find now.

>
> PUTTING NON-ALKALINE BATTERIES IN BACKWARDS CAN DAMAGE THE 95LX?
> According to an HP Tech Support person, the 95LX does have
> reverse battery protection, but the circuit has been tested only
> with alkaline batteries, and HP will give no assurances that it
> will work or not self-destruct if a user installs Ni-Cds or
> equivalent. That is, if you install alkaline batteries
> backwards, the circuit will protect the 95LX without burning up,
> while all bets are off if you use Ni-Cds.
>
> Victor D Roberts
>
> CompuServe ID: [70413,1423]

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 17:23:00 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: NO luck getting online. :/
Comments: To: hplx@TWU.NET
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

How are you running Nettamer on your LX? Have you terminated
System Manager so your LX is a "pure" DOS computer? If Nettamer
runs on your laptop, it should work the same way on your LX as
long as System Manager is not interfering with the serial port.
(I assume you know that System Manager will interfere with the
serial port unless you shut it down or use one of a few special
programs to prevent it from interfering with the serial port.)

Victor Roberts


On Sat, 23 Mar 2002 16:41:30 -0600, Jessica Blank <hplx@TWU.NET> wrote:

> I have had great success via NetTamer on my laptop-- with the SAME copy of
> NetTamer and the SAME PCMCIA modem (Noteworthy 14.4 xjack) I am trying on
> the LX. It works on the laptop-- on the LX, it dials out, connects,
> logs in, then FREEZES (I need to
> ctrl-alt-del to get out of it) when it sets up the nameserver's IP
> address.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 17:46:11 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: Around The World Info
Comments: To: stan.hplx@VERIZON.NET
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Wed, 27 Mar 2002 20:02:57 -0500, Stanley Dobrowski <stan.hplx@VERIZON.NET> wrote:

> I grew up in New Jersey, USA and currenly live in Rutherford,
NJ.

And, those of us who were born and live in New York don't hold
that against you <G>.

Vic

P.S.  Stan really is a great friend and a good sailor.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 17:46:08 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: OT: Re: Important Yahoo! Mail Service Announcement
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Wed, 27 Mar 2002 21:26:36 +0200, Daniel Hertrich <daniel.hertrich@GMX.DE> wrote:

> I like these systems where the provider offer a basic service for free
> but if you want more, you have to pay. So they win because they reach a
> lot of people, and we win because we can have a lot of small services
> for free.

I use these sometimes also. For example I use the free efax
service at www.efax.com. They also have a service with more
features for a monthly fee. However, the free service is
sometimes not reliable. I do wish they had a paid service
that was not as expensive as their full service. I would pay a
modest amount per month to get the right to complain about
poor service <g>

Vic Roberts

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 02:52:46 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: Sega AC adapter perfect for LX
Comments: To: Russell Hemery <rhemery@POWERUP.COM.AU>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Russell Hemery wrote:
> I just found an AC adapter at a garage sale that is a perfect match for the
> LX.
>
> Its an adapter for use with the Sega megadrive. Listed as 10 Volts 1.2 amps
> voltage actual is 12.25V with the right size plug and correct polarity
> (negative tip).

Is that REGULATED voltage?
Did you perform your measurements under load?

I'm glad I got several of the HP AC adapters when they were
available cheap.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Wed, 27 Mar 2002 23:49:18 -0500
Reply-To:     Dario Draiman <dario200@MAIL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Dario Draiman <dario200@MAIL.COM>
Subject:      Re: OT: Re: Important Yahoo! Mail Service Announcement
Content-Type: text/plain; charset="ISO-8859-1"
Content-Transfer-Encoding: 7bit
MIME-Version: 1.0

I tried to get an account on GMX because Yahoo.com and mail.com no longer provide POP access for free, but it's all in german and I can't understand a word, I think I will end up to buying a german dictionary if I can't find I decent free email provider
:)

> Typical example is my email provider GMX. The basic services they offer
> for free are more than enough for me. Okay, no large attachments
> accepted, but for that purpose I have another mailnox at a provider
> where I PAY for the service (and email is only a secondary service of
> them, main service is the DSL access and web hosting).
>
> Of course these free basic services are all on a best-effort basis, no
> guaranteed services. But usually it works.
>
> GTX
> daniel
>

--

_______________________________________________
Sign-up for your own FREE Personalized E-mail at Mail.com
http://www.mail.com/?sr=signup

Win the Ultimate Hawaiian Experience from Travelocity.
http://ad.doubleclick.net/clk;4018363;6991039;n?http://svc.travelocity.com/promos/winhawaii/

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 11:11:27 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      EMI news!!
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi friends,

good news about the EMI problem
( http://www.daniel-hertrich.de/emi )

I have disassembled an Omnigo 700LX and really found another IR
receiver design in there! So HP was aware of the EMI problem, too, and
solved it: They used an IR transceiver chip instead of the IR LED and
the photo diode combined with the external circuit. AND: They shielded
all the stuff with metal.
The transceiver chip looks like the HP HSDL1001, but I am not sure
about this.

See http://www.daniel-hertrich.de/700lx

Another new aspect is that a German LX user (not on this list (yet))
has sent me a _very_detailled_ description of how he interprets the
200LX IR receiver circuit, and how he would try to solve the problem.
I will try it with his suggestions. Maybe this weekend, maybe later.
But be sure that I'll report the results!

Other thoughts about the EMI problem:

I don't think we should invest too much time and effort, because
actually the EMI problem is only relevant to Siemens phone users.
Ericsson and Nokia phones have stronger IR ports which lets us put them
in more distance from the HPLX's IR port, so the phones cannot cause
EMI anymore.
But if a solution can easily be done, as the suggestions of that LX
user seem to show, we should of course make it perfect and offer the
solution on the web.
The 700LX solution is not easily applyable to the 200LX. I have tried a
similar thing (using a Temic TFDS6500 transceiver chip) some time ago,
and it failed. But of course it _may_ also be possible with a huge
amount of effort. I definitely won't do that, though.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 14:06:22 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      To Franklin Eekhout (re: 700LX)
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Franklin,

I saw your 700LX pictures on HPLX.NET
(www.hplx.net/feature.700lx.html). You also have these manual circuit
corrections on your motherboard. Please let me know the serial number
of your 700LX! I'm curious if this is on all 700LX motherboards or jsut
the earlier ones...

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 14:17:31 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: OT: Re: Important Yahoo! Mail Service Announcement
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Dario

On Wed, 27 Mar 2002 23:49:18 -0500, Dario Draiman <dario200@MAIL.COM> wrote:

> I tried to get an account on GMX because Yahoo.com and mail.com no longer provide POP access for free, but it's all in german and I can't understand a word, I think I will end up to buying a german dictionary if I can't find I decent free email provid
e
> r :)

GMX has olso other language interfaces than German.

....

At least they had. You could choose betweek English, French, German,
Turkish.... I'm just visiting www.gmx.net and looking for the switch,
but cannot find it anymore! Even if you go to www.gmx.co.uk or
www.gmx.com, everything is in German! :-(
Does anyone know how to choose another language?

In the URL there is, if you click onto "Mitglied werden" (=become a
member) the language abbreviation "de". I remember that I could replace
that by other abbreviations (en, fr?) and that gave another language.
But now, all I get is a 404 error.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 09:09:12 -0500
Reply-To:     Gary Hodge <grh@UNITY.NCSU.EDU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Gary Hodge <grh@UNITY.NCSU.EDU>
Subject:      compuserve pricing
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

I use Compuserve when traveling to provide email service
internationally.  My billing plan is $9.95 per month for five hours
which is plenty for me to upload and download email.  I seem to remember
someone on the list saying that if you tell them you will cancel the
account they may offer other pricing plans, perhaps a per-call
arrangment.  Can someone provide details on this?  Under the per-call
plan are there still the surcharges for using non-CS networks?

GRH
--
Gary R Hodge
Associate Professor
CAMCORE, NC State University

919-515-6427
fax 919-515-6430
grh@unity.ncsu.edu

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 09:07:48 -0500
Reply-To:     Steve <novosad@SERVER030.FWB.SAIC.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Steve <novosad@SERVER030.FWB.SAIC.COM>
Subject:      Re: Fluff: WWW vs. Usenet)
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"

Barry wrote:

> They're similar.  A lot of the same people are on both.  Each
> has a few different people.  On alt.lang.asm they sometimes try
> to keep it general and not centered around the x86 cpu but for
> the most part the people there are x86 programmers and examples
> are usually given in x86 code.  The difference is small.

Barry,

   Thanks for replying.  I guess I'll continue to look at c.l.a.x
then.

> There are some long winded discussions about the "proper" way to
> code and the proper way to organize a program.  I usually enjoy
> these for a while and then ignore them when they get repetitive.

   I guess those go below my radar.  I haven't followed too
many of those recently.  (And I follow the contrary path to
the most vocal anyway. ;))

> A lot of the discussion, on both groups, is about how to get
> some particular thing done.

   That's what I generally look for in all the groups I follow,
except for the TV show of course.

> What keeps both groups interesting is the knowlegable people
> that frequent it.  A few jerks participate now and then and
> sometimes one is so loquacious that I'll stop reading till he
> goes away.  But not usually.  It's normally a pretty polite
> group.  Not as polite as this list, but then not many lists are
> this polite either.

   I agree 100%.  The PostScript and TV show groups are generally
polite.  The OS/2 groups get ugly every so often.  It's bad (sad)
when the knowledgable and intelligent get pushed out.

> Every couple of weeks I'll read comp.graphics.algorithms, which
> is often over my head since my math is limited, but I learn a
> lot every time.  Not that I do much programming anymore but I
> still enjoy learning about new things.

   I tend to follow that one.  Trying to work out what they're
talking about does burn the carbon out of the old cylinders at
times.  I've even worked up enough nerve to post there.  Great
way to look like a fool.  Every once in a while they come out
with a real gem.  Though my programming has fallen off of late,
it's still good to be familar with the problem solving techniques.

   You've pointed out some groups that might be worth a look.
Thanks.  And the news server I get posts from seems to only get
about half of the posts.  That can make getting sense out of a
thread problematic.

   This group (HPLX) has a better mix of interests than most
anything else on average, and it's varied enough to wade through
the extraneous posts.  So I guess it has a good standard
deviation as well as a good average. <g>

Steve

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 15:26:12 +0100
Reply-To:     radek.svagr@LGPHILIPS-DISPLAYS.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Radek Svagr <radek.svagr@LGPHILIPS-DISPLAYS.COM>
Subject:      power consumption
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

I measured a power consumption of my DS 5MB 200lx.
I know it was done before many times but I found something interesting.


Switched ON without any card inserted - 40mA
Switched ON with CF Transcend 128MB - 100mA
Switched ON with CF Sundisk 10MB - 120 mA
Switched ON with PCMCIA HP Flashcard 10MB /Sundisk/ - 40mA!!!

Everything measured when no acess to disk.

Why the flash PCMCIA card takes no power when not in use? It is a really big difference!

The only differnce I see between CF and Flash card is different voltage used /5 - 12V/ which means
different power supply of 200lx is used. Does it mean, that 5V supply cannot be switched off, when
the 200lx is ON?

Radek

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 15:50:54 +0100
Reply-To:     Michel Bel <michel.bel@ZONNET.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michel Bel <michel.bel@ZONNET.NL>
Subject:      Re: 700LX
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Daniel Hertrich wrote:
> I'm curious if this is on all 700LX motherboards or jsut
> the earlier ones...
I have a SG63... version,
Also has the manual corrections on the motherboard..
Michel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 17:42:25 +0100
Reply-To:     Jan Brandt <jebrandt@XS4ALL.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jan Brandt <jebrandt@XS4ALL.NL>
Subject:      Re: IR connection to Ericsson T39
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

I have no luck connecting my LX and my Ericsson T39 via Infrared.
In order to take it step by step I am concentrating on connecting the
two using Andreas Garzottos IR.EXE,
to see if I can establish a connection and perhaps transfer for instance
a vcard.

My LX is a double speed 200LX. According to the documentation of the
IR.EXE program an appropriate
baud rate should be 38400, but if I try that nothing at all works.
So I set the IR.CFG file to

[oget]
Mode=4
Baud=19200

I make sure the infrared port in the T39 is set to "ON".
I tell my T39 to send my own business card via infrared.
I then start the IR.EXE program on the LX with the following command
line:

ir oget > vcard.vcf

The IR program replies:
IR/LX 0.2 by A. Garzotto, Sep, 1999

Opening IrDA for OBEX receive...
Talking with "T39"...
IrDA connection established (9600 baud).
Closing IrDA connection...

So on the LX it seems like everything has worked (although I don't
understand why it reports 9600 baud),
but the T39 display says:

Connecting...
then after 2 seconds:
Connection failed
then
No device found
Search again ?

The vcard.vcf file that has been created in the LX is empty.

I know that the LX sees "something", because if I remove the T39 from
the line of sight
it never gets past the "Opening IrDA for OBEX receive..." message.

Am I missing something obvious here ? What am I supposed to see if this
works. Can the infrared port
be disabled in the LX ? On the other hand as described above the LX
seems to see the T39 alright, so
that's probably not the problem. Is there a handshake problem ?

Is this setup very sensitive to the relative position of the devices ?
I have tried holding them up almost against each other (obviously with
the IR ports facing each other),
I have tried placing them with a distance of 30 cm, and I have tried
anything in between.

I know that some people use this all the time, so if somebody could let
me know if this is supposed to
work "out of the box", or I need to tweak some settings somewhere, I
would appreciate it.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 17:52:25 +0100
Reply-To:     Lillebjorn Nilsen <bjni@ONLINE.NO>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Lillebjorn Nilsen <bjni@ONLINE.NO>
Subject:      FLUFF: Netscape 2.11
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

For most of my communication needs I use
my trusty 200LX. But I regularely visit
the Web and do FTP with my Toshiba laptop running
Windows 3.11 and Netscape 2.01.

(The reason why this is never upgraded:
it has worked for my needs, the
harddisk is almost filled and I hate
ugrading Windows programs...)

Lately Nestcape has failed: The dialer
calls my ISP and seems to connect OK.
Then Netscape is passive til I get the
message:

'Netscape is unable to locate the
server: so.and.so.com The server does
not have a DNS entry. Check the server
name in the Location [URL] and try
again.'

Some times I get through with these same
URL's. Any ideas?

 -----------------
 Lillebjorn Nilsen, Oslo Norway
 http://home.online.no/~bjni/lillebjorn.html
 http://bjni.home.online.no

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 18:52:36 +0100
Reply-To:     Zoran Vignjevic <zoranv@GOV.YU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Zoran Vignjevic <zoranv@GOV.YU>
Subject:      Re: FLUFF: Netscape 2.11
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Try again right after, and maybe again, in the middle of previous
request...Lately I used to get the same thing with Netscape 4.x and
win98, when I asked for some URL which DN is not defined locally in my
DNS server, I got the prompt answer like you, and when I repeated the
request it went to connecting...Maybe there is a problem with Netscape,
or routing...

Lillebjorn Nilsen wrote:
>
> For most of my communication needs I use
> my trusty 200LX. But I regularely visit
> the Web and do FTP with my Toshiba laptop running
> Windows 3.11 and Netscape 2.01.
>
> (The reason why this is never upgraded:
> it has worked for my needs, the
> harddisk is almost filled and I hate
> ugrading Windows programs...)
>
> Lately Nestcape has failed: The dialer
> calls my ISP and seems to connect OK.
> Then Netscape is passive til I get the
> message:
>
> 'Netscape is unable to locate the
> server: so.and.so.com The server does
> not have a DNS entry. Check the server
> name in the Location [URL] and try
> again.'
>
> Some times I get through with these same
> URL's. Any ideas?
>
>  -----------------
>  Lillebjorn Nilsen, Oslo Norway
>  http://home.online.no/~bjni/lillebjorn.html
>  http://bjni.home.online.no
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

--

Regards, Zoranv
http://albums.photopoint.com/j/AlbumList?u=10099
http://www.geocities.com/Heartland/Park/5906/

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 20:31:27 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: compuserve pricing
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Gary

On Thu, 28 Mar 2002 09:09:12 -0500, Gary Hodge <grh@UNITY.NCSU.EDU> wrote:

> which is plenty for me to upload and download email.  I seem to remember
> someone on the list saying that if you tell them you will cancel the
> account they may offer other pricing plans, perhaps a per-call
> arrangment.

Yes, I reported that. When I wanted to cancel my account they asked me
if I wanted to continue the accout on a by-call basis and since that
was exactly what I needed I agreed. Now I really pay nothing, except
when I'm travelling and using their service (which is only once for a
few weeks per year).
Maybe somply call them, say you want to cancel your account, and if
they want to go on to delete your data, quickly say you have
reconsidered and now don't want to cancel it anymore. ;-)
Then ask directly for the by-call service.

> Can someone provide details on this?  Under the per-call
> plan are there still the surcharges for using non-CS networks?

To be honest, I don't know. I have used the service only to access the
GMX POP/SMPT servers and I didn't really care about what they charged
me.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 13:38:59 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: FLUFF: Netscape 2.11
Comments: To: Lillebjorn Nilsen <bjni@ONLINE.NO>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Thu, 28 Mar 2002 17:52:25 +0100, Lillebjorn Nilsen <bjni@ONLINE.NO> wrote:

[snip]

> Lately Nestcape has failed: The dialer
> calls my ISP and seems to connect OK.
> Then Netscape is passive til I get the
> message:
>
> 'Netscape is unable to locate the
> server: so.and.so.com The server does
> not have a DNS entry. Check the server
> name in the Location [URL] and try
> again.'

I do not believe this is a Netscape problem. The problem is
related to the software you use to dial into your ISP and
establish a network connection. In Win9x this would be the DUN.
What are you using in Win 3.11?

Vic Roberts

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 22:38:11 -0000
Reply-To:     "Richard E. McEvoy" <remce@GOFREE.INDIGO.IE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Richard E. McEvoy" <remce@GOFREE.INDIGO.IE>
Subject:      Re: 200LX display
Comments: cc: Tony Kan <tony.kan@CLEAR.NET.NZ>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

My 200LX is a 32 mb DS (formerly 2mb) which has a superbly contrasty display
with a green background. Perhaps the year of manufacture has something to do
with it - the number is SG60500337. Somebody explained the numbering some
time ago, but I can't remember whether the 605 means June of 1995, or May of
1996 : ) I bought it in London on June 14th 1996.

Richard.

----- Original Message -----
From: "Tony Kan" <tony.kan@CLEAR.NET.NZ>
To: <HPLX-L@UCONNVM.UCONN.EDU>
Sent: Wednesday, March 27, 2002 10:14 PM
Subject: Re: 200LX display


> Strangely my experience is more similar to Curtis Cameron's i.e. my 2Mb
> version has the slightly green/yellow background and my 4Mb machine has a
> silvery gray background.  I use the 2Mb machine and assigned the 4Mb as a
> backup because of the better contrast.
>
> >
> > HP changed the display on the 4MB units. The 4MB ones had noticable
> > better contrast then the 2MB unit machines.
> >
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 23:00:04 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: OT: Re: Important Yahoo! Mail Service Announcement
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Dario Draiman wrote:
> I tried to get an account on GMX because Yahoo.com and
> mail.com no longer provide POP access for free, but it's all in
> german and I can't understand a word, I think I will end up to
> buying a german dictionary if I can't find I decent free email provide

GMX recently changed to German only.  Fortunately my girlfriend
speaks German so I have a local translator whenever I get mail
from GMX or have to use their web site.

Their service has been good; I've been using GMX as an alternate
email address for over a year now.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 17:19:30 -0500
Reply-To:     stan.hplx@VERIZON.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Stanley Dobrowski <stan.hplx@VERIZON.NET>
Subject:      Re: AW: charging system
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Axel,

The 100LX and 200LX require a regulated 12 volts DC.  You
cannot expect it to work normally when you give it anything
different.  You should stop playing around with different
voltages and just conform to the HP specification.


Stan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 19:46:48 -0500
Reply-To:     Bob Newins <bnew@ATTBI.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Newins <bnew@ATTBI.COM>
Subject:      Compuserve & ACCIS 4.0c
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

A couple of months ago I changed my Compuserve password.  Big mistake.
Can't seem to log on anymore.  Did something change in the script in the
last few months?  I have since changed my password many times.  No luck.

ACCIS starts, dials, connects.  "Logging onto compuserve".  Then I keep
getting "Incorrect User ID or Password" error message.  I have even
entered the password manually into the ACCIS configuration file.  So,
something must be wrong with the script?

Would someone using ACCIS with compuserve send me a copy of the first
part of their log-on script.  Other suggestions?  Thanks.    =Bob=

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 03:52:52 +0100
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: Compuserve & ACCIS 4.0c
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

As far as I can make out, there were no changes, recent or otherwise. The
login script from the ROM of our HPs still works fine for me - can't do
anything anymore once I am logged in, but that's not relevant here.
What I fear you might have inadvertantly done while changing your password:
Compuserve want us off their traditional service, which they now call
"classic" and onto their proprietary new stuff and same as when shoving
people off vt100 access they do tend to use rather devious ways to achieve
it. So now your access may be not only "windows only" but rather "windows
plus proprietary installed software only".

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 21:24:19 -0800
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      GPRS and 6310
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

There seems to be some problems with this combo for one person here...

Here is something that may be interesting from Andreas:

======

I have no problems with it. For a normal connection, do the same as for
any other phone. For GPRS, use something like (change numbers etc):

[GPRS]
Port=-1
PPP=1
Modem=1
Script=CHAP_Script
My_IP=192.168.210.1
DNS_IP=130.59.10.30
DNS2_IP=0.0.0.0
Login=gprs
Password=
Baud=38400
ModemInit=AT&F
;ModemInit=AT&F+CGDCONT=1,"IP","gprs.swisscom.ch"
Dial=*99#
Magic=0
Compress=0

Important are the last 2 since they implemented a minimap PPP server in
the phone.

Andreas

==========

Hope this helps.

Avi


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 22:31:10 -0800
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      GMX Webpage
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

try this: http://www.google.com and look for the link to language tools on
the right.  click it. Then go to the TRANSLATE box (second box down the
page. The bottom prompt will take a url and you can select the translation
you need. I guarantee you a rather stilted translation - German is very
hard to translate by machine. But I think there is enough in the
translation to make sense and let you decided. Good luck!

    avi


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 21:20:42 -0800
Reply-To:     bobv <bobv@SOS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         bobv <bobv@SOS.NET>
Subject:      voltage reduction
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

I have an ac adapter with a 24 volt dc output.

Can I just put in a resistor to drop it down to the 12V needed by the
200LX?

Thanks

Bob

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 08:09:52 +0100
Reply-To:     "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Subject:      Re: EMI news!!
In-Reply-To:  <HPLX-L%2002032805100472@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Hello,

I just checked your pictures and found on picture of the assembled 700lx
(03150055.jpg) quite disturbing. It look like ther's some kind of a world
map on the lower left portion of the keyboard. I don't have that on my 700lx
(German SG63)? I made a (BIG) picture of it:
http://www.compuseum.de/pub/700lx.jpg (557kb).

Second question: I have a Nokia Infrared link JLP-1. It consists of an
IR-transceiver for a Nokia 8110 and another one for a Nokia Datacard. On
Your pictures you can see the connectors of the datacard.... and they're
completely different to what they're supposed to look like for my IR-Link
:-( Are there different datacards with different connectors?

regards,
Oliver

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 09:15:54 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      registering domain name
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Hi Daniel, Bob, Bob, Avi, Stefan, Russel, Nathalie, and all
others  !

what is the best way to register a .com domain name ?

important : this to be done without credit card .. thru bank
transfer only

we don't have on line validated credit cards rampantly
available in india !

..pk

(also other opinions .. pricing, reliability, features, page
hosting, webspace ..)

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Thu, 28 Mar 2002 23:29:04 -0800
Reply-To:     Marta Pierce <Marta1@attbi.com>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marta Pierce <Marta1@ATTBI.COM>
Organization: Family
Subject:      Nextel  i85s connectivity?
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Hello HPLX,

  I just purchased a Nextel  i85s phone, and was wondering if anyone
  had used it w/ the hp200 ?  The manual states that you can use the
  phone as a modem.  I looked on Daniel's page, and didn't see this
  particular phone listed anywhere.

  TIA

--
Best regards,
 Marta                          mailto:Marta1@attbi.com

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 03:13:31 -0500
Reply-To:     LEONG Ka Tai <leongkt@HKIPP.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         LEONG Ka Tai <leongkt@HKIPP.ORG>
Subject:      Re: compuserve pricing
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Gary R Hodge wrote:

> I use Compuserve when traveling to provide email service
> internationally.  My billing plan is $9.95 per month for five hours
> which is plenty for me to upload and download email.  I seem to remember
> someone on the list saying that if you tell them you will cancel the
> account they may offer other pricing plans, perhaps a per-call
> arrangment.  Can someone provide details on this?  Under the per-call
> plan are there still the surcharges for using non-CS networks?

I used to subscribe to Compuserve. It was quite good 10 years
ago. The surcharges are horrendous though. I live in Asia, and
when I travelled, the surcharges can come to more than US$1 per
minute. Then they started to cut down the network. So I
unsubscribed.

Compuserve will most probably keep the surcharges on non-CIS
networks since they have to pay access fees. And they probably
make a bundle on the mark up.

I now have mailboxes accessible by POP and the web. There are
cybercafes everywhere, or one can always borrow time on a
computer. Just be sure to delete history and clear the cache
after using the browser.

I have also tried iPASS on my last trip. It worked fine.

Just my $.02's worth.

Ka Tai

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 10:32:00 +0100
Reply-To:     xmarc@free.fr
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marc BERLIOUX <xmarc@FREE.FR>
Subject:      Re: registering domain name
In-Reply-To:  <006b01c1d6d4$3bd7e520$6674c5cb@pk>
Content-Type: text/plain; charset="iso-8859-1"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit

> what is the best way to register a .com domain name ?

try this :

http://www.gandi.net

--
Marc BERLIOUX
"Sans technique, un don n'est qu'une sale manie" G.Brassens

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 10:36:18 +0100
Reply-To:     xmarc@free.fr
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marc BERLIOUX <xmarc@FREE.FR>
Subject:      Re: voltage reduction
In-Reply-To:  <3CA3F9AA.C75DEAD1@sos.net>
Content-Type: text/plain; charset="iso-8859-1"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit

> I have an ac adapter with a 24 volt dc output.
> Can I just put in a resistor to drop it down to the 12V needed by
> the 200LX?

better is to put a bridge rectifier + a 20005F capacitor + a voltage
regulator (7812CT) for example.

--
Marc BERLIOUX
"Les statistiques sont formelles :
 Il y a de plus en plus d'itrangers dans le monde"

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 10:28:03 +0100
Reply-To:     xmarc@free.fr
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marc BERLIOUX <xmarc@FREE.FR>
Subject:      Re: FLUFF: Netscape 2.11
Comments: To: Lillebjorn Nilsen <bjni@ONLINE.NO>
In-Reply-To:  <200203281652.RAA01604@mail47.fg.online.no>
Content-Type: text/plain; charset="iso-8859-1"
MIME-Version: 1.0
Content-Transfer-Encoding: 8bit

Try to specify your provider's Domain Name Servers (DNS) in your
TCP/IP settings (or PPP settings), if not done.

--
          Marc BERLIOUX -- M.C.S.E
- Minesweeper Consultant & Solitaire Expert -

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 09:53:03 +0100
Reply-To:     Michel Bel <michel.bel@ZONNET.NL>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michel Bel <michel.bel@ZONNET.NL>
Subject:      Re: AW: charging system
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

----- Original Message -----
From: "Stanley Dobrowski" <stan.hplx@VERIZON.NET>
--snip--
> The 100LX and 200LX require a regulated 12 volts DC.  You
> cannot expect it to work normally when you give it anything
> different.

The Specs clearly say ( Page B-6 in the User's Guide):

  Minimum voltage +9.6 V
  Nominal Voltage +12V
  Maximum Voltage +14.4 V

I have used a 10.5 V, 1A miniature switched  supply for over a year now,
without problems.

Michel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 11:05:02 +0100
Reply-To:     xmarc@free.fr
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marc BERLIOUX <xmarc@FREE.FR>
Subject:      test
Content-Type: text/plain; charset="utf-8"
MIME-Version: 1.0
Content-Transfer-Encoding: quoted-printable

sorry for the noise

=C2=B9~#{[|`\^@]}
=E2=82=AC=C2=A3$=C2=B5*%=C3=B9
=C3=A9=C3=A8=C3=A7=C3=A0=C2=A7


--=20
          Marc BERLIOUX -- M.C.S.E
- Minesweeper Consultant & Solitaire Expert -

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 12:52:05 +0530
Reply-To:     pksharma <pksharma@CAL.VSNL.NET.IN>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         pksharma <pksharma@CAL.VSNL.NET.IN>
Subject:      Re: registering domain name
Comments: To: xmarc@free.fr
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

tks marc

..pk

----- Original Message -----
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Friday, March 29, 2002 3:02 PM
> try this :
> http://www.gandi.net

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 14:08:43 +0200
Reply-To:     Nigel R <nigel@KEEPSMILING.CO.ZA>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Nigel R <nigel@KEEPSMILING.CO.ZA>
Organization: STRATEGIC ALLIANCE CONSULTING
Subject:      Siemens IC35; An HP companion?
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Hi everyone, Nigel R from sunny South Africa again!

I came across the Siemens IC35 device awhile back and wondered if it could
be as useful as my 95LX but physically smaller...  I even hunted down a SDK
pack and lots of other related info (including a PC based emulator) but
seems the device never became popular(?).  I may have a chance to acquire a
new unit at a low price now that locally there is (or would seem that way)
no support or active promotion.  Does anyone have any experience or comments
relating to the IC35 and if there would be any value in interfacing to the
HP palm?  The physical size of the unit is certainly more practical than
many other PDA's but applications seem to be limited...

Till the next time, KEEP SMILING :-)

Nigel R

HP95LX (1Mb + 2Mb PCMCIA card!)

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 13:07:24 +0000
Reply-To:     Stefan.Peichl@T-ONLINE.DE
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Stefan Peichl <Stefan.Peichl@T-ONLINE.DE>
Subject:      Re: power consumption
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Radek Svagr wrote:

> Switched ON without any card inserted - 40mA
> Switched ON with CF Transcend 128MB - 100mA
> Switched ON with CF Sundisk 10MB - 120 mA
> Switched ON with PCMCIA HP Flashcard 10MB /Sundisk/ - 40mA!!!

Did you always wait for 2-3 seconds after power on before
measuring the voltage? At least the Sundisk cards should
power down by themselves after some seconds (my 96 MB CF card
does). LXCIC/S can also tell you, if your card powered down.

Access the card and call immediately LXCIC/S. It will tell you
"Card powered". Then wait for 2 seconds and call LXCIC/S again.
My Sundisk CF now reports "Card power down".

Indeed you have to run LXCIC from your C: drive and your path
should have no A: references, otherwise loading LXCIC from the
card or searching the card would always power it on.

Stefan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 14:40:11 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: Siemens IC35; An HP companion?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Nigel

On Fri, 29 Mar 2002 14:08:43 +0200, Nigel R <nigel@KEEPSMILING.CO.ZA> wrote:

> no support or active promotion.  Does anyone have any experience or comments
> relating to the IC35 and if there would be any value in interfacing to the
> HP palm?  The physical size of the unit is certainly more practical than
> many other PDA's but applications seem to be limited...

I used the IC35 for a few days, and I can only say, that it is IMO a
good organizer and SMS keyboard for a Siemens phone.
AFAIK it also has an email client, so it may be good for email either.
But the keyboard is really crap, compared to the HP palmtops, and the
lacking DOS compatibility makes it far less flexible.
So I sold mine again.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 14:40:12 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: EMI news!!
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Oliver

On Fri, 29 Mar 2002 08:09:52 +0100, "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE> wrote:

.> I just checked your pictures and found on picture of the assembled 700lx
> (03150055.jpg) quite disturbing. It look like ther's some kind of a world
> map on the lower left portion of the keyboard. I don't have that on my 700lx
> (German SG63)? I made a (BIG) picture of it:
> http://www.compuseum.de/pub/700lx.jpg (557kb).
>

Aha!
Well, I'm glad you recognize it as a world map. Indeed it is. When I
first saw it, I thought is was a kind of chemical reaction of the case
plastic with something else, until I looked from a bigger distance and
saw it is a world map.

What you _also_ have on the case plastic are these little stars (left
of the left hinge, for example). Mine is a SG60... unit, that seems to
mean that mine is really an early machine (beginning of 1996) and only
three weeks later they produced them without this decoration.
How about other 700LX owners? Do you have this world map on the
keyboard frame? What are the serial numbers of your machines?


> Second question: I have a Nokia Infrared link JLP-1. It consists of an
> IR-transceiver for a Nokia 8110 and another one for a Nokia Datacard. On
> Your pictures you can see the connectors of the datacard.... and they're
> completely different to what they're supposed to look like for my IR-Link
> :-( Are there different datacards with different connectors?

I don't know.
I have never seen a Nokia datacard before I bought and npened this
700LX.
But another thing which was interesting about my 700LX Nokia data card
is that it seems to be made from plastic, nut fro mmetal, as PCMCIA
card are usually made. Maybe this is a special edition for the 700LX.
But then it is strange that they left the conector. They could have
removed it, because it's not needed in the 700LX.

Well, the 700LX seems to be a mystic machine. :-)

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 14:40:14 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: voltage reduction
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Bob

On Thu, 28 Mar 2002 21:20:42 -0800, bobv <bobv@SOS.NET> wrote:

> Can I just put in a resistor to drop it down to the 12V needed by the
> 200LX?

No. The voltage the resistor would reduce the 24V by would vary
depending on the currect the LX needs (Ohm's law).
You need a voltage regulator, or simply buy another AC adapter. Would
be the easiest and maybe the cheapest option.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 13:16:09 +0100
Reply-To:     xmarc@free.fr
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marc BERLIOUX <xmarc@FREE.FR>
Subject:      [OT] need a german translator
Content-Type: text/plain; charset="iso-8859-1"
MIME-Version: 1.0
Content-Transfer-Encoding: quoted-printable

I need translation for the following german text.
As i know there are plenty of smart and helpful german guys on the=20
list, if one of them has a few minutes...

-----------------------------------------------
Die Schaltung

Die Schaltung ist vollst=E4ndig analog aufgebaut, es kommen nur=20
Standardbauteile zum Einsatz. Den Aufbau =FCber Software habe ich=20
verworfen, weil die Schaltung echtzeittauglich und auch au=DFerhalb=20
eines Computers laufen sollte. Diese Schaltung ist allerdings von mir=20
nicht praktisch realisiert, sondern nur simuliert worden (mit dem=20
Simulationsprogramm electonic workbench 5.0, ein Mixed-Mode=20
Simulationsprogramm, das auf einen Spice-Kern basiert). D.h. es ist=20
wahrscheinlich, da=DF die Schaltung funktioniert, aber nicht sicher.=20
Deshalb existiert auch leider (noch) keine Platine. Sie wird=20
vielleicht nachgeliefert. Sollte jemand die Schaltung praktisch=20
umsetzen, w=E4re ich ihm dankbar, wenn er mir den Platinenentwurf=20
zukommen lie=DFe (mail an mich).

Sollte jemand diese Schaltung nachbauen, weise ich ausdr=FCcklich=20
darauf hin, da=DF ich die Schaltung zwar nach bestem Wissen entworfen=20
habe, sie aber weder testete noch 100% sicher bin, da=DF sie exakt den=20
original Dolby-Encodern enstpricht. Au=DFerdem m=FCssen f=FCr den=20
praktischen Einsatz dieses Encoders nat=FCrlich alle Schutzrechte von=20
Dolby beachtet werden.=20
-----------------------------------------------

thanks

--=20
Marc BERLIOUX
"Y a des ann=E9es o=F9 on a rien envie de faire"

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 15:27:23 +0100
Reply-To:     "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Subject:      Re: EMI news!!
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
In-Reply-To:  <HPLX-L%2002032908384572@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

> What you _also_ have on the case plastic are these little stars (left
> of the left hinge, for example).

The stars on the display-portion of the screen are present, I'm only missing
the world map :-( Anyone willing to donate his shell?

> What are the serial numbers of your machines?

SG63200081

> But another thing which was interesting about my 700LX Nokia data card
> is that it seems to be made from plastic, nut fro mmetal, as PCMCIA
> card are usually made. Maybe this is a special edition for the 700LX.

Mine is made out of plastic, too. I've seel several nokia datacards on
internet auctions (they all had a metal casing), but I've never seen the
connectors. The connector should be about 15mm wide, compared to the one in
the 700lx.

> But then it is strange that they left the conector. They could have
> removed it, because it's not needed in the 700LX.

They made quite some efforts to put in a second PCMCIA-connector. Why didn't
HP dump the whole datacard stuff in favor of a "on board" solution? The
700lx could be *much* slimmer ;-)

> Well, the 700LX seems to be a mystic machine. :-)

;-)

regards,
Oliver

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 06:38:48 -0800
Reply-To:     Longden_Loo@CANDLE.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Longden Loo <Longden_Loo@CANDLE.COM>
Subject:      Re: 200LX display
MIME-Version: 1.0
Content-type: text/plain; charset=us-ascii

> My 200LX is a 32 mb DS (formerly 2mb) which has a superbly contrasty
display
> with a green background. Perhaps the year of manufacture has something to
do
> with it - the number is SG60500337. Somebody explained the numbering some
> time ago, but I can't remember whether the 605 means June of 1995, or May
of
> 1996 : ) I bought it in London on June 14th 1996.

Neither.  According to the FAQ, it was the 337th unit made in the 5th week
of 1996 (Jan-Feb).

SG y ww nnnnn

- Longden (who has an SG6 also)

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 16:31:26 +0100
Reply-To:     Jacques Belin <jbelin@ALTERN.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jacques Belin <jbelin@ALTERN.ORG>
Subject:      [OT] Re: registering domain name
In-Reply-To:  <02032910320001.01376@obelix.gaulois>
MIME-Version: 1.0
Content-Type: text/plain; charset="ISO-8859-1"
Content-Transfer-Encoding: 8bit

Le Fri, 29 Mar 2002 10:32:00 +0100
Marc BERLIOUX <xmarc@FREE.FR> a icrit:

> > what is the best way to register a .com domain name ?
>
> try this :
>
> http://www.gandi.net

Possible, but not really easy. From their web site :

    "You can pay by credit card (MasterCard, or Visa - but not Visa
    Electron), or by bank check (only if drawn on a French bank, in
    Euros). Except for transfers for which you must pay by credit card
    for now (we are working on this).

    Domain name owner and the payer can be different people."

Anyway, I will see some of the Gandi folks next thursday. If I see
Valentin Lacambre (who is in charge of the money matters), I will ask
him if he has some experience with indian domain owners...


Jacques.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 17:01:40 +0100
Reply-To:     Jacques Belin <jbelin@ALTERN.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jacques Belin <jbelin@ALTERN.ORG>
Subject:      Re: 200LX display
In-Reply-To:  <OFC691563E.B7E5B968-ON88256B8B.004FE08F@candle.com>
MIME-Version: 1.0
Content-Type: text/plain; charset="ISO-8859-1"
Content-Transfer-Encoding: 8bit

Le Fri, 29 Mar 2002 06:38:48 -0800
Longden Loo <Longden_Loo@CANDLE.COM> a icrit:

> SG y ww nnnnn

SG means that it was manufactured in the Singapore HP's plant.

Jacques.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 17:01:40 +0100
Reply-To:     Jacques Belin <jbelin@ALTERN.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jacques Belin <jbelin@ALTERN.ORG>
Subject:      Re: test
In-Reply-To:  <02032911050205.01376@obelix.gaulois>
MIME-Version: 1.0
Content-Type: text/plain; charset="UTF-8"
Content-Transfer-Encoding: 8bit

Le Fri, 29 Mar 2002 11:05:02 +0100
Marc BERLIOUX <xmarc@FREE.FR> a icrit:

> B9~#{[|`\^@]}
> b ,B#$B5*%C9
> C)C(C'C B'

Missed..

'charset="utf-8" ' : Not a standard, according to the RFCs..

You should try ISO-8859-15 (Latin 9) which includes the euro symbol, and is
a valid charset...


Jacques.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 10:41:47 -0800
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: [OT] need a german translator
Comments: To: xmarc@free.fr
In-Reply-To:  <02032913160900.01688@obelix.gaulois>
Mime-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"; format=flowed
Content-Transfer-Encoding: quoted-printable

Google.com Language Tools link yields this:

The circuit

The circuit is developed completely similarly, it comes only standard=20
construction units to the employment.  I rejected the structure over=20
software, because the circuit should run real time-suited and also outside=
=20
of a computer.  This circuit is however realized of me not practically, but=
=20
only simulated (with the simulator routine electonic workbench 5,0, a mix=20
OD mode simulator routine, which is based on a Spice core).  I.e. it is=20
probable that the circuit functions, but not surely.  Therefore (still) no=
=20
plate also unfortunately exists.  It is perhaps delivered subsequently.  If=
=20
someone should convert the circuit practically, I would be grateful, if he=
=20
gave the plate draft me (mail to me).  If someone should copy this circuit,=
=20
I point out expressly that I sketched the circuit after best knowledge, her=
=20
however neither tested nor 100% am safe that she enstpricht accurately the=
=20
original Dolby Encodern.  In addition all patent rights must be naturally=20
considered by Dolby for the field use of this Encoders.

At 3/29/02 +0100, you wrote:
>I need translation for the following german text.
>As i know there are plenty of smart and helpful german guys on the
>list, if one of them has a few minutes...
>
>-----------------------------------------------
>Die Schaltung
>
>Die Schaltung ist vollst=E4ndig analog aufgebaut, es kommen nur
>Standardbauteile zum Einsatz. Den Aufbau =FCber Software habe ich
>verworfen, weil die Schaltung echtzeittauglich und auch au=DFerhalb
>eines Computers laufen sollte. Diese Schaltung ist allerdings von mir
>nicht praktisch realisiert, sondern nur simuliert worden (mit dem
>Simulationsprogramm electonic workbench 5.0, ein Mixed-Mode
>Simulationsprogramm, das auf einen Spice-Kern basiert). D.h. es ist
>wahrscheinlich, da=DF die Schaltung funktioniert, aber nicht sicher.
>Deshalb existiert auch leider (noch) keine Platine. Sie wird
>vielleicht nachgeliefert. Sollte jemand die Schaltung praktisch
>umsetzen, w=E4re ich ihm dankbar, wenn er mir den Platinenentwurf
>zukommen lie=DFe (mail an mich).
>
>Sollte jemand diese Schaltung nachbauen, weise ich ausdr=FCcklich
>darauf hin, da=DF ich die Schaltung zwar nach bestem Wissen entworfen
>habe, sie aber weder testete noch 100% sicher bin, da=DF sie exakt den
>original Dolby-Encodern enstpricht. Au=DFerdem m=FCssen f=FCr den
>praktischen Einsatz dieses Encoders nat=FCrlich alle Schutzrechte von
>Dolby beachtet werden.
>-----------------------------------------------
>
>thanks
>
>--
>Marc BERLIOUX
>"Y a des ann=E9es o=F9 on a rien envie de faire"
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 17:40:23 +0000
Reply-To:     castorlw@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Larry Castor <castorlw@YAHOO.COM>
Subject:      Re: compuserve pricing
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Gary,

> I use Compuserve when traveling to provide email service
> internationally.  My billing plan is $9.95 per month for five hours =
which is plenty for me to upload and download email.  I seem to remember =
someone on the list saying that if you tell them you will cancel the =
account they may offer other pricing plans, perhaps a per-call arrangment.=
  Can someone provide details on this?<<

I had the same plan and am trying to go to the per-call arrangement.  =
Actually, I called to do this and was told it was not possible BUT, I =
could cancel "classic" go to their new service and then cancel there new =
service and the per-call would be in place. So, I said okay, send me the =
cd and I will do that.  The cd never came!  But last month there was no =
compuserve charge either and I am still getting email via post/lx.  So, =
I'm waiting till I get this months bill and then I will test to see if I =
still have access with accis4. And at what cost.

Larry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 13:11:18 -0500
Reply-To:     Bob Penick <bnj@MYREALBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Penick <bnj@MYREALBOX.COM>
Subject:      Re: EMI news!!
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

> Well, I'm glad you recognize it as a world map. Indeed it is. When I
> first saw it, I thought is was a kind of chemical reaction of the case
> plastic with something else, until I looked from a bigger distance and
> saw it is a world map.
>

I bought my first off eBay and when it arrived I initially wondered what
kind of accident could have caused such "damage" to the case.  I later
recognized that was a decoration(?), but I'm still not sure it is an image
of the planet I live on.  I've looked and held it at different angles while
comparing it to a globe, trying to figure out where on the Earth they had
pictured.  The only conclusion was reached by my wife as she looked at ME
and shook her head knowing that I had surely lost what sanity I had been
maintaining until then.

> mean that mine is really an early machine (beginning of 1996) and only
> three weeks later they produced them without this decoration.
> How about other 700LX owners? Do you have this world map on the
> keyboard frame? What are the serial numbers of your machines?
>
SG615XXXXX originally from South Africa & SG618XXXXX originally from
Scotland and they both have the celestial decorations.

Later,
bob

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 08:14:28 -1000
Reply-To:     Renato de Vega <r.devega@WORLDNET.ATT.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Renato de Vega <r.devega@WORLDNET.ATT.NET>
Subject:      using the 200LX to write and get email with a Verizon ADSL
              connection
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Hi All,

I am considering having Verizon DSL installed in my house because my
children's use of the Internet with my present dial-up connection is tying
up the phone line. Before I do this, I want to make sure that I can still
use my 200LX to access email.

I have stuck with AT&T as my ISP because I can access email with my 200LX
from just about anywhere. I don't know if I can still do the same if I have
Verizon DSL installed.

Verizon cannot help me with my question. The tech help sounded as if I was
talking strange when I told him about the 200LX. I told myself I better
consult the HPLX List where I wouldn't seem too strange. Thus, my request
for help.

Thanks in advance for any assistance.

Renato de Vega
Mililani, HI

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 19:34:42 +0100
Reply-To:     "M. L." <lennartz-mi@GMX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "M. L." <lennartz-mi@GMX.NET>
Subject:      Re: Siemens IC35
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8Bit

Hallo

the IC35 was one of my favorites, before I 've got to know the HP. But... you must know, that it has a Z80 heart. I love the Z80-processor (worked some years with it), but it nobody can create a good organizer with 64kByte RAM. The Siemens-engineers did a
trick: They have some RAM-banks and switch between the banks. So you can use only 4 kByte for a note or memo or e-mail. The emulation for the PC had some failures (may be, the original has the same ones).

(all concluded from the documents, because I didn't buy a organizer, which allows only 4 kByte messages).

BTW: The gameboy has a Z80-processor, too.

My question: The Sharp SE-500 is a organizer with e-mail-functions. Are there any good or bad experiences?

Mit freundlichem Gru_
Michael Lennartz
www.lennartz-online.net
lennartz-mi@gmx.net
Fax: +49 89 244 34 52 57


>----- Urspr|ngliche Nachricht -----
 (Nigel R <nigel@KEEPSMILING.CO.ZA>; Fri, 29 Mar 2002 14:08:43 +0200)
>Hi everyone, Nigel R from sunny South Africa again!
>
>I came across the Siemens IC35 device awhile back and wondered if >it could
>be as useful as my 95LX but physically smaller...  I even hunted down >a SDK
>pack and lots of other related info (including a PC based emulator) but
>seems the device never became popular(?).  I may have a chance to >acquire a
>new unit at a low price now that locally there is (or would seem that >way)
>no support or active promotion.  Does anyone have any experience or >comments
>relating to the IC35 and if there would be any value in interfacing to >the
>HP palm?  The physical size of the unit is certainly more practical than
>many other PDA's but applications seem to be limited...
>
>Till the next time, KEEP SMILING :-)
>
>Nigel R
>
>HP95LX (1Mb + 2Mb PCMCIA card!)
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 19:34:07 +0100
Reply-To:     "Helmuth E. Guenther" <h_e_guenther@ATTGLOBAL.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Helmuth E. Guenther" <h_e_guenther@ATTGLOBAL.NET>
Subject:      Re: using the 200LX to write and get email with a Verizon
              ADSL,connection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Renato

I am using DSL here too.

DSL comes in and is connected to a SMC DSL gateway. On the other side
it is a standard 10/100 LAN.

So the kids and everybody connecting to the internet are using this
gateway. This gateway supports dhcp and fixed addresses.

I connect the hp200lx to the LAN using an Accton 2216-1 network card
and post/lx based on www/lx.

Enjoy it!

Kind regards

Helmuth



> Hi All,
>
> I am considering having Verizon DSL installed in my house because my
> children's use of the Internet with my present dial-up connection is tying
> up the phone line. Before I do this, I want to make sure that I can still
> use my 200LX to access email.
>
> I have stuck with AT&T as my ISP because I can access email with my 200LX
> from just about anywhere. I don't know if I can still do the same if I have
> Verizon DSL installed.
>
> Verizon cannot help me with my question. The tech help sounded as if I was
> talking strange when I told him about the 200LX. I told myself I better
> consult the HPLX List where I wouldn't seem too strange. Thus, my request
> for help.
>
> Thanks in advance for any assistance.
>
> Renato de Vega
> Mililani, HI
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 19:01:57 +0100
Reply-To:     xmarc@free.fr
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Marc BERLIOUX <xmarc@FREE.FR>
Subject:      Re: [OT] need a german translator
In-Reply-To:  <5.1.0.14.2.20020329104055.00a5b840@pop.mail.yahoo.com>
Content-Type: text/plain; charset="iso-8859-1"
MIME-Version: 1.0
Content-Transfer-Encoding: quoted-printable

thanks all
i've got what i needed

--=20
Marc BERLIOUX
"i ever thought german was not a language, just a throat disease..."=20
;o))

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 12:46:26 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: using the 200LX to write and get email with a Verizon ADSL
              connection
In-Reply-To:  <004d01c1d74d$c2352140$17035f0c@default>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Fri, 29 Mar 2002, Renato de Vega wrote:

> I am considering having Verizon DSL installed in my house because my
> children's use of the Internet with my present dial-up connection is tying
> up the phone line. Before I do this, I want to make sure that I can still
> use my 200LX to access email.

Good question!  I was in the same boat with two teenage boys.  For
Christmas I set up a LAN and bought ADSL.  My DSL connection is by
Verizon, but I connect to a local ISP.

In short, it is not only possible, but great!  I bought a LinkSys
4 port "router" (~$80) to connect the LAN to the DSL modem.  On the
200LX I use the Accton Ethernet Drivers (by Yoichiro UENO) from SUPER,
and the LXTCP suite of apps.

With this setup I can run ssh, telnet, pop, nntp, and smtp directly
from my palmtop, but I usually just use lxtelnet to log on to my
Linux box, and then work from there.

If you decide to try something similar, I'd be glad to help answer
questions as best I can.

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 19:48:05 +0100
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: using the 200LX to write and get email with a Verizon
              ADSLconnection
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

You will always be able to plug in a modem where the phones go. It may be
that through the several conversions 56 k modems will not reach the speeds
they do on real analogue lines - the limit tends to be 28.8k - but for a
200 that's hardly relevant.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 13:53:28 -0500
Reply-To:     Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Eduardo Seudsnimo <ohdamnthathurts@YAHOO.COM>
Subject:      Re: using the 200LX to write and get email with a Verizon ADSL
              connection
In-Reply-To:  <004d01c1d74d$c2352140$17035f0c@default>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: quoted-printable

First of all I would not recommend Verizon DSL because the service is =
terrible and overpriced. They also make you use this WinPoet software =
that does something like a dialup instead of just being connected all =
the time. I used to use Verizon and switched to comcast. It was $20 =
cheaper for me, faster, more reliable and easier to use.

If you must use Verizon then I suggest you get a broadband router that =
supports PPoE (PPP over Ethernet). They can be had for about $100 and =
will allow you to connect many computers to the Internet/DSL at the same =
time via a LAN. (You can also do this with Linux (or BSD) and an old =
pentium but it requires a lot of homework if you've never done it =
before.)

As far as the 200LX goes, i think you have two choices:

You can get the Aacton ethernet card and connect it directly to an =
ethernet hub. This is only practical if you have a 4MB or biiger LX as =
you can't have the flash card in at the same time. You also have to use =
a package that supports packet drivers.

You can install MochaPPP on a desktop machine and have the LX access the =
Internet through the serial port. This is the option I prefer as it is =
reasonably fast and let's you d/load stuff right to the flash card.=20


BTW: Nettamer will not work over ethernet and will only work with PPP if =
you trick it into thinking it's a modem on the line. Nettamer is =
hard-wired to work with a modem only. It needs to send modem AT commands =
and see reult codes before it will start the PPP protocol. I've done =
both of the above with www/lx.


> -----Original Message-----
> From: HPLX Mailing List [mailto:HPLX-L@uconnvm.uconn.edu]On Behalf Of
> Renato de Vega
> Sent: Friday, March 29, 2002 1:14 PM
> To: HPLX-L@uconnvm.uconn.edu
> Subject: using the 200LX to write and get email with a Verizon ADSL
> connection
>=20
>=20
> Hi All,
>=20
> I am considering having Verizon DSL installed in my house because my
> children's use of the Internet with my present dial-up connection is =
tying
> up the phone line. Before I do this, I want to make sure that I can =
still
> use my 200LX to access email.
>=20
> I have stuck with AT&T as my ISP because I can access email with my =
200LX
> from just about anywhere. I don't know if I can still do the same=20
> if I have
> Verizon DSL installed.
>=20
> Verizon cannot help me with my question. The tech help sounded as if I =
was
> talking strange when I told him about the 200LX. I told myself I =
better
> consult the HPLX List where I wouldn't seem too strange. Thus, my =
request
> for help.
>=20
> Thanks in advance for any assistance.
>=20
> Renato de Vega
> Mililani, HI
>=20
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>=20

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 19:53:16 +0100
Reply-To:     "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "Oliver W. Leibenguth" <Oliver@COMPUSEUM.DE>
Subject:      Re: Siemens IC35; An HP companion?
In-Reply-To:  <00fb01c1d71b$01e8b000$395cef9b@co.za>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

Hi,

> Does anyone have any experience or comments
> relating to the IC35

To say it in three words: The IC35 sucks!
I've played with one for about an hour and found nothing a HPLX couldn't do
better. Stick with your 95lx and save the money.

regards,
Oliver

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 14:05:54 -0500
Reply-To:     Francois G <matrix@SHOT.ORG>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Francois G <matrix@SHOT.ORG>
Subject:      Re: [OT] Re: registering domain name
In-Reply-To:  <20020329160510.38A8.JBELIN@altern.org>; from Jacques Belin on
              Fri, Mar 29, 2002 at 04:31:26PM +0100
Mime-Version: 1.0
Content-Type: text/plain; charset=us-ascii

On Fri, Mar 29, 2002 at 04:31:26PM +0100, Jacques Belin wrote:
> Le Fri, 29 Mar 2002 10:32:00 +0100
> Marc BERLIOUX <xmarc@FREE.FR> a icrit:
>
> > > what is the best way to register a .com domain name ?
> >
> > try this :
> >
> > http://www.gandi.net

I've been very  fond of stargateinc.com for domain name purchases.  can't
beat the price and have always had good service.

--francois

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 13:33:50 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Re: using the 200LX to write and get email with a Verizon ADSL
              connection
In-Reply-To:  <BMEDJPEHPGEIFEKEBFNOKENOCAAA.ohdamnthathurts@yahoo.com>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Fri, 29 Mar 2002, Eduardo Seudsnimo wrote:

> As far as the 200LX goes, i think you have two choices:
>
> You can get the Aacton ethernet card and connect it directly to an
> ethernet hub...
>
> You can install MochaPPP on a desktop machine and have the LX access
> the Internet through the serial port...

Actually, you can also continue to use a standard modem, as Axel
pointed out.  I can verify that this works, through personal
experience.

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 20:36:57 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: compuserve pricing
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Gary and Larry

On Fri, 29 Mar 2002 17:40:23 +0000, Larry Castor <castorlw@YAHOO.COM> wrote:

> I had the same plan and am trying to go to the per-call arrangement.  Actually, I called to do this and was told it was not possible BUT, I
> could cancel "classic" go to their new service and then cancel there new service and the per-call would be in place. So, I said okay, send me the
> cd and I will do that.  The cd never came!  But last month there was no compuserve charge either and I am still getting email via post/lx.  So,
> I'm waiting till I get this months bill and then I will test to see if I still have access with accis4. And at what cost.

Maybe I should mention that I always only used WWW/LX to access
Compuserve Internet services. I only used their access point (in Spain
and in Canada so far) to get access to POP/SMTP servers, nothing more.
No Compuserve forums or something like that.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 20:36:58 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: using the 200LX to write and get email with a Verizon
              ADSL,connection
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Renato

On Fri, 29 Mar 2002 08:14:28 -1000, Renato de Vega <r.devega@WORLDNET.ATT.NET> wrote:

> I am considering having Verizon DSL installed in my house because my
> children's use of the Internet with my present dial-up connection is tying
> up the phone line. Before I do this, I want to make sure that I can still
> use my 200LX to access email.

You cannot directly connect the 200LX via DSL to an ISP, because there
is no PPPOE (PPP over Ethernet) software available for the 200LX.

However, there are several other ways:

1. If you have an Ethernet card for the palmtop, you can buy a DSL
router, which lets you connect whatever computer you like via Ethernet
to the DSL line. The router does all the PPPOE stuff and to the
machines it looks like an Ethernet connection.

2. (cheaper): You can use your desktop computer as the router. This
means the desktop computer must be running everytime you want to
connect the 200LX to DSL. Then simply connect the palmtop via serial
cable to the desktop.
If you run Windows, MochaPPP does the routing job, and if you run
Linux, PPPD and IP masquerading / forwarding does all you need (see
http://www.daniel-hertrich.de/internet_sharing ).

3. Of course you can still use a modem to connect the 200LX via
analogue phone line to the ISP. I don't know the details of the DSL
service you plan to use, but usually you still have the base band phone
line available for normal phone calls, so you can use a modem, too.
If they convert your analogue phone line into an ISDN line, you would
need a special ISDN-analogue adapter to connect a modem....

GTX
daniel


--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 13:20:40 -0700
Reply-To:     Michael Kopplin <kopplin@TECHNOIR.NU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Kopplin <kopplin@TECHNOIR.NU>
Subject:      Re: using the 200LX to write and get email with a Verizon
              ADSL,connection
In-Reply-To:  <HPLX-L%2002032914353162@UCONNVM.UCONN.EDU>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

> 3. Of course you can still use a modem to connect the 200LX via
> analogue phone line to the ISP. I don't know the details of the DSL
> service you plan to use, but usually you still have the base band phone
> line available for normal phone calls, so you can use a modem, too.

I think this was what the original question was about, actually
being able to access email from anywhere, not just over the DSL
line. Yes, you can use a modem over the same line as DSL, but
the problem with some ISP's is that you no longer have dialup
access if you go with DSL. With my previous ISP, I was allowed
10 hours dialup a month. With some, dialup is available, but at
an added cost.

Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 21:48:40 +0100
Reply-To:     Alexander Schreiber <als@THANGORODRIM.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Alexander Schreiber <als@THANGORODRIM.DE>
Subject:      Re: [OT] need a german translator
In-Reply-To:  <5.1.0.14.2.20020329104055.00a5b840@pop.mail.yahoo.com>
Mime-Version: 1.0
Content-Type: text/plain; charset=iso-8859-1
Content-Transfer-Encoding: 8bit

On Fri, Mar 29, 2002 at 10:41:47AM -0800, A Meshar wrote:
> Google.com Language Tools link yields this:
>
> The circuit
>
> The circuit is developed completely similarly, it comes only standard
> construction units to the employment.  I rejected the structure over
> software, because the circuit should run real time-suited and also outside
> of a computer.  This circuit is however realized of me not practically, but
> only simulated (with the simulator routine electonic workbench 5,0, a mix
> OD mode simulator routine, which is based on a Spice core).  I.e. it is
> probable that the circuit functions, but not surely.  Therefore (still) no
> plate also unfortunately exists.  It is perhaps delivered subsequently.  If
> someone should convert the circuit practically, I would be grateful, if he
> gave the plate draft me (mail to me).  If someone should copy this circuit,
> I point out expressly that I sketched the circuit after best knowledge, her
> however neither tested nor 100% am safe that she enstpricht accurately the
> original Dolby Encodern.  In addition all patent rights must be naturally
> considered by Dolby for the field use of this Encoders.

Wow, this machine translation is rather ... creative in some parts.

> At 3/29/02 +0100, you wrote:
> >I need translation for the following german text.
> >As i know there are plenty of smart and helpful german guys on the
> >list, if one of them has a few minutes...
> >
> >-----------------------------------------------
> >Die Schaltung
> >
> >Die Schaltung ist vollstdndig analog aufgebaut, es kommen nur
> >Standardbauteile zum Einsatz. Den Aufbau |ber Software habe ich
> >verworfen, weil die Schaltung echtzeittauglich und auch au_erhalb
> >eines Computers laufen sollte. Diese Schaltung ist allerdings von mir
> >nicht praktisch realisiert, sondern nur simuliert worden (mit dem
> >Simulationsprogramm electonic workbench 5.0, ein Mixed-Mode
> >Simulationsprogramm, das auf einen Spice-Kern basiert). D.h. es ist
> >wahrscheinlich, da_ die Schaltung funktioniert, aber nicht sicher.
> >Deshalb existiert auch leider (noch) keine Platine. Sie wird
> >vielleicht nachgeliefert. Sollte jemand die Schaltung praktisch
> >umsetzen, wdre ich ihm dankbar, wenn er mir den Platinenentwurf
> >zukommen lie_e (mail an mich).
> >
> >Sollte jemand diese Schaltung nachbauen, weise ich ausdr|cklich
> >darauf hin, da_ ich die Schaltung zwar nach bestem Wissen entworfen
> >habe, sie aber weder testete noch 100% sicher bin, da_ sie exakt den
> >original Dolby-Encodern enstpricht. Au_erdem m|ssen f|r den
> >praktischen Einsatz dieses Encoders nat|rlich alle Schutzrechte von
> >Dolby beachtet werden.
> >-----------------------------------------------

Ok, quick manual translation:

-------------------------------------------------------------

The circuit

The circuit is build completely analog, only standard components are
used. I rejected the design by software because the circuit should be
suitable for realtime and it should work outside of a computer. The
circuit was not built by me, only simulated (using the simulation
software eletronic workbench, a mixed mode simulation software based
on a Spice-core). So, the circuit will probably work, but it's not
guaranteed. Therefore, no printed circuit board exists (so far), it might
be available later. Should anybody actually build this circuit I'd
appreciate getting a copy of the PCB design (mail to me).

Should anybody actually build this circuit, then I insist on having
designed the circuit according to the best of my knowledge but I
neither did I test it nor am I 100% sure that it works exactly like the
original Dolby encoders. Of course you have to respect the intellectual
property of Dolby if you use this encoder.

-------------------------------------------------------------


Regards,
       Alex.
--
We're gonna be body guards for teen rock-stars. Wouldn't the cause of freedom
be better served if we killed them instead?
                        -- Schlock from the ''Schlock Mercenary'' comic strip

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 21:06:57 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: voltage reduction
Comments: To: bobv <bobv@SOS.NET>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

bobv wrote:
> I have an ac adapter with a 24 volt dc output.
> Can I just put in a resistor to drop it down to the 12V needed by the
> 200LX?

If the LX always drew a constant current then it is possible to
just use a resistor (although you might have trouble finding one
of the necessary calculated ohms).

Since the LX does not pull a constant current, any resistor will
drop a varying amount of voltage which means the LX would see
the remaining varying amount of voltage.  If the voltage swings
were too great you could exceed safe levels for the LX.

A good AC adapter is CHEAP insurance.  It isn't worth risking an
EXPENSIVE LX just to save a few dollars on a questionable AC
power supply.

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 22:30:34 +0100
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: Siemens IC35
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> the IC35 [...] has a Z80 heart.

Hey, that sounds interesting - didn't know it. Does anybody know if it is
at all possible to get CP/M running on it?

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 17:33:50 -0500
Reply-To:     Martin Bergvill <hplx@BERGVILL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Martin Bergvill <hplx@BERGVILL.COM>
Subject:      Re: MindMap/LX
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Mon, 25 Mar 2002 22:17:24 +0200, Daniel Hertrich wrote:

> Hi friends,

Hello there

> BTW: Anyone interested in that map (about almost all aspects of
> telecommunication networks, from POTS and ISDN over Ethernet, xDSL, all
> the used protocols, ISO-OSI reference model, Routing, Bridging......)
> let me know - I'll gladly share it with you. It's in German, and the
> final size will probably be around 45-50 kB.

I would like a copy. I remember back in school I had this green book by
Tennembaum I think that described a lot of these things. But the book
is a little bit large to carry with me.:-)

Maybe I start the process of translating your map to english

Please email it to me on hplx@bergvill.com

TIA

Regards



--
Martin Bergvill ,Narvik Norway

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 18:14:46 -0500
Reply-To:     Bob Newins <bnew@ATTBI.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Newins <bnew@ATTBI.COM>
Subject:      Re: compuserve pricing
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Larry or anyone using ACCIS 4.0c on a DS 200LX with compuserve, could
you send me a copy of the compuserve log-on script that works so I can
compare it with mine.  Still no working for me.   Thanks.  =Bob=

> I had the same plan and am trying to go to the per-call arrangement.  Actually, I called to do this and was told it was not possible BUT, I could cancel "classic" go to their new service and then cancel there new service and the per-call would be in
place. So, I said okay, send me the cd and I will do that.  The cd never came!  But last month there was no compuserve charge either and I am still getting email via post/lx.  So, I'm waiting till I get this months bill and then I will test to see if I
still have access with accis4. And at what cost.
>
> Larry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 17:20:30 -0600
Reply-To:     Hal Goldstein <hal_goldstein@THADDEUS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Hal Goldstein <hal_goldstein@THADDEUS.COM>
Subject:      HP 720LXs from Thaddeus
Comments: cc: Wayne Kneeskern <wayne_kneeskern@thaddeus.com>
MIME-Version: 1.0
Content-Type: text/plain

Hi Everyone,

We (Thaddeus Computing) just purchased 150 brand new, sealed in original
packaging, HP Jornada 720s for resale. We got them from a company that is
probably going out of business. I do not believe HP will introduce a
replacement any time soon. MobilePlanet sells the 720 for $899.

We will sell them for $775. We've already pre-sold 30 to one customer, and
we don't expect them to last very long.

If you wish to trade in HP 100LX, 200LX, or 1000CX for the HP 720, email
wayne@thaddeus.com and he will give you an extra $50 credit over what we
would normally pay.

We (end-of-day Friday) are updating the site, but you should still be able
to order even if it reads funny:
http://www.palmtoppaper.com/store/asp/home.asp

Hal from Thaddeus

-----Original Message-----
From: Martin Bergvill [mailto:hplx@BERGVILL.COM]
Sent: Friday, March 29, 2002 4:34 PM
To: HPLX-L@UConnVM.UConn.Edu
Subject: Re: MindMap/LX


On Mon, 25 Mar 2002 22:17:24 +0200, Daniel Hertrich wrote:

> Hi friends,

Hello there

> BTW: Anyone interested in that map (about almost all aspects of
> telecommunication networks, from POTS and ISDN over Ethernet, xDSL,
> all the used protocols, ISO-OSI reference model, Routing,
> Bridging......) let me know - I'll gladly share it with you. It's in
> German, and the final size will probably be around 45-50 kB.

I would like a copy. I remember back in school I had this green book by
Tennembaum I think that described a lot of these things. But the book is a
little bit large to carry with me.:-)

Maybe I start the process of translating your map to english

Please email it to me on hplx@bergvill.com

TIA

Regards



--
Martin Bergvill ,Narvik Norway

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 18:20:04 -0500
Reply-To:     Bob Newins <bnew@ATTBI.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Newins <bnew@ATTBI.COM>
Subject:      Re: using the 200LX to write and get email with a
              VerizonADSL,connection
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Anybody know a source for the Accton 2216-1 network cards?  Thanks.
=Bob=

"Helmuth E. Guenther" wrote:
>
> Renato
>
> I am using DSL here too.
>
> DSL comes in and is connected to a SMC DSL gateway. On the other side
> it is a standard 10/100 LAN.
>
> So the kids and everybody connecting to the internet are using this
> gateway. This gateway supports dhcp and fixed addresses.
>
> I connect the hp200lx to the LAN using an Accton 2216-1 network card
> and post/lx based on www/lx.
>
> Enjoy it!
>
> Kind regards
>
> Helmuth
>
> > Hi All,
> >
> > I am considering having Verizon DSL installed in my house because my
> > children's use of the Internet with my present dial-up connection is tying
> > up the phone line. Before I do this, I want to make sure that I can still
> > use my 200LX to access email.
> >
> > I have stuck with AT&T as my ISP because I can access email with my 200LX
> > from just about anywhere. I don't know if I can still do the same if I have
> > Verizon DSL installed.
> >
> > Verizon cannot help me with my question. The tech help sounded as if I was
> > talking strange when I told him about the 200LX. I told myself I better
> > consult the HPLX List where I wouldn't seem too strange. Thus, my request
> > for help.
> >
> > Thanks in advance for any assistance.
> >
> > Renato de Vega
> > Mililani, HI
> >
> > ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
> >
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Fri, 29 Mar 2002 19:06:12 -0800
Reply-To:     Larry Mittell <lmittel@ATTGLOBAL.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Larry Mittell <lmittel@ATTGLOBAL.NET>
Subject:      Re: using the 200LX to write and get email with a Verizon ADSL
              connection
In-Reply-To:  <BMEDJPEHPGEIFEKEBFNOKENOCAAA.ohdamnthathurts@yahoo.com>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Interesting. I have Verizon DSL and none of those things is true for me.
The service is good, the support isn't terrible, the price is competitive
and I use IE for surfing and Eudora for email on my Windoze machines. No
Verizon-unique software is required. Perhaps they've turned over a new leaf
since you were with them?

Larry Mittell

At 10:53 AM 3/29/02, Eduardo Seudsnimo wrote:
>First of all I would not recommend Verizon DSL because the service is
>terrible and overpriced. They also make you use this WinPoet software that
>does something like a dialup instead of just being connected all the time.
>I used to use Verizon and switched to comcast. It was $20 cheaper for me,
>faster, more reliable and easier to use.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 04:12:45 +0000
Reply-To:     fjkaufman@WORLDNET.ATT.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "F. Kaufman" <fjkaufman@WORLDNET.ATT.NET>
Subject:      Re: dictionary pcmcia and food analyst card hack?
Comments: To: "William T. Hole" <wth@NLM.NIH.GOV>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

> A long time ago, I copied my Personal Food Analyst to my flash card,
> which then still insisted on the original card.  I examined the code with debug
> and changed the explicit references to the drive and directory, which then
> let me put the files where I want except, as I recall, the path
> length in the old
> references couldn't be change and that restricted where I could put the files.
>
> Not for the faint of heart!

And, if I can remember back that far, that is also what I did for Food
analyst and why I had some of those peculiar directory/subdir structures
due to the hard coded paths in the original versions.

If I recall, though, the dictionary has some kind of "execute in place"
which makes it impossible to merely copy the files even tweaking the
innards of the programs to look for files on other than the hardcoded
card.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 08:49:28 +0100
Reply-To:     Yves Leurquin <leurquin@BIGFOOT.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Yves Leurquin <leurquin@BIGFOOT.COM>
Subject:      MindMap/LX Crash
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

Hi,

I am now using MM/LX extensively to take meeting notes on the fly. From =
time
to time I encounter a strange bug which is drawing horizontal dotted =
lines
from the top to the bottom of the screen. It totally crashed the 200LX =
and I
have to resort to CTRL-Shift-On to recover the system (running under SC).

Has anyone seen the same behaviour, is it related to MM/LX or some other =
part
of my setup ?

   \/
   /ves



_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 05:53:22 -0500
Reply-To:     Kevin Ford <200lx@GNOSYS.BIZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Kevin Ford <200lx@GNOSYS.BIZ>
Subject:      TECH: Problems with HP-IRDA and 200LX
Content-Type: text/plain; charset=US-ASCII; format=flowed
Mime-Version: 1.0 (Apple Message framework v481)
Content-Transfer-Encoding: 7bit

Hi All-

I'm running a 200LX that has the 64MB RAM upgrade and the doublespeed
clock upgrade from Times2Tech.  Aside from 200.EXE and associated
applications, the only other programs in memory are an old Buddy TSR
(version 2.1a), ZANSI.SYS, KBUF128.SYS (although I've tried unloading
these in case there are interferences---no luck).  There are also some
drivers associated with the 64MB RAM upgrade and the doublespeed
upgrade.  I've not removed these from memory for hopefully obvious
reasons.  Could the problem be here, though?

With the utility below installed at either COM1 or COM2 as documented
(I've tried both, but the driver complains when I attempt to use it with
COM2), I'm trying to print using the 200LX IR port to an HP LaserJet 6MP
and having no luck in spite of trying many solutions.

I've seen several posts in the archives of this list on doing the same,
but none shed any light (no pun intended) on my dilemma.

What I have tried and the results:

I've tried printing to the same printer using an IrDA laptop and get
success, so I know the printer and its IR port work.

I've tried connecting two 200LX machines together using their IR ports
and get success, so I know that the IR hardware and software on both
200LX's is working.  Both of these 200LX's have the 64MB and the
doublespeed upgrades.  Could the problem be associated with timing and
the communications over the serial ports?  I thought that the
doublespeed driver corrected for this...

Redundant check of the IR port of the 200LX using a standard video
camera indicates light being emitted from the IR port, so I know with
extra certainty that the IR port on the 200LX is working (thanks to
Peter W. Borders on this list for this idea).

Using the JETUTIL.EXE utility included with the software below, I get a
message indicating that the driver is enabled.

Using the 200LX setup utility, I've configured the printer (F3) to use
each of the IR port, the COM1 port, and the COM2 port (I'm guessing that
the JetEye driver would like this setting to be COM1 and for the driver
to be installed at COM1, but that is not clear to me from the driver
docs) for Interface, the HP LaserJet printer driver, and various baud
rates (from 300 up to 19200).

With the above settings in the 200LX setup utility, I tried printing to
the LaserJet 6MP from the MEMO application.  No success, but I can see
light being emitted from the 200LX IR port if I observe with the video
camera.

With the same characteristics in the 200LX setup utility, I've tried
printing to the 6MP from the Lotus123 application and get no success,
although I do see light being emitted.

So, I'm at my wit's end.  Does anyone have this working?  If so, any
thoughts on what I'm doing wrong?

If you by chance have this driver working on your 200LX and haven't a
clue as to what I'm doing wrong, would you mind sending me the details
of your 200LX setup utility (for printing, ie. baud rate, interface,
printer driver), the printer setup characteristics from Lotus123 (by
touching "/PP" and reading the information following the word,
"Interface"), the relevant lines from your CONFIG.SYS and AUTOEXEC.BAT,
and any other details you think might be helpful?  I'll be forever
grateful.

FWIW, I seem to have discovered that immediately after a reboot (with
printer settings in the 200LX setup utility as above), an attempt to
print from MEMO does generate light at the IR port.  However, if I start
FILER, then switch back to MEMO and attempt the exact same print
operation (no other changes to any aspect of the 200LX), the same print
operation generates NO light at the IR port.  If I then switch back to
the FILER and quit the FILER, then try to print, I still get no light
generated at the IR port.  It seems that starting the FILER operates a
toggle switch that only toggles in one direction (to turn the IR light
from enabled to disabled).  I halfway expect this sort of behavior with
Buddy 2.1a loaded (there is a handy feature to turn off the comm ports
with the touch of the + or - keys), but I get the same behavior with or
without Buddy loaded.  Any idea what's going on here?  Does FILER run
the d:\bin\serctl command or something?

Sorry for such a long post, but I figured more detail is better than
less.

TIA for any help.

ksf


IRDA DOS Print Driver (18 KB) added 12/29/1998 (Connectivity)
Version 1.0 by Extended Systems

HP-IRDA is a utility that will allow you to print from DOS programs
(including the built-in Lotus 123) through the palmtop's IR port. It
loads as a device driver and can be run in separate Software Carousel
sessions. Copyright 1994 Extended Systems.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 07:59:00 +0000
Reply-To:     hpstaber@compuserve.com
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Hans Peter Staber <hpstaber@COMPUSERVE.COM>
Subject:      AW: Compuserve & ACCIS 4.0c
MIME-Version: 1.0
Content-Type: text/plain; charset=iso-8859-1
Content-Transfer-Encoding: quoted-printable

Bob,

>A couple of months ago I changed my Compuserve password.  Big mistake.
>Can't seem to log on anymore.  Did something change in the script in the
>last few months?  I have since changed my password many times.  No luck.

You have two login procedures :
a) to the CIS network with your numeric CIS ID as login and a password which were both assigned to you by CIS upon registration. You cannot change these and they are required in acCIS for login.
b) to the POP3 mailbox of CIS if you have opted to switch to NEWMAIL. This is what you may change at your will but you must not use it with acCIS.

I am sure you mixed that.

HP

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 07:58:24 -0800
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: using the 200LX to write and get email with a
              VerizonADSL,connection
Comments: To: Bob Newins <bnew@ATTBI.COM>
In-Reply-To:  <3CA4F6A4.EF17E3A6@attbi.com>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Bob, LanMarket in Irvine CA used to be my source, and they are still on
ACCTON's distributor's list, but their website www.lanmarket.com is not
"occupied" by a domain seller, it appears.

I have an email to a friend who I know has 2 of them, to see id she uses
them. Interested?

Avi



At 3/29/02 -0500, you wrote:
>Anybody know a source for the Accton 2216-1 network cards?  Thanks.
>=Bob=
>
>"Helmuth E. Guenther" wrote:
> >
> > Renato
> >
> > I am using DSL here too.
> >
> > DSL comes in and is connected to a SMC DSL gateway. On the other side
> > it is a standard 10/100 LAN.
> >
> > So the kids and everybody connecting to the internet are using this
> > gateway. This gateway supports dhcp and fixed addresses.
> >
> > I connect the hp200lx to the LAN using an Accton 2216-1 network card
> > and post/lx based on www/lx.
> >
> > Enjoy it!
> >
> > Kind regards
> >
> > Helmuth
> >
> > > Hi All,
> > >
> > > I am considering having Verizon DSL installed in my house because my
> > > children's use of the Internet with my present dial-up connection is
> tying
> > > up the phone line. Before I do this, I want to make sure that I can still
> > > use my 200LX to access email.
> > >
> > > I have stuck with AT&T as my ISP because I can access email with my 200LX
> > > from just about anywhere. I don't know if I can still do the same if
> I have
> > > Verizon DSL installed.
> > >
> > > Verizon cannot help me with my question. The tech help sounded as if
> I was
> > > talking strange when I told him about the 200LX. I told myself I better
> > > consult the HPLX List where I wouldn't seem too strange. Thus, my request
> > > for help.
> > >
> > > Thanks in advance for any assistance.
> > >
> > > Renato de Vega
> > > Mililani, HI
> > >
> > > ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
> > >
> >
> > ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 08:05:42 -0800
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: MindMap/LX Crash
Comments: To: Yves Leurquin <leurquin@BIGFOOT.COM>
In-Reply-To:  <HPLX-L%2002033002484153@UCONNVM.UCONN.EDU>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Yves,

Sorry about the trouble. You think it comes from MM/LX because it is the
last used program? It simply fills the screen with dotted lines? Hmmm...

At 3/30/02 +0100, you wrote:
>Hi,
>
>I am now using MM/LX extensively to take meeting notes on the fly. From time
>to time I encounter a strange bug which is drawing horizontal dotted lines
>from the top to the bottom of the screen. It totally crashed the 200LX and I
>have to resort to CTRL-Shift-On to recover the system (running under SC).
>
>Has anyone seen the same behaviour, is it related to MM/LX or some other part
>of my setup ?
>
>    \/
>    /ves
>
>
>
>_________________________________________________________
>Do You Yahoo!?
>Get your free @yahoo.com address at http://mail.yahoo.com
>
>
>** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 15:21:26 +0100
Reply-To:     Tamas Feher <etomcat@FREEMAIL.HU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tamas Feher <etomcat@FREEMAIL.HU>
Subject:      My 200LX fell and quit working.
MIME-Version: 1.0
Content-type: text/plain; charset=US-ASCII
Content-transfer-encoding: 7BIT

Dear all,

Today my already battered 200LX/2MB suffered a fall from about 5ft
(1.5m). It was in closed position and landed flat on a a stack of 70
sheets of paper on the floor, then came to rest lying upside down.

The battery compartment door and the 2 AA NiCads were ejected,
but the PCMCIA card remained in place. The long slope (wedge),
which is situated between top of keyboard and the screen rod, was
separated from the rod about half of its lenght.

The LX now seems to be dead, the only sign I got was two short
beeps when I plugged in the wall adapter and even this did not
repeat. I managed to put the screen rod into alignment with the
base unit by pressing firmly, but it did not help. I took the machine
apart, but I cannot see anything suspicious.

Maybe the keyboard is damaged (including the ON key) or the
screen is malfunctioning? I did not yet open these, because I
assume the cover plastic sheet may not stick again after a removal.

What would you recommend trying, in order to revive this 200LX?

I have a basic handheld electric multimeter, a 50W soldering
station with digital temperature dial and the set of tooling /
accessories, commonly found in a home.

Thank you in advance, Sincerely: Tamas Feher.

PS: I feel the LX case designers should have opted for a latch
mechanism with two hooks, one in both corners. The single centre
latch does not seem to really hold the two shells together and
allows for deformation / twisting of the whole palmtop.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 11:12:18 -0600
Reply-To:     Hal Goldstein <hal_goldstein@THADDEUS.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Hal Goldstein <hal_goldstein@THADDEUS.COM>
Subject:      Re: Databases for the Database Repository
Comments: To: Daniel Hertrich <daniel.hertrich@GMX.DE>
MIME-Version: 1.0
Content-Type: text/plain

Hi Daniel,

Sorry for not responding. Haven't been reading the list for a while, but it
is sure fun to see old friends and posts. I will try to be more regular.

<<The database repository is stored at www.thaddeus.com and I think Hal is
the right person to contact here. But of course I can put the (also) on
SUPER, if you wish. For that purpose, please post the databases to
super@palmtop.net. I will get a copy (besides the other SUPER team members)
and will put them online with the next SUPER update, which is planned for
this weekend, maybe next week.

Well - Hal, there are lots of databases already on SUPER, AND you have a lot
on www.thaddeus.com. I would suggest that we put all the databases in one
place, avoiding confusion and double entries.

What do you think?>>

You are welcome to swipe any of the databases from our site and put them on
SUPER.

BTW -- in case anyone was concerned, our 200LX repair/upgrade/resell
business continues to be strong. In fact we could easily handle another 2000
HP Palmtops to refurbish and resell -- if anyone has a lead on a large
number of them. We expect to be in the business for a long time.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 12:44:26 -0500
Reply-To:     Ulrich Allen <Ulrich.Allen@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Ulrich Allen <Ulrich.Allen@GMX.DE>
Subject:      Re: GPRS and 6310
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: quoted-printable

I am the one person with the combo problem.
New to me is magic=3D0 and compress=3D0.
But even that didn't help so far.
The third part of the combo is VIAGInterkom as provider.
At present time I don't know the DNS of VI.
That is the last part which differs from Andreas G's setup.
I'll try to get the IP-adress and let you know.
Thank you for caring Avi anyway.
Uli

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 18:59:17 +0100
Reply-To:     "M. L." <lennartz-mi@GMX.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         "M. L." <lennartz-mi@GMX.NET>
Subject:      Re: Siemens IC35
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8Bit

I think, it is impossible.

Mit freundlichem Gru_
Michael Lennartz
www.lennartz-online.net
lennartz-mi@gmx.net
Fax: +49 89 244 34 52 57

>----- Urspr|ngliche Nachricht -----
 (Axel Berger <Axel-Berger@NexGo.De>; Fri, 29 Mar 2002 19:50:59 +0100)
>> the IC35 [...] has a Z80 heart.
>
>Hey, that sounds interesting - didn't know it. Does anybody know if it is
>at all possible to get CP/M running on it?
>
>Axel
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 19:54:33 +0200
Reply-To:     Daniel Hertrich <daniel.hertrich@GMX.DE>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Daniel Hertrich <daniel.hertrich@GMX.DE>
Subject:      Re: MindMap/LX Crash
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Hi Yves

On Sat, 30 Mar 2002 08:49:28 +0100, Yves Leurquin <leurquin@BIGFOOT.COM> wrote:

> I am now using MM/LX extensively to take meeting notes on the fly. From time
> to time I encounter a strange bug which is drawing horizontal dotted lines
> from the top to the bottom of the screen. It totally crashed the 200LX and I
> have to resort to CTRL-Shift-On to recover the system (running under SC).

I think I know what you mean.
Do you speak of pixel lines, filled from left to right and from top to
bottom slowly with obviously random pixels?
I get this behaviour if I press keys too fast or in a non-functional
order (menu - e - o for example, maybe only when I press menu twice or
so... I haven't found the real reason yet).

I'm running MM/LX 2.0 under Software Carousel, with SC swapping to EMS.

GTX
daniel

--
http://www.daniel-hertrich.de/contact

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 15:01:42 -0500
Reply-To:     Jim Westley <jwestley@BELLSOUTH.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jim Westley <jwestley@BELLSOUTH.NET>
Subject:      FS: PCMCIA Card Dock
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

I apologize for the "for sale" message, but I thought someone on this list
may benefit from this item, so I thought I'd give you guys first crack.

I have a Card Dock GS220x/I20 PCMCIA card reader\writer that I got new a
couple of years ago, and I don't need it. In fact, after I got it, I never
used it. It is made by Greystone, and I am not sure if they still exist.

If anyone wants it, I will sell it for $10.00, and that includes shipping
(in the US). Outside the US, what ever the true shipping charges are.

This includes an 16 bit controller card, four 40 pin ribbon cables and a
drive that mounts in a 5 1/4" bay. If your desktop only has PCI slots, then
this won't work.

It has room for 4 full size type II cards, but the literature says that 2
of them are optional, and looking in the bay it looks like only two sockets
are there.

I assume it works, but I have never put it in a computer, so I'm not sure.

First one who asks, gets it.

Jim

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 16:42:06 -0500
Reply-To:     Jim Westley <jwestley@BELLSOUTH.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Jim Westley <jwestley@BELLSOUTH.NET>
Subject:      Re: FS: PCMCIA Card Dock
In-Reply-To:  <4.2.0.58.20020330144718.00999340@mail.clt.bellsouth.net>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Unbelievable! You guys are amazing.

The card dock was claimed 6 minutes after I sent the message.

Jim

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 10:43:10 +1200
Reply-To:     Tony Kan <tony.kan@CLEAR.NET.NZ>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Tony Kan <tony.kan@CLEAR.NET.NZ>
Subject:      OT:  RE: FS: PCMCIA Card Dock
Comments: To: jwestley@BELLSOUTH.NET
MIME-version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding:  7bit

What I find truly amazing is someone with a PC that still has an ISA
slot!!!! <g>
Tony.

> Date: Sun 31-Mar-2002 09:42
> To: HPLX-L@UConnVM.UConn.Edu (Tony Kan)
> From: jwestley@BELLSOUTH.NET (Jim Westley)
> Subject: RE: FS: PCMCIA Card Dock
>
> Unbelievable! You guys are amazing.
>
> The card dock was claimed 6 minutes after I sent the message.
>
> Jim
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml
>
>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 17:17:37 -0600
Reply-To:     Barry <barry@FBTC.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Barry <barry@FBTC.NET>
Subject:      Re: OT:  RE: FS: PCMCIA Card Dock
Comments: To: Tony Kan <tony.kan@CLEAR.NET.NZ>
MIME-Version: 1.0
Content-Type: text/plain; charset="iso-8859-1"
Content-Transfer-Encoding: 7bit

----- Original Message -----
From: "Tony Kan" <tony.kan@CLEAR.NET.NZ>
To: <HPLX-L@UConnVM.UConn.Edu>
Sent: Saturday, March 30, 2002 4:43 PM
Subject: OT: RE: FS: PCMCIA Card Dock


> What I find truly amazing is someone with a PC that still has
an ISA
> slot!!!! <g>
> Tony.

I still have (and occasionally use) an old Compaq 486sx desktop.
Well, not "still".  I bought it about a year ago for $29, I
think.  I wanted something with a 5.25 drive because the one in
my regular computer was getting flaky and I was thinking of
removing it to get the slot.

By the way, I've switched from getting the digest to getting
seperate emails so nothing is the same for me and I'll have to
develop all new habits in the list.  I hope when I make a
mistake you'll all flame me so I'll know.  :)

Barry

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 18:18:51 -0500
Reply-To:     Martin Bergvill <hplx@BERGVILL.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Martin Bergvill <hplx@BERGVILL.COM>
Subject:      Re: Nextel  i85s connectivity?
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

On Thu, 28 Mar 2002 23:29:04 -0800, Marta Pierce wrote:

> Hello HPLX,
>
>   I just purchased a Nextel  i85s phone, and was wondering if anyone
>   had used it w/ the hp200 ?  The manual states that you can use the
>   phone as a modem.  I looked on Daniel's page, and didn't see this
>   particular phone listed anywhere.

Hi

I have never heard of this phone. But does it have irda? If it has you
could get it to work. For email there is only WWW/LX that will work
over irda.

Regards

--
Martin Bergvill ,Narvik Norway

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 17:22:42 -0600
Reply-To:     Theodore Heise <theise@NETINS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Theodore Heise <theise@NETINS.NET>
Subject:      Fluff: OT: FS: PCMCIA Card Dock
In-Reply-To:  <001c01c1d841$294bec80$920d22d1@oemcomputer>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Sat, 30 Mar 2002, Barry wrote:

> > What I find truly amazing is someone with a PC that still has
> an ISA
> > slot!!!! <g>
> > Tony.

I just upgraded from a 286 (with all ISA slots) to a P-100 (with
several of each).


> By the way, I've switched from getting the digest to getting
> seperate emails so nothing is the same for me and I'll have to
> develop all new habits in the list.  I hope when I make a
> mistake you'll all flame me so I'll know.  :)

Oh, don't you worry about *that*!  <grin>

--
Ted Heise      <theise@netins.net>      West Lafayette, IN, USA

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 01:05:47 +0000
Reply-To:     Russel Brooks <rlbrooks@POBOX.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Russel Brooks <rlbrooks@POBOX.COM>
Subject:      Re: OT:  RE: FS: PCMCIA Card Dock
Comments: To: Tony Kan <tony.kan@CLEAR.NET.NZ>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Tony Kan wrote:
> What I find truly amazing is someone with a PC that still has an ISA
> slot!!!! <g>

That's all mine has, along with a 486 and it runs IBM DOS 5.0.
It's a good companian for a 200LX.  :-)

Cheers... Russ

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 20:58:22 -0500
Reply-To:     Bob Newins <bnew@ATTBI.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Newins <bnew@ATTBI.COM>
Subject:      Re: AW: Compuserve & ACCIS 4.0c
Comments: To: h@attbi.com
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

HP,

Thanks for the reply.  You gave me an idea.  I tried just getting email
AND just getting to the Palmtop forum.  Neither worked.  The problem
seems to appear before that.

When trying to log on I can't even get in the door.  Get:"Connecting to
Compuserve Network"
                                                         "Logging onto Compuserve . . .
                                                         "Incorrect User ID or password"
It retries a few time and aborts.  I am only using my original User #
that never changed.  I have called 4 times and tried 4 sets of new
passwords with no luck.  I requested that the passwords work with the
old classic system.  That is why I wanted to see a working script file
as perhaps something is different.  Anybody have any new idea??  Thanks
=Bob=

Hans Peter Staber wrote:
>
> Bob,
>
> >A couple of months ago I changed my Compuserve password.  Big mistake.
> >Can't seem to log on anymore.  Did something change in the script in the
> >last few months?  I have since changed my password many times.  No luck.
>
> You have two login procedures :
> a) to the CIS network with your numeric CIS ID as login and a password which were both assigned to you by CIS upon registration. You cannot change these and they are required in acCIS for login.
> b) to the POP3 mailbox of CIS if you have opted to switch to NEWMAIL. This is what you may change at your will but you must not use it with acCIS.
>
> I am sure you mixed that.
>
> HP
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 22:35:45 -0800
Reply-To:     hplxmail@YAHOO.COM
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         A Meshar <hplxmail@YAHOO.COM>
Subject:      Re: using the 200LX to write and get email with
              aVerizonADSL,connection
Comments: To: Bob Newins <bnew@attbi.com>
In-Reply-To:  <3CA66FDC.36A12123@attbi.com>
Mime-Version: 1.0
Content-Type: text/plain; charset="us-ascii"; format=flowed

Hi Bob,

At 3/30/02 -0500, you wrote:
>Avi,
>
>Hi there!  Yes.  Thanks.
>
>The only other lead I had was gretchen_tai@yahoo.com but the manual was
>in Japanese.|-(

I'll let you know as soon as I hear from her.


_________________________________________________________
Do You Yahoo!?
Get your free @yahoo.com address at http://mail.yahoo.com


** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 00:05:21 -0500
Reply-To:     WEB <geologist@MINDSPRING.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         WEB <geologist@MINDSPRING.COM>
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

I have three 200LX palmtops. The 200LX 1mb SS displays the least
contrast. The 4mb SS and 2mb DS with 64mb installed are equal in
their high contrast display characteristics. HP evidently
changed the display to a higher contrast when they started
manufacturing the 2mb model.

The 1mb model I have was manufacured in 1995, while the 2mb and
4mb models were manufactured 1999 and 1997 respectively.

William

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sat, 30 Mar 2002 22:02:53 -0700
Reply-To:     Michael Kopplin <kopplin@TECHNOIR.NU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Kopplin <kopplin@TECHNOIR.NU>
Subject:      Re: using the 200LX to write and get email with a
              VerizonADSL,connection
In-Reply-To:  <3CA4F6A4.EF17E3A6@attbi.com>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Fri, 29 Mar 2002, Bob Newins wrote:
> Anybody know a source for the Accton 2216-1 network cards?  Thanks.

There is a dutch auction for some of the Socket LP-E cards on
ebay. Looks like the ruggedized model, with the non-removable
cord. They work well in the LX. No experience with the seller.

http://cgi.ebay.com/ws/eBayISAPI.dll?ViewItem&item=2013130191

Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 07:54:13 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Fluff:  FS: PCMCIA Card Dock
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

I keep an "old" tower system around because it has a 5 1/4"
floppy drive and I still have lots of stuff on 5 1/4" floppy
disks that I want to archive on CDs "someday". This system has
both ISA and PCI slots.

Vic Roberts

On Sun, 31 Mar 2002 10:43:10 +1200, Tony Kan <tony.kan@CLEAR.NET.NZ> wrote:

> What I find truly amazing is someone with a PC that still has an ISA
> slot!!!! <g>

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 18:37:06 +0200
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: AW: Compuserve & ACCIS 4.0c
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> Anybody have any new idea??

How do you get the web? I can access my cis classic account using the
standard W98 dialer and the CIS.scp provided. I entered my numeric userid
with comma, the two word all capitals (I assume you checked that for your
passwords) and can get perfect access with a modem - cis makes weird
assumptions for ISDN. If you try that you immediately eliminate all machine
or script dependant problems.

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 00:10:13 -0800
Reply-To:     bobv <bobv@SOS.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         bobv <bobv@SOS.NET>
Subject:      Re: voltage reduction
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Thanks to the many replies on why I couldn't add a resistor to drop the
voltage on an existing ac power adapter.

bob

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 18:52:20 -0500
Reply-To:     Bob Newins <bnew@ATTBI.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Newins <bnew@ATTBI.COM>
Subject:      Re: AW: Compuserve & ACCIS 4.0c
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Axel,

Yes I am using the numeric id with the comma and the all caps Password
from ACCIS 4.0c and the 200lx.  This all was working for yrs. until the
NEW password.|-(   =Bob=

Axel Berger wrote:
>
> > Anybody have any new idea??
>
> How do you get the web? I can access my cis classic account using the
> standard W98 dialer and the CIS.scp provided. I entered my numeric userid
> with comma, the two word all capitals (I assume you checked that for your
> passwords) and can get perfect access with a modem - cis makes weird
> assumptions for ISDN. If you try that you immediately eliminate all machine
> or script dependant problems.
>
> Axel
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 15:53:48 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: AW: Compuserve & ACCIS 4.0c
Comments: To: Bob Newins <bnew@ATTBI.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Bob,

Remind me again what you are trying to do. Are you using Accis
or Datacomm? I don't use Accis and don't use scripts with
Datacomm but still use Tapcis for HMI access and believe I can
long in manually with Datacomm. (I can probably get you the
Tapcis login script.) You do remember that the login must be
done with 7-bit odd parity I believe. Have you tried your new
password with CIS software or with any Web browser at
www.compuserve.com? If you have never logged in with your new
password it is possible that you mistyped it when you changed
it or the Caps Lock key was on.

Vic Roberts

On Sat, 30 Mar 2002 20:58:22 -0500, Bob Newins <bnew@ATTBI.COM> wrote:

> When trying to log on I can't even get in the door.  Get:"Connecting to
> Compuserve Network"
>                                                          "Logging onto Compuserve . . .
>                                                          "Incorrect User ID or password"
> It retries a few time and aborts.  I am only using my original User #
> that never changed.  I have called 4 times and tried 4 sets of new
> passwords with no luck.  I requested that the passwords work with the
> old classic system.  That is why I wanted to see a working script file
> as perhaps something is different.  Anybody have any new idea??  Thanks

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 19:05:59 -0500
Reply-To:     Bob Newins <bnew@ATTBI.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Newins <bnew@ATTBI.COM>
Subject:      Re: AW: Re: AW: Compuserve & ACCIS 4.0c
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

HP,

When you call CSI all they will do is provide you will another new
password.  I have done this 4 times with 4 different NEW passwords to no
avail.  They can't seem to tell you what your current password is, they
don't have access to thet information.  If anyone knows a way of getting
your current password out of them I would like to know how!

That was the original problem.  I had to restore the 800CT HD where my
backups for the 200LX were stored and couldn't remember the 1991
Compuserve password to restore the CSI 3.0 software on the 800CT.  It is
encrypted on the 200LX in ACCIS so I couldn't see it there.  I had them
change it for the 800CT and now I can't get either one working. |-(
=Bob=

hpstaber@compuserve.com wrote:
>
> >It retries a few time and aborts.  I am only using my original User #
> >that never changed.  I have called 4 times and tried 4 sets of new
> >passwords with no luck.  I requested that the passwords work with the
> >old classic system.  That is why I wanted to see a working script file
> >as perhaps something is different.  Anybody have any new idea??  Thanks
>
> For acCIS login you need to specify
>  Login : 123456,789
>  and
>  PWD : the one you were given when you signed up.
>
> There is only ONE password, not several. If you are not sure call CSI and ask them to provide you your RPN password again. YOU cannot change it.

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Mon, 1 Apr 2002 02:10:30 +0200
Reply-To:     Axel-Berger@NexGo.De
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Axel Berger <Axel-Berger@NEXGO.DE>
Subject:      Re: AW: Compuserve & ACCIS 4.0c
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

> This all was working for yrs. until the NEW password.|-(   =Bob=

That was the point of my suggestion. If you use the the windows dialer,
just for once doing it their way, and it still doesn't work, the helpline
might understand your questions. Another thing that should work is
datacomm:
use compuserve.dcf from ROM and the provided script. It not not in ROM as I
misremebered so I think I typed it from the handbook. That combo gets you
logged on and lets you read "we only worship Bill Gates" or some such.
The thing to do is separate the account from the software and test each
separately.

Axel

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 19:18:25 -0500
Reply-To:     Bob Newins <bnew@ATTBI.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Newins <bnew@ATTBI.COM>
Subject:      Re: using the 200LX to write and get email with
              aVerizonADSL,connection
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Mike,

So, I take it that (Socket LP-E) means low power - ethernet from the
company Socket?(G)

How does that compare with the Accton 2216-1?  More power/less
power/about the same??

Is there any magic to get it going?  Drivers, files, etc.?  Which ones
and where do do put them on the LX?

BYW, thanks for the reference to them!     =Bob=

Michael Kopplin wrote:
>
> On Fri, 29 Mar 2002, Bob Newins wrote:
> > Anybody know a source for the Accton 2216-1 network cards?  Thanks.
>
> There is a dutch auction for some of the Socket LP-E cards on
> ebay. Looks like the ruggedized model, with the non-removable
> cord. They work well in the LX. No experience with the seller.
>
> http://cgi.ebay.com/ws/eBayISAPI.dll?ViewItem&item=2013130191
>
> Mike
>
> ** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 17:04:48 -0800
Reply-To:     Victor Roberts <RobertsV@EARTHLINK.NET>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Victor Roberts <RobertsV@EARTHLINK.NET>
Subject:      Re: AW: Re: AW: Compuserve & ACCIS 4.0c
Comments: To: Bob Newins <bnew@ATTBI.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

What am I missing here? If they give you a new password, can't
you just enter that in Accis and be back on line? Also, you
could reinstall the CIS software on your 800CT and provide it
with the same new password. There must be more to this that I
am not seeing.

Vic

On Sun, 31 Mar 2002 19:05:59 -0500, Bob Newins <bnew@ATTBI.COM> wrote:

> HP,
>
> When you call CSI all they will do is provide you will another new
> password.  I have done this 4 times with 4 different NEW passwords to no
> avail.  They can't seem to tell you what your current password is, they
> don't have access to thet information.  If anyone knows a way of getting
> your current password out of them I would like to know how!

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 20:13:28 -0500
Reply-To:     Bob Newins <bnew@ATTBI.COM>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Bob Newins <bnew@ATTBI.COM>
Subject:      Re: AW: Compuserve & ACCIS 4.0c
MIME-Version: 1.0
Content-Type: text/plain; charset=us-ascii
Content-Transfer-Encoding: 7bit

Vic,

I am trying to get Accis working again.  Played with Datacomm briefly
the other day but couldn't remember the bit/parity thing.  Good idea,
will try with browser at compuserve .com.
Larry Castor sent me his log-on scripts, so when I have more time I will
dig into it.  Thanks everyone for the help.   =Bob=
Victor Roberts wrote:
>
> Bob,
>
> Remind me again what you are trying to do. Are you using Accis
> or Datacomm? I don't use Accis and don't use scripts with
> Datacomm but still use Tapcis for HMI access and believe I can
> long in manually with Datacomm. (I can probably get you the
> Tapcis login script.) You do remember that the login must be
> done with 7-bit odd parity I believe. Have you tried your new
> password with CIS software or with any Web browser at
> www.compuserve.com? If you have never logged in with your new
> password it is possible that you mistyped it when you changed
> it or the Caps Lock key was on.
>
> Vic Roberts
>
> On Sat, 30 Mar 2002 20:58:22 -0500, Bob Newins <bnew@ATTBI.COM> wrote:
>
> > When trying to log on I can't even get in the door.  Get:"Connecting to
> > Compuserve Network"
> >                                                          "Logging onto Compuserve . . .
> >                                                          "Incorrect User ID or password"
> > It retries a few time and aborts.  I am only using my original User #
> > that never changed.  I have called 4 times and tried 4 sets of new
> > passwords with no luck.  I requested that the passwords work with the
> > old classic system.  That is why I wanted to see a working script file
> > as perhaps something is different.  Anybody have any new idea??  Thanks

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 20:25:13 -0500
Reply-To:     stan.hplx@VERIZON.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Stanley Dobrowski <stan.hplx@VERIZON.NET>
Subject:      Re: Is 2X worth it?  Maybe, Maybe Not.
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

> The best authority
> would be someone who has had a known machine upgraded who could comment
> on whether or not the contrast was affected

I have personally upgraded (meaning I have soldered in the
crystal myself) several 100LX and 200LX palmtops for myself and
others and have never noticed a difference in the screen
contrast before and after the surgery.


Stan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 20:59:06 -0500
Reply-To:     stan.hplx@VERIZON.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Stanley Dobrowski <stan.hplx@VERIZON.NET>
Subject:      Re: voltage reduction
Comments: To: bobv <bobv@SOS.NET>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

> Can I just put in a resistor to drop it down to the 12V needed by the
> 200LX?

NO!!!!!!!!!

The current draw the the 200Lx varies from 10 ma to over 200ma.
  There is no way you could put in a resister to drop the 24
 volts with such a variying current load.

Don't risk damaging your 200LX just to save $10 on an AC
adapter.


Stan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 20:59:08 -0500
Reply-To:     stan.hplx@VERIZON.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Stanley Dobrowski <stan.hplx@VERIZON.NET>
Subject:      Re: AW: charging system
Comments: To: Michel Bel <michel.bel@ZONNET.NL>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Michel wrote:

> The Specs clearly say ( Page B-6 in the User's Guide):
>   Minimum voltage +9.6 V
>   Nominal Voltage +12V
>   Maximum Voltage +14.4 V
> I have used a 10.5 V, 1A miniature switched  supply for over a year now,
> without problems

I understand.  But you were talking about fooling around with a
regulated variable output power supply and using 10.5 volts and
having some troubles.  I was trying to suggest that you use the
nominal spec.

I also understand that a 10.5 volt supply would most likely
work fine.  But at the lower voltage (than the nominal 12
volts), the power supply conversion circuits inside the palmtop
have to draw more current at that lower voltage and could
therefore run hotter.

Also, HP's own AC power adapter puts out 12 volts, so I read
that as an indication that 12 volts is the best to give to the
100/200LX.  I have been using HP's regulated 12 volt adapters
for many years - since my first 100LX one month after they were
introduced - and have never had a problem.


Stan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 20:59:11 -0500
Reply-To:     stan.hplx@VERIZON.NET
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Stanley Dobrowski <stan.hplx@VERIZON.NET>
Subject:      Re: Compuserve & ACCIS 4.0c
Comments: To: Bob Newins <bnew@ATTBI.COM>
MIME-Version: 1.0
Content-Type: text/plain; charset=ISO-8859-1
Content-Transfer-Encoding: 8bit

Bob Newins wrote:

> Can't seem to log on anymore.  Did something change in the script in the
> last few months?

No, CompuServe did not change anything here in the USA as far
as scripts go.  I'd bet money that the trouble is not the
script.

> ACCIS starts, dials, connects.  "Logging onto compuserve".  Then I keep
> getting "Incorrect User ID or Password" error message.  I have even
> entered the password manually into the ACCIS configuration file

The password is encoded in the ACCIS.CFG file - you can't edit
the file manually to change the password.  You need to use
AcCIS's ACCSETUP program to change you password.  Use the F2
(User) button to change the password.  And then use the F5
(Phone) button to go into the phone entries and change the
password for each of your dialup entries.


Stan

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

=========================================================================
Date:         Sun, 31 Mar 2002 19:25:57 -0700
Reply-To:     Michael Kopplin <kopplin@TECHNOIR.NU>
Sender:       HPLX Mailing List <HPLX-L@UCONNVM.UCONN.EDU>
From:         Michael Kopplin <kopplin@TECHNOIR.NU>
Subject:      Re: using the 200LX to write and get email with
              aVerizonADSL,connection
In-Reply-To:  <3CA7A751.92673EBA@attbi.com>
MIME-Version: 1.0
Content-Type: TEXT/PLAIN; charset=US-ASCII

On Sun, 31 Mar 2002, Bob Newins wrote:
> Mike,
>
> So, I take it that (Socket LP-E) means low power - ethernet from the
> company Socket?(G)

Yes, Socket Communications, see www.socketcom.com, although the
cards being sold on ebay are not a current model so you won't
find any information there.

> How does that compare with the Accton 2216-1?  More power/less
> power/about the same??

I don't have the specs available at the moment, but I seem to
recall the socket cards run about 65ma active, and the accton
cards a bit more. The new socket models draw 19ma, which would
be nice, but there not $20.

> Is there any magic to get it going?  Drivers, files, etc.?  Which ones
> and where do do put them on the LX?

All you need is lxcic and lxen2216, same with an accton card,
see super and lxeth.hplx.net. I put them both in a directory on
my command path. that way I can use them from both my lxtcp
setup and www/lx. If they're not on your path you could always
invoke them with full path.

No real magic. If you can configure lxtcp, or www/lx, you
shouldn't have a problem using either card.

> BYW, thanks for the reference to them!     =Bob=

You're welcome. If you get a card, let me know if you have
troubles and I'll see if I can help.

By the way, the socket cards also work in the early omnibooks,
while the accton cards don't.

Mike

** HPLX-L LIST Info at http://www.sp.uconn.edu/~mchem1/HPLX.shtml

