# MS-DOS Troubleshooting

- Make sure you’re using the correct and most recent drivers for this adapter.

- If you’re replacing an existing adapter, make sure the LINK statement in your NET.CFG is correct for the new adapter.

- Verify that the frame type in your NET.CFG file matches your network.

- Test the adapter by running the Diag100.EXE diagnostics program. Additional testing is
  available by using a responder.

- Check the online User's Guide for DOS client instructions.

`Last modified on 7/23/02 10:21a Revision 2`