# PCI Hot Plug Support for Sunsoft Solaris* 7 and 8

Intel® PRO/1000 network adapters are enabled for use in selected servers equipped with PCI Hot Plug support and running Sunsoft Solaris* 7 and 8.

| NOTE: If you replace an adapter in a Hot Plug slot, do not place the removed adapter back into the same network until the server has rebooted. The two adapters may have the same virtual MAC address and create a conflict.
| NOTE: Hot Plug only works between identical Intel network adapters.

Software Requirements:

- Solaris 7 11/99 or later operating system

Hardware Requirements:

- Processor that supports Hot Plug

`Last modified on 11/07/02 10:16a Revision 5`