# System Requirements

Before installing the network adapter, check your system for the following minimum configuration requirements for Intel® PRO/1000 adapters.

## Hardware Compatibility - Gigabit Adapters

- One of the following slot types, depending on your adapter:

  - One open PCI bus master slot, 32-bit or 64-bit, operating at 33 or 66 MHz

  - One open PCI-X slot operating at 66, 100 or 133 MHz (recommended)

  - The PRO/1000 MT Quad Port Server adapter requires a 3.3 volt slot. It cannot be installed in a 5.0 volt slot.

- 64 MB of system memory

- The latest BIOS for your computer

`Last modified on 6/16/04 1:15p Revision 3`